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Company vehicles shall be checked at the beginning of each hitch to assure that all parts,
equipment and accessories are free of damage and in safe operating condition. A copy of
the Vehicle Safety Checkiist (below) should be in all vehicles. Reportall defects to the
responsible department manager or the individual responsible for the vehicle. Correct all
defects before the vehicle is placed in service.

X

ime Helicopters

Vehicle Maintenance Safety Checklist
DAILY GHEGKLIST
A Outside the Vehicle Yos Mo
1. Tires are not low r at; tread s not o away
2. Windshieid wipers work;suffcent leaning fid n reservor
3.Noleaks under ne vencie
4. Minors, directicnal Sgnals, head,tail, and brake ights are clean and ne brcken.

B. Incido the Vahicls Yos Mo
1. All doors are fully ciosed and locked.
2. Seatand head restraint comfortably adjusted,
3. Driver and passengers correctly beted
. Mlimors, vents, indows and heatiair property adjustod
5. Gauges work and accurately refiect engine conditons.
6. Drveris mentally and physially ready to drive.

WEEKLY CHECKLIST (First day of each hitch) Yos Mo

1.0l Lovel ~ Check the ol before stating the vehicie (whils the engine s cool):
Pullout the dipstik, wipe & of and reinsert. Pullt ut again o check the ol evel. A s376 GTIRveT
indication s betneenthe tpper and lower level marks. I the feveis belon the lower merk,actia
quart of of it the o reservoi and check your owner's manual.

2 Chesk coolant level.
3. Washer Fluid Lovel - Check the lavel of fluid n the holder. A good habitto

developisto il the fuid reservor when i s halfful

4. Tires — Check et e e re ol i Crescnesresmery. |||

i you i the gas tank,

5. \Windhieid Wper Blades (Replace blades ifhard, cracked, or bite).
. Checktires (Chack awner's manual for tre rtation Insiructions).
7. Power Stesring fui levels (Add i according to owner's manual directions).
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