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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0550.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 206L MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 206L MP
	

	
	
	

	C 0550.2 AAI LIGHTWEIGHT EMERGENCY FLOATS – ICA407-11

	
	
	

	2.1 Visually inspect LH and RH float assemblies for damaged areas. Any break or hole in the coated fabric covers must be suspect of internal damage and should be investigated.
	
	

	2.2 Visually inspect all exposed hoses for cuts or kinks.
	
	

	
	
	

	2.3 Check cylinder for security and condition. Check the pressure gauge mounted on the cylinder valve. The gauge shall read 4185 psi ±50 psi @ 70º F (see Table 3 for pressure v temperature differentials). Recharge cylinder if pressure is below minimum allowable.
	
	

	
	
	

	2.4 Unsnap float covers. Inspect the covers for any cuts or tears. If the cover is damaged in any way, remove and replace it.
	
	

	
	
	

	2.5 Conduct Float Leak Test and inspect for chafing or damaged areas.
	
	

	
	
	

	2.6 Inflate all chambers of the assembly using shop air to 2.0 psi. (Inflate in 0.5 psi increments.) Measure pressure in each compartment with mercury manometer or pressure gauge (calibrated in increments not greater than 0.10 psi) connected to topping valve.
	
	

	
	
	

	2.7 Allow the float to remain undisturbed for 8 hours. The maximum allowable pressure drop is 0.50 psi (or allow float to stand for 24 hours and the maximum allowable pressure drop is 1.0 psi) after correction for temperature and barometric variations
	
	

	
	
	

	2.8 Record the compartment pressures, the temperature and barometric reading at the end of the pressure test. Correct for temperature variations by subtracting 0.10 psi for every 3°F rise in temperature, or adding 0.10 psi for every 3°F drop.
	
	

	
	
	

	2.9 Correct for barometric conditions by adding 0.10 psi to the final gauge reading for every 0.20 inches of mercury that the barometric pressure had increased, or subtract 0.10 psi from final reading for every 0.20 inches of mercury that the barometer has fallen.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	2.10 Conduct Pressure Relief /Topping Valve Leakage Test. This valve may be checked as part of the float pressure test while it is inflated to 2.0 psi.
	
	

	
	
	

	2.11 Conduct Pressure Relief /Topping Valve Leakage Test. This valve may be checked as part of the float pressure test while it is inflated to 2.0 psi.
	
	

	
	
	

	2.12 If leakage is due to valve not seating properly, remove and replace.
	
	

	
	
	

	2.13 Fill the relief valve aperture with clean water. Slowly raise the compartment pressure and watch for bubbles indicating that the valve opens. Then reduce pressure watching for the elimination of bubbles. The valve should open at 4.0 psi ±0.25 psi and should close by 3.0 psi.
	
	

	
	
	

	2.14 If valve operates improperly, apply leak solution in aperture of valve. If bubbles indicate a leak at this location, remove valve from base flange and check threads in flange base and on valve. If threads in flange are damaged, return float to factory for repair/replacement. If valve threads are damaged, replace as specified.
	
	

	
	
	

	2.15 Conduct Inlet Check Valve Test. This valve may be checked as part of the float pressure test while it is inflated to 2.0 psi.
	
	

	
	
	

	2.16 Apply leak solution with soft nylon bristle brush at mounting patch to float location. If bubbles indicate a leak, return to factory.
	
	

	
	
	

	2.17 Apply leak solution with a soft nylon bristle brush to valve body. If bubbles indicate a leak, return to factory.
	
	

	
	
	

	2.18 Deflate Float Bags and repack (see 7.0 Float Bag Packing Section)
	
	

	
	
	

	C 0550.3 POST INSPECTION

	
	
	

	3.1 Inspect for operation and leaks.
	
	

	
	
	

	3.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	3.3 Perform Functional Check Flight if required per Rotorcraft Flight Manual and/or Manufacturer ICA.
	BHT-206L-FM-1
	

	
	
	

	3.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 206L Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 206L Series AAIP – C 0550 – 500 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


