Items to add to the 407 AAIP
Inspection				reference			interval 
Paravion blade fold kit inspection	PR-407BF-120M		300hr  Done
Barrier filter inspection (check)	(check)				100hr - Done
AAI Locking fuel Cap		AA

Items to remove from the 407 AAIP
Inspection				reference			interval 
Barrier filter inspection		(check)				300hr cleaning
Servo 12 and 24 month inspections (if a servo is removed or replaced) – Removed, tracked by component.
A-2500. This inspection is tracked under the component – Remove, tracked by component.
A-6010. This inspection is tracked under the component – Remove, tracked by component.
A-6020. This inspection is tracked under the component. – Remove, tracked by component.
A-6030. This inspection is tracked under the component – Remove, tracked by component.
[bookmark: _GoBack]A-6040. This inspection is tracked under the component – Remove, tracked by component.



