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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 407 MM-1

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1700.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 1700.2 GENERAL

	
	
	

	2.1 Ensure that one complete cycle (A0051 – A0056) of the AAIP inspections have been completed in the last 12 calendar month period.
	
	

	
	
	

	2.2 Inspect all fuel system, oil system, and hydraulic system filler caps for proper functioning and sealing. Make sure the sealing o-rings within the filler caps are in good condition. Repair or replace the filler caps or replace the sealing o-rings as required.
	
	

	
	
	

	2.3 Perform a dynamic balance of the main rotor hub and blade assembly.
	Chapter 18
	

	
	
	

	2.4 Remove interior trim and access panels necessary to gain access. Examine the areas following (starting with item A 1700.3):
	Chapters 25 & 53
	

	
	
	

	A 1700.3 FORWARD FUSELAGE 

	
	
	

	3.1 Examine the controls for condition, security and correct operation. Examine them in the locations that follow:
	Chapter 67

	

	
	
	

	3.1.1 Pedestal. 
	
	

	
	
	



	MARITIME HELICOPTERS
	Bell 407 AAIP

	
	

	Page No:
	1

	Revision:
	6

	Issue Date:
	11/30/19

	SECTION:
	
	A 1700 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	12 MONTH INSPECTION

	NOTE:
	
	




	

	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	3.1.2 Crew seats.
	
	

	
	
	

	3.1.3 Tunnel.
	
	

	
	
	

	3.1.4 Roof beam.
	
	

	
	
	

	3.1.5 Hat bin.
	
	

	
	
	

	3.2 Examine the components of the airspeed-actuated pedal stop for condition, security and correct operation. Examine the following components:
	Chapter 67
	

	
	
	

	3.2.1 Solenoid.
	
	

	
	
	

	3.2.2 Cam.
	
	

	
	
	

	3.2.3 Release cable.
	
	

	
	
	

	3.3 Operate the airspeed-actuated pedal stop manual cable release mechanism for the cam. Examine for correct operation and free movement of cable. Safety the cable release handle with lockwire (C-554). 
	
	

	
	
	

	3.4 Perform pedal restrictor control system functional test.
	Chapter 96
	

	
	
	

	3.5 Examine all fluid flexible and rigid lines for condition, leaks, and security. Examine them in the locations that follow:
	Chapter 67
	

	
	
	

	3.5.1 Vertical tunnel.
	
	

	
	
	

	3.5.2 The roof beam.
	
	

	
	
	

	3.5.3 Hat bin.
	
	

	
	
	

	3.6 Examine the throttle control cable for condition and security. Examine it in the locations that follow:
	Chapter 76
	

	
	
	

	3.6.1 Crew seats.
	
	

	
	
	

	3.6.2 Vertical tunnel.
	
	

	
	
	

	3.6.3 Roof beam.
	
	

	
	
	

	3.7 Replace the 1.5 volt dry cell battery located at the back of the instrument panel digital clock (S/N 53000 through 54299). NOTE: N/A if Clock is Hardwired.
	Chapter 95
	

	CAUTION
ANY CRACK, CORROSION, OR LOOSE OR SHEARED RIVET IS CAUSE FOR IMMEDIATE GROUNDING OF THE HELICOPTER UNTIL THE PROBLEM IS CORRECTED.
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	MECHANIC’S
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	3.8 Examine the structure for condition in the locations that follow:
	Chapter 53
	

	
	
	

	3.8.1 Pedestal.
	
	

	
	
	

	3.8.2 Crew seats.
	
	

	
	
	

	3.8.3 Bulkhead at fuselage station 81.08.
	
	

	
	
	

	3.8.4 Vertical tunnel.
	
	

	
	
	

	3.8.5 Roof beam.
	
	

	
	
	

	3.8.6 Hat bin.
	
	

	
	
	

	3.8.7 Bulkhead at fuselage station 142.715.
	
	

	
	
	

	3.9 Examine the electrical harness for condition and security in the locations that follow:
	Chapter 96
	

	
	
	

	3.9.1 Pedestal.
	
	

	
	
	

	3.9.2 Crew seats.
	
	

	
	
	

	3.9.3 Vertical tunnel. 
	
	

	
	
	

	3.10 Examine the internal structure of forward and side engine mount attachment points for condition and security. 
	Chapter 53
	

	
	
	

	3.11 Examine the internal structure of frame at fuselage station 199.039 (WL 72.602) for condition and security.
	
	

	
	
	

	A 1700.4 FUEL SYSTEM

	
	
	

	4.1 Do a fuel low annunciator circuit operational check.
	Chapter 96
	

	
	
	

	4.2 Examine the operation of the check valves for the forward fuel cell transfer pumps. Turn on each transfer/boost pump assembly individually and visually confirm flow of fuel from outlet of fuel transfer line in aft fuel cell. Fuel system may have to be defueled until fuel level is below transfer line outlet. 
	Chapter 28
	

	
	
	

	4.3 Examine the fuel system shutoff valve and components for condition, leaks, and security.
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	MECHANIC’S
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	REFERENCE
	

	
	
	

	A 1700.5 TAILBOOM

	
	
	

	5.1 Examine the following for condition and security:
	
	

	
	
	

	5.1.1 Ballast.
	Chapter 8
	

	
	
	

	5.1.2 Controls.
	Chapter 67
	

	
	
	

	5.1.3 Horizontal stabilizer including slats and auxiliary finlets. 
	Chapter 53
	

	
	
	

	5.1.4 Vertical fin including tail stinger and weight.
	
	

	
	
	

	5.1.5 Electrical harness.
	Chapter 96
	

	
	
	

	A 1700.6 ENGINE

	
	
	

	6.1 Do a MGT indicator functional check in Normal Mode and Start Mode (S/N 53000 through 54299).
	Chapter 95
	

	
	
	

	A 1700.7 TRANSMISSION

	
	
	

	7.1.1 Perform inspection of the transmission corner mounts using work aid 407-240-013-101.
	Chapter 63-53
	

	
	
	

	A 1700.8 POST INSPECTION

	
	
	

	8.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-407-FM-1/2
	

	
	
	

	8.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	8.3 Perform Functional Check Flight if required per Bell 407 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	8.4 Download, then clear all the past faults from FADEC.
	
	

	
	
	

	8.5 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – A 1700 – 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




