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	SECTION:
	
	A 0130 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	25 HOUR INSPECTION

	
	
	



	Registration No.:
	N
	Start:
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  AEC AS 350 BA Maintenance Program 05.20.02.105
	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A0130.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies.  Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	AS 350BA Maintenance Program 5.99
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	AS 350BA Maintenance Program 5.10
	

	
	
	

	1.5 Inspect the areas of the aircraft open for this inspection for signs of corrosion.  If corrosion is evident, or if aircraft has been operating in a known corrosive environment, conduct a searching inspection for corrosion.
	Advisory 
Circular 
AC 43-4A
	

	A0130.2 MAIN ROTOR BLADE 62-10

	
	
	

	2.1 MAIN ROTOR BLADE – Cleaning the blades.
	MET 62.10.00.302
	

	Effectivity: Tropical and damp atmosphere.
	

	2.2 MAIN ROTOR BLADE. – Cleaning the blades.
	MET 62.10.00.302
	

	Effectivity: Salt-laden atmosphere.
NOTE:   After hovering or low-altitude flight, this operation should be carried out during the ALF check.
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A0130.3 TAIL ROTOR 64-10

	3.1 TAIL ROTOR BLADE – Check for erosion and perform cleaning.
	MET 64.10.00.601
	

	Effectivity: Tropical, damp, salt and dust-laden atmosphere
	

	A0520.16 POST INSPECTION

	
	
	

	16.1 Inspect for operation and leaks.
	
	

	
	
	

	16.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	16.1 Perform Functional Check Flight if required per AMC General Maintenance Manual, AS350 MM, or RFM as appropriate.
	
	

	
	
	

	16.1 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Air Methods’ Model AS 350 BA Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made the entry below in the Aircraft Log Book or a similarly worded statement:

I certify that this aircraft has been inspected in accordance with Air Methods’ AS 350 BA AAIP – 25 Hour Airframe Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End:
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	Certificate Type & No:
	


