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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  AW119MKII Maintenance Planning Manual Chapter 05-40

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0050.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	A 0050.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chp 11
	

	
	
	

	[image: ]




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0050.3 AREA 1 - HELICOPTER NOSE

	
	
	

	3.1 Battery and relative mount attachments for condition and security.
	
	

	
	
	

	3.2 Vent lines for condition and obstruction.
	
	

	
	
	

	3.3 Nose compartment electrical/avionic components, relative mounts and floor attachment area for condition, cracks and security.
	
	

	
	
	

	3.4 Ventilation air intake screen and ducts for condition.
	
	

	
	
	

	A 0050.4 AREA 2 - FUSELAGE – RH SIDE

	
	
	

	4.1 SAS pitch and roll actuators for unusual play, condition and security; electrical connections for condition and security.
	
	

	
	
	

	4.2 Fuel system drain lines and valves for leaks.
	
	

	
	
	

	4.3 Landing skid for damage, condition and forward and rear saddles connecting skid to crossbeams for sealing integrity.
	
	

	
	
	

	4.4 Landing skid damper for condition and leaks. Support for condition.
	
	

	
	
	

	4.5 Rear crosstube and central support for condition and security (visible parts).
	
	

	
	
	

	4.6 Forward crosstube and fuselage attaching clamps for condition and security.
	
	

	
	
	

	4.7 Main rotor grips (2 places) for condition.
	
	

	
	
	

	4.8 Main rotor elastomeric bearings for separation or loss of bearing elements, eventual blowing and/or rubber extruding and absence of oil or grease.
	
	

	NOTE: If contaminated, refer to Para 62-21-50 for cleaning
	
	

	4.9 Check interrupter and magnetic pick-up for condition and security (provision for main rotor balance and track).
	
	

	
	
	

	4.10 Main rotor dampers (2 places) for condition, security, unusual play of bearings and correct fluid level.
	
	

	
	
	

	4.11 Ground jumpers between pitch control lever (inside grip) and damper and between damper and attachment bracket to hub for condition.
	
	

	
	
	

	4.12 Main rotor pitch change links for condition, security, corrosion and fretting of the spherical bearings, loss of part of the liner and unusual play (check axial play by moving the pitch link by hand and the radial play by rotating the blade along its pitch axis and by acting from the tip cap area).
	
	

	
	
	

	4.13 Inspect swashplate upper and lower boots for condition, integrity and absence of grease on external surfaces. Lubricate main swashplate (2 places).
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.14 Main rotor hub and blades (2 places) for condition, damage and cleanliness.
	
	

	
	
	

	4.15 Main rotor damper fittings (2 places) for condition, unusual play and cracks in the area of the attachment point to the hub.
	
	

	
	
	

	4.16 Main transmission and accessories for condition, security and leaks of lubricant.
	
	

	
	
	

	4.17 Engine to transmission drive shaft (visible part) for condition and security of attaching hardware. Check bolts attaching shaft flange to the engine and to the main transmission for integrity of slippage marks.
	
	

	
	
	

	4.18 Visible parts of flight controls, levers and supports for condition and security.
	
	

	
	
	

	4.19 Main rotor servo actuator (1 place) for condition, security and leaks. Inspect bleed hole for leaks, lower spherical bearing for looseness and upper bearing for abnormal play.
	
	

	
	
	

	4.20 Forward and aft engine supports and rods for condition and security.
	
	

	
	
	

	4.21 Engine exhaust duct for condition, security and cracks.
	
	

	
	
	

	4.22 Ventilation air intake screen and ducts for condition.
	
	

	
	
	

	4.23 Main rotor hub cover for condition and security.
	
	

	
	
	

	4.24 Swashplate and rotating scissor for condition, security and unusual play.
	
	

	NOTE:  Ref. to para 62-31-9; in case of doubt ref. to para 62-31-9A
	
	

	4.25 Flap and drop restrainers for condition, freedom of movement and integrity of lockwire Inspect floating ring and droop stop plates for condition and check that grease is present in contact area.
	
	

	
	
	

	4.26 Lubricate main rotor floating ring and droop stop.
	
	

	
	
	

	4.27 Hydraulic pump for leaks.
	
	

	
	
	

	4.28 Fuel tank sump cover for condition and security.
	
	

	
	
	

	4.29 Anti-collision light for condition, security and cracks.
	
	

	
	
	

	A 0050.5 AREA 3 - TAIL BOOM & STABILIZER – RH SIDE

	
	
	

	5.1 Tail boom exterior (pay particular attention to tail boom and fuselage attachment areas) and stabilizer for cracks, dents, missing and/or loose rivets and screws.
	
	

	
	
	

	5.2 Position and anti-collision lights for condition, security and cracks.
	
	

	
	
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0050.6 AREA 4 - FINS, 90° GEARBOX, TAIL ROTOR, TAIL SKID

	
	
	

	6.1 External fuselage for cracks, dents, missing and/or loose rivets and screws.
	
	

	
	
	

	6.2 Tail rotor hub and blades for condition, contamination of oil/grease, security and freedom of flapping. Flap stop bumpers and boots for condition and damage. Tail rotor hub for unusual play along flap axis. Tail rotor blades for condition, scratches and dents.
	
	

	
	
	

	6.3 Tail rotor pitch change mechanism for condition, security and unusual play. 
	
	

	
	
	

	6.4 Lubricate pitch change mechanism duplex bearing.
	
	

	
	
	

	6.5 Tail rotor (90°) gearbox for condition, security, oil leaks.
	
	

	
	
	

	A 0050.7 AREA 5 - TAIL BOOM & STABOLIZER – LH SIDE

	
	
	

	7.1 Tail rotor drive shafts for condition, security, proper bonding of balancing weights and rings in contact with dampers.
	
	

	
	
	

	7.2 Tail rotor drive shaft bearing for condition and excessive grease leakage. In case excessive grease leakage is detected inspect for roughness to rotation. Lubricate drive shaft bearing.
	
	

	
	
	

	7.3 Tail rotor drive shaft Thomas couplings for condition and cracks of visible surfaces.
	
	

	
	
	

	7.4 Tail rotor drive shaft dampers for condition and freedom of movement.
	
	

	
	
	

	7.5 Tail boom exterior (pay particular attention to tail boom and fuselage attachment areas) and stabilizer for cracks, dents, missing and/or loose rivets and screws.
	
	

	
	
	

	7.6 Position lights for condition, security and cracks.
	
	

	
	
	

	A 0050.8 AREA 6 - FUSELAGE – LH SIDE

	8.1 Fuel system drain lines and valves for leaks.
	
	

	
	
	

	8.2 Landing skid for damage, condition and forward and rear saddles connecting skid to crossbeams for sealing integrity.
	
	

	
	
	

	8.3 Rear crosstube and central support for condition and security (visible parts).
	
	

	
	
	

	8.4 Landing skid damper for condition and leaks. Support for condition.
	
	

	
	
	

	8.5 Forward crosstube and fuselage attaching clamps for condition and security.
	
	

	
	
	

	8.6 Inspect cargo hook components, structure and electrical connection for condition and security
	25-92-15
	

	
	
	

	8.7 Check operation of emergency cargo release system. Leave hook in stowed position.
	25-92-7
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	8.8 Main rotor grips (2 places) for condition.
	
	

	
	
	

	8.9 Flap and drop restrainers for condition, freedom of movement and integrity of lockwire.
	
	

	
	
	

	8.10 Main rotor dampers (2 places) for condition, security, unusual play of bearings and correct fluid level.
	
	

	
	
	

	8.11 Ground jumpers between pitch control lever (inside grip) and damper and between damper and attachment bracket to hub for condition (2 places).
	
	

	
	
	

	8.12 Main rotor pitch change links (2 places) for condition, security, corrosion and fretting of the spherical bearings, loss of part of the liner and unusual play (check axial play by moving the pitch link by hand and the radial play by rotating the blade along its pitch axis and by acting from the tip cap area).
	
	

	
	
	

	8.13 Swashplate upper and lower boots for condition, integrity and absence of grease on external surfaces.
	
	

	
	
	

	8.14 Main rotor damper fittings (2 places) for condition, unusual play and cracks in the area of the attachment point to the hub.
	
	

	
	
	

	8.15 Fan and oil cooler for condition and security.
	
	

	
	
	

	8.16 Transmission to fan drive shaft for condition, security and freedom of axial movement.
	
	

	
	
	

	8.17 Main transmission and accessories for condition, security and leaks of lubricant.
	
	

	
	
	

	8.18 Check rotor brake assembly for security of attachments.
	
	

	
	
	

	8.19 Visible parts of flight controls, levers and supports for condition and security.
	
	

	
	
	

	8.20 Forward and aft engine supports and rods for condition and security.
	
	

	
	
	

	8.21 Engine exhaust duct for condition, security and cracks.
	
	

	
	
	

	8.22 Ventilation air intake screen and ducts for condition.
	
	

	
	
	

	8.23 Main rotor hub cover for condition and security.
	
	

	
	
	

	8.24 Swashplate and rotating scissor for condition, security and unusual play.
	
	

	NOTE:  Ref. to para 62-31-9; in case of doubt ref. to para 62-31-9A
	
	

	8.25 Main rotor hub and blades (2 places) for condition, damage and cleanliness.
	
	

	
	
	

	8.26 Main rotor servo actuator (2 places) for condition, security and leaks. Inspect bleed hole for leaks, lower spherical bearing for looseness and upper bearing for abnormal play.
	
	

	
	
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	8.27 Hydraulic pump for leaks.
	
	

	
	
	

	8.28 Main rotor elastomeric bearings for separation or loss of bearing elements, eventual blowing and/or rubber extruding and absence of oil or grease;
	
	

	NOTE:  If contaminated ref. to Para 62-21-50 for cleaning.
	
	

	8.29 Tail rotor servo actuator for condition, security and leaks.
	
	

	
	
	

	8.30 Fuel tank sump cover for condition and security
	
	

	
	
	

	8.31 Engine oil filter and housing for condition, leaks and security.
	
	

	
	
	

	8.32 Gas Generator Control lever rigging check
	76-11-29A
	

	
	
	

	A 0050.9 AREA 7 - CABIN INTERIOR

	
	
	

	9.1 Magnetic compass for level of fluid. Correction card for legibility.
	
	

	
	
	

	9.2 Safety belts for condition. Release mechanism for operation.
	
	

	
	
	

	9.3 Passenger seats for condition and security.
	
	

	
	
	

	9.4 Check the contents of the first aid kit onboard and expiring date of all the components.
	
	

	
	
	

	9.5 Set radio master (RAD MSTR) switch to on and check that avionic cooler fan (nose compartment) operates.
	
	

	
	
	

	A 0050.10 POST INSPECTION

	
	
	

	11.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	11.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	
	

	
	
	

	11.3 Perform Functional Check Flight if required per AW119MKII MPM Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	11.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

[bookmark: _Hlk529367719]I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ AW119MKII Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

[bookmark: _Hlk529367746]I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ AW119MKII AAIP – A 0050NT – 50 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
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