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	2
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	SECTION:
	
	A 0600 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	600 HOUR INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 407 MM-1 Chapter 5

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0600.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 407 MP
	

	
	
	

	A 0600.2 ROTOR BRAKE

	
	
	

	2.1 Inspect the rotor brake if installed
	BHT-407-CR&O-V
	

	NOTE:
Inspection information for the caliper assemblies and disc is contained in Northwest Dynamics Document N. B0223-OM, B0223-OM4, B0224-OM as identified in Table 5-2  
	

	2.1.1 Caliper Assembly
	
	

	
	
	

	2.1.2 Disk
	
	

	
	
	

	A 0600.3 MAIN ROTOR FRAHM (If installed) 

	NOTE:
Not required if the Frahm has been removed 
in accordance with TB 407-03-51
	

	3.1 Remove main rotor Frahm.
	
	

	
	
	

	3.2 Inspect Frahm assembly for condition.
	
	

	
	
	

	A 0600.4 POST INSPECTION

	
	
	

	4.1 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-407-FM-1/2
	

	
	
	

	4.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	4.3 Perform Functional Check Flight if required per Bell 407 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	4.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 407 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 407 AAIP – A 0600 – 600 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




