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	Page No:
	1

	Revision:
	Orig

	Issue Date:
	04/15/19

	SECTION:
	
	C 0120 – ICA OF INSTALLED EQUIPMENT

	TYPE:
	
	12 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0120.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	C 0120.2 TANNIS HEATER - TCA0003

	
	
	

	2.1 Perform visual inspection for serviceability and security of attachment of the following:
	AC43.13-1B

TCA Chp 11
	

	
	
	

	2.1.1 Security of attachment by following cable leads from the shore power plug to each element.
	
	

	
	
	

	2.1.2 Connectors and junctions for signs of heat damage or deformities.
	
	

	
	
	

	2.1.3 Wire/cable for signs of fatigue, chafing, flexing, heat damage, and vibration, re-secure, and or repair as needed.
	
	

	
	
	

	2.1.4 Pad heat elements for security of attachment and bonding.
	
	

	
	
	

	2.1.5 Threaded elements for security of installation.
	
	

	
	
	

	2.1.6 Wire to element transition point, where the lead enters the element body, for signs of heat damage or broken wires, and inspect the connector for security   of attachment and deformities.
	
	

	
	
	

	2.1.7 Cleaned as needed.
	
	

	
	
	

	2.2 Perform a Functional System check of each pad.
	Section 15
	

	
	TCA
	

	C 0120.3 DART CABLE CUTTER KIT – ICA119-2

	
	
	

	3.1 Thoroughly clean cutter assemblies, deflectors, and all associated components before conducting inspection.
	
	

	
	
	

	3.2 Inspect all surfaces and edges of the kit for damage. If damage is found, remove and replace parts per Section 5.0.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	3.3 Inspect the cutter assemblies, cutter blades, deflectors, brackets, struts, and attachment hardware for any corrosion.
	
	

	
	
	

	3.4 Reinstall any removed or replaced parts per applicable portions of Section 5.0 and return aircraft to operational condition.
	
	

	
	
	

	C 0120.4 AAI TAIL ROTOR PEDAL LOCKOUT KIT – AA-99032

	
	

	4.1 TAIL ROTOR PEDALS LOCKED OUT
	

	
	

	4.1.1 Inspect Lockout Bracket Assembly for condition and security of attachment.
	
	

	
	
	

	4.1.2 Verify the Expandable pins are properly positioned in the Bellcrank and Safety Clips are properly latched.
	
	

	
	
	

	4.1.3 Verify the Links are fully seated and locked on the Lockout bracket Assembly.
	
	

	
	
	

	4.2 TAIL ROTOR PEDALS ENGAGED
	

	
	

	4.2.1 Inspect Warning Decal for condition and security of attachment.
	
	

	
	
	

	4.2.2 Inspect Cable Assembly (Lanyard) for condition and security.
	
	

	
	
	

	4.2.3 Verify the Expandable Pins are seated on top of the Links.
	
	

	
	
	

	4.2.4 Verify the Safety Clips are properly latched.
	
	

	
	
	

	4.2.5 Verify there is no play between the Expandable Pins, Links and Bellcrank.
	
	

	
	
	

	4.2.6 Position each Tail Rotor Pedal, one at a time, to the full forward position. Verify there is no Pedal-to-Expandable Pin contact. Verify there is no right Expandable Pin contact with the Control Tube.
	
	

	
	
	

	C 0120.5 EXTERNAL ITT & TORQUE INDICATING SYSTEM – MMS407001 

	
	
	

	5.1 Perform a function test of the rotorcraft torque indicating system
	P&W
	

	
	EMM
	

	5.2 Perform an engine temperature compensator verification (ITT trim value) test of the rotorcraft ITT indicating system.
	P& W

EMM
	

	
	
	

	C 0120.6 HELICOPTER PERFORMANCE MONITORING SYSTEM – MMS403001

	
	
	

	6.1 Perform a detailed visual structural inspection of the MPMS and the associated modified aircraft structure using a 10X magnifying glass.
	2.1
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0120.7 POST INSPECTION

	
	
	

	7.1 Inspect for operation and leaks.
	
	

	
	
	

	7.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	7.3 Perform Functional Check Flight if required per Rotorcraft Flight Manual and/or Manufacturer ICA.
	
	

	
	
	

	7.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ AW119MKII Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ AW119MKII AAIP – C 0120 – 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


