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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
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	Aircraft Start Total Cycles:
	



	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0351.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	C 0351.2 DART BEARPAWS  D119-647

	
	
	

	2.1 Remove as per chapter 32 of these instructions and inspect the bearpaws and clamps for damage and/or wear.
	
	

	
	
	

	2.2 In the shaded region of Figure 5-2, the bearpaw may be worn by a maximum of 0.125” (3.18mm) down to the minimum allowable values specified in Table 5-1. Outside the shaded region of Figure 5-2, it is acceptable to have worn areas up to a maximum of 0.125” (3.18mm) deep over a maximum area of 2 sq. in (1290 sq. mm). The edge of a damaged region must be a minimum of 2” (51mm) away from the edge of nearest damaged region.
	Table 5-1
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	2.3 Cracks are acceptable in the unshaded portion of Figure 5-2 as long as they are restricted to the pockets of the bearpaws. Cracks that penetrate the stiffening ribs of the unshaded regions are unacceptable. Stop drill all cracks up to 0.50” (12.7mm) long with ∅0.188” (∅4.78mm) drill.
	
	

	
	
	

	2.4 Report all damage in excess of indicated limits to Dart Aerospace USA, Inc. for evaluation and disposition.
	
	

	
	
	

	2.5 Replace damaged or worn parts per chapter 32 of ICA.
	
	

	
	
	



	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0351.3 DONALSON IBF SYSTEM – AFS-AA119-IBF

	CAUTION: NEVER INSTALL A FILTER ASSEMBLY AND/OR OPERATE AN AIRCRAFT WITH A FILTER INSTALLED WHERE THE FILTER MEDIA HAS NOT BEEN PROPERLY OILED.
	

	
	
	

	3.1 Filter Assembly; Filter frame and filter media and all associated seals/fasteners.
	Fig 4
	

	
	
	

	3.1.1 Perform a visual inspection checking for deformation, buckling, corrosion, cracks, dents, tears, or other signs of damage and repair in accordance with the procedures.
	Chp 8
	

	
	
	

	3.1.2 Service filter – Observe all cautions
	7.3
	

	
	
	

	3.1.3 Visually inspect the pleats on both sides of the filter. If you cannot see the bottom of the pleat, when sighting the length, or depth of the pleat, straightening of the pleat is required.
	
	

	
	
	

	3.1.4 Inspect the filter assembly frame for cracks, gouges, distortion or deformation, corrosion, loose or missing fasteners, and missing or deteriorated protective coating. Refer to “Repair” for criteria / disposition.
	
	

	
	
	

	3.1.5 Inspect the filter seal for any tears, nicks, gouges, missing pieces or a permanent set or flattening of the seal. If the seal exhibits any of these conditions, repair or replace the seal. Refer to “Filter Seal” procedures.
	
	

	
	
	

	3.1.6 Visually inspect the assemblies for corrosion in accordance with AC 43.13-1, Chapter 6 and Table 8-1.
	
	

	
	
	

	3.2 Structural Components; Fore and Aft Frames, Filter Frames, FMA Bracket, Lower Supports, and Actuator Supports.
	8.4.1.2

8.4.2.2
	

	
	
	

	3.2.1 Visually inspect all structural components for oversized or elongated holes, deformation, cracks, corrosion, missing fasteners or components, fretting, galling, etc. Any component exhibiting these conditions requires repair or replacement.
	
	

	
	
	

	3.2.2 Visually inspect fasteners for damaged or missing threads, in both the bolt or screw and the nut or nut plate. If a self-locking fastener can be fully threaded by hand, replace the self-locking fastener.
	
	

	
	
	

	3.2.3 Visually inspect all electrical connections for security, corrosion, arcing, breakdown of insulation, and overheating. Repair or replace components exhibiting defects. Inspect and repair components per Agusta technical manuals or AC 43.13-1B, Chapter 11.
	
	

	
	
	

	3.2.4 Cracking. Visually inspect the assemblies for cracking using a 10x magnification glass at the corners, radiuses, and transitions in part thickness. Inspect suspect areas carefully using the 10x magnification. No cracks are allowed in the assemblies. If cracks are found, Filter Housing Assembly must be replaced.
	
	

	
	
	



	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	3.2.5 Visually inspect the assemblies for warping or distortion. Any warping or distortion that keeps the Upper or Side Filter Assemblies from creating a seal to the frame Assemblies requires disposition instructions from AFS or replacement.
	8.4.1.2
	

	
	
	

	3.2.6 Visually inspect the assemblies for missing, damaged, or “scratched through” protective coatings. Re-apply protective coatings per Table 8-1.
	
	

	
	
	

	3.2.7 Inspect the Actuator Supports and the Upper Filter Actuator Support for cracks, damage, corrosion, security, and serviceability.
	
	

	
	
	

	3.3 Systems and Electrical Components; Filter Assembly; Wiring, Connectors, Backshells, Circuit Breaker, Cockpit Indicator/switch, Differential Pressure Switch, Filter Maintenance Aid, and Actuator.
	
	

	
	
	

	3.3.1 Inspect circuit breaker for proper functioning.
	
	

	
	
	

	3.3.2 Inspect circuit breaker for security, damage, overheating, or corrosion. If component is suspect, replace defective component or contact AFS for disposition.
	
	

	
	
	

	3.3.3 Visually inspect all electrical connections for security, corrosion, arcing, breakdown of insulation, and overheating. Repair or replace components exhibiting defects. Inspect and repair components per Agusta technical manuals or AC 43.13-1B, Chapter 11.
	
	

	
	
	

	3.3.4 Wiring harness and associated components - Perform a visual inspection for evidence of chafing, damage, corrosion and insuring the circuit breaker and all pins, connectors, and backshells are secure. Inspect wiring, wiring harness and associated components per AC 43.13-1, Chapter 11.
	
	

	
	
	

	3.3.5 Inspect Cockpit Indicator/Switch for proper functioning. 
	8.5.2.5
	

	
	
	

	3.3.6 Inspect Cockpit Indicator/Switch for security, damage, overheating, corrosion, or distortion. Replace defective component or contact AFS for disposition.
	
	

	
	
	

	3.3.7 Inspect Actuator for cracks, damage, corrosion, and serviceability.
	
	

	
	
	

	3.3.8 Inspect the Circular Connector for damage, security, corrosion and serviceability.
	
	

	
	
	

	C 0351.4  CABIN CRAFTERS - CCI4744-11

	
	
	

	4.1 Visually check all Main Cabin Liners for general condition, operation and security.
	
	

	
	
	



	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0351.5 PARAVION BLADE FOLDING KIT – PR-1A109BF-120M

	
	
	

	5.1 Forward Receivers 
	Fig 1
	

	
	
	

	5.1.1 Inspect for indication of stress, cracks, or corrosion.
	
	

	
	
	

	5.1.2 Clean and remove corrosion. Replace receiver if necessary.
	Fig 2
	

	
	
	

	5.2 Windscreen Clevis
	
	

	
	
	

	5.2.1 Inspect for indications of stress, cracks or corrosion. Clean and remove corrosion. Replace clevis if necessary.
	
	

	
	
	

	5.2.2 Inspect aircraft structure at attachment points. Evidence of movement will require clevis removal and inspection and, if necessary, repair of aircraft structure in accordance with approved procedures.
	
	

	
	
	

	5.3 Left and Right-Side Aft Receivers
	Fig 3
	

	
	
	

	5.3.1 Inspect for indications of stress, cracks or corrosion. Clean and remove corrosion. Replace receiver if necessary.
	
	

	
	
	

	5.3.2 Inspect aircraft structure at attachment points. Evidence of movement will require receiver removal and inspection and, if necessary, repair of aircraft structure in accordance with approved procedures.
	
	

	
	
	

	5.4 Left Side Aft Receiver Installation
	Fig 4
	

	
	
	

	5.4.1 Inspect for indications of stress, cracks or corrosion. Clean and remove corrosion. Replace receiver if necessary.
	
	

	
	
	

	5.4.2 Inspect aircraft structure at attachment points. Evidence of movement will require receiver removal and inspection and, if necessary, repair of aircraft structure in accordance with approved procedures
	
	

	
	
	

	C 0351.6 DART BUBBLE WINDOW – ICA-D119-755

	
	
	

	6.1 Inspect all parts of the D119-755 installation for mechanical damage (scratches, nicks, cracks) and suitability for continued serves
	
	

	
	
	

	6.2 Inspect seals for deterioration/weathering and suitability for continued service.  Cracks in seals are unacceptable; replace as required.
	
	

	
	
	

	6.3 Verify that the doors are opening, closing, locking and sealing properly.
	
	

	
	
	

	6.4 Inspect the doors for wear and damage in accordance with the aircraft MM
	
	

	
	
	



	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0351.7 POST INSPECTION

	
	
	

	7.1 Inspect for operation and leaks.
	
	

	
	
	

	7.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	7.3 Perform Functional Check Flight if required per Rotorcraft Flight Manual and/or Manufacturer ICA.
	
	

	
	
	

	7.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ AW119MKII Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ AW119MKII AAIP – C 0351 – 300 Hour 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


