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	Page No:
	3

	Revision:
	Orig

	Issue Date:
	04/15/19

	SECTION:
	
	A 0250RT – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	200 HOUR / 12 MONTH INSPECTION

	NOTE:
	
	This Inspection is restricted to +10 Hours/2 Months whichever occurs first.



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  AW119MKII MPM Chapter 05, 05-70
	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0250.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	A 0250.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	
	
	

	A 0250.3 ROTOR DRIVE

	
	

	3.1 MAIN TRANSMISSION STRUCTURAL FWD AND AFT LOWER FITTINGS
	

	
	

	3.1.1 Inspect main transmission structural fwd and aft lower fittings for corrosion, cracks and proper condition of joints.
	63-31-10
	

	
	
	

	3.2 Lubricate main rotor servo actuators (3 places)
	
	

	
	
	

	3.3 Lubricate main rotor swashplate (2 places) with C594 or C009 Do not mix!
	12-20-5
	

	Note: Select which lubrication;    ____ 1st        ____ 2nd        ____ 3rd         ____ 4th
	
	

	Type of Grease ______________________
	

	3.4 In regards to the above, every 4th lubrication:
	

	
	

	3.4.1 On upper swashplate bellow cut lower safety wire (ref. Fig. 62-45, detail A1), or remove the clamp (whatever installed), and lift the bellow to expose bellow ring support. Lift ring support bellow and remove all visible grease extruding from duplex bearing seat.
	12-20-5
	

	CAUTION
DO NOT MIX GREASE C594 WITH C009. MAKE AN APPROPRIATE ENTRY IN HELICOPTER LOG BOOK TO INDICATE THE GREASE USED TO PREVENT SUBSEQUENT SERVICING WITH A DIFFERENT BRAND
	





	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0250.4 FLIGHT CONTROLS

	
	
	

	4.1 Service servo hydraulic system accumulators (2 places) with nitrogen
	12-20-13
	

	
	
	

	A 0250.5 POST INSPECTION

	
	
	

	5.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	5.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	
	

	
	
	

	5.3 Perform Functional Check Flight if required per AW119MKII MPM Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	5.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ AW119MKII Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ AW119MKII MPM AAIP – A 0250RT – 200 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	


	




