	MARITIME HELICOPTERS
	AgustaWestland Model AW119 AAIP

	
	

	Page No:
	3

	Revision:
	Orig

	Issue Date:
	04/15/19

	SECTION:
	
	A 0800RT – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	800 HOUR INSPECTION

	NOTE:
	
	This Inspection is Restricted to +30 Hours



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  AW119MKII Maintenance Planning Manual Chapter 05-40-10

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0800.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	A 0800.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	
	
	

	A 0800.3 FUEL

	
	
	

	3.1 Fuel flexible and rigid tubes for condition, leaks and chafing.
	
	

	
	
	

	A 0800.4 HYDRAULIC POWER

	
	
	

	4.1 Clean the hydraulic filter elements.
	29-11-31
	

	
	
	

	A 0800.5 FUSELAGE

	
	
	

	5.1 Tail boom attachment bolts for correct torque.
	53-31-8
	

	
	
	

	5.2 Inspect main transmission structural aft lower fittings, for condition of attachment bolts and condition of surrounding structure, verify correct torque.
	63-31-9
	

	
	
	

	A 0800.6 MAIN ROTOR

	
	
	

	6.1 Main rotor head ring nut bolts for correct torque.
	62-21-13
	

	
	
	

	6.2 Swashplate for correct friction.
	62-31-28
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0800.7 MAIN ROTOR DRIVE

	
	
	

	7.1 POWER PLANT AND OIL COOLER FAN - Splined adapters of transmission to fan drive shaft for excessive radial play and Thomas couplings for cracks and corrosion of laminates.
	63-11-14
	

	
	
	

	7.2 Inspect main transmission mounts for condition and/or chafing with tubing.
	
	

	
	
	

	7.3 Inspect bolt P/N NAS 625-14 and -18 securing main transmission support fittings to the structure for correct torque.
	63-31-8
63-31-9

	

	
	
	

	A 0800.8 TAIL ROTOR DRIVE

	
	
	

	8.1 [bookmark: _GoBack]Inspect free bearing adapter of tail rotor drive shaft.
	65-11-9
	

	8.2 Inspect bearing for roughness and freedom of rotation.
	65-11-25
	

	
	
	

	8.3 Remove tail rotor drive shaft forward and aft sections.
	65-11-10
	

	
	65-11-14
	

	8.4 Clean and inspect shafts, adapters and Thomas couplings.
	65-11-11/15
	

	
	
	

	8.5 Check drive shaft dampers for dimension, correct friction setting and integrity of supports.
	65-11-29
	

	
	
	

	A 0800.9 ROTORS FLIGHT CONTROL

	
	
	

	9.1 Lower spherical bearing of main rotor servo actuators for freedom of movement and correct rotation moment.
	67-31-9
	

	
	
	

	9.2 Upper rod-end bearing of main rotor servo actuators for radial play.
	67-31-9
	

	
	
	

	9.3 Main rotor servo actuators dowel pin seats for wear, elongation and/or distortion.
	67-31-9
	

	NOTE:  The following inspection is applicable to main rotor servo actuators P/N 109-0110-42-124/-125/-126 up to S/N 2331 included. The subject servo actuators repaired or overhauled by Magnaghi after 13 may 1999 (date shown on the related assembly historical record) do not require compliance with this inspection.
	
	

	9.4 Remove main rotor servo actuators and inspect bolts securing the two half-bodies.
	67-31-12
	

	
	
	

	A 0800.10 POWER PLANT

	
	
	

	10.1 Attaching hardware securing engine mount and relative fittings secured to fuselage for correct torque.
	Figure 71-9
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0800.11 OIL

	
	
	

	11.1 Oil flexible and rigid tubes for condition, leaks and chafing.
	
	

	
	
	

	11.2 Detach fan from oil cooler and thoroughly clean oil cooler mating surface with fan.
	
	

	
	
	

	A 0800.12 POST INSPECTION

	
	
	

	12.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	12.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	
	

	
	
	

	12.3 Perform Functional Check Flight if required per AW119MKII MPM Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	12.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

[bookmark: _Hlk529367719]I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ AW119MKII Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

[bookmark: _Hlk529367746]I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ AW119MKII AAIP – A 0800RT – 800 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	


	

