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	Page No:
	3
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	Orig

	Issue Date:
	04/15/19

	SECTION:
	
	A 1701RT – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	12 MONTH INSPECTION

	NOTE:
	
	This Inspection is Restricted to +2 Months



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  AW119MKII Maintenance Planning Manual Chapter 05-50

	
	
	MECHANIC’S
INITIALS

	[bookmark: _GoBack]MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1701.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	AW119MKII MPM
	

	
	
	

	A 1701.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	
	
	

	A 1701.3 FUEL

	
	
	

	3.1 Drain and vent lines for condition and obstructions.
	
	

	
	
	

	A 1701.4 NAVIGATION

	
	
	

	4.1 Antenna(s) for condition and security. Check sealant for voids and condition.
	
	

	
	
	

	4.2 Drain pitot static and dynamic lines.
	
	

	
	
	

	A 1701.5 DOORS

	
	
	

	5.1 Remove pilot doors and inspect jettison mechanism for correct operation.
	52-11-10
	

	
	
	

	A 1701.6 FUSELAGE

	
	
	

	6.1 Fuselage and tail boom exterior for general condition, corrosion, visual evidence of distortion and defective and/or missing rivets.
	
	

	
	
	

	6.2 Service steps, wire ropes and related fixing area on fuselage for condition, security and integrity.
	
	

	
	
	

	6.3 Inspect placards and decals for integrity and legibility.
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	6.4 Inspect cockpit floor and cabin floor for cleanliness, corrosion, dents and damage.
	
	

	NOTE: Liner removal is required.
	

	6.5 Tail skid for wear. Inspect tail skid attachment area for corrosion, cracks and damage.
	
	

	
	
	

	A 1701.7 STABILIZERS

	
	
	

	7.1 Inspect stabilizer for condition, cracks and distortions, dents, corrosion, defective and/or missing rivets (pay particular attention to the attachment area)
	55-00-7
	

	NOTE: Tail plane removal is required.
	

	A 1701.8 POST INSPECTION

	
	
	

	8.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	8.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	
	

	
	
	

	8.3 Perform Functional Check Flight if required per AW119MKII MPM Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	8.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

[bookmark: _Hlk529367719]I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ AW119MKII Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

[bookmark: _Hlk529367746]I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ AW119MKII AAIP – A 1701RT – 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	


	

