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	SECTION:
	
	A 1272 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	1200 HOUR / 72 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Location:
	


Reference:  Eurocopter B0-105 Series MM Chapter 101

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1272.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	1.4 Overhaul all components that have completed published operating limits.
	Eurocopter 
	

	
	BO-105 MP
	

	A 1272.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	
	

	A 1272.3 CORROSION CONTROL

	3.1 Perform corrosion inspection in any area’s access during this AAIP inspection.
	
	

	A 1272.4 MAIN ROTOR BLADE

	
	
	

	4.1 Remove, clean and inspect primary and secondary bolts for cracks and condition.
	14-4, 14-5
	

	NOTE:  Note following when inspecting erosion protective shells for debonding:
When first-time debonds are found, or existing debonds have increased in area. the inspection shall be repeated after 50Fh. Only when an inspection has revealed no further debonding do the periodic inspection intervals re-apply.
	

	A 1272.5 TAIL ROTOR

	
	33-16, step 1.
	

	5.1 Measure play between blade mounting fork and inner sleeve
	
	

	
	
	

	5.2 Remove bolts connecting laminated strap pack to blade mounting forks, and inspect for condition
	33-16, step 5.
	

	
	
	

	A 1272.6 TAIL ROTOR CONTROLS

	
	
	

	6.1 Inspect tail rotor controls for condition.
	42-3
	

	
	
	

	A 1272.7 ELECTRICAL

	
	
	

	7.1 Inspect components of electrical l system for condition
	92-4
	

	
	
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 1272.8 ENGINE

	
	
	

	8.1 Remove engine mounts and inspect for condition.
	61-8 thru 61 -19
	

	NOTE:  If the associated engine is to be removed within 600Fh after the inspection is due, the inspection can be performed concurrently with engine removal. 

	

	A 1272.9 POST INSPECTION

	
	
	

	9.1 Ensure applicable servicing requirements have been carried out.
	
	

	
	
	

	9.2 Check oil level of transmission, hydraulic tank, engine and rail rotor gearbox prior to running helicopter.
	
	

	
	
	

	9.3 Complete a ground run at 100% NR to check for leaks and confirm system operation and parameters are within Flight Manual limitations. – Qualified pilot only.
	
	

	
	
	

	9.4 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	9.5 Perform Functional Check Flight if required per BO-105 Maintenance Manual  or RFM as appropriate.
	
	

	
	
	

	9.6 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	







Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-105 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Eurocopter BO-105 Series AAIP – A 1272 – 1200 Hour / 72 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Log Page Number:
	



	Signature:
	
	
	Certificate Type & No:
	




