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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0150.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	BO -105 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	BO -105 MP
	

	
	
	

	C 0150.2 DART REPLACEMENT SKID TUBES – D105-674

	Note:  Removal of Skid Tubes from the helicopter is not required for inspection
	

	Note:  If excessive corrosion/wear/damage has occurred, perform the detailed 600 hour inspection.
	

	Note: It is acceptable to have nicks, scratches, or corrosion damage up to 0.015” (0.4 mm) deep over 30% of the total surface area of the skidtube.
	

	2.1 Inspect the skid tubes for scratches, nicks, dents, corrosion or excessive wear/damage.
	
	

	2.2 Inspect the sides of the tubes for excessive wear/damage.
	
	

	
	
	

	2.3 Inspect the area between the saddles for bow or sharp bends.
	
	

	
	
	

	2.4 Inspect the aft cap for damage.
	
	

	
	
	

	2.5 Inspect ground handling hardware for serviceability
	
	

	
	
	

	2.6 Inspect all areas of the skidtube for suitability of the paint finish and the anti-skid surface.
	
	

	
	
	

	C 0150.3 DUKANE UNDERWATER BEACON  03-TM-0037

	
	
	

	3.1 Clean the switch end of the beacon with a soft cloth and mild detergent, then dry thoroughly with a clean cloth.
	
	

	
	
	

	3.2 Clean the switch end insulator to prevent leakage currents from occurring across the switch.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0150.4 ONBOARD CARGO HOOK – ICA 123-022-00

	
	
	

	CAUTION

Energizing the cargo hook release solenoid continuously in excess of 20 seconds will cause it to overheat, possibly causing permanent damage.
	

	
	
	

	4.1 Activate the electrical system and press the Cargo Release button to ensure the cargo hook electrical release system is operating correctly- The cargo hook must release.
	Section 5
	

	4.2 Reset the hook by hand after release. If the hook does not release or re-latch, do not use the unit until the problem is fixed.
	
	

	4.3 Activate the hydraulic release system by pulling the release lever located on the collective in the cockpit. The mechanism should operate smoothly and the cargo hook must release.
	
	

	4.4 After release, return the load beam to its closed and locked position by hand. Verify that the hook lock indicator on the side of the hook returns to the fully locked position.
	
	

	4.5 In the fully locked position the hook lock indicator should align with the lines on the manual release cover…
[image: image1.png]



If the hook does not release or re-latch, do not use the unit until the

problem is resolved.

	
	

	4.6 Visually inspect for presence and security of fasteners and electrical connections.
	
	

	4.7 Check the fluid level in the master cylinder with the collective against the lower stop. The Master Cylinder features a transparent lid through which the fluid level can be checked. Hydraulic fluid must be visible over the baffle surface.
	
	

	4.8 Visually inspect for oil leaks in the hydraulic release system. Some seeping or dampness is acceptable, but if drips or areas cleaned by oil leaking are present the hook must not be used until the condition is repaired.
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.9 Visually inspect for corrosion on the exterior of cargo hook and link assembly components. 
	
	

	Note:  Corrosion on the cargo hook side plates is cause for immediate overhaul. Additionally, any exfoliation corrosion in the upper attach lug area of the cargo hook is cause for immediate replacement of the side plate. 
	

	4.10 Visually inspect for presence and security of fasteners and electrical connections.
	
	

	
	
	

	4.11 Visually inspect the external electrical wire harnesses and their connectors for damage and security.
	
	

	
	
	

	4.12 Visually inspect the hydraulic hose for damage and security.
	
	

	
	
	

	4.13 Visually inspect the electrical harness strain relief at the load cell (if installed) for damage.
	
	

	
	
	

	4.14 Verify calibration of the load cell (if installed) by lifting a load of known weight.
	
	

	
	
	

	4.15 Visually inspect the manual release cable for damage and security.
	
	

	
	
	

	4.16 Visually inspect the external electrical release harness and load weigh harness (if installed) for damage and security.
	
	

	
	
	

	C 0150.5 ARTEX ELT 570-5060

	
	
	

	5.1 ELT and mount for improper installation;
	FAR Part 43, 
	

	
	Appendix D
	

	5.2 Wiring and conduits for improper routing, insecure mounting, and obvious defects;
	
	

	
	
	

	5.3 Bonding and shielding for improper installation and poor condition;
	
	

	
	
	

	5.4 Antenna, including trailing antenna, for poor condition, insecure mounting, and improper operation.
	
	

	
	
	

	C 0150.6 POST INSPECTION

	
	
	

	6.1 Inspect for operation and leaks.
	
	

	
	
	

	6.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	6.3 Perform Functional Check Flight if required per Rotorcraft Flight Manual and/or Manufacturer ICA.
	
	

	
	
	

	6.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Eurocopter BO-105 Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Eurocopter BO-105  Series AAIP – C 0150 – 100 Hour / 6 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


