The last one went with out the attachment. 
I have N/A ed those that do not apply, and added a couple notes. 
I will send half and then the other half, then look at the other email you mentioned.
I will add a couple things. The Borg Warner Freewheel has an inspection 1200 hrs after new, then 600 hrs thereafter. At 1200 hrs the look like they will make it another 600 but what should happen is to send them in to Borg warner, and they refurbish them and then you can go another 1200. If you put them back in the probability of them deteriorating and pieces going thru the trans is very high.
Also, the trans filter should be checked each 100 hrs. when it starts giving trouble, non ferrous metal goes thru and gets caught in the filter. so the chip detector does no good.
I also recommend a supplimental inspection, like our 10 day PMI, As I have mentioned the BO is a vibrating machine. We have caught many pretty serious problems on that inspection, cracks, leaks, etc. because it required removing all cowls to have a serious look at things that can't be seen otherwise. It is not a Bell, and requires constant attention, even though these don't fly a lot. 

