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	SECTION:
	
	C 0001 – ICA OF INSTALLED EQUIPMENT

	TYPE:
	
	12 MONTHS AVIONICS INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  Various Avionics Installation and Operations Manuals.
	
	
	

	MAINTENANCE ACTION
	REFERENCE
	MECHANIC’S

	
	
	INITIALS

	C 0001.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	
	

	
	
	

	C 0001.2 FUSELAGE — COCKPIT SECTION

	2.1 Clean Instruments, avionics and electrical panels with damp, lint-free, static free cloths.  Take care to prevent moisture from entering components.
	
	

	
	
	

	2.2 Instrument Panel (Original or Altered) – Check for damage and security.
	
	

	
	
	

	2.3 Avionics consoles and extensions (Original or Altered) – Check for damage and security.
	
	

	
	
	

	2.4 Pilot’s Artificial Horizon – Check for damage, security and normal operation.
	
	

	
	
	

	2.5 Pilot’s Altimeter – Check for damage, security and normal operation. Set baro window, check field elevation.
	
	

	
	
	

	2.6 Pilot’s (Instantaneous) Vertical Speed Indicator – Check indicator to read zero on ground, adjust if necessary.
	
	

	
	
	

	2.7 Pilot’s Airspeed Indicator – Check for damage, security and normal operation.
	
	

	
	
	

	2.8 Pilot’s HSI – Check for damage and security, normal operation.
	
	

	
	
	

	2.9 Pilots Audio Panel – Check for damage, security and normal operation.
	
	

	
	
	

	2.10 Copilot’s Artificial Horizon – Check for damage, security and normal operation.
	
	

	
	
	

	2.11 Copilot’s Altimeter – Check for damage, security and normal operation. Set baro window, check field elevation.
	
	

	
	
	

	2.12 Copilot’s Instantaneous Vertical Speed Indicator – Check indicator to read zero on ground, adjust if necessary.
	
	

	
	
	

	2.13 Copilot’s Airspeed Indicator – Check for damage, security and normal operation.
	
	

	
	
	


	
	
	

	MAINTENANCE ACTION
	REFERENCE
	MECHANIC’S

	
	
	INITIALS

	2.14 Copilot’s HSI – Check for damage and security, normal operation.
	
	

	
	
	

	2.15 Copilots Audio Panel – Check for damage, security and normal operation.
	
	

	
	
	

	2.16 Crew Audio Panel – Check for damage, security and normal operation.
	
	

	
	
	

	2.17 Marker Beacon – Check for damage, security and normal operation, Self test.
	
	

	
	
	

	2.18 Standby Artificial Horizon – Check for damage, security and normal operation.
	
	

	
	
	

	2.19 Storm Scope/Weather Radar – Check for damage, security and normal operation, Self test.
	
	

	
	
	

	2.20 Radar Altimeter - Check for damage, security and normal operation, Self test.
	
	

	
	
	

	2.21 VOR/RMI/Localizer Indicator - Check for damage, security.
	
	

	
	
	

	2.22 Turn and Bank Indicator – Check for damage, security and normal operation.
	
	

	
	
	

	2.23 DME – Check for damage, security and normal operation.
	
	

	
	
	

	2.24 GPS 1 – Check for current data base, damage, security and normal operation, Self test.
	
	

	NOTE: Data base currency is required for IFR aircraft only.
	
	

	2.25 GPS 2 – Check for current data base, damage, security and normal operation, Self test.
	
	

	NOTE: Data base currency is required for IFR aircraft only.
	
	

	2.26 VHF Comm 1 – Check for damage, security and normal operation, Self test.
	
	

	
	
	

	2.27 VHF Comm 2 – Check for damage, security and normal operation, Self test.
	
	

	
	
	

	2.28 Nav 1 - Check for damage, security.
	
	

	
	
	

	2.29 Nav 2 - Check for damage, security.
	
	

	
	
	

	2.30 ADF – Check for damage, security and normal operation.
	
	

	
	
	

	2.31 FM Control(s) – Check for damage, security and normal operation.
	
	

	
	
	

	2.32 VHF – Lo Band(s) – Check for damage, security and normal operation.
	
	

	
	
	

	2.33 VHF – Hi Band(s) – Check for damage, security and normal operation.
	
	

	
	
	

	2.34 400 MHz Radio(s) – Check for damage, security and normal operation.
	
	

	
	
	

	2.35 800 MHz Radio(s) – Check for damage, security and normal operation.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	2.36 Multi Band Radio(s) – Check for damage, security and normal operation.
	
	

	
	
	

	2.37 Dual Tone Multi-Frequency (DTMF) Encoder – Check for damage, security and normal operation.
	
	

	
	
	

	2.38 Satellite Tracking system and Controls – Check for damage, security, self test and normal operation, to include verification of airspeed and altitude tracking.
	
	

	
	
	

	2.39 Terrain Display Unit – Check for damage, security, and normal operation.
	
	

	
	
	

	2.40 Terrain Awareness Annunciation Control Unit – Check for damage, security, and normal operation.
	
	

	
	
	

	2.41 Traffic alert and Collision Avoidance System – Check for damage, security, and normal operation.
	
	

	
	
	

	2.42 Multi-function Display – Proper display and function of controls.
	
	

	
	
	

	2.43 Satellite Weather Display – Proper display and function of controls and muting of signal with aircraft/engine warning.
	
	

	
	
	

	2.44 Handheld Radio Provisions – Check for damage, security, and normal operation.
	
	

	
	
	

	2.45 #1 Inverter – Check for damage, security and normal operation.
	
	

	
	
	

	2.46 #2 Inverter – Check for damage, security and normal operation.
	
	

	
	
	

	2.47 Standby Inverter – Check for damage, security and normal operation.
	
	

	
	
	

	2.48 Auto Pilot – Refer to Autopilot Operator’s Manual or Aircraft Flight Manual Supplement to check for damage, security, self test, and normal operation.
	
	

	
	
	

	2.49 ELT and control – Check for damage, security and normal operation. Check per FAR 91.207 and manufactures instructions.
	
	

	
	
	

	2.50 Loud Hailer/P.A. Control – Check for damage, security and normal operation.
	
	

	
	
	

	2.51 Hour Meter (Hobbs) – Check for damage, security and normal operation.
	
	

	
	
	

	2.52 Maintenance Hour Meter (Hobbs) – Check for damage, security and normal operation.
	
	

	
	
	

	2.53 Audio Advisory System (such as P2 Inc.) – Check for damage, security and normal ops.
	
	

	
	
	

	2.54 AM/FM Radio  – Check for damage, security and normal operation.
	
	

	
	
	

	2.55 Remote Digital Recorder and Aural Warming System – Check for damage, security and normal operation.
	
	

	
	
	


	
	
	

	MAINTENANCE ACTION
	REFERENCE
	MECHANIC’S

	
	
	INITIALS

	2.56 Inspect the cockpit voice and flight data recorder for security of installation.
	
	

	
	
	

	2.57 Check CVFDR for function.
	
	

	
	
	

	2.58 Avionics Fan (s) – Check for damage, security and normal operation.
	
	

	
	
	

	2.59 LT-100 Power Supply – Check for damage, electrical wiring, circuit breaker, reset retentions, security and normal operation.
	
	

	
	
	

	C 0001.3 AVIONICS COMPARTMENT(S)

	3.1 Raise cowling or cover and inspect avionics components for:
	

	3.1.1 Security of installation for all avionics.
	
	

	
	
	

	3.1.2 Damage.
	
	

	
	
	

	3.1.3 Condition of electrical wire bundles and chafe protection.
	
	

	
	
	

	3.1.4 Evidence of moisture entering area.
	
	

	
	
	

	3.1.5 Weather Radar – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	3.1.6 EGPWS  – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	3.1.7 Avionics Fan (s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	C 0001.4 FUSELAGE

	4.1 Flux Valve(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.2 Navigation Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.3 Marker Beacon Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.4 Comm Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.5 DME Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.6 GPS Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.7 ADF Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.8 Loran Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.9 ELT Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.10 Transponder Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	


	
	
	

	MAINTENANCE ACTION
	REFERENCE
	MECHANIC’S

	
	
	INITIALS

	4.11 Radio Altimeter Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.12 Glide Slope Antenna – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.13 FM Communications Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.14 Storm Scope Antenna – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.15 Satellite Tracking system Antennas – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.16 Upper Traffic Advisory System (TAS) Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.17 Lower Traffic Advisory System (TAS) Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.18 Check external components of the Avalanche Victim Search System.
	
	

	
	
	

	4.19 All other Antenna(s) – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	4.20 Loud Hailer/P.A. Speaker – Inspect for security of installation and evidence of damage.
	
	

	
	
	

	C 0001.5 COMPASS COMPENSATION

	5.1 Compensate Wet Compass(s) and install new correction card.
	
	

	
	
	

	5.2 Check compensation of flux valve (s)
	
	

	
	
	

	C 0001.6 ELT

	6.1 Inspect the unit for security of attachment, knobs and buttons for legibility
	
	

	
	
	

	6.2 Inspect condition of wiring, routing, bonding, shielding and attachment/clamping
	
	

	
	
	

	C 0001.7  CONCLUSIVE WORK

	7.1 Inspect all wiring, harnesses and electrical connections for chafing, security and condition before reinstalling panels/cowlings.
	
	

	C 0001.8 FINAL STEPS

	8.1 Inspect for operation and leaks.
	
	

	8.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	8.3 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Air Methods’ Model AS 350 SERIES Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been competed and have made the following entry in the Aircraft Log Book:

.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters AW119 AAIP – C0001 – 12 Months Avionics ICA Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


