	AIR METHODS CORPORATION
	Eurocopter Model AS 350 SERIES AAIP

	
	

	Page No:
	1

	Revision:
	Rev. 6

	Issue Date:
	02/15/11

	SECTION:
	
	C 0002 – ICA OF INSTALLED EQUIPMENT 

	TYPE:
	
	24 MONTHS AVIONICS INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  Various Avionics Installation and Operations Manuals.
	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0002.1 GENERAL

	
	
	

	1.1 Complete AS350 Series AAIP C-0001 ICA Of Installed Equipment – Avionics 12 Months Inspection
	
	

	
	
	

	C 0002.2 NAVIGATION RECEIVERS AND INDICATORS VOR/ILS/GLIDESLOPE/RNAV/RECEIVERS AND INDICATORS COUPLED THERE TO) (CHECK ALL UNITS)

	
	
	

	2.1 Check receiver for proper ground operation, audio quality and volume.
	1
	

	
	2
	

	2.2 Check ident function(s).
	1
	

	
	2
	

	2.3 Open and close circuit protection device(s) to ensure proper operation
	1
	

	
	2
	

	C 0002.3 MARKER BEACONS

	
	
	

	3.1 Check operation of marker beacon(s) with regards to proper lights and tones
	1
	

	
	2
	

	3.2 Check receiver(s) audio quality and volume
	1
	

	
	2
	

	3.3 Open and close circuit protection device(s) to ensure proper operation
	1
	

	
	2
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0002.4 ADF RECEIVERS (AND ALL INDICATORS COUPLED THERE TO)

	
	
	

	4.1 Check ADF(s) pointing operation including proper pointing, no excessive hunting
	1
	

	
	2
	

	4.2 Check BFO (Beat Frequency Oscillator)
	1
	

	
	2
	

	4.3 Check receiver(s) audio quality and volume
	1
	

	
	2
	

	4.4 Check self-test features
	1
	

	
	2
	

	4.5 Open and close circuit protection device(s) to ensure proper operation
	1
	

	
	2
	

	C 0002.5 DME’S (AND ALL INDICATORS COUPLED THERE TO)

	
	
	

	5.1 Check for proper ground operation
	1
	

	
	2
	

	5.2 Check receiver(s) audio quality
	1
	

	
	2
	

	5.3 Open and close circuit protection device(s) to ensure proper operation
	1
	

	
	2
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0002.6 RADAR ALTIMETERS AND ALTITUDE ALERTS (AND ALL INDICATORS COUPLED THERE TO)

	
	
	

	6.1 Check for ground proper operation.
	1
	

	
	2
	

	6.2 Check self-test function(s)
	1
	

	
	2
	

	6.3 Open and close circuit protection device(s) to ensure proper operation
	1
	

	
	2
	

	C 0002.7 WEATHER RADAR AND THUNDERSTORM DETECTION EQUIPMENT

	
	
	

	7.1 Check self-test function(s).
	1
	

	
	2
	

	7.2 Check for proper operation.
	1
	

	
	2
	

	7.3 Open and close circuit protection device(s) to ensure proper operation
	1
	

	
	2
	

	C 0002.8 ATTITUDE GYROS

	
	
	

	8.1 Check for proper indication, flags, and lack of precession
	1
	

	
	2
	

	8.2 Check for proper “Quick Erect”
	1
	

	
	2
	

	8.3 Open and close circuit protection device(s) to ensure proper operation
	1
	

	
	2
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0002.9 INVERTER CHECK

	9.1 Check for proper operations of the AC Inverters.
	1
	

	
	2
	

	9.2 Check for proper buss transfer
	1
	

	
	2
	

	9.3 Check operation of fault indicators and annunciators
	1
	

	
	2
	

	9.4 Open and close circuit protection device(s) to ensure proper operation
	1
	

	
	2
	

	C 0002.10 FLIGHT CHECK

	10.1 Check VHF Comm Radio(s) for proper operation.
	
	

	
	
	

	10.2 Check Nav Radio(s) for proper operation with regard to VOR tracking.
	
	

	
	
	

	10.3 Check Nav Radio(s) for proper operation with regard to ILS tracking, if available.
	
	

	
	
	

	10.4 Check Nav Radio(s) for proper operation with regard to GS tracking, if available.
	
	

	
	
	

	10.5 Check DME(s) for proper operation, if available.
	
	

	
	
	

	10.6 Check Marker Beacon for proper operation, if available.
	
	

	
	
	

	10.7 Check Radar Altimeter for proper indication in flight.
	
	

	
	
	

	10.8 Check Flight Director/Autopilot for proper operation.
	
	

	
	
	

	10.9 Check for proper coupling of Radar/Thunderstorm Detection Equipment to compass(es) systems and vertical gyros for heading and tilting
	
	

	C 0002.11 CONCLUSIVE WORK

	11.1 Inspect all wiring, harnesses and electrical connections for chafing, security and condition before reinstalling panels/cowlings.
	
	

	C 0002.12 POST INSPECTION

	
	
	

	12.1 Inspect for operation and leaks.
	
	

	
	
	

	12.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	12.3 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Air Methods’ AS350 B2 Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made the entry below in the Aircraft Log Book:

I certify that this aircraft has been inspected in accordance with Air Methods’ AS350 B2 AAIP – C0002 – 24 Month Avionics ICA Inspection and was determined to be in an airworthy condition.
	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	



