	AIR METHODS CORPORATION
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	Page No:
	1

	Revision:
	Rev. 6

	Issue Date:
	02/15/11

	SECTION:
	
	C ? – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	100 HOUR INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	C 0100.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	AS350BA MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	AS350BA MP
	

	
	
	

	C 0100.2 

	
	
	

	2.1 
	
	

	
	
	

	2.1.1 
	
	

	
	
	

	2.1.1.1 
	
	

	
	
	

	2.2 
	
	

	
	
	

	2.3 
	
	

	
	
	

	C 0100.3  

	
	
	

	3.1 
	
	

	
	
	

	3.2 
	
	

	
	
	

	3.3 
	
	

	
	
	

	3.4 
	
	

	
	
	

	3.5 
	
	

	
	
	

	C 0100.4  

	
	
	

	4.1 
	
	

	
	
	

	4.2 
	
	

	
	
	

	4.3 
	
	

	
	
	

	4.4 
	
	

	
	
	

	4.5 
	
	

	
	
	

	C 0100.5 

	
	
	

	5.1 
	
	

	
	
	

	5.2 
	
	

	
	
	

	5.3 
	
	

	
	
	

	5.4 
	
	

	
	
	

	5.5 
	
	

	
	
	

	C 0100.6 

	
	
	

	6.1 
	
	

	
	
	

	6.2 
	
	

	
	
	

	6.3 
	
	

	
	
	

	6.4 
	
	

	
	
	

	6.5 
	
	

	
	
	

	C 0100.7 

	
	
	

	7.1 
	
	

	
	
	

	7.2 
	
	

	
	
	

	7.3 
	
	

	
	
	

	7.4 
	
	

	
	
	

	7.5 
	
	

	
	
	


	C 0100.8 POST INSPECTION

	
	
	

	8.1 Inspect for operation and leaks.
	
	

	
	
	

	8.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	8.3 Perform Functional Check Flight if required per AMC Operations Manual.
	
	

	
	
	

	8.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Air Methods’ AS350 BA Series Approved Aircraft Inspection Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Air Methods’ AS 350 BA AAIP – C ???? – ??? Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


