	MARITIME HELICOPTERS
	DCH-6 CONTINUOUS AIRWORTHINESS MAINTENANCE PROGRAM

	
	

	Page No:
	1

	Revision:
	Original

	Issue Date:
	12/15/19

	CHECK:
	
	A 0125 – BASIC INSPECTION

	FREQUENCY:
	
	Every 125 Hours 

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  DHC-6 Maintenance Program, PSM 1-64-2 Maintenance Manual
	MAINTENANCE ACTION
	REF
	MECH INITIALS
	RII INITIALS

	A 0125.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	DHC-6-400

MP
	
	

	1.4 Overhaul all components that have completed published operating limits.
	DHC-6-400

MP
	
	

	A 0125.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	
	
	
	

	A 0125.3 CORROSION CONTROL

	
	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s accessed during this CAMP inspection.
	
	
	

	
	
	
	

	A 0125.4 PREPARATION

	
	
	
	

	4.1. Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	


	MAINTENANCE ACTION
	REF
	MECH INITIALS
	RII INITIALS

	A 0125.5 61 - PROPELLERS -RH

	
	
	
	

	5.1. Bata backup carbon block retaining pin for free movement.  Lubricate
	61-02b-2
	
	

	5.2. Overspeed governor for condition, security and leakage. 
	61-03-1

61-04-1
	
	

	Note:  Refer to AD 70-16-01, if applicable.
	
	
	

	5.3. Constant speed governor for condition, security and leakage. 
	61-03-1

61-04-1
	
	

	5.4. Propeller blades for condition, blades for freedom of movement on hub pitot tubes by rocking slightly using counterweights as levers; grease blade clamps.
	61-05a-2
	
	

	5.5. Gas generator tachometer and propeller generator for condition and security of installation.
	61-07

77-05
	
	

	5.6. Engine propeller synchronizer master speed pickup for condition and security.
	61-09a
	
	

	A 0125.6 61 - PROPELLERS -LH

	
	
	
	

	6.1 Bata backup carbon block retaining pin for free movement.  Lubricate
	61-02b-2
	
	

	6.2          Overspeed governor for condition, security and leakage. 
	61-03-1

61-04-1
	
	

	Note:  Refer to AD 70-16-01, if applicable.
	
	
	

	6.1 6.3         Constant speed governor for condition, security and leakage. 
	61-03-1
61-04-1
	
	

	6.4         Propeller blades for condition, blades for freedom of movement on hub pitot tubes by rocking slightly using counterweights as levers; grease blade clamps.
	61-05a-2
	
	

	6.5        Gas generator tachometer and propeller generator for condition and security of installation.
	61-07
77-05
	
	

	6.6        Engine propeller synchronizer master speed pickup for condition and security.
	61-09a
	
	

	A 0125.7 71 - POWEPLANT -LH

	7.1. Engine cowling fire seals for condition and security
	71-07
	
	

	7.2. Engine pipes, leads and controls; pipes for condition, security and leakage, controls for security and operation, clams and brackets for condition, leads for condition and security.  Clean as required.
	71-10
	
	

	A 0125.8 71 - POWEPLANT -RH

	8.1. Engine cowling fire seals for condition and security
	71-07
	
	

	8.2. Engine pipes, leads and controls; pipes for condition, security and leakage, controls for security and operation, clams and brackets for condition, leads for condition and security.  Clean as required.
	71-10
	
	


	MAINTENANCE ACTION
	REF
	MECH INITIALS
	RII INITIALS

	A 0125.9 72 - ENGINE - LH

	9.1. Engine external tubing for condition, cracks bulges and evidence of fuel and oil leakage.
	72-01
	
	

	9.2. Engine gas generator case for condition, cracks, bulges and evidence of hot spots
	72-04

72-05
	
	

	9.3. Power section and turbine exhaust for duct for condition, cracks and distortion.
	72-07
	
	

	A 0125.10 72 - ENGINE - RH

	10.1. Engine external tubing for condition, cracks bulges and evidence of fuel and oil leakage.
	72-01
	
	

	10.2. Engine gas generator case for condition, cracks, bulges and evidence of hot spots
	72-04

72-05
	
	

	10.3. Power section and turbine exhaust for duct for condition, cracks and distortion.
	72-07
	
	

	A 0125.11 73 - ENGINE FUEL AND CONTROL - LH

	
	
	
	

	11.1. Fuel pump for security and evidence of leakage.

Note: Refer to A.D 69-23-06 or 80-08-12, if applicable
	73-03
	
	

	11.2. Fuel pump filter screen (inlet). Remove, inspect and install. Clean or replace as required and leak check (power on).

CAUTION: Whenever any component upstream of the filter is replaced, check screen after run up or first flight
	73-01a
	
	

	11.3. Fuel pump filter screen (outlet). Remove, inspect and install. Clean or replace as required and leak check (power on).

Note: Refer to PWC Service Bulletin No. 1155
	73-01b-1
	
	

	11.4. Fuel control unit for condition, security, linkages, sense lines and heaters for condition, security and leakage.

Note: Refer to A.D 69-23-06 or 80-08-12, if applicable
	73-01

73-03
	
	

	11.5. Remove High Pressure fuel filter element, inspect and install. Clean or replace as required and leak check.
	73-01b-1
	
	

	11.6. Starting control unit for security and leakage
	73-07
	
	

	11.7. Compressor discharge P3 filter – clean filter element ultrasonically.

Effectivity: Mod SOO 6177
	73-09-1
	
	


	MAINTENANCE ACTION
	REF
	MECH INITIALS
	RII INITIALS

	A 0125.12 73 - ENGINE FUEL AND CONTROL - RH

	
	
	
	

	12.1. Fuel pump for security and evidence of leakage.

Note: Refer to A.D 69-23-06 or 80-08-12, if applicable
	73-03
	
	

	12.2. Fuel pump filter screen (inlet). Remove, inspect and install. Clean or replace as required and leak check (power on).
CAUTION: Whenever any component upstream of the filter is replaced, check screen after run up or first flight
	73-01a
	
	

	12.3. Fuel pump filter screen (outlet). Remove, inspect and install. Clean or replace as required and leak check (power on).

Note: Refer to PWC Service Bulletin No. 1155
	73-01b-1
	
	

	12.4. Fuel control unit for condition, security, linkages, sense lines and heaters for condition, security and leakage.
Note: Refer to A.D 69-23-06 or 80-08-12, if applicable
	73-01
73-03
	
	

	12.5. Remove High Pressure fuel filter element, inspect and install. Clean or replace as required and leak check.
	73-01b-1
	
	

	12.6. Starting control unit for security and leakage
	73-07
	
	

	12.7. Compressor discharge P3 filter – clean filter element ultrasonically.

Effectivity: Mod SOO 6177
	73-09-1
	
	

	A 0125.13 76 – ENGINE CONTROLS - LH

	
	
	
	

	13.1. Lubricate power control mechanism and linkage interconnecting rod ball ends.
	76-03-1
	
	

	Note: Refer to Service Bulletin 6/387 and A.A 80-04-02, if applicable.
	
	
	

	A 0125.14 76 – ENGINE CONTROLS - RH

	
	
	
	

	14.1. Lubricate power control mechanism and linkage interconnecting rod ball ends.
	76-03-1
	
	

	Note: Refer to Service Bulletin 6/387 and A.A 80-04-02, if applicable.
	
	
	

	A 0125.15 77 – ENGINE INDICATING - LH

	
	
	
	

	15.1. Torque pressure transmitter for condition and security.
	77-02
	
	

	15.2. Gas generator tachometer and propeller generator for condition and

security of installation.
	61-07

7-705
	
	

	A 0125.16 77 – ENGINE INDICATING - RH

	
	
	
	

	16.1. Torque pressure transmitter for condition and security
	77-02
	
	

	16.2. Gas generator tachometer and propeller generator for condition and

security of installation.
	61-07
7-705
	
	


	MAINTENANCE ACTION
	REF
	MECH INITIALS
	RII INITIALS

	A 0125.17 79 - OIL - LH

	
	
	
	

	17.1. Engine oil filter remove and check for foreign matter. Install a serviceable filter.
	79-01


	
	

	Note: Clean or renew filter according to instruction in the Engine Maintenance Manual. Change oil I/A/W UACL Service Bulletin No. 1001.
	
	
	

	17.2. Test magnetic chip detector in reduction gearbox for electrical continuity.
	79-03a
	
	

	
	
	
	

	17.3. Leak check engine oil filter after installation.
	79-03
	
	

	
	
	
	

	A 0125.18 79 - OIL - RH

	
	
	
	

	18.1. Engine oil filter remove and check for foreign matter. Install a serviceable filter.
	79-01


	
	

	Note: Clean or renew filter according to instruction in the Engine Maintenance Manual. Change oil I/A/W UACL Service Bulletin No. 1001.
	
	
	

	18.2. Test magnetic chip detector in reduction gearbox for electrical continuity.
	79-03a
	
	

	
	
	
	

	18.3. Leak check engine oil filter after installation.
	79-03
	
	

	A 0125.19 80 - STARTING - LH

	
	
	
	

	19.1. Starter generator for security of installation, electrical connectors for security.  Clean as required
	80-01-1
	
	

	
	
	
	

	1.2. Glow plug current regulators (ballast tubes) condition and security, ignition leads for security
	
	
	

	A 0125.20 80 - STARTING - RH

	
	
	
	

	20.1. Starter generator for security of installation, electrical connectors for security.  Clean as required
	80-01-1
	
	

	
	
	
	

	20.2. Glow plug current regulators (ballast tubes) condition and security, ignition leads for security.
	80-03
	
	

	
	
	
	


	MAINTENANCE ACTION
	REF
	MECH INITIALS
	RII INITIALS

	A 0125.21 OPERATIONAL CHECKS

	
	

	21.1 Perform the following Operational Checks;
	

	NOTE

Electrical power for the following tests is obtained by

connecting a ground power source or by running the

engines, whichever is more convenient
	

	21.1.1 Fuel emergency shutoff valve - Return switches to NORMAL after test. Power on.
	28-06-2
	
	

	21.1.2 Fuel crossfeed valve and (if installed), position indicator (Pre Mod 6/2009).
	28-07-2
28-07a-2
	
	

	21.1.3 HP fuel filter for leaks after element installation.
	73-06-1
	
	

	21.1.4 Fuel pump for leaks after inlet filter screen and outlet filter installation.
	73-01a
	
	

	Note: Refer to PWC Service Bulletin No. 155
	73-01b
	
	

	21.1.5 Oil filter for leaks after installation.
	79-03
	
	

	21.1.6 Fwd avionics compartment cooling fans (Mod 6/2045). (Power on).
	21-20-2
	
	

	21.1.7 DAU cooling fans (Mod 6/2045). (Power on).
	21-21-2
	
	

	21.1.8 Reversion control panel (Mod 6/2049) switch.
	31-06-3
	
	

	21.1.9 ADAHRS #1 and #2 (Mod 6/2049) reversion switches. (
	34-22-4
34-22a-4
	
	

	A 0125.22 POST INSPECTION

	
	
	
	

	21.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	21.2 Clean aircraft and engine once maintenance is completed.
	
	
	

	
	
	
	

	21.3 Perform functional check flight if required per Pratt & Whitney MM or AFM as appropriate.
	
	
	

	21.4 Check oil levels of hydraulic tank, engine prior to running aircraft.
	
	
	

	21.5 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters Viking DHC-6-400 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6-400 – A 0125 – 125 Hour Basic Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


