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Reference:  DHC-6 Maintenance Program
	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	C 1000.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	DHC-6-400
MP
	
	

	
	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	DHC-6-400

MP
	
	

	
	
	
	

	C 1000.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	
	
	
	

	C 1000.3  CORROSION CONTROL

	
	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	Appendix
C
	
	

	C 1000.4  PREPARATION

	
	
	
	

	4.1 Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	C 1000.5 21 – AIR CONDITIONING 

	
	
	
	

	5.1 Forward avionics compartment air filter for condition, security and free of obstruction.  Clean as required.
	
	
	

	Effectivity: Mod 6/2049 or 6/2014
	
	
	

	5.2 DAU cooling fan for condition and security, bonding wires for condition, security and security of attachment.
	
	
	

	Effectivity: Mod 6/2049
	
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	C 1000.6 22 – AUTO FLIGHT 

	
	
	
	

	6.1 Directional indicator and caging mechanism for proper operation, condition and security, electrical connection for security and hoses, if required, for condition and security. Clean as required.
	
	
	

	Effectivity: Pre Mod 6/2049
	
	
	

	6.2 Slaving indicator for proper operation, condition and security, electrical connection for security and hoses, if required, for condition and security. Clean as required.
	
	
	

	
	
	
	

	6.3 SM3000 Aileron servo for grounding of unit wiring bundle shield braid to airframe structure (<7.5 milliohms) .

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6221
	
	
	

	6.4 SM3000 Aileron servo for bonding of the mating surfaces between servo mount and airframe structure (<2.5 milliohms) .

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6221
	
	
	

	6.5 AFCS (Autopilot) SM3000 elevator system servo. Check bridle cable tensions.
	
	
	

	
	
	
	

	6.6 AFCS (Autopilot) SM3000 rudder system servo. Check bridle cable tensions and verify no slippage of clamps has occurred.
	
	
	

	
	
	
	

	6.7 SM3000 rudder servo for grounding of unit wiring bundle shield braid to airframe structure (<7.5 milliohms) .

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6221
	
	
	

	6.8 SM3000 Aileron servo for bonding of the mating surfaces between servo mount and airframe structure (<2.5 milliohms) .

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6221
	
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	
	
	

	6.9 KS 272A pitch trim servo for grounding of unit wiring bundle shield braid to airframe structure (<7.5 milliohms) .

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6221
	
	
	

	6.10 KS 272A pitch trim servo for bonding of the mating surfaces between servo mount and airframe structure (<2.5 milliohms) .

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6221
	22-54g
	
	

	6.11 KS 272A pitch trim system servo. Check bridle cable tensions and verify no slippage of clamps has occurred.
	22-54h
	
	

	
	
	
	

	C 1000.7 23 – COMMUNICATIONS 

	
	
	
	

	7.1 VHF upper antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	23-02c-2
	
	

	7.2 VHF upper aft antenna for condition and security, control and indicators for condition, wiring and connector for security.  Clean as required.
	23-02c-1
	
	

	Effectivity: Mod 6/2003
	
	
	

	7.3 VHF forward antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	23-02d-2
	
	

	7.4 VHF lower aft antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003 & Mod 6231
	23-02e-2
	
	

	7.5 VHF lower aft antenna for condition and security, control and indicators for condition, wiring and connector for security.  Clean as required.
	23-02e-1
	
	

	Effectivity: Mod 6/2003, SOO 6231
	
	
	

	7.6 VHF-FM antenna for condition and security, control and indicators for condition, wiring and connector for security.  Clean as required.
	23-02f-1
	
	

	Effectivity: Mod SOO 6296
	
	
	

	7.7 VHF-FM antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6296
	23-02f-2
	
	

	7.8 Pilots audio panel (KMA 29), for condition and security, bonding wires for condition and security.
	23-05-1
	
	

	Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.9 Pilots audio panel (KMA 29), for bonding of the mating surfaces between mounting tray and airframe (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6209, Mod 6/2049
	
	
	

	7.10 Co-Pilots audio panel (KMA 29), for condition and security, bonding wires for condition and security.
	23-05-1
	
	

	Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.11 Co-Pilots audio panel (KMA 29), for bonding of the mating surfaces between mounting tray and airframe (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6209, Mod 6/2049
	
	
	

	7.12 Pilot audio panel (KMA 29), emergency switch operational test.
	23-05-3
	
	

	Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.13 Co-Pilot audio panel (KMA 29), emergency switch operational test.
	23-05-3
	
	

	Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.14 Audio system (NAT 247) isolation amplifier for bonding of the mating surfaces between antenna and airframe (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	23-06-2
	
	

	7.15 Audio system (NAT 247) isolation amplifier for condition and security, bonding wires for condition and security.
	23-06-1
	
	

	Effectivity: Mod 6/2049
	
	
	

	7.16 MMDR #1 for bonding of the mating surfaces between antenna and airframe (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	23-07a-2
	
	

	7.17 MMDR #2 for condition and security, bonding wires for condition and security.
	23-07b-1
	
	

	Effectivity: Mod 6/2049
	
	
	

	7.18 MMDR #2 for bonding of the mating surfaces between antenna and airframe (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	23-07b-2
	
	

	7.19 MMDR #1 for condition and security, bonding wires for condition and security.
	23-07a-1
	
	

	Effectivity: Mod 6/2049
	
	
	

	7.20 Emergency frequency com tuning switch operational test.
	23-08
	
	

	
	
	
	

	7.21 GPS/IRIDIUM/WiFi Antenna for condition, security and corrosion, condition of external fillet seal, condition of coaxial cables and connectors and security of attachment of coaxial cables.
	23-09-1
	
	

	
	
	
	

	7.22 GPS/IRIDIUM/WiFi Antenna for bonding of the mating surfaces between antenna baseplate and airframe (<3 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: SOO 6288 or 6298
	23-09-2
	
	

	C 1000.8 24 – ELECTRICAL POWER 

	
	
	
	

	8.1 External power receptacle for condition and security. Clean as required.
	24-12
	
	

	
	
	
	

	8.2 External power receptacle for condition and security. Clean as required.
	24-12-1
	
	

	Effectivity: SOO 6371
	
	
	

	8.3 Grounding and bonding wires for condition and security. Clean as required.
	24-13
	
	

	
	34-07c
	
	

	8.4 Voltage regulators for condition and security. Clean as required.
	24-14
	
	

	
	
	
	

	C 1000.9 25 - EQUIPMENT/FURNISHINGS 

	
	
	
	

	9.1 ELT for bonding of the mating surfaces between the backshell and airframe (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	23-02c-2
	
	

	9.2 ELT Antenna bonding of the mating surfaces between the antenna and airframe (<3 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	25-07a-2
	
	

	
	
	
	

	9.3 Flight compartment axe and axe storage;
	

	9.3.1 Axe handle retention strap and elastic webbing for damage or deterioration (loss of elastic properties). Replace on condition.
	25-15a
	
	

	9.3.2 Condition and security of axe stowage structure. Condition and security of axe cutting edge and pike to axe handle.
	25-15b
	
	

	C 1000.10 27 – FLIGHT CONTROLS 


	10.1 Inspect control column (Mod 6/1433) as follows;
	

	
	

	10.1.1 Condition, security and full and free movement.
	27-01-1
	
	

	
	
	
	

	10.1.2 Brackets for condition and security, centering strut for condition, proper operation and security.
	27-01a
	
	

	
	
	
	

	10.1.3 Remove covers.
	
	
	

	
	
	
	

	10.1.4 Check for evidence of binding, chain alignment with control wheel sprockets, sprockets for condition, security and teeth wear, turnbuckles for safety.
	27-01b
	
	

	
	
	
	

	10.1.5 Control column floor boot for condition and security.
	27-01c
	
	

	
	
	
	

	10.1.6 Lubricate.
	
	
	

	
	
	
	

	10.1.7 Reinstall covers.
	
	
	

	
	
	
	

	10.2 Rudder torque tube and quadrats for condition and security, linkage and push rod installation for security.
	27-02
	
	

	
	
	
	

	10.3 Gust lock control for condition and proper operation, brackets and connecting rods for cracks, buckling and security.
	27-02a
	
	

	Note 1: Refer to Service Bulletin N. 6/508, if applicable.
	
	
	

	10.4 Rudder pedal support assembly, push rods, levers and linkage for condition and security; pedals for full and free movement; condition and security; pedals for cracking as shown in PSM 1-6-7, Part 1 Figure 2. Replace if cracked.
	27-03-1
	
	

	
	
	
	

	10.5 Inspect rudder, elevator and aileron primary control cables as follows;

Note 1: Refer to Service Bulletin N. 6/523, if applicable.

Note 2: Ensure adequate clearance with adjacent electrical conduits, structure and other systems, making allowance for vibratory motion of cable under tension.

Note 3: In the event of early or abnormal cable wear at pulley(s), replace the worn cable(s) and the corresponding pulley(s).
	

	
	

	10.5.1 Cables (from beneath flight compartment) floor to wings and empennage) for fraying corrosion, flattening, proper attachment and security.
	27-04-1
	
	

	
	
	
	

	10.5.2 Pulleys for condition and freedom of movement, pulley brackets and guides for condition and security, turnbuckles for security.
	27-04-1
	
	

	
	
	
	

	10.5.3 Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	27-04-1
	
	

	
	
	
	

	10.6 Inspect rudder flight control cables as follows
	

	
	

	10.6.1 Control and tab cables, flap/elevator interconnect and elevator trim cables for fraying kinks, flattening, corrosion and security of attachments.
	27-10c-1
	
	

	
	
	
	

	10.6.2 Cable ends with nylon sheathing, (where applicable) for condition.
	
	
	

	
	
	
	

	10.6.3 Turnbuckles for security. Replace cable where evidence of damage is found.
	27-04-1
	
	

	
	
	
	

	10.6.4 Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	27-05-1
	
	

	
	
	
	

	10.7 Inspect aileron L/H wing flight control cables as follows
	

	
	

	10.7.1 Fraying, flattening, corrosion, proper attachment and security.
	27-04-1
	
	

	
	
	
	

	10.7.2 Pulleys for condition and freedom of movement, pulley brackets and guides for condition and security, turnbuckles for security.
	27-04-1
	
	

	
	
	
	

	10.7.3 Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	27-04-1
	
	

	
	
	
	

	10.8 Inspect aileron R/H wing flight control cables as follows
	

	
	

	10.8.1 Fraying, flattening, corrosion, proper attachment and security.
	27-04-1
	
	

	
	
	
	

	10.8.2 Pulleys for condition and freedom of movement, pulley brackets and guides for condition and security, turnbuckles for security.
	27-04-1
	
	

	
	
	
	

	10.8.3 Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	27-04-1
	
	

	
	
	
	

	10.9 Inspect rudder and elevator trim tab controls as follows;
	

	
	

	10.9.1 Full and freedom of movement, cables for fraying, kinks, flattening, proper attachment and security.
	27-05-1
	
	

	
	
	
	

	10.9.2 Pulleys for freedom of operation and pulley brackets for condition and security.
	
	
	

	
	
	
	

	10.10 Do a detailed visual inspection of cable terminals as follows;
	27-05-1
	

	
	
	

	10.10.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	10.10.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	10.10.3 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	10.10.4 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	10.10.5 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.1.15.1, rig the control system.
	
	
	

	
	
	
	

	10.10.6 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	10.11 Inspect rudder gear tab mechanism as follows;
	

	
	

	10.11.1 Gearbox for condition and security of mounting plate installation and cover, tab pushrod for security and evidence of irregular operation during rudder movement.
	27-07a-1
	
	

	
	
	
	

	10.11.2 Gearbox to rudder linkage for condition and security, pushrod for security of attachments.
	27-07b

27-06b
	
	

	
	
	
	

	10.12 Inspect L/H aileron trim tab actuator as follows;
	

	
	

	10.12.1 Smooth operation and security. 
	27-08a
	
	

	
	
	
	

	10.12.2 Electrical wiring and connections for security.
	27-08b
	
	

	
	
	
	

	10.12.3 Linkages for damage, safety and security.
	27-08c
	
	

	
	
	
	

	10.12.4 Position transmitter for cleanliness, loose connections and security of mounting.
	27-08c
	
	

	
	
	
	

	10.13 Inspect R/H aileron trim tab actuator as follows;
	

	
	

	10.13.1 Smooth operation and security. 
	27-08a
	
	

	
	
	
	

	10.13.2 Electrical wiring and connections for security.
	27-08b
	
	

	
	
	
	

	10.13.3 Linkages for damage, safety and security.
	27-08c
	
	

	
	
	
	

	10.13.4 Position transmitter for cleanliness, loose connections and security of mounting.
	27-08c
	
	

	
	
	
	

	10.14 Aileron trim tab position indicator for condition and security, wiring and connectors for condition and security.
	27-08d-1
	
	

	Effectivity: Mod 6/2047
	
	
	

	10.15 Rubber, elevator and aileron position voltage check.
	27-17e

27-18e
	
	

	Effectivity: Mod 6/2047
	27-8f
	
	

	10.16 Position transmitter, inspect for security of mounting and brackets, wiring and connections for security. Clean as required.
	27-08g
27-09g
	
	

	Effectivity: Mod 6/2047
	27-17a&b
27-18a&b
	
	

	10.17 Flap position cable for fraying, flattening, corrosion and security of attachment, spring for condition, tension and security. 
	27-09f
	
	

	
	
	
	

	10.18 Flap position indicator for smooth operation.
	27-09f
	
	

	Effectivity: Mod 6/2048
	
	
	

	10.19 Flap position dracon cable cord at window frame small pulley locations for condition.
	27-09f
	
	

	
	
	
	

	10.20 Rudder pedal support assembly, push rods, levers and linkage for condition and security.
	27-03-1
	
	

	
	
	
	


	10.21 Flap/elevator interconnect, elevator trim cables and flap indicator cables for condition, fraying, corrosion, flattening and security of attachment, turnbuckles for security, pulleys for condition, security and freedom of operation.
	27-10c-1
	
	

	
	
	
	

	10.22 Do a detailed visual inspection as follows;
	27-04-4
	

	
	
	

	10.22.1 Fuselage aileron, elevator and rudder flight control cables.
	27-05-2
	
	

	
	
	
	

	10.22.2 Flap to elevator interconnect tab cables
	27-09c-2
	
	

	
	
	
	

	10.22.3 Flap selector valve and follow up cables.
	27-10c-2
	
	

	
	
	
	

	10.23 Do a detailed visual inspection of cable terminals as follows;
	27-10c-1
	

	
	
	

	10.23.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	10.23.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	10.23.3 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	10.23.4 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	10.23.5 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.18.1, rig the control system.
	
	
	

	
	
	
	

	10.23.6 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	10.24 Inspect rudder flight control cables as follows;

Note 1: Refer to Service Bulletin N. 6/523, if applicable.

Note 2: Ensure adequate clearance with adjacent electrical conduits, structure and other systems, making allowance for vibratory motion of cable under tension.

Note 3: In the event of early or abnormal cable wear at pulley(s), replace the worn cable(s) and the corresponding pulley(s).
	

	
	

	10.24.1 Cables and tab cables, flap/interconnect and elevator trim cables for fraying corrosion, kinks, flattening, proper attachment and security.
	27-10c-1
	
	

	
	
	
	

	10.24.2 Cable ends with nylon sheathing, (where applicable), for condition.
	27-4-1
	
	

	
	
	
	

	10.24.3 Turnbuckles for security. Replace cable where evidence of damage is found.
	27-5-1
	
	

	
	
	
	

	10.24.4 Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	
	
	
	

	10.25 Overhead console flight control and flap selector (Mod 6/1895) aluminum quadrants for condition and security, freedom of movement, cable attachment for security, pulley for smooth and freedom of operation.
	27-11c
76-06a
	
	

	
	
	
	

	10.26 Aileron flight control cable quadrants in cabin roof for condition and security, bearings for condition, cable guides for security. Clean as required.
	27-11d
	
	

	
	
	
	


	10.27 Elevator control lever and connecting rod for full and free movement, attaching brackets for cracks and distortion.
	27-12
	
	

	
	
	
	

	10.28 L/H wing root rib/flap pushrod support rollers for condition, wear and security, proper clearance between rod surface and roller and freedom of operation. Lubricate inside of spacer and bolt.
	27-14

27-14a
	
	

	Effectivity: Post Mod 6/1707
	
	
	

	10.29 R/H wing root rib/flap pushrod support rollers for condition, wear and security, proper clearance between rod surface and roller and freedom of operation. Lubricate inside of spacer and bolt.

	27-14

27-14a
	
	

	Effectivity: Post Mod 6/1707
	
	
	

	10.30 Stall warning cam limit microswitch mechanism and propeller reset limit switch for condition and security, connector for security.
	27-15d

61-08f
	
	

	Effectivity: Post Mod 6/1701
	
	
	

	10.31 Rudder position transmitter, inspect for security of mounting and brackets, wiring and connections for security. Clean as required.
	27-08g

27-09g

27-17a&b
	
	

	Effectivity: Mod 6/2047
	27-18a&b
	
	

	10.32 Elevator position transmitter, inspect for security of mounting and brackets, wiring and connections for security. Clean as required.
	27-08g

27-09g

27-17a&b
	
	

	Effectivity: Mod 6/2047
	27-18a&b
	
	

	C 1000.11  28 – FUEL 

	
	
	
	

	11.1 Fuel system pipes for condition, connections and hoses for security and leakage, sump plates for corrosion and leakage.  Clean as required
	28-2-2
28-10d
	
	

	Note: Refer to Service Bulletin No. 6/269 and A.D. 71-16-01, if applicable.
	
	
	

	11.2 Do a detailed visual inspection of the fuel manifold as follows;
	28-02-3
	

	Effectivity: Mod 6/2389
	
	

	11.2.1 Bonding clamp sealant and terminal lug sealant for condition and integrity, peeling, cracking or evidence of corrosion.
	
	
	

	
	
	
	

	11.2.2 Inspect bonding jumpers for condition, security, integrity and corrosion.
	
	
	

	
	
	
	

	11.2.3 If damaged, replace component, re-apply sealant.
	
	
	

	
	
	
	

	11.3 Do a detailed visual inspection of the booster pumps as follows;
	28-03-1
	

	
	
	

	11.3.1 Condition, security, corrosion and cleanliness. 
	
	
	

	
	
	
	

	11.3.2 Wiring for condition, corrosion, signs of overheat or arcing.
	
	
	

	
	
	
	

	11.3.3 Radio noise filters for security, condition and corrosion.
	
	
	

	Effectivity: Pre Mod 6/2267
	
	
	

	11.3.4 Electrical terminals for condition and deterioration of sealant.
	
	
	

	
	
	
	

	11.3.5 Electronic EMI noise filters for condition, security, sign of overheat. Resistance check and condition of electrical termination.
	28-03-3
	
	

	Effectivity: Pre Mod 6/2267
	
	
	

	11.3.6 Bleed resistors for condition, security, sign of overheat. Resistance check and condition of electrical termination.
	28-03-3
	
	

	Effectivity: Pre Mod 6/2267
	
	
	

	11.4 Fuel ejectors for condition and security. 
	28-4
	
	

	
	
	
	

	11.5 Crossfeed valve for corrosion, security and evidence of leakage.
	28-07-1
	
	

	
	
	
	

	11.6 Fuel system pipes for condition, connections and hoses for security and leakage, sump plates for corrosion and leakage.  Clean as required.
	28-2-2
28-10d
	
	

	Note: Refer to Service Bulletin No. 6/269 and A.D. 71-16-01, if applicable.
	
	
	

	11.7 Fuel low pressure switches for condition, leakage and security, electrical connector for security.
	28-11
	
	

	
	
	
	

	11.8 Coaxial electrical wiring in fuel gallery for condition, connectors for condition and security.  Clean as required.
	28-13
	
	

	For Mod 6/2390, do a detailed visual inspection of the environmental wrap for condition, integrity (split, tear or removal etc.). If deterioration is evident, remove the environmental wrap and inspect underlying components for general condition, corrosion, wiring, terminations, shield terminations. Replace damaged components and install new environmental wrap (refer to PSM1-64-2, Chapter 20-50-03).
For Mod 6/2395, do a detailed visual inspection of the backshell and backshell sealant for deterioration in the seal cavities. If deterioration is evident, clean and reseal backshell. Replace if deterioration is severe.
	
	
	

	11.9 Grounding and bounding leads for fraying, broken wires, loose connections, cleanliness.
	28-13
	
	

	For Mod 6/2390, do a detailed visual inspection of the environmental wrap for condition, integrity (split, tear or removal etc.). If deterioration is evident, remove the environmental wrap and inspect underlying components for general condition, corrosion, wiring, terminations, shield terminations. Replace damaged components and install new environmental wrap (refer to PSM1-64-2, Chapter 20-50-03).
For Mod 6/2395, do a detailed visual inspection of the backshell and backshell sealant for deterioration in the seal cavities. If deterioration is evident, clean and reseal backshell. Replace if deterioration is severe.
	
	
	

	C 1000.12  29 – HYDRAULIC POWER 

	
	
	
	

	12.1 Hydraulic accumulators for leakage and security.
	29-01b-2
	
	

	
	
	
	

	12.2 Hydraulic brake system pressure relief valve for leakage and security.
	29-01e


	
	

	
	
	
	

	12.3 Hydraulic system pressure relief valve for leakage and security.
	29-05
	
	

	
	
	
	

	12.4 Flap system thermal relief valves for leakage and security.
	29-04
	
	

	
	
	
	

	12.5 Main leg hydraulic lines for condition, leakage, loose clamps and connections for security.
	29-07
	
	

	
	
	
	

	12.6 Main leg flexible hoses for condition, leakage and connections for security.
	29-07
	
	

	
	
	
	

	C 1000.13  30 – ICE AND RAIN PROTECTION 

	
	
	
	

	13.1 Heated windshield elements and wiring for condition and security.
	30-1b
	
	

	
	
	
	

	13.2 Airframe deicing timer and connectors for condition and security.
	30-03e
	
	

	
	
	
	

	13.3 Do a detailed visual inspection of the horizontal stabilizer deicing system as follows;
	

	
	

	13.3.1 Ejector for condition and security, clear of obstruction. Clean as required.
	30-03k
	
	

	
	
	
	

	13.3.2 Distributor valve for condition, security and leakage.
	30-03f
	
	

	
	
	
	

	13.3.3 Distributor valve heating jacket for security, electrical connections for corrosion and security.
	30-03g
	
	

	
	
	
	

	13.3.4 Horizontal stabilizer pressure system indicating switches for security, electrical connections for security.
	30-03h
	
	

	
	
	
	

	13.3.5 Pipe for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	30-03j
	
	

	
	
	
	

	13.4 Do a detailed visual inspection of the L/H wing deicing system as follows;
	

	
	

	13.4.1 Distributor valves for leaks and security.
	30-03f
	
	

	
	
	
	

	13.4.2 Distributor valves heater jackets for security, electrical connections for corrosion and security.
	30-03g
	
	

	
	
	
	

	13.4.3 Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	30-03j
	
	

	
	
	
	

	13.5 Do a detailed visual inspection of the R/H wing deicing system as follows;
	

	
	

	13.5.1 Distributor valves for leaks and security.
	30-03f
	
	

	
	
	
	

	13.5.2 Distributor valves heater jackets for security, electrical connections for corrosion and security.
	30-03g
	
	

	
	
	
	

	13.5.3 Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	30-03j
	
	

	
	
	
	

	13.6 Do a detailed visual inspection of the horizontal stabilizer deicing system as follows;
	

	
	

	13.6.1 Ejector for condition and security, clear of obstructions. Clean s required.
	30-03k
	
	

	
	
	
	

	13.6.2 Distributor valves for leaks and security.
	30-03f
	
	

	
	
	
	

	13.6.3 Distributor valves heater jackets for security, electrical connections for corrosion and security.
	30-03g
	
	

	
	
	
	

	13.6.4 Pressure system indicating switches for security, electrical connections for security.
	30-03h
	
	

	
	
	
	

	13.6.5 Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	30-03j
	
	

	
	
	
	

	13.6.6 Caution light panel and cockpit dome light for condition and security.
	33-01b&c
	
	

	
	
	
	

	13.6.7 Deicing boot pressure warning lights for condition and security.
	30-03i
	
	

	Effectivity: Pre Mod 6/2028
	
	
	

	13.7 Do a detailed visual inspection of the airframe deicing system as follows;
	

	
	

	13.7.1 Timer and connectors for condition and security
	30-03e
	
	

	
	
	
	

	13.7.2 Distributor valves for leaks and security.
	30-03f
	
	

	
	
	
	

	13.7.3 Distributor valves heater jackets for security, electrical connections for corrosion and security.
	30-03g
	
	

	
	
	
	

	13.7.4 Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	30-03j
	
	

	
	
	
	

	13.7.5 Pressure system indicating switches for security, electrical connections for security.
	30-03h
	
	

	
	
	
	

	13.7.6 Ejector for condition and security, clear of obstructions. Clean s required.
	30-03k
	
	

	
	
	
	

	13.7.7 Deicing pressure and suction indicator for condition, leakage and security.
	30-03l
	
	

	
	
	
	

	C 1000.14  31 – INSTRUMENTS 

	
	
	
	

	14.1 Primary flight display unit KDU 1080 or KDU 1080-2 for condition and security, bonding wires for condition and security of attachment.
	31-03-1
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.2 Primary flight display unit KDU 1080 or KDU 1080-2, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	31-03-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	14.3 Primary flight display controller KMC2210 for condition and security, bonding wires for condition and security of attachment.
	31-03a-1
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.4 Primary flight controller KMC2210, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	31-03a-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	14.5 Multi-function display unit KDU 1080 or KDU 1080-2 for condition and security, bonding wires for condition and security of attachment
	31-04-2
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.6 Multi-function display controller KMC2220, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	31-04a-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	14.7 Multi-function display controller KMC2220 for condition and security, bonding wires for condition and security of attachment
	31-04a-1
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.8 Flight controller KMC9200 for condition and security, bonding wires for condition and security of attachment.
	31-05-1
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.9 Flight controller KMC9200, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	31-05-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	14.10 Reversion control panel for displays, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	31-06-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	14.11 Reversion control panel for displays for condition and security, bonding wires for condition and security of attachment.
	31-06-1
	
	

	
	
	
	

	14.12 ESIS display for condition and security, bonding wires for condition and security of attachment.
	31-07-1
	
	

	Effectivity: Mod 6/2049, Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.13 
	
	
	

	
	
	
	

	14.14 ESIS display, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	31-07-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.15 ESIS battery for condition and security, bonding wires for condition and security of attachment.
	31-07a-1
	
	

	Effectivity: Mod 6/2049, Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.16 ESIS battery, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	31-07a-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.17 ESIS magnetometer for condition and security, bonding wires for condition and security of attachment.
	31-07b-1
	
	

	Effectivity: Mod 6/2049 & Mod SOO 6209
	
	
	

	14.18 ESIS magnetometer, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
	31-07b-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.19 ESIS magnetometer, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
	31-07b-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.20 MAU for condition and security, bonding wires for condition and security of attachment.
	31-08-1
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.21 MAU, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
	31-08-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	14.22 MAU, verify ferrite beads are installed on the LAN wires inside the backshells of all the NIC’s (bead P/N is a Ferronics 21-727-B).
	31-08-3
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.23 MAU, visually inspect the mesh covering the air intake for dust and debris. Clean as required.
	31-08-4
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.24 MAU power supplies, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
	31-08a-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.25 MAU power supplies for condition and security, bonding wires for condition and security of attachment.
	31-08a-1
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.26 CVR for condition and security, bonding wires for condition and security of attachment.
	31-09-1
	
	

	Effectivity: Mod 6/2049 & Mod SOO 6384
	
	
	

	14.27 CVR, inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
	31-09-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.28 FDR for condition and security, bonding wires for condition and security of attachment.
	31-10-1
	
	

	Effectivity: Mod SOO 6385 Mod 6/2049 & Mod SOO 6385
	
	
	

	14.29 FDR, inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
	31-10-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6385 Mod 6/2049 & Mod SOO 6385
	
	
	

	14.30 DAU #1 & #2 for condition and security, bonding wires for condition and security of attachment.
	31-11-1
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.31 DAU #1 & #2, inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
	31-11-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	14.32 Master warning and caution indication and control inspect for condition and security, bonding wires for condition and security of attachment.
	31-12-1
	
	

	Effectivity: Mod 6/2028
	
	
	

	14.33 ECTM/FOQA (IONode 100) (SOO 6288) for condition, security and corrosion; electrical wires and connectors for security of attachment.
	31-13-1
	
	

	
	
	
	

	14.34 Inspect FDR (Mod SOO 6385) (Mod 6/2049) (Post Mod 6/2332) for;
	

	
	

	14.34.1 Condition and security; bonding wires for condition and security of attachment.
	31-10-1
	
	

	
	
	
	

	14.34.2 Bonding of the mating surfaces between the unit and airframe (< 2.5 milliohms).
	31-10-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	C 1000.15 32 – LANDING GEAR  

	
	
	

	15.1 Inspect the nosewheel steering cables forward of Sta. 60 and beneath cockpit floor as follows; 
	32-04c
	

	Effectivity: Mod 6/1800
	
	

	15.1.1 Condition, kinks, flattening, proper attachment and security.
	
	
	

	
	
	
	

	15.1.2 Pulleys for condition, freedom of operation and security.
	
	
	

	
	
	
	

	15.1.3 Turnbuckles for security.
	
	
	

	
	
	
	

	15.1.4 Do a detailed visual inspection of nosewheel cable terminals as follows;
	

	
	

	15.1.5 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	15.1.6 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	15.1.7 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	15.1.8 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	15.1.9 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.1.15.1, rig the control system.
	
	
	

	
	
	
	

	15.1.10 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	15.2 Inspect the nosewheel steering lever as follows; 
	32-06

32-04d
	

	Effectivity: Mod 6/1800
	
	

	15.2.1 Remove control column cover.
	
	
	

	
	
	
	

	15.2.2 Cables for condition, kinks, flattening, proper attachment and security.
	
	
	

	
	
	
	

	15.2.3 Pulleys for condition, freedom of operation and security.
	
	
	

	
	
	
	

	15.2.4 Turnbuckles for security.
	
	
	

	
	
	
	

	15.2.5 Do a detailed visual inspection of nosewheel cable terminals as follows;
	

	
	

	15.2.6 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	15.2.7 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	15.2.8 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	15.2.9 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	15.2.10 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.1.15.1, rig the control system.
	
	
	

	
	
	
	

	15.2.11 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	15.2.12 Steering cables for tension.
	32-07
	
	

	
	
	
	

	15.2.13 Install control column cover.
	
	
	

	
	
	
	

	15.3 Remove nose wheel.
	32-09a-3
	
	

	Note: Refer also to Special Inspection Card SP1 if applicable.
	
	
	

	15.4 Remove tire from wheel and examine for visible cracks or chipping on rims.
	
	
	

	
	
	
	

	15.5 Lubricate bearings as required.
	
	
	

	
	
	
	

	15.6 Install serviceable tire on wheel.
	
	
	

	
	
	
	

	15.7 Install serviceable nose wheel.
	
	
	

	
	
	
	

	15.8 Remove L/H main wheel.
	32-11-3
	
	

	Note: Refer also to Special Inspection Card SP1 if applicable.
	
	
	

	15.9 Remove tire from wheel and examine for visible cracks or chipping on rims.
	
	
	

	
	
	
	

	15.10 Lubricate bearings as required.
	
	
	

	
	
	
	

	15.11 Install serviceable tire on wheel.
	
	
	

	
	
	
	

	15.12 Install serviceable L/H main wheel.
	
	
	

	
	
	
	

	15.13 Remove R/H main wheel.
	32-11-3
	
	

	Note: Refer also to Special Inspection Card SP1 if applicable.
	
	
	

	15.14 Remove tire from wheel and examine for visible cracks or chipping on rims.
	
	
	

	
	
	
	

	15.15 Lubricate bearings as required.
	
	
	

	
	
	
	

	15.16 Install serviceable tire on wheel.
	
	
	

	
	
	
	

	15.17 Install serviceable R/H main wheel.
	
	
	

	
	
	
	

	15.18 Do a detailed visual inspection of L/H brake system as follows;
	32-13

32-12b
	

	15.18.1 Remove console cover.
	
	
	

	
	
	
	

	15.18.2 Parking brake rods and linkage for signs of wear and security.
	
	
	

	
	
	
	

	15.18.3 Lubricate cams.
	
	
	

	
	
	
	

	15.18.4 Wheel brake valve for leakage and security.
	
	
	

	
	
	
	

	15.18.5 Clean as required.
	
	
	

	
	
	
	

	15.18.6 Reinstall console cover.
	
	
	

	
	
	
	

	15.19 Do a detailed visual inspection of R/H brake system as follows;
	32-13

32-12b
	

	15.19.1 Remove console cover.
	
	
	

	
	
	
	

	15.19.2 Parking brake rods and linkage for signs of wear and security.
	
	
	

	
	
	
	

	15.19.3 Lubricate cams.
	
	
	

	
	
	
	

	15.19.4 Wheel brake valve for leakage and security.
	
	
	

	
	
	
	

	15.19.5 Clean as required.
	
	
	

	
	
	
	

	15.19.6 Reinstall console cover.
	
	
	

	
	
	
	

	15.20 Do a detailed visual inspection of main gear fairings as follows;
	32-14-

1 thru 3
	

	15.20.1 Remove center fairings.
	
	
	

	
	
	
	

	15.20.2 Cracks, delamination and security.
	
	
	

	
	
	
	

	15.20.3 Seals for tears, deterioration and security.
	
	
	

	
	
	
	

	15.20.4 Fairing supporting structure for cracks, corrosion, buckling and loose anchor nuts.
	
	
	

	
	
	
	

	15.20.5 Roller blind assembly for adequate spring tension, blind for fraying, tears and security.
	
	
	

	
	
	
	

	15.20.6 Roller for free running and security.
	
	
	

	
	
	
	

	15.20.7 Welds for cracks at tubes, lugs, pivot fittings and brake flange ale housing.
	32-14-04
	
	

	Note: Refer to PSM1-6-7 Part 3, Figure 8 for leg weld locations.
	
	
	

	15.20.8 Reinstall center fairings.
	
	
	

	
	
	
	

	15.21 Inspect shock absorber blocks for condition, free from oil, grease, deterioration, splitting on surface adjacent to bolt holes and displacement of blocks. Discard blocks that have sustained permanent set due to displacement beyond edge of scuff plate. Clean as required.
	32-15-1
	
	

	Note: Displacement within boundaries of scuff plate edge is allowable and not detrimental to aircraft safety. Inspect for bubbles close to vertical surface of block by smearing surface with water and using a strong light viewed from opposite side of block. For bubble criteria, refer to Maintenance Manual.
	
	
	

	15.22 Main landing gear upper and lower fuselage attachment fittings for condition and security.
	32-18
	
	

	
	
	
	

	C 1000.16 33 – LIGHTS 

	
	
	
	

	16.1 Pilot/Co-pilot panel and instrument lights for condition and security.
	33-01a
	
	

	Effectivity: Pre Mod 6/2028
	
	
	

	16.2 Caution light panel for condition and security.
	33-01b
33-01c
	
	

	16.3 Horizontal stabilizer deicing boot pressure warning lights for condition and security.
	30-03i
	
	

	Effectivity: Pre Mod 6/2028
	
	
	

	16.4 Co-pilot dimming control rheostat for condition and clear from cable routing
	33-01d
	
	

	Effectivity: Pre Mod 6/2028
Note: Refer to Service Bulletin No. 6/401, if applicable.
	
	
	

	16.5 Do a visual inspection of the following lights for condition and security, bonding wires for condition and security of attachment;

Effectivity: Mod 6/2028
	

	16.5.1 Instrument panel, panel overlay and compass
	33-1e-1
33-1f-1
	
	

	16.5.2 Flight compartment flood lights, aisle, eye reference, avionics CB post, instrument panel and visor lights.
	33-1g-1
	
	

	
	
	
	

	16.5.3 Flight compartment instrument panel, trim panel static valve post and selector lights.
	33-1g-1
	
	

	
	
	
	

	16.5.4 Flight compartment dome
	33-1h-1
	
	

	
	
	
	

	16.5.5 Map lights
	33-1i-1
	
	

	
	
	
	

	16.5.6 Caution lights dimming
	33-1j-1
	
	

	
	
	
	

	16.6 Do a visual inspection of the following exterior lights for condition and security, bonding wires for condition and security of attachment;

Effectivity: Mod 6/2028
	

	16.6.1 Position and strobe
	33-2f-1
	
	

	
	
	
	

	16.6.2 Aircraft exterior position and strobe
	33-2f-1
	
	

	
	
	
	

	16.6.3 Wing tip position and strobe for condition and security, wing tip rib installation for condition.
	33-02a-1

	
	

	Effectivity: Pre Mod 6/1513 AND 6/2028

Note: Refer to Service Bulletin No. 6/318 and A.D 76-13-06, if applicable (Pre Mod 6/2028)
	33-02e
	
	

	16.6.4 Aircraft exterior beacon
	33-2g-1
	
	

	
	
	
	

	16.6.5 Aircraft exterior landing
	33-2h-1
	
	

	Effectivity: Mod 6/2028, 6/2285, 6/2407
	
	
	

	16.6.6 Aircraft exterior wing inspection lights
	33-2i-1
	
	

	
	
	
	

	16.6.7 Position, anti-collision and strobe for condition and security.
	33-02a-1


	
	

	Effectivity: Pre Mod 6/1513 AND 6/2028

Note: Refer to Service Bulletin No. 6/57 and A.D 67-33-01 (Pre Mod 6/116), if applicable (Pre Mod 6/2028)
	33-02b-1&2

33-02d-1


	
	

	16.7 Passenger Warning and passenger lights for condition and security.
	33-03a&b
	
	

	Effectivity: Pre Mod 6/2028
	
	
	

	16.8 Cabin interior boarding lights
	33-3c-1
	
	

	Effectivity: Mod 6/2028
	
	
	

	16.9 Cabin interior lighting
	33-3d-1
	
	

	Effectivity: Mod 6/2028, 6/2427
	
	
	

	16.9.1 
	
	
	

	
	
	
	

	C 1000.17 34 - NAVIGATION 

	
	
	
	

	17.1 #1 ADF loop antenna cover for condition, moister ingress and security, connectors and insulation for security. Clean as required.
	34-01c
	
	

	Effectivity: Pre Mod 6/2003
	
	
	

	17.2 #2 ADF loop antenna cover for condition, moister ingress and security, connectors and insulation for security. Clean as required.
	34-01c
	
	

	Effectivity: Pre Mod 6/2049
	
	
	

	17.3 #1 ADF indicator for condition and security, cables and connectors for security. Clean as required.
	34-01f
	
	

	Effectivity: Pre Mod 6/2049
	
	
	

	17.4 #2 ADF indicator for condition and security, cables and connectors for security. Clean as required.
	34-01f
	
	

	Effectivity: Pre Mod 6/2049
	
	
	

	17.5 #1 VOR antenna for evidence of leakage at structure and loose connections, antenna disconnect for security.
	34-02b
	
	

	Effectivity: Pre Mod 6/2003
	
	
	

	17.6 #2 VOR antenna for evidence of leakage at structure and loose connections, antenna disconnect for security.
	34-02b
	
	

	Effectivity: Pre Mod 6/2003
	
	
	

	17.7 #1 VOR antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	34-02d
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	17.8 #2 VOR antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	34-02d
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	17.9 #1 Glide Slope antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	34-03c
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	17.10 #2 Glide Slope antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	34-03c
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	17.11 Marker beacon antenna for condition, loose connections, entry of moisture and security.
	34-04c
	
	

	
	
	
	

	17.12 Marker beacon antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	34-04d
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	17.13 Weather radar transmitter and receiver (RDR2000) inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
	34-06e
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	17.14 Nav systems grounding and bonding wires for condition and security.  Clean as required.
	24-13
34-07c
	
	

	
	
	
	

	17.15 Do a visual inspection of the following navigation instruments for condition and security, electrical connection for security and hoses, if required, for condition and security. Clean as required.;

Effectivity: Mod 6/2028
	

	17.15.1 Turn and Slip indicator
	34-08a-1
	
	

	Effectivity: Pre Mod 6/2049
	
	
	

	17.15.2 Directional indicator and caging mechanism for proper operation.
	34-08b-1
22-43a
	
	

	Effectivity: Pre Mod 6/2049
	
	
	

	17.15.3 Airspeed Indicator.
	34-08c-1
	
	

	Effectivity: Pre Mod 6/2049
	
	
	

	17.15.4 Attitude indicator and caging mechanism for proper operation.
	34-08d-1
	
	

	Effectivity: Pre Mod 6/2049
	
	
	

	17.15.5 Vertical speed Indicator.
	34-08e
	
	

	Effectivity: Pre Mod 6/2049
	
	
	

	17.15.6 Altimeter.
	34-08f-1
	
	

	Effectivity: Pre Mod 6/2049

Note: Refer to Serice Bulletin No. 6/349, if apllicable.
	
	
	

	17.15.7 Standby Compass.
	34-08g-1
	
	

	
	
	
	

	17.15.8 Radio Magnetic Indicator and Annunciator (if fitted).
	34-08j&k

22-43
	
	

	Effectivity: Pre Mod 6/2049

Note: Refer to Serice Bulletin No. 6/349 and A.D 76-07-09, if apllicable.
	
	
	

	17.15.9 C14 Gyro Compass Control Head Unit.
	34-14a
	
	

	Effectivity: Pre Mod 6/2049
	
	
	

	17.16 Transponders; KXP 2290 or 2290A
	
	
	

	
	
	
	

	17.16.1 Perform a power on operational test.
	34-15-2
	
	

	
	
	
	

	17.16.2 Inspect bonding of mating surfaces between mounting tray and the nearest airframe ground. (<2.5 milliohms).
	34-15-3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.16.3 #1 lower antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	34-15a-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.16.4 #2 lower antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	34-15a-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.16.5 #1 upper antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	34-15b-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.16.6 #2 upper antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	34-15b-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.17 #1 GPS (KGS 200)
	

	Effectivity: Mod 6/2049, Post Mod 6/2304 & Mod SOO 6388
	

	17.17.1 Inspect for condition and security, bonding wires for condition and security of attachment.
	34-16-1
	
	

	
	
	
	

	17.17.2 Perform a power on operational test.
	34-16-2
	
	

	
	
	
	

	17.17.3 Inspect antenna bonding of mating surfaces between mounting tray and the nearest airframe ground. (<3.0 milliohms).
	34-16b-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.17.4 Antenna for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
	34-16b-1
	
	

	Effectivity: Mod SOO 6388 and Mod 6/2003
	
	
	

	17.18 #2 GPS (KGS 200)
	

	Effectivity: Mod 6/2049, Post Mod 6/2304 & Mod SOO 6388
	

	17.18.1 Inspect for condition and security, bonding wires for condition and security of attachment.
	34-16a-1
	
	

	
	
	
	

	17.18.2 Perform a power on operational test.
	34-16a-2
	
	

	
	
	
	

	17.18.3 Inspect antenna bonding of mating surfaces between mounting tray and the nearest airframe ground. (<3.0 milliohms).
	34-16c-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.18.4 Antenna for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
	34-16c-1
	
	

	Effectivity: Mod SOO 6388 and Mod 6/2003
	
	
	

	17.19 #1 DME (KN63)
	

	Effectivity: Mod 6/2049 & Mod SOO 6388
	

	17.19.1 Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	34-17-1
	
	

	
	
	
	

	17.19.2 Perform power on operational test of transceiver unit.
	34-17-2
	
	

	
	
	
	

	17.19.3 Inspect transceiver unit bonding of mating surfaces between mounting tray and the nearest airframe ground. (<2.5 milliohms).
	34-17-3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.19.4 Inspect center fuselage antenna bonding of mating surfaces between mounting tray and the nearest airframe ground. (<3.0 milliohms).
	34-17a-3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.20 #2 DME (KN63)
	

	Effectivity: Mod 6/2049 & Mod SOO 6388
	

	17.20.1 Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	34-17a-1
	
	

	
	
	
	

	17.20.2 Perform power on operational test of transceiver unit.
	34-17a-2
	
	

	
	
	
	

	17.20.3 Inspect transceiver unit bonding of mating surfaces between mounting tray and the nearest airframe ground. (<2.5 milliohms).
	34-17a-3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.20.4 Inspect antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	34-17c-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.21 #1 Radar Altimeter Unit
	

	Effectivity: Mod 6/2049 & Mod SOO 6388
	

	17.21.1 Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	34-18-1
	
	

	
	
	
	

	17.21.2 Perform power on operational test of radar altimeter unit.
	34-18-2
	
	

	
	
	
	

	17.21.3 Inspect bonding of mating surfaces between mounting tray airframe ground. (<2.5 milliohms).
	34-18-3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.21.4 Inspect antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	34-18b-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003 & Mod SOO 6388
	
	
	

	17.22 #2 Radar Altimeter Unit
	

	Effectivity: Mod 6/2049 & Mod SOO 6218
	

	17.22.1 Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	34-18a-1
	
	

	
	
	
	

	17.22.2 Perform power on operational test of radar altimeter unit.
	34-18a-2
	
	

	
	
	
	

	17.22.3 Inspect bonding of mating surfaces between mounting tray and airframe ground. (<2.5 milliohms).
	34-18a-3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.22.4 Inspect antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	34-18c-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003 & Mod SOO 6388
	
	
	

	17.23 #1 TCAS I Processor Unit (KTA 970)
	

	Effectivity: Mod 6/2049 & Mod SOO 6382
	

	17.23.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	34-19-1
	
	

	
	
	
	

	17.23.2 Perform power on operational test of processor unit.
	34-19-2
	
	

	
	
	
	

	17.23.3 Inspect bonding of mating surfaces between mounting tray airframe ground. (<2.5 milliohms).
	34-19-3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.23.4 Inspect upper antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	34-19b-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003 & Mod SOO 6382
	
	
	

	17.23.5 Inspect lower antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	34-19d-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003 & Mod SOO 6382
	
	
	

	17.24 #2 TCAS II Processor Unit (KTA 970)
	

	Effectivity: Mod 6/2049 & Mod SOO 6219
	

	17.24.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	34-19a-1
	
	

	
	
	
	

	17.24.2 Perform power on operational test of processor unit.
	34-19a-2
	
	

	
	
	
	

	17.24.3 Inspect bonding of mating surfaces between mounting tray and airframe ground. (<2.5 milliohms).
	34-19a-3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.24.4 Inspect upper antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	34-19c-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003 & Mod SOO 6219
	
	
	

	17.25 EGPWS (MK VI)
	

	Effectivity: Mod 6/2049 & Mod SOO 6387
	

	17.25.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	34-20-1
	
	

	
	
	
	

	17.25.2 Perform power on operational test of EGPWS unit.
	34-20-2
	
	

	
	
	
	

	17.25.3 Inspect bonding of mating surfaces between mounting tray and airframe ground. (<2.5 milliohms).
	34-20-3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.26 #1 ADAHRS (KSG 7200)
	

	Effectivity: Mod 6/2049
	

	17.26.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	34-22-1
	
	

	
	
	
	

	17.26.2 Perform power on operational test of EGPWS unit.
	34-22--2
	
	

	
	
	
	

	17.26.3 Inspect bonding of mating surfaces between mounting tray and airframe ground. (<1.0 milliohms).
	34-22--3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.27 #2 ADAHRS (KSG 7200)
	

	Effectivity: Mod 6/2049 & Mod SOO 6209
	

	17.27.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	34-22a-1
	
	

	
	
	
	

	17.27.2 Perform power on operational test of EGPWS unit.
	34-22a--2
	
	

	
	
	
	

	17.27.3 Inspect bonding of mating surfaces between mounting tray and airframe ground. (<1.0 milliohms).
	34-22a--3
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.28 ADAHRS (KSG 7210)
	

	Effectivity: Mod 6/2049 & Mod SOO 6209 and Pre Mod 6/2171
	

	17.28.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	34-22b-1
	
	

	
	
	
	

	17.28.2 Inspect bonding of mating surfaces between mounting feet and airframe structure. (<2.5 milliohms).
	34-22b-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.29 #1 ADF Antenna
	

	Effectivity: Mod 6/2003 & Mod SOO 6209
	

	17.29.1 Inspect bonding of mating surfaces between the antenna and the airframe ground. (<3.0 milliohms).
	34-23-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.30 #2 ADF Antenna
	

	Effectivity: Mod 6/2003 & Mod SOO 6209
	

	17.30.1 Inspect bonding of mating surfaces between the antenna and the airframe ground. (<3.0 milliohms).
	34-24-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.30.2 
	
	
	

	
	
	
	

	C 1000.18 36 - PNEUMATIC 

	
	
	
	

	18.1 Instrument pneumatic system filter for long nose aircraft with (Mod 6/1046) bleed air or (Mod 6/1166) engine driven pump systems.
	36-02e
	
	

	
	
	
	

	18.2 Remove and install new filters and leak check.
	36-03i
	
	

	
	
	
	

	18.3 
	36-02h
	
	

	
	
	
	

	C 1000.19 44 – CABIN SYSTEMS 

	
	
	
	

	19.1.1 Inspect grounding of cabin speakers and airframe structure. (<2.5 milliohms).
	44-01-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6/221 & Mod 6/2049
	
	
	

	19.2 NAT 245 PA Amplifier
	

	Effectivity: Mod SOO 6/2010 & Mod 6/2049
	

	19.2.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	44-02-1
	
	

	
	
	
	

	19.2.2 Inspect grounding of unit wire bundle shield braid to airframe structure. (<2.5 milliohms).
	44-02-2
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	19.3 
	
	
	

	
	
	
	

	C 1000.20 52 – DOORS

	
	
	
	

	20.1 Flight compartment RH and LH doors to airframe for bonding. (<10 milliohms).
	52-01b
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2024
	
	
	

	20.2 Cabin RH and LH doors to airframe for bonding. (<10 milliohms).
	52-02b
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2024
	
	
	

	20.3 Airstair door to airframe for bonding. (<10 milliohms).
	52-03e
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2024
	
	
	

	20.4 Aft baggage compartment door to airframe for bonding. (<10 milliohms).
	52-05c
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2024
	
	
	

	20.5 Fwd baggage compartment door to airframe for bonding. (<10 milliohms).
	52-05c
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2020 & Mod 6/2161
	
	
	

	C 1000.21 53 – FUSELAGE 

	
	
	
	

	21.1 External structure for dents, scores, fretting and cracks, fasteners for security.
	53-01-2
	
	

	
	
	
	

	21.2 Radome for condition, cracks, delamination and security.
	53-03
	
	

	
	
	
	

	21.3 Nose baggage compartment to radome joint diverter strip (qty 4) for electrical bonding. (<10 milliohms).
	53-03a
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	21.4 Radio equipment racks for cracks, buckling and corrosion.  Vibration isolators for deterioration.  Clean as required.
	53-05-2
	
	

	
	
	
	

	21.5 Rear baggage compartment for condition. Equipment shelves for cracks, buckling and corrosion.  Clean as required.
	53-05-3
	
	

	Note:  In addition, when Mod 6/2020 or Mod 6/2160 is installed at STA 44.0 nose attachment, pay particular attention for the corrosion to the exterior aluminum joint straps and fasteners common to the carbon nose.
	
	
	

	21.6 Fuel gallery structure for corrosion.
	53-05-4
	
	

	
	
	
	

	21.7 Inspect fuel gallery access panels and seals for damage. Repair or replace as required.
	53-05-5
	
	

	Effectivity: Mod 6/2408
	
	
	

	21.8 Nose baggage bulkhead at STA 15.45 for condition, security and corrosion between aluminum brackets and fasteners attached to the carbon nose.
	53-05-6
	
	

	
	
	
	

	21.9 Cargo tie-downs located on STA 15.45 bulkhead for condition and security.
	53-05-7
	
	

	
	
	
	

	21.10 Fuselage forward spar adapters for condition, corrosion, cracks and fasteners for security.
	53-12
	
	

	Effectivity: Pre Mod 6/1189
	
	
	

	21.11 Inspect the nose baggage compartment weather radar wiring metal conduit to airframe for electrical bonding. (<10 milliohms).
	53-19-1
	
	

	Effectivity: Mod 6/2020 & 6/2160
	
	
	

	21.12 Inspect the nose baggage compartment fuselage circumferential aluminum strap joint for electrical bonding. (<10 milliohms).
	53-19-2
	
	

	Effectivity: Mod 6/2020 & 6/2160
	
	
	

	21.13 Ensure bonding jumpers in nose baggage compartment have no sign of corrosion, braid damage such as kinks, fretting or fraying, cracked or broken terminal ends.
	53-19-3
	
	

	
	
	
	

	21.14 Inspect forward avionics compartment shelves to airframe for bonding. (<2.5 milliohms).
	53-20-1
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2005
	
	
	

	21.15 Inspect forward avionics compartment shelves bonding jumpers have no sign of corrosion, braid damage such as kinks, fretting or fraying, cracked or broken terminal ends. 

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	53-20-2
	
	

	Effectivity: Mod 6/2005
	
	
	

	21.16 Inspect aft avionics compartment shelves to airframe for bonding. (<2.5 milliohms).
	53-21-1
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2028
	
	
	

	21.17 Ensure aft avionics equipment shelves bonding jumpers have no sign of corrosion, braid damage such as kinks, fretting or fraying, cracked or broken terminal ends.
	53-21-2
	
	

	Effectivity: Mod 6/2028
	
	
	

	21.18 
	
	
	

	
	
	
	

	C 1000.22 54 – NACELLE - LH

	
	
	
	

	22.1 Nacelle fairing to airframe for bonding. (<10 milliohms).
	54-01a
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2021
	
	
	

	22.2 
	
	
	

	
	
	
	

	C 1000.23 54 – NACELLE - RH

	
	
	
	

	23.1 Nacelle fairing to airframe for bonding. (<10 milliohms).
	54-01a
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2021
	
	
	

	23.2 .
	
	
	

	
	
	
	

	C 1000.24 55 – STABILIZER - LH

	
	
	
	

	24.1 Mid hinge arm adapter place for condition, corrosion, fasteners for security and bearings for condition
	55-02f-1
	
	

	Effectivity: Pre Mod 6/1341
	
	
	

	24.2 .
	
	
	

	
	
	
	

	C 1000.25 55 – STABILIZER - RH

	
	
	
	

	25.1 Mid hinge arm adapter place for condition, corrosion, fasteners for security and bearings for condition
	55-02f-1
	
	

	Effectivity: Pre Mod 6/1341
	
	
	

	25.2 .
	
	
	

	
	
	
	

	C 1000.26 56 – WINDOWS

	
	
	
	

	26.1 Flight compartment windshield and door windows for condition, crazing and security, retaining strips for condition and security of attachment. For SOO 6320 or 6321, if installed, inspect vent for condition and security of attachment. Replace as required.
	56-01a-2
56-01b
	
	

	
	
	
	

	26.2 Flight compartment LH and RH doors to airframe for bonding. (<10 milliohms).
	52-01b
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6024
	
	
	

	26.3 Cabin windows for condition, crazing and security. Inspect vents (SOO 6368) for condition and security of attachment.  Replace if required.
	56-02b
	
	

	
	
	
	

	26.4 Cabin side escape hatch windows for condition, crazing and security. Replace if required.
	56-02c
	
	

	
	
	
	

	26.5 Cabin door windows for condition, crazing and security. Replace if required.
	56-02d
	
	

	
	
	
	

	26.6 .
	
	
	

	
	
	
	

	C 1000.27 57 – WING – LH 

	
	
	
	

	27.1 All accessible electrical wiring for deterioration, chafing, bonding wire for fraying, corrosion and security of attachment, connector for cleanliness and security.
	57-07-2
	
	

	
	
	
	

	27.2 Outboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
	57-15a
	
	

	
	
	
	

	27.3 Inboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
	57-15a
	
	

	
	
	
	

	27.4 Outboard foreflap pushrod fork attachment for corrosion and security of attachment.
	57-20a
	
	

	
	
	
	

	27.5 Inboard foreflap pushrod fork attachment for corrosion and security of attachment.
	57-20a
	
	

	
	
	
	

	27.6 Do a detailed visual inspection of the aileron as follows;
	

	
	

	27.6.1 Nose and tail skins for condition, dents, scores, abrasions and fasteners for security.
	57-17a
	
	

	
	
	
	

	27.6.2 Trim and gear tab hinge adapter for corrosion, wear, security and freedom of movement. Lubricate.
	57-17e
	
	

	
	
	
	

	27.6.3 Bellcrank structure channels for condition, fasteners for security, bearings for freedom of operation and security.
	57-18
	
	

	
	
	
	

	27.6.4 Aileron trim and gear tab skins for condition, buckling and fasteners for security.
	57-19a
	
	

	
	
	
	

	27.6.5 Hing arms for condition, corrosion and security.
	57-19b
	
	

	
	
	
	

	27.6.6 Trim tab hinge for condition, corrosion, wear and freedom of movement. Lubricate.
	57-19c
	
	

	
	
	
	

	27.6.7 
	
	
	

	
	
	
	

	C 1000.28 57 – WING – RH 

	
	
	
	

	28.1 All accessible electrical wiring for deterioration, chafing, bonding wire for fraying, corrosion and security of attachment, connector for cleanliness and security.
	57-07-2
	
	

	
	
	
	

	28.2 Outboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
	57-15a
	
	

	
	
	
	

	28.3 Inboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
	57-15a
	
	

	
	
	
	

	28.4 Outboard foreflap pushrod fork attachment for corrosion and security of attachment.
	57-20a
	
	

	
	
	
	

	28.5 Inboard foreflap pushrod fork attachment for corrosion and security of attachment.
	57-20a
	
	

	
	
	
	

	28.6 Do a detailed visual inspection of the aileron as follows;
	

	
	

	28.6.1 Nose and tail skins for condition, dents, scores, abrasions and fasteners for security.
	57-17a
	
	

	
	
	
	

	28.6.2 Trim and gear tab hinge adapter for corrosion, wear, security and freedom of movement. Lubricate.
	57-17e
	
	

	
	
	
	

	28.6.3 Bellcrank structure channels for condition, fasteners for security, bearings for freedom of operation and security.
	57-18
	
	

	
	
	
	

	28.6.4 Aileron trim and gear tab skins for condition, buckling and fasteners for security.
	57-19a
	
	

	
	
	
	

	28.6.5 Hing arms for condition, corrosion and security.
	57-19b
	
	

	
	
	
	

	28.6.6 Trim tab hinge for condition, corrosion, wear and freedom of movement. Lubricate.
	57-19c
	
	

	
	
	
	

	28.6.7 
	
	
	

	
	
	
	

	C 1000.29 61 – PROPELLERS – LH 

	
	
	
	

	29.1 Stall warning cam limit microswitch mechanism and propeller reset limit switch for condition and security, connect for security.
	27-15d

61-08f
	
	

	
	
	
	

	C 1000.30 61 – PROPELLERS – RH 

	
	
	
	

	30.1 Stall warning cam limit microswitch mechanism and propeller reset limit switch for condition and security, connect for security.
	27-15d
61-08f
	
	

	
	
	
	

	C 1000.31 71 – POWERPLANT - LH

	
	
	
	

	31.1 Remove intake deflector air line filters at inlet and return ports of air control valves.
	71-01f
	
	

	
	
	
	

	31.2 Inspect intake deflector air line filters at inlet and return ports of air control valves.
	71-01f
	
	

	
	
	
	

	31.3 Install intake deflector air line filters at inlet and return ports of air control valves.
	71-01f
	
	

	
	
	
	

	C 1000.32 71 – POWERPLANT - RH

	
	
	
	

	32.1 Remove intake deflector air line filters at inlet and return ports of air control valves.
	71-01f
	
	

	
	
	
	

	32.2 Inspect intake deflector air line filters at inlet and return ports of air control valves.
	71-01f
	
	

	
	
	
	

	32.3 Install intake deflector air line filters at inlet and return ports of air control valves.
	71-01f
	
	

	
	
	
	

	C 1000.33 73 – ENGINE FUEL AND CONTROL – LH 

	
	
	
	

	33.1 Remove and discard P3 filter element.
	73-09-2
	
	

	
	
	
	

	33.2 Install new P3 filter element.
	73-09-2
	
	

	
	
	
	

	C 1000.34 73 – ENGINE FUEL AND CONTROL – RH 

	
	
	
	

	34.1 Remove and discard P3 filter element.
	73-09-2
	
	

	
	
	
	

	34.2 Install new P3 filter element.
	73-09-2
	
	

	
	
	
	

	C 1000.35 76 – ENGINE CONTROLS 

	
	
	
	

	35.1 Overhead console flight control and flap selector aluminum quadrants for condition and security, freedom of movement, cable attachment for security.
	27-11c
	
	

	
	
	
	

	35.2 Overhead console flight control and flap selector pulleys for smoothness and freedom of operation.
	76-06a
	
	

	
	
	
	

	C 1000.36 80 – STARTING – LH 

	
	
	
	

	36.1 Starter generator brushes for condition and wear.
	80-01-2
	
	

	
	
	
	

	36.2 Drive splines for wear. Lubricate
	80-01-2
	
	

	
	
	
	

	36.3 Spark igniters for condition and security. Check for operation.
	80-04a
	
	

	
	
	
	

	36.4 Spark ignitor box for condition and security.
	80-04b
	
	

	
	
	
	

	36.5 Starter generator electrical wiring for condition, insulation for deterioration and connectors for security. Clean as required.
	80-05
	
	

	
	
	
	

	C 1000.37 

	
	
	
	

	37.1 
	
	
	

	
	
	
	

	37.2 
	
	
	

	
	
	
	

	37.3 
	
	
	

	
	
	
	

	C 1000.38 POST INSPECTION

	
	
	
	

	38.1 Inspect for operation and leaks.
	
	
	

	
	
	
	

	38.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	38.3 Clean aircraft and engine once maintenance is completed.
	
	
	

	
	
	
	

	38.4 Perform Functional Check Flight if required per DHC-6-400 Maintenance Manual or AFM as appropriate.
	
	
	

	
	
	
	

	38.5 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	

	
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6-400 – C 1000RT – 1000 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


