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1
AIRWORTHINESS LIMITATIONS
NOTE: The entire airframe must be removed from service at or before the end of the validated life at 66,000 flight Hours, or 312,000 Flight Cycles, whichever occurs first.
1.1 Compliance of all airworthiness Inspections must be completed by the limits specified in the below table.  Each inspection shall be entered either in a work order or the aircraft log book as appropriate and remain a permanent record until repeated.
1.2 The appropriate maintenance manual shall be referenced when performing each event. 

	TASK
	ITEM DESCRIPTION
	EFFECTIVITY/

CONFIGURATION
	AIRWORTHINESS LIMITATIONS
	ACTION NOTES

	
	
	
	SAFE LIFE LIMIT EXCEPTIONS FROM AIRFRAME LIMIT
	MODIFICATION LIMIT
	INSPECTION OR OVERHAUL
	

	
	
	
	
	
	INITIAL
	REPEAT
	


	32 – FLIGHT CONTROLS

	27-002
	Elevator and Rudder

Primary Flight

Control Cables
	Landplanes
	60 Months
	-
	-
	-
	Replace

	27-004
	Elevator and Rudder

Primary Flight

Control Cables below

Baggage Floor
	All Configurations

If spillage occurs

when operating with

corrosive cargo
	Within 2 Months of

spillage
	-
	-
	-
	Replace

	27-006
	Aileron Primary Flight

Control Cables
	All Configurations
	60 Months
	-
	-
	-
	Replace

	27-007
	Elevator and Rudder

Cable Pulleys at

Sta 270.3
	All Configurations
	60 Months
	-
	-
	-
	Replace

	32 – LANDING GEAR

	32-001
	Main Landing

Gear Leg
	All Configurations

with New Main

Landing Gear Leg

with No Previous

Overhaul and No

Previous Repair
	Safe Life Limit

Not Applicable
	-
	24,000

Landings or 120

Months

whichever

occurs first
	-
	Remove

Overhaul in

accordance with

TB V6/00063 Rev. NC

or later

	32-002
	Main Landing

Gear Leg
	All Configurations

with Previous

Overhaul or

Previous Repair
	Safe Life Limit

Not Applicable
	-
	
	7,000

Landings or

60 Months

whichever

occurs first
	Remove

Overhaul in

accordance with

TB V6/00063

Rev. NC or later

	53 – FUSELAGE

	53-005
	Fuselage Frame

Assembly, Sta. 218.8,

Part No. C6FSM2582–1
	Post Mod 6/1173
	-
	39,000 Flight

Hours or 78,000

Flight Cycles

whichever

occurs first
	-
	-
	Remove this frame

assembly from

service and replace

with a new assembly

C6MK1553–1 
or –3

Incorporating

Mod 6/1553

(Refer to SB 6/354)


	TASK
	ITEM DESCRIPTION
	EFFECTIVITY/

CONFIGURATION
	AIRWORTHINESS LIMITATIONS
	ACTION NOTES

	
	
	
	SAFE LIFE LIMIT EXCEPTIONS FROM AIRFRAME LIMIT
	MODIFICATION LIMIT
	INSPECTION OR OVERHAUL
	

	
	
	
	
	
	INITIAL
	REPEAT
	


	53 – FUSELAGE (Cont’d)

	53-006
	Fuselage Frame

Assembly, 
Sta. 239
	All Configurations
	-
	-
	1,200 Flight

Hours or

12 Months

whichever

occurs first
	Every 1,200

Flight Hours or

12 Months

whichever

occurs first
	If cracks are within limits in accordance

with SB 6/521 Rev. C or

later, inspect every 600 Flight Hours or

6 Months whichever

occurs first. Replace or

repair if cracks are out of limits.

	54 – NACELLES

	54-002
	Engine Nacelle

Structure
	All Configurations
	-
	-
	3,000 Flight

Hours or 6,000

Flight Cycles

whichever

occurs first
	Every 3,000

Flight Hours or

6,000 Flight

Cycles

whichever

occurs first
	Inspect the left side of each nacelle structure

(Refer to 
PSM 1-6-7

Part 3)

	54-009
	Engine Nacelle

Lower Longerons
	Aircraft that are not

addressed by

54-003 through

54-008
	-
	-
	400 
Flight Hours
	Every 400 Flight Hours
	Inspect lower

longerons for buckles or

cracks on each nacelle structure

(Refer to SB 6/509)

	54-010
	Engine Nacelle

Lower Longerons
	All Configurations

After Hard Landing
	-
	-
	Immediate
	Immediate
	Inspect lower

longerons for buckles or

cracks on each nacelle structure

(Refer to SB 6/509)

	57 – WINGS

	57-026
	Wing Assembly

C6W1001–33, –35,

& subsequent

Wing Box

C6W1002–67, –69,

& subsequent
	Post Mod 6/1117

and

Pre Mod 6/1630

and

Pre Mod 6/1318
	-
	12,000 Flight

Hours or 24,000

Flight Cycles
	-
	-
	Incorporate Mod 6/1318

(Refer to 
SB 6/268)

	57-027
	Wing Assembly

C6W1001–33, –35,

& subsequent

Wing Box

C6W1002–67, –69,

& subsequent
	Post Mod 6/1117

and

Pre Mod 6/1630

and

Pre Mod 6/1318
	-
	-
	12,000 Flight

Hours or 24,000

Flight Cycles

whichever

occurs first
	Every 1,200

Flight Hours or

2,400 Flight

Cycles

whichever

occurs first
	Inspect Main Spar at

Station 152.8

(Refer to 

PSM 1-6-7

Part 3)


	TASK
	ITEM DESCRIPTION
	EFFECTIVITY/

CONFIGURATION
	AIRWORTHINESS LIMITATIONS
	ACTION NOTES

	
	
	
	SAFE LIFE LIMIT EXCEPTIONS FROM AIRFRAME LIMIT
	MODIFICATION LIMIT
	INSPECTION OR OVERHAUL
	

	
	
	
	
	
	INITIAL
	REPEAT
	


	57 – WINGS (Cont’d)

	57-029
	Wing Assembly

C6W1001–33, –35,

& subsequent

Wing Box

C6W1002–67, –69,

& subsequent
	Post Mod 6/1117

and

Pre Mod 6/1630
	33,000 Flight

Hours or 66,000

Flight Cycles

whichever

occurs first
	-
	-
	-
	Incorporate Mod 6/1630

to extend service life

(Refer to 
SB 6/362)

	57-030
	C6W1002–

Replacement Box

(Replaces 67, –69,

& subsequent
	Post Mod 6/1117

and when installed

into C6W1001 as

part of Mod 6/1630

and

Pre Mod 6/1318
	-
	12,000 Flight

Hours or 24,000

Flight Cycles
	-
	-
	Incorporate Mod 6/1318

(Refer to SB 6/268)

	57-031
	C6W1002–

Replacement Box

(Replaces 67, –69,

& subsequent
	Post Mod 6/1117

and when installed

into C6W1001 as

part of Mod 6/1630
	-
	-
	12,000 Flight

Hours or 24,000

Flight Cycles

whichever

occurs first
	Every 1,200

Flight Hours or

2,400 Flight

Cycles

whichever

occurs first
	Inspect Main Spar at

Sta. 152.8

(Refer to 

PSM 1-6-7

Part 3)

	57-032
	C6W1002–

Replacement Box

(Replaces 67, –69,

& subsequent
	Post Mod 6/1117

and when installed

into C6W1001 as

part of Mod 6/1630
	-
	-
	24,000 Flight

Hours or 48,000

Flight Cycles

whichever

occurs first
	Every 1,200

Flight Hours or

2,400 Flight

Cycles

whichever

occurs first
	Inspect Lwr Skin at WS185, Lwr Wing Skin,

Stringers and Aft Spar Lwr Flange from WS122 to WS263

(ribs 8 to 20)

(Refer to 
PSM 1-6-7

Part 3)

	57-033
	Wing Assembly

C6W1001–33, –35

& subsequent
	Post Mod 6/1117

and

Post Mod 6/1630
	66,000 Flight

Hours or 132,000

Flight Cycles

whichever

occurs first
	-
	-
	-
	-

	57-037
	Wing Strut Assembly

C6W1005–9, –10

Link Assembly

C6WM1409–1, –3
	Post Mod 6/1172

and

Post Mod 6/1174
	36,000 Flight

Hours or 72,000

Flight Cycles

whichever

occurs first
	-
	-
	-
	Remove these

wing strut and link assemblies, including all attachment bolts,

from service and

replace with new parts

C6W1005–9, and –10 (strut), C6WM1409–3

(link), and attachment

bolts C6WM1411–27

(one per strut) and –29

(two per strut)


	TASK
	ITEM DESCRIPTION
	EFFECTIVITY/

CONFIGURATION
	AIRWORTHINESS LIMITATIONS
	ACTION NOTES

	
	
	
	SAFE LIFE LIMIT EXCEPTIONS FROM AIRFRAME LIMIT
	MODIFICATION LIMIT
	INSPECTION OR OVERHAUL
	

	
	
	
	
	
	INITIAL
	REPEAT
	


	57 – WINGS (Cont’d)

	57-038
	Wing Flap Hinge Arm

Attachment Fittings at

Wing Sta. 97.5
	Landplanes and

Floatplanes that

have been used

in Landplane

configuration
	-
	-
	31,800 Flight

Hours or 63,600

Flight Cycles

whichever

occurs first
	Every 2,400

Flight Hours or

4,800 Flight

Cycles

whichever

occurs first
	Inspections of the lower

attachment fittings

C6W1045

(Refer to 

PSM 1-6-7)

	57-041
	Wing Upper Surface

Inspection for Disbonding
	All Configurations
	-
	-
	20 years
	Every 5 years
	As per

SB V6/0018

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	

	
	
	
	
	
	
	
	


