
	MARITIME HELICOPTERS
	DHC-6 CONTINUOUS AIRWORTHINESS MAINTENANCE PROGRAM

	
	

	Page No:
	

	Revision:
	Original
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	CHECK:
	
	S 0850NT – SPECIAL INSPECTION

	FREQUENCY:
	
	Every 800 Hours or 12 Months, whichever occurs first

	NOTE:
	
	No Tolerance




	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  DHC-6 Maintenance Program 

	
	
	MECH
INITIALS
	RII
INTIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	S 0850.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	DHC-6
MP
	
	

	
	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	DHC-6
 MP
	
	

	
	
	
	

	S 0850.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 
	
	
	

	
	
	
	

	2.1.1 
	
	
	

	
	
	
	

	2.1.1.1  CORROSION CONTROL

	
	
	
	

	2.2 
	
	
	

	
	
	
	

	2.3 
	
	
	

	
	
	
	

	S 0850.3  FLIGHT CONTROLS

	
	
	
	

	3.1 Flap Push Rods – Wing flap material pushrods with sleeves incorporated for cracks.
	
	
	

	Note: refer to Service bulletin No’s. 6/388 and 6/381 and A.D. CF-79-22 or 80-03-08, if applicable.
	
	
	

	3.2 Flight Control Pushrods – flight control material pushrods with sleeves incorporated for cracks.
	
	
	

	Note: refer to Service bulletin No’s. 6/390 and 6/502 and A.D. CF-80-03 or 80-13-11, if applicable.
	
	
	

	3.3 
	
	
	

	
	
	
	

	3.4 
	
	
	

	
	
	
	

	3.5 
	
	
	

	
	
	
	

	S 0850.4 

	
	
	
	

	4.1 
	
	
	

	
	
	
	

	4.2 
	
	
	

	
	
	
	

	4.3 
	
	
	

	
	
	
	

	4.4 
	
	
	

	
	
	
	

	4.5 
	
	
	

	
	
	
	

	S 0850.5 

	
	
	
	

	5.1 
	
	
	

	
	
	
	

	5.2 
	
	
	

	
	
	
	

	5.3 
	
	
	

	
	
	
	

	5.4 
	
	
	

	
	
	
	

	5.5 
	
	
	

	
	
	
	

	S 0850.6 

	
	
	
	

	6.1 
	
	
	

	
	
	
	

	6.2 
	
	
	

	
	
	
	

	6.3 
	
	
	

	
	
	
	

	6.4 
	
	
	

	
	
	
	

	6.5 
	
	
	

	
	
	
	

	S 0850.7 

	
	
	
	

	7.1 
	
	
	

	
	
	
	

	7.2 
	
	
	

	
	
	
	

	7.3 
	
	
	

	
	
	
	

	7.4 
	
	
	

	
	
	
	

	7.5 
	
	
	

	
	
	
	

	S 0850.8 

	
	
	
	

	8.1 
	
	
	

	
	
	
	

	8.2 
	
	
	

	
	
	
	

	8.3 
	
	
	

	
	
	
	

	8.4 
	
	
	

	
	
	
	

	8.5 
	
	
	

	
	
	
	

	S 0850.9 FINAL CLOSE UP

	
	
	
	

	9.1 
	
	
	

	
	
	
	

	9.2 
	
	
	

	
	
	
	

	9.3 
	
	
	

	
	
	
	

	9.4 
	
	
	

	
	
	
	

	9.5 
	
	
	

	
	
	
	

	S 0850.10 POST INSPECTION

	
	
	
	

	10.1 Inspect for operation and leaks.
	
	
	

	
	
	
	

	10.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	10.3 Perform Functional Check Flight if required per DHC - 6 Maintenance Manual or AFM as appropriate.
	
	
	

	
	
	
	

	10.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	

	
	
	
	




Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters Viking DHC-6-400 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6-400 CAMP – S 0850NT – 800 Hour / 12 Monh Special Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




