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Reference:  DHC-6 Maintenance Program, Viking PSM 1-64-2 Maintenance Manual

	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	C 1000.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	DHC-6-400
MP
	
	

	
	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	DHC-6-400

MP
	
	

	
	
	
	

	C 1000.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	
	
	
	

	C 1000.3  CORROSION CONTROL

	
	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	Appendix

B
	
	

	C 1000.4  PREPARATION

	
	
	
	

	4.1 Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	C 1000.5 21 – AIR CONDITIONING 

	
	
	
	

	5.1 Forward avionics compartment air filter for condition, security and free of obstruction.  Clean as required.
	
	
	

	Effectivity: Mod C10-06/2014
	
	
	

	5.2 DAU cooling fan for condition and security, bonding wires for condition, security and security of attachment.
	
	
	

	Effectivity: Mod 6/2049
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	C 1000.6 22 – AUTO FLIGHT 

	
	
	
	

	6.1 SM3000 Aileron servo for grounding of unit wiring bundle shield braid to airframe structure (<7.5 milliohms).
 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod SOO 6221
	
	
	

	6.2 SM3000 Aileron servo for bonding of the mating surfaces between servo mount and airframe structure (<2.5 milliohms). 

 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod SOO 6221
	
	
	

	6.3 AFCS (Autopilot) SM3000 aileron system servo. Check bridle cable tensions and verify no slippage of clamps has occurred.
	
	
	

	
	
	
	

	6.4 AFCS (Autopilot) SM3000 elevator system servo. Check bridle cable tensions and verify no slippage of clamps has occurred.
	
	
	

	
	
	
	

	6.5 AFCS (Autopilot) SM3000 rudder system servo. Check bridle cable tensions and verify no slippage of clamps has occurred.
	
	
	

	
	
	
	

	6.6 SM3000 rudder servo for grounding of unit wiring bundle shield braid to airframe structure (<7.5 milliohms) .

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6221
	
	
	

	6.7 SM3000 Aileron servo for bonding of the mating surfaces between servo mount and airframe structure (<2.5 milliohms) .

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6221
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	6.8 KS 272A pitch trim servo for grounding of unit wiring bundle shield braid to airframe structure (<7.5 milliohms) .

 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod SOO 6221
	
	
	

	6.9 KS 272A pitch trim servo for bonding of the mating surfaces between servo mount and airframe structure (<2.5 milliohms) .

 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod SOO 6221
	
	
	

	6.10 KS 272A pitch trim system servo. Check bridle cable tensions and verify no slippage of clamps has occurred.
	
	
	

	C 1000.7 23 – COMMUNICATIONS 

	
	
	
	

	7.1 VHF upper antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).

 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

  Effectivity: Mod 6/2003
	
	
	

	7.2 VHF upper aft antenna for condition and security, control and indicators for condition, wiring and connector for security.  Clean as required.
	
	
	

	Effectivity: Mod 6/2003
	
	
	

	7.3 VHF forward antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).

 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2003
	
	
	

	7.4 VHF lower aft antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).

 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2003 & Mod 6231
	
	
	

	7.5 VHF lower aft antenna for condition and security, control and indicators for condition, wiring and connector for security.  Clean as required.
	
	
	

	 Effectivity: Mod 6/2003, SOO 6231
	
	
	

	7.6 VHF-FM antenna for condition and security, control and indicators for condition, wiring and connector for security.  Clean as required.
	
	
	

	 Effectivity: Mod SOO 6296
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	7.7 VHF-FM antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).

 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod SOO 6296
	
	
	

	7.8 Pilots audio panel (KMA 29), for condition and security, bonding wires for condition and security.
	
	
	

	 Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.9 Pilots audio panel (KMA 29), for bonding of the mating surfaces between mounting tray and airframe (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6209, Mod 6/2049
	
	
	

	7.10 Co-Pilots audio panel (KMA 29), for condition and security, bonding wires for condition and security.
	
	
	

	 Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.11 Co-Pilots audio panel (KMA 29), for bonding of the mating surfaces between mounting tray and airframe (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6209, Mod 6/2049
	
	
	

	7.12 Pilot audio panel (KMA 29), emergency switch operational test.
	
	
	

	Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.13 Co-Pilot audio panel (KMA 29), emergency switch operational test.
	
	
	

	 Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.14 Audio system (NAT 247) isolation amplifier for bonding of the mating surfaces between antenna and airframe (<2.5 milliohms).

 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2049
	
	
	

	7.15 Audio system (NAT 247) isolation amplifier for condition and security, bonding wires for condition and security.
	
	
	

	Effectivity: Mod 6/2049
	
	
	

	7.16 MMDR #1 for bonding of the mating surfaces between antenna and airframe (<2.5 milliohms).

 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2049
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	7.17 MMDR #2 for condition and security, bonding wires for condition and security.
	
	
	

	Effectivity: Mod SOO 6209, Mod 6/2049
	
	
	

	7.18 MMDR #2 for bonding of the mating surfaces between antenna and airframe (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod SOO 6209, Mod 6/2049
	
	
	

	7.19 MMDR #1 for condition and security, bonding wires for condition and security.
	
	
	

	Effectivity: Mod 6/2049
	
	
	

	7.20 Emergency frequency com tuning switch operational test.
	
	
	

	
	
	
	

	7.21 GPS/IRIDIUM/WiFi Antenna for condition, security and corrosion, condition of external fillet seal, condition of coaxial cables and connectors and security of attachment of coaxial cables.
	
	
	

	
	
	
	

	7.22 GPS/IRIDIUM/WiFi Antenna for bonding of the mating surfaces between antenna baseplate and airframe (<3 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: SOO 6288 or 6298
	
	
	

	7.23 SkyNode SAT COM Panel/Dialer (RC6000/A), for condition, security and corrosion; electrical wires and connectors for condition and security of attachment.
	
	
	

	Effectivity: SOO 6298
	
	
	

	C 1000.8 24 – ELECTRICAL POWER 

	
	
	
	

	8.1 External power receptacle for condition and security. Clean as required.
	
	
	

	
	
	
	

	8.2 Grounding and bonding wires for condition and security. Clean as required.
	
	
	

	
	
	
	

	8.3 Voltage regulators for condition and security. Clean as required.
	
	
	

	
	
	
	

	C 1000.9 25 - EQUIPMENT/FURNISHINGS 

	
	
	
	

	9.1 ELT for bonding of the mating surfaces between the backshell and airframe (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
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	9.2 ELT Antenna bonding of the mating surfaces between the antenna and airframe (<3 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	9.3 Flight compartment axe and axe storage;
	

	9.3.1 Axe handle retention strap and elastic webbing for damage or deterioration (loss of elastic properties). Replace on condition.
	
	
	

	9.3.2 Condition and security of axe stowage structure. Condition and security of axe cutting edge and pike to axe handle.
	
	
	

	C 1000.10 27 – FLIGHT CONTROLS 

	10.1 Inspect control column (Mod 6/1433) as follows;
	

	
	

	10.1.1 Condition, security and full and free movement.
	
	
	

	
	
	
	

	10.1.2 Brackets for condition and security, centering strut for condition, proper operation and security.
	
	
	

	
	
	
	

	10.1.3 Remove covers.
	
	
	

	
	
	
	

	10.1.4 Check for evidence of binding, chain alignment with control wheel sprockets, sprockets for condition, security and teeth wear, turnbuckles for safety.
	
	
	

	
	
	
	

	10.1.5 Control column floor boot for condition and security.
	
	
	

	
	
	
	

	10.1.6 Lubricate.
	
	
	

	
	
	
	

	10.1.7 Reinstall covers.
	
	
	

	
	
	
	

	10.2 Rudder torque tube and quadrats for condition and security, linkage and push rod installation for security.
	
	
	

	
	
	
	

	10.3 Gust lock control for condition and proper operation, brackets and connecting rods for cracks, buckling and security.
	
	
	

	Note 1: Refer to Service Bulletin N. 6/508, if applicable.
	
	
	

	10.4 Rudder pedal support assembly, push rods, levers and linkage for condition and security; pedals for full and free movement; condition and security; peda
10.5 ls for cracking as shown in PSM 1-6-7, Part 1 Figure 2. Replace if cracked.
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	10.6 Inspect rudder, elevator and aileron primary control cables as follows;

Note 1: Refer to Service Bulletin N. 6/523, if applicable.

Note 2: Ensure adequate clearance with adjacent electrical conduits, structure and other systems, making allowance for vibratory motion of cable under tension.

Note 3: In the event of early or abnormal cable wear at pulley(s), replace the worn cable(s) and the corresponding pulley(s).
	

	
	

	10.6.1 Cables (from beneath flight compartment) floor to wings and empennage) for fraying corrosion, flattening, proper attachment and security.
	
	
	

	
	
	
	

	10.6.2 Pulleys for condition and freedom of movement, pulley brackets and guides for condition and security, turnbuckles for security.
	
	
	

	
	
	
	

	10.6.3 Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	
	
	
	

	10.7 Inspect rudder flight control cables as follows
	

	
	

	10.7.1 Control and tab cables, flap/elevator interconnect and elevator trim cables for fraying kinks, flattening, corrosion and security of attachments.
	
	
	

	
	
	
	

	10.7.2 Cable ends with nylon sheathing, (where applicable) for condition.
	
	
	

	
	
	
	

	10.7.3 Turnbuckles for security. Replace cable where evidence of damage is found.
	
	
	

	10.7.4 Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	
	
	
	

	10.8 Inspect aileron L/H wing flight control cables as follows
	

	
	

	10.8.1 Fraying, flattening, corrosion, proper attachment and security.
	
	
	

	
	
	
	

	10.8.2 Pulleys for condition and freedom of movement, pulley brackets and guides for condition and security, turnbuckles for security.
	
	
	

	
	
	
	

	10.8.3 Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	
	
	
	

	10.9 Inspect aileron R/H wing flight control cables as follows
	

	
	

	10.9.1 Fraying, flattening, corrosion, proper attachment and security.
	
	
	

	
	
	
	

	10.9.2 Pulleys for condition and freedom of movement, pulley brackets and guides for condition and security, turnbuckles for security.
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	10.9.3 Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	
	
	
	

	10.10 Inspect rudder and elevator trim tab controls as follows;
	

	
	

	10.10.1 Full and freedom of movement, cables for fraying, kinks, flattening, proper attachment and security.
	
	
	

	
	
	
	

	10.10.2 Pulleys for freedom of operation and pulley brackets for condition and security.
	
	
	

	
	
	
	

	10.11 Do a detailed visual inspection of cable terminals as follows;
	

	
	

	10.11.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	10.11.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	10.11.3 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	10.11.4 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	10.11.5 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.1.15.1, rig the control system.
	
	
	

	
	
	
	

	10.11.6 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	10.12 Inspect rudder gear tab mechanism as follows;
	

	
	

	10.12.1 Gearbox for condition and security of mounting plate installation and cover, tab pushrod for security and evidence of irregular operation during rudder movement.
	
	
	

	
	
	
	

	10.12.2 Gearbox to rudder linkage for condition and security, pushrod for security of attachments.
	
	
	

	
	
	
	

	10.13 Inspect L/H aileron trim tab actuator as follows;
	

	
	

	10.13.1 Smooth operation and security. 
	
	
	

	
	
	
	

	10.13.2 Electrical wiring and connections for security.
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	10.13.3 Linkages for damage, safety and security.
	
	
	

	
	
	
	

	10.13.4 Position transmitter for cleanliness, loose connections and security of mounting.
	
	
	

	
	
	
	

	10.14 Inspect R/H aileron trim tab actuator as follows;
	

	
	

	10.14.1 Smooth operation and security. 
	
	
	

	
	
	
	

	10.14.2 Electrical wiring and connections for security.
	
	
	

	
	
	
	

	10.14.3 Linkages for damage, safety and security.
	
	
	

	
	
	
	

	10.14.4 Position transmitter for cleanliness, loose connections and security of mounting.
	
	
	

	
	
	
	

	10.15 Aileron trim tab position indicator for condition and security, wiring and connectors for condition and security.
	
	
	

	 Effectivity: Mod 6/2047
	
	
	

	10.16 Rubber, elevator and aileron position voltage check.
	
	
	

	Effectivity: Mod 6/2047
	
	
	

	10.17 Position transmitter, inspect for security of mounting and brackets, wiring and connections for security. Clean as required.
	
	
	

	 Effectivity: Mod 6/2047
	
	
	

	10.18 Flap position cable for fraying, flattening, corrosion and security of attachment, spring for condition, tension and security. 
	
	
	

	
	
	
	

	10.19 Flap position indicator for smooth operation.
	
	
	

	 Effectivity: Mod 6/2048
	
	
	

	10.20 Flap position dracon cable cord at window frame small pulley locations for condition.
	
	
	

	
	
	
	

	10.21 Flap/elevator interconnect, elevator trim cables and flap indicator cables for condition, fraying, corrosion, flattening and security of attachment, turnbuckles for security, pulleys for condition, security and freedom of operation.
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	10.22 Do a detailed visual inspection as follows;
	

	
	

	10.22.1 Fuselage aileron, elevator and rudder flight control cables.
	
	
	

	
	
	
	

	10.22.2 Flap to elevator interconnect tab cables
	
	
	

	
	
	
	

	10.22.3 Flap selector valve and follow up cables.
	
	
	

	
	
	
	

	10.23 Do a detailed visual inspection of cable terminals as follows;
	

	
	

	10.23.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	 Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	10.23.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	10.23.3 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	10.23.4 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	10.23.5 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.18.1, rig the control system.
	
	
	

	
	
	
	

	10.23.6 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	10.24 Inspect rudder flight control cables as follows;

Note 1: Refer to Service Bulletin N. 6/523, if applicable.

Note 2: Ensure adequate clearance with adjacent electrical conduits, structure and other systems, making allowance for vibratory motion of cable under tension.

Note 3: In the event of early or abnormal cable wear at pulley(s), replace the worn cable(s) and the corresponding pulley(s).
	

	
	

	10.24.1 Cables and tab cables, flap/interconnect and elevator trim cables for fraying corrosion, kinks, flattening, proper attachment and security.
	
	
	

	
	
	
	

	10.24.2 Cable ends with nylon sheathing, (where applicable), for condition.
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	10.24.3 Turnbuckles for security. Replace cable where evidence of damage is found.
	
	
	

	
	
	
	

	10.24.4 Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	
	
	
	

	10.25 Overhead console flight control and flap selector (Mod 6/1895) aluminum quadrants for condition and security, freedom of movement, cable attachment for security, pulley for smooth and freedom of operation.
	
	
	

	
	
	
	

	10.26 Aileron flight control cable quadrants in cabin roof for condition and security, bearings for condition, cable guides for security. Clean as required.
	
	
	

	
	
	
	

	10.27 Elevator control quadrants for cleanliness, damage, corrosion and security; bearings for corrosion, cleanliness and security; stops for damage.
	
	
	

	
	
	
	

	10.28 Elevator control lever and connecting rod for full and free movement, attaching brackets for cracks and distortion.
	
	
	

	
	
	
	

	10.29 L/H wing root rib/flap pushrod support rollers for condition, wear and security, proper clearance between rod surface and roller and freedom of operation. Lubricate inside of spacer and bolt.
	
	
	

	 Effectivity: Post Mod 6/1707
	
	
	

	10.30 R/H wing root rib/flap pushrod support rollers for condition, wear and security, proper clearance between rod surface and roller and freedom of operation. Lubricate inside of spacer and bolt.

	
	
	

	 Effectivity: Post Mod 6/1707
	
	
	

	10.31 Stall warning cam limit microswitch mechanism and propeller reset limit switch for condition and security, connector for security.
	
	
	

	 Effectivity: Post Mod 6/1701
	
	
	

	10.32 Rudder position transmitter, inspect for security of mounting and brackets, wiring and connections for security. Clean as required.
	
	
	

	 Effectivity: Mod 6/2047
	
	
	

	10.33 Elevator position transmitter, inspect for security of mounting and brackets, wiring and connections for security. Clean as required.
	
	
	

	 Effectivity: Mod 6/2047
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	C 1000.11  28 – FUEL 

	
	
	
	

	11.1 Fuel system pipes for condition, connections and hoses for security and leakage, sump plates for corrosion and leakage.  Clean as required
	
	
	

	Note: Refer to Service Bulletin No. 6/269 and A.D. 71-16-01, if applicable.
	
	
	

	11.2 Do a detailed visual inspection of the fuel manifold as follows;
	

	Effectivity: Mod 6/2389
	

	11.2.1 Bonding clamp sealant and terminal lug sealant for condition and integrity, peeling, cracking or evidence of corrosion.
	
	
	

	
	
	
	

	11.2.2 Inspect bonding jumpers for condition, security, integrity and corrosion.
	
	
	

	
	
	
	

	11.2.3 If damaged, replace component, re-apply sealant.
	
	
	

	
	
	
	

	11.3 Do a detailed visual inspection of the booster pumps as follows;
	
	

	
	
	

	11.3.1 Condition, security, corrosion and cleanliness. 
	
	
	

	
	
	
	

	11.3.2 Wiring for condition, corrosion, signs of overheat or arcing.
	
	
	

	
	
	
	

	11.3.3 Radio noise filters for security, condition and corrosion.
	
	
	

	 Effectivity: Pre Mod 6/2267
	
	
	

	11.3.4 Electrical terminals for condition and deterioration of sealant.
	
	
	

	
	
	
	

	11.3.5 Electronic EMI noise filters for condition, security, sign of overheat. Resistance check and condition of electrical termination.
	
	
	

	 Effectivity: Pre Mod 6/2267
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	11.3.6 Bleed resistors for condition, security, sign of overheat. Resistance checks and condition of electrical termination.
	
	
	

	Effectivity: Pre Mod 6/2267
	
	
	

	11.4 Fuel ejectors for condition and security. 
	
	
	

	
	
	
	

	11.5 Crossfeed valve for corrosion, security and evidence of leakage.
	
	
	

	
	
	
	

	11.6 Fuel system pipes for condition, connections and hoses for security and leakage, sump plates for corrosion and leakage.  Clean as required.
	
	
	

	Note: Refer to Service Bulletin No. 6/269 and A.D. 71-16-01, if applicable.
	
	
	

	11.7 Fuel low pressure switches for condition, leakage and security, electrical connector for security.
	
	
	

	
	
	
	

	11.8 Coaxial electrical wiring in fuel gallery for condition, connectors for condition and security.  Clean as required.
	
	
	

	For Mod 6/2390, do a detailed visual inspection of the environmental wrap for condition, integrity (split, tear or removal etc.). If deterioration is evident, remove the environmental wrap and inspect underlying components for general condition, corrosion, wiring, terminations, shield terminations. Replace damaged components and install new environmental wrap (refer to PSM1-64-2, Chapter 20-50-03).
For Mod 6/2395, do a detailed visual inspection of the backshell and backshell sealant for deterioration in the seal cavities. If deterioration is evident, clean and reseal backshell. Replace if deterioration is severe.
	
	
	

	11.9 Grounding and bounding leads for fraying, broken wires, loose connections, cleanliness.
	
	
	

	For Mod 6/2390, do a detailed visual inspection of the environmental wrap for condition, integrity (split, tear or removal etc.). If deterioration is evident, remove the environmental wrap and inspect underlying components for general condition, corrosion, wiring, terminations, shield terminations. Replace damaged components and install new environmental wrap (refer to PSM1-64-2, Chapter 20-50-03).
For Mod 6/2395, do a detailed visual inspection of the backshell and backshell sealant for deterioration in the seal cavities. If deterioration is evident, clean and reseal backshell. Replace if deterioration is severe.
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	C 1000.12  29 – HYDRAULIC POWER 

	
	
	
	

	12.1 Hydraulic accumulators for leakage and security.
	
	
	

	
	
	
	

	12.2 Hydraulic brake system pressure relief valve for leakage and security.
	
	
	

	
	
	
	

	12.3 Hydraulic system pressure relief valve for leakage and security.
	
	
	

	
	
	
	

	12.4 Flap system thermal relief valves for leakage and security.
	
	
	

	
	
	
	

	12.5 Main leg hydraulic lines for condition, leakage, loose clamps and connections for security.
	
	
	

	
	
	
	

	12.6 Main leg flexible hoses for condition, leakage and connections for security.
	
	
	

	
	
	
	

	C 1000.13  30 – ICE AND RAIN PROTECTION 

	
	
	
	

	13.1 Heated windshield elements and wiring for condition and security.
	
	
	

	
	
	
	

	13.2 Airframe deicing timer and connectors for condition and security.
	
	
	

	
	
	
	

	13.3 Do a detailed visual inspection of the horizontal stabilizer deicing system as follows;
	

	
	

	13.3.1 Ejector for condition and security, clear of obstruction. Clean as required.
	
	
	

	
	
	
	

	13.3.2 Distributor valve for condition, security and leakage.
	
	
	

	
	
	
	

	13.3.3 Distributor valve heating jacket for security, electrical connections for corrosion and security.
	
	
	

	
	
	
	

	13.3.4 Horizontal stabilizer pressure system indicating switches for security, electrical connections for security.
	
	
	

	
	
	
	

	13.3.5 Pipe for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	
	
	

	
	
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	

	13.4 Do a detailed visual inspection of the L/H wing deicing system as follows;
	

	
	

	13.4.1 Distributor valves for leaks and security.
	
	
	

	
	
	
	

	13.4.2 Distributor valves heater jackets for security, electrical connections for corrosion and security.
	
	
	

	
	
	
	

	13.4.3 Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	
	
	

	
	
	
	

	13.5 Do a detailed visual inspection of the R/H wing deicing system as follows;
	

	
	

	13.5.1 Distributor valves for leaks and security.
	
	
	

	
	
	
	

	13.5.2 Distributor valves heater jackets for security, electrical connections for corrosion and security.
	
	
	

	
	
	
	

	13.5.3 Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	
	
	

	
	
	
	

	13.6 Do a detailed visual inspection of the horizontal stabilizer deicing system as follows;
	

	
	

	13.6.1 Ejector for condition and security, clear of obstructions. Clean s required.
	
	
	

	
	
	
	

	13.6.2 Distributor valves for leaks and security.
	
	
	

	
	
	
	

	13.6.3 Distributor valves heater jackets for security, electrical connections for corrosion and security.
	
	
	

	
	
	
	

	13.6.4 Pressure system indicating switches for security, electrical connections for security.
	
	
	

	
	
	
	

	13.6.5 Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	
	
	

	
	
	
	

	13.6.6 Caution light panel and cockpit dome light for condition and security.
	
	
	

	
	
	
	

	13.6.7 Deicing boot pressure warning lights for condition and security.
	
	
	

	 Effectivity: Pre Mod 6/2028
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	13.7 Do a detailed visual inspection of the airframe deicing system as follows;
	

	
	

	13.7.1 Timer and connectors for condition and security
	
	
	

	
	
	
	

	13.7.2 Distributor valves for leaks and security.
	
	
	

	
	
	
	

	13.7.3 Distributor valves heater jackets for security, electrical connections for corrosion and security.
	
	
	

	
	
	
	

	13.7.4 Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	
	
	

	
	
	
	

	13.7.5 Pressure system indicating switches for security, electrical connections for security.
	
	
	

	
	
	
	

	13.7.6 Ejector for condition and security, clear of obstructions. Clean s required.
	
	
	

	
	
	
	

	13.7.7 Deicing pressure and suction indicator for condition, leakage and security.
	
	
	

	
	
	
	

	C 1000.14  31 – INSTRUMENTS 

	
	
	
	

	14.1 Primary flight display unit KDU 1080 or KDU 1080-2 for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod 6/2049
	
	
	

	14.2 Primary flight display unit KDU 1080 or KDU 1080-2, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2049
	
	
	

	14.3 Primary flight display controller KMC2210 for condition and security, bonding wires for condition and security of attachment.
	
	
	

	Effectivity: Mod 6/2049
	
	
	

	14.4 Primary flight controller KMC2210, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	14.5 Multi-function display unit KDU 1080 or KDU 1080-2 for condition and security, bonding wires for condition and security of attachment
	
	
	

	Effectivity: Mod 6/2049
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	14.6 Multi-function display controller KMC2220, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2049
	
	
	

	14.7 Multi-function display controller KMC2220 for condition and security, bonding wires for condition and security of attachment
	
	
	

	 Effectivity: Mod 6/2049
	
	
	

	14.8 Flight controller KMC9200 for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod 6/2049
	
	
	

	14.9 Flight controller KMC9200, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2049
	
	
	

	14.10 Reversion control panel for displays, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2049
	
	
	

	14.11 Reversion control panel for displays for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	14.12 ESIS display for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod 6/2049, Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.13 ESIS display, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.14 ESIS battery for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod 6/2049, Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
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	14.15 ESIS battery, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.16 ESIS magnetometer for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod 6/2049 & Mod SOO 6209
	
	
	

	14.17 ESIS magnetometer, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.18 ESIS magnetometer, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.19 MAU for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod 6/2049
	
	
	

	14.20 MAU, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2049
	
	
	

	14.21 MAU, verify ferrite beads are installed on the LAN wires inside the backshells of all the NIC’s (bead P/N is a Ferronics 21-727-B).
	
	
	

	 Effectivity: Mod 6/2049
	
	
	

	14.22 MAU, visually inspect the mesh covering the air intake for dust and debris. Clean as required.
	
	
	

	 Effectivity: Mod 6/2049
	
	
	

	14.23 MAU power supplies, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.24 MAU power supplies for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod 6/2049
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	14.25 CVR for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod 6/2049 & Mod SOO 6384
	
	
	

	14.26 CVR, inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.27 FDR for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod SOO 6385 Mod 6/2049 & Mod SOO 6385
	
	
	

	14.28 FDR, inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod SOO 6385 Mod 6/2049 & Mod SOO 6385
	
	
	

	14.29 DAU #1 & #2 for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod 6/2049
	
	
	

	14.30 DAU #1 & #2, inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2049
	
	
	

	14.31 Master warning and caution indication and control inspect for condition and security, bonding wires for condition and security of attachment.
	
	
	

	 Effectivity: Mod 6/2028
	
	
	

	14.32 ECTM/FOQA (IONode 100) (SOO 6288) for condition, security and corrosion; electrical wires and connectors for security of attachment.
	
	
	

	
	
	
	

	14.33 Inspect FDR (Mod SOO 6385) (Mod 6/2049) (Post Mod 6/2332) for;
	

	
	

	14.33.1 Condition and security; bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	14.33.2 Bonding of the mating surfaces between the unit and airframe (< 2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
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	C 1000.15 32 – LANDING GEAR  

	
	

	15.1 Inspect the nosewheel steering cables forward of Sta. 60 and beneath cockpit floor as follows; 
	

	 Effectivity: Mod 6/1800
	

	15.1.1 Condition, kinks, flattening, proper attachment and security.
	
	
	

	
	
	
	

	15.1.2 Pulleys for condition, freedom of operation and security.
	
	
	

	
	
	
	

	15.1.3 Turnbuckles for security.
	
	
	

	
	
	
	

	15.1.4 Do a detailed visual inspection of nosewheel cable terminals as follows;
	

	
	

	15.1.5 Remove and discard the lockwire from the cable terminals.
	
	
	

	 Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	15.1.6 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	15.1.7 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	15.1.8 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	15.1.9 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.1.15.1, rig the control system.
	
	
	

	
	
	
	

	15.1.10 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	15.2 Inspect the nosewheel steering lever as follows; 
	

	 Effectivity: Mod 6/1800
	

	15.2.1 Remove control column cover.
	
	
	

	
	
	
	

	15.2.2 Cables for condition, kinks, flattening, proper attachment and security.
	
	
	

	
	
	
	

	15.2.3 Pulleys for condition, freedom of operation and security.
	
	
	

	
	
	
	

	15.2.4 Turnbuckles for security.
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	15.2.5 Do a detailed visual inspection of nosewheel cable terminals as follows;
	

	
	

	15.2.5.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	 Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	15.2.5.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	15.2.5.3 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	15.2.5.4 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	15.2.5.5 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.1.15.1, rig the control system.
	
	
	

	
	
	
	

	15.2.5.6 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	15.2.5.7 Steering cables for tension.
	
	
	

	
	
	
	

	15.2.5.8 Install control column cover.
	
	
	

	
	
	
	

	15.3 Remove nose wheel.
	
	
	

	 Note: Refer also to Special Inspection Card SP1 if applicable.
	
	
	

	15.3.1 Remove tire from wheel and examine for visible cracks or chipping on rims.
	
	
	

	
	
	
	

	15.3.2 Lubricate bearings as required.
	
	
	

	
	
	
	

	15.3.3 Install serviceable tire on wheel.
	
	
	

	
	
	
	

	15.3.4 Install serviceable nose wheel.
	
	
	

	
	
	
	

	15.4 Remove L/H main wheel.
	
	
	

	 Note: Refer also to Special Inspection Card SP1 if applicable.
	
	
	

	15.4.1 Remove tire from wheel and examine for visible cracks or chipping on rims.
	
	
	

	
	
	
	

	15.4.2 Lubricate bearings as required.
	
	
	

	
	
	
	

	15.4.3 Install serviceable tire on wheel.
	
	
	

	
	
	
	

	15.4.4 Install serviceable L/H main wheel.
	
	
	

	
	
	
	

	15.5 Remove R/H main wheel.
	
	
	

	 Note: Refer also to Special Inspection Card SP if applicable.
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	15.5.1 Remove tire from wheel and examine for visible cracks or chipping on rims.
	
	
	

	
	
	
	

	15.5.2 Lubricate bearings as required.
	
	
	

	
	
	
	

	15.5.3 Install serviceable tire on wheel.
	
	
	

	
	
	
	

	15.5.4 Install serviceable R/H main wheel.
	
	
	

	
	
	
	

	15.6 Do a detailed visual inspection of L/H brake system as follows;
	

	15.6.1 Remove console cover.
	
	
	

	
	
	
	

	15.6.2 Parking brake rods and linkage for signs of wear and security.
	
	
	

	
	
	
	

	15.6.3 Lubricate cams.
	
	
	

	
	
	
	

	15.6.4 Wheel brake valve for leakage and security.
	
	
	

	
	
	
	

	15.6.5 Clean as required.
	
	
	

	
	
	
	

	15.6.6 Reinstall console cover.
	
	
	

	
	
	
	

	15.7 Do a detailed visual inspection of R/H brake system as follows;
	

	15.7.1 Remove console cover.
	
	
	

	
	
	
	

	15.7.2 Parking brake rods and linkage for signs of wear and security.
	
	
	

	
	
	
	

	15.7.3 Lubricate cams.
	
	
	

	
	
	
	

	15.7.4 Wheel brake valve for leakage and security.
	
	
	

	
	
	
	

	15.7.5 Clean as required.
	
	
	

	
	
	
	

	15.7.6 Reinstall console cover.
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	15.8 Do a detailed visual inspection of main gear fairings as follows;
	

	15.8.1 Remove center fairings.
	
	
	

	
	
	
	

	15.8.2 Cracks, delamination and security.
	
	
	

	
	
	
	

	15.8.3 Seals for tears, deterioration and security.
	
	
	

	
	
	
	

	15.8.4 Fairing supporting structure for cracks, corrosion, buckling and loose anchor nuts.
	
	
	

	
	
	
	

	15.8.5 Roller blind assembly for adequate spring tension, blind for fraying, tears and security.
	
	
	

	
	
	
	

	15.8.6 Roller for free running and security.
	
	
	

	
	
	
	

	15.8.7 Welds for cracks at tubes, lugs, pivot fittings and brake flange ale housing.
	
	
	

	 Note: Refer to PSM1-6-7 Part 3, Figure 8 for leg weld locations.
	
	
	

	15.8.8 Reinstall center fairings.
	
	
	

	
	
	
	

	15.9 Inspect shock absorber blocks for condition, free from oil, grease, deterioration, splitting on surface adjacent to bolt holes and displacement of blocks. Discard blocks that have sustained permanent set due to displacement beyond edge of scuff plate. Clean as required.
	
	
	

	Note: Displacement within boundaries of scuff plate edge is allowable and not detrimental to aircraft safety. Inspect for bubbles close to vertical surface of block by smearing surface with water and using a strong light viewed from opposite side of block. For bubble criteria, refer to Maintenance Manual.
	
	
	

	15.10 Main landing gear upper and lower fuselage attachment fittings for condition and security.
	
	
	

	
	
	
	

	C 1000.16 33 – LIGHTS 

	
	
	
	

	16.1 Caution light panel and cockpit dome light for condition and security.
	
	
	

	16.2 Horizontal stabilizer deicing boot pressure warning lights for condition and security.
	
	
	

	Effectivity: Pre Mod 6/2028
	
	
	

	16.3 Co-pilot dimming control rheostat for condition and clear from cable routing
	
	
	

	Effectivity: Pre Mod 6/2028
Note: Refer to Service Bulletin No. 6/401, if applicable.
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	16.4 Do a visual inspection of the following lights for condition and security, bonding wires for condition and security of attachment;

 Effectivity: Mod 6/2028
	

	16.4.1 Instrument panel, panel overlay and compass
	
	
	

	16.4.2 Flight compartment flood lights, aisle, eye reference, avionics CB post, instrument panel and visor lights.
	
	
	

	
	
	
	

	16.4.3 Flight compartment instrument panel, trim panel static valve post and selector lights.
	
	
	

	
	
	
	

	16.4.4 Flight compartment dome
	
	
	

	
	
	
	

	16.4.5 Map lights
	
	
	

	
	
	
	

	16.4.6 Caution dimming lights
	
	
	

	
	
	
	

	16.5 Do a visual inspection of the following exterior lights for condition and security, bonding wires for condition and security of attachment;

 Effectivity: Mod 6/2028
	

	16.5.1 Position and strobe
	
	
	

	
	
	
	

	16.5.2 Aircraft exterior position and strobe
	
	
	

	
	
	
	

	16.5.3 Aircraft exterior beacons
	
	
	

	
	
	
	

	16.5.4 Aircraft exterior landing
	
	
	

	Effectivity: Mod 6/2028, 6/2285, 6/2407
	
	
	

	16.5.5 Aircraft exterior wing inspection lights
	
	
	

	
	
	
	

	16.5.6 Position, anti-collision and strobe for condition and security.
	
	
	

	 Effectivity: Pre Mod 6/1513 AND 6/2028

 Note: Refer to Service Bulletin No. 6/57 and A.D 67-33-01 (Pre Mod 6/116), if applicable (Pre Mod 6/2028)
	
	
	

	16.6 Passenger Warning and passenger lights for condition and security.
	
	
	

	 Effectivity: Pre Mod 6/2028
	
	
	

	16.7 Cabin interior boarding lights
	
	
	

	 Effectivity: Mod 6/2028
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	16.8 Cabin interior lighting
	
	
	

	 Effectivity: Mod 6/2028, 6/2427
	
	
	

	C 1000.17 34 - NAVIGATION 

	
	
	
	

	17.1 #1 VOR antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	17.2 #2 VOR antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	17.3 #1 Glide Slope antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	17.4 #2 Glide Slope antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	17.5 Marker beacon antenna for condition, loose connections, entry of moisture and security.
	
	
	

	
	
	
	

	17.6 Marker beacon antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	17.7 Weather radar transmitter and receiver (RDR2000) inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2049
	
	
	

	17.8 Nav systems grounding and bonding wires for condition and security.  Clean as required.
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	17.9 Transponders; KXP 2290 or 2290A;
	

	
	

	17.9.1 Condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.9.2 Perform a power on operational test (Power On).
	
	
	

	
	
	
	

	17.9.3 Inspect bonding of mating surfaces between mounting tray and the nearest airframe ground. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.9.4 Inspect grounding of unit wiring bundle shield brain to airframe structure. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.9.5 #1 lower antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.9.6 #2 lower antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.9.7 #1 upper antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.9.8 #2 upper antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.10 #1 GPS (KGS 200)
	

	 Effectivity: Mod 6/2049, Post Mod 6/2304 & Mod SOO 6388
	

	17.10.1 Inspect for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.10.2 Perform a power on operational test (Power On).
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	17.10.3 Inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.10.4 Inspect antenna bonding of mating surfaces between mounting tray and the nearest airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.10.5 Antenna for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
	
	
	

	 Effectivity: Mod SOO 6388 and Mod 6/2003
	
	
	

	17.11 #2 GPS (KGS 200)
	

	 Effectivity: Mod 6/2049, Post Mod 6/2304 & Mod SOO 6388
	

	17.11.1 Inspect for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.11.2 Perform a power on operational test.
	
	
	

	
	
	
	

	17.11.3 Inspect antenna bonding of mating surfaces between mounting tray and the nearest airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.11.4 Inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.11.5 Antenna for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
	
	
	

	 Effectivity: Mod SOO 6388 and Mod 6/2003
	
	
	

	17.12 #1 DME (KN63)
	

	 Effectivity: Mod 6/2049 & Mod SOO 6388
	

	17.12.1 Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.12.2 Perform power on operational test of transceiver unit.
	
	
	

	
	
	
	

	17.12.3 Inspect transceiver unit bonding of mating surfaces between mounting tray and the nearest airframe ground. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
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	17.12.4 Inspect center fuselage antenna bonding of mating surfaces between mounting tray and the nearest airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.13 #2 DME (KN63)
	

	Effectivity: Mod 6/2049 & Mod SOO 6388
	

	17.13.1 Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.13.2 Perform power on operational test of transceiver unit.
	
	
	

	
	
	
	

	17.13.3 Inspect transceiver unit bonding of mating surfaces between mounting tray and the nearest airframe ground. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.13.4 Inspect antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.14 Inspect center fuselage antenna bonding of mating surfaces between antenna and airframe ground. (<3.0 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.15 #1 Radar Altimeter Unit
	

	 Effectivity: Mod 6/2049 & Mod SOO 6388
	

	17.15.1 Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.15.2 Perform power on operational test of radar altimeter unit.
	
	
	

	
	
	
	

	17.15.3 Inspect bonding of mating surfaces between mounting tray airframe ground. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.15.4 Inspect antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2003 & Mod SOO 6388
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	17.16 #2 Radar Altimeter Unit
	

	Effectivity: Mod 6/2049 & Mod SOO 6218
	

	17.16.1 Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.16.2 Perform power on operational test of radar altimeter unit.
	
	
	

	
	
	
	

	17.16.3 Inspect bonding of mating surfaces between mounting tray and airframe ground. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.16.4 Inspect antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6/2003 & Mod SOO 6388
	
	
	

	17.17 Inspect Radar Altimeter unit antenna’s #3 & #4 bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003 & Mod SOO 6388
	
	
	

	17.18 #1 TCAS I Processor Unit (KTA 970)
	

	 Effectivity: Mod 6/2049 & Mod SOO 6382
	

	17.18.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.18.2 Perform power on operational test of processor unit (Power On).
	
	
	

	
	
	
	

	17.18.3 Inspect bonding of mating surfaces between mounting tray airframe ground. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7,  Para 12 for details.
	
	
	

	17.18.4 Inspect upper antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003 & Mod SOO 6382
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	17.18.5 Inspect lower antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003 & Mod SOO 6382
	
	
	

	17.19 #2 TCAS II Processor Unit (KTA 970)
	

	 Effectivity: Mod 6/2049 & Mod SOO 6219
	

	17.19.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.19.2 Perform power on operational test of processor unit.
	
	
	

	
	
	
	

	17.19.3 Inspect bonding of mating surfaces between mounting tray and airframe ground. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.19.4 Inspect upper antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003 & Mod SOO 6219
	
	
	

	17.20 EGPWS (MK VI)
	

	 Effectivity: Mod 6/2049 & Mod SOO 6387
	

	17.20.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.20.2 Perform power on operational test of EGPWS unit.
	
	
	

	
	
	
	

	17.20.3 Inspect bonding of mating surfaces between mounting tray and airframe ground. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.21 #1 ADAHRS (KSG 7200)
	

	 Effectivity: Mod 6/2049
	

	17.21.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.21.2 Perform power on operational test of EGPWS unit.
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	17.21.3 Inspect bonding of mating surfaces between mounting tray and airframe ground. (<1.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.22 #2 ADAHRS (KSG 7200)
	

	 Effectivity: Mod 6/2049 & Mod SOO 6209
	

	17.22.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.22.2 Perform power on operational test of EGPWS unit.
	
	
	

	
	
	
	

	17.22.3 Inspect bonding of mating surfaces between mounting tray and airframe ground. (<1.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.23 ADAHRS - Magnetometer (KSG 7210)
	

	 Effectivity: Mod 6/2049 & Mod SOO 6209 and Pre Mod 6/2171
	

	17.23.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.23.2 Inspect bonding of mating surfaces between mounting feet and airframe structure. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.24 ADAHRS - Magnetometer (KSG 7210)
	

	 Effectivity: Mod 6/2049 & Mod SOO 6209 and Post Mod 6/2171
	

	17.24.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	17.24.2 Inspect bonding of mating surfaces between mounting feet and airframe structure. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.25 #1 ADF Antenna
	

	 Effectivity: Mod 6/2003 & Mod SOO 6209
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	17.25.1 Inspect bonding of mating surfaces between the antenna and the airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.26 #2 ADF Antenna
	

	 Effectivity: Mod 6/2003 & Mod SOO 6209
	

	17.26.1 Inspect bonding of mating surfaces between the antenna and the airframe ground. (<3.0 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.27 XM antenna - Inspect bonding of mating surfaces between the antenna and the airframe ground. (<2.5 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2003
	
	
	

	C 1000.18 36 - PNEUMATIC 

	
	
	
	

	18.1 Instrument pneumatic system filter for long nose aircraft with (Mod 6/1046) bleed air or (Mod 6/1166) engine driven pump systems.
	
	
	

	
	
	
	

	18.2 Remove and install new filters and leak check.
	
	
	

	
	
	
	

	C 1000.19 44 – CABIN SYSTEMS 

	
	
	
	

	19.1.1 Inspect grounding of cabin speakers and airframe structure. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod SOO 6/221 & Mod 6/2049
	
	
	

	19.2 NAT 245 PA Amplifier
	

	 Effectivity: Mod SOO 6/2010 & Mod 6/2049
	

	19.2.1 Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	
	
	
	

	19.2.2 Inspect grounding of unit wire bundle shield braid to airframe structure. (<2.5 milliohms).
	
	
	

	 Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
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	C 1000.20 52 – DOORS

	
	
	
	

	20.1 Flight compartment LH and RH doors to airframe for bonding. (<10 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2024
	
	
	

	20.2 Cabin LH and RH doors to airframe for bonding. (<10 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2024
	
	
	

	20.3 Airstair door to airframe for bonding. (<10 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2024
	
	
	

	20.4 Aft baggage compartment door to airframe for bonding. (<10 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2024
	
	
	

	20.5 Fwd baggage compartment door to airframe for bonding. (<10 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2020 & Mod 6/2161
	
	
	

	C 1000.21 53 – FUSELAGE 

	
	
	
	

	21.1 External structure for dents, scores, fretting and cracks, fasteners for security.
	
	
	

	
	
	
	

	21.2 Radome for condition, cracks, delamination and security.
	
	
	

	
	
	
	

	21.3 Nose baggage compartment to radome joint diverter strip (qty 4) for electrical bonding. (<10 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	21.4 Radio equipment racks for cracks, buckling and corrosion.  Vibration isolators for deterioration.  Clean as required.
	
	
	

	
	
	
	

	21.5 Rear baggage compartment for condition. Equipment shelves for cracks, buckling and corrosion.  Clean as required.
	
	
	

	Note:  In addition, when Mod 6/2020 or Mod 6/2160 is installed at STA 44.0 nose attachment, pay particular attention for the corrosion to the exterior aluminum joint straps and fasteners common to the carbon nose.
	
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	
	
	

	21.6 Fuel gallery structure for corrosion.
	
	
	

	
	
	
	

	21.7 Inspect fuel gallery access panels and seals for damage. Repair or replace as required.
	
	
	

	Effectivity: Mod 6/2408
	
	
	

	21.8 Nose baggage bulkhead at STA 15.45 for condition, security and corrosion between aluminum brackets and fasteners attached to the carbon nose.
	
	
	

	
	
	
	

	21.9 Cargo tie-downs located on STA 15.45 bulkhead for condition and security.
	
	
	

	
	
	
	

	21.10 Inspect the nose baggage compartment weather radar wiring metal conduit to airframe for electrical bonding. (<10 milliohms).
	
	
	

	Effectivity: Mod 6/2020 & 6/2160
	
	
	

	21.11 Inspect the nose baggage compartment fuselage circumferential aluminum strap joint for electrical bonding. (<10 milliohms).
	
	
	

	Effectivity: Mod 6/2020 & 6/2160
	
	
	

	21.12 Ensure bonding jumpers in nose baggage compartment have no sign of corrosion, braid damage such as kinks, fretting or fraying, cracked or broken terminal ends.
	
	
	

	
	
	
	

	21.13 Inspect forward avionics compartment shelves to airframe for bonding. (<2.5 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2005
	
	
	

	21.14 Inspect forward avionics compartment shelves bonding jumpers have no sign of corrosion, braid damage such as kinks, fretting or fraying, cracked or broken terminal ends. 

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	Effectivity: Mod 6/2005
	
	
	

	21.15 Inspect aft avionics compartment shelves to airframe for bonding. (<2.5 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2028
	
	
	

	21.16 Ensure aft avionics equipment shelves bonding jumpers have no sign of corrosion, braid damage such as kinks, fretting or fraying, cracked or broken terminal ends.
	
	
	

	Effectivity: Mod 6/2028
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	C 1000.22 54 – NACELLE - LH

	
	
	
	

	22.1 Nacelle fairing to airframe for bonding. (<10 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2021
	
	
	

	C 1000.23 54 – NACELLE - RH

	
	
	
	

	23.1 Nacelle fairing to airframe for bonding. (<10 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

Effectivity: Mod 6/2021
	
	
	

	C 1000.24 55 – STABILIZER - LH

	
	
	
	

	24.1 Mid hinge arm adapter place for condition, corrosion, fasteners for security and bearings for condition
	
	
	

	Effectivity: Pre Mod 6/1341
	
	
	

	C 1000.25 55 – STABILIZER - RH

	
	
	
	

	25.1 Mid hinge arm adapter place for condition, corrosion, fasteners for security and bearings for condition
	
	
	

	Effectivity: Pre Mod 6/1341
	
	
	

	C 1000.26 56 – WINDOWS

	
	
	
	

	26.1 Flight compartment windshield and door windows for condition, crazing and security, retaining strips for condition and security of attachment. For SOO 6320 or 6321, if installed, inspect vent for condition and security of attachment. Replace as required.
	
	
	

	
	
	
	

	26.2 Flight compartment LH and RH doors to airframe for bonding. (<10 milliohms).
	
	
	

	Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.

 Effectivity: Mod 6024
	
	
	

	26.3 Cabin windows for condition, crazing and security. Inspect vents (SOO 6368) for condition and security of attachment.  Replace if required.
	
	
	

	
	
	
	

	26.4 Cabin side escape hatch windows for condition, crazing and security. Replace if required.
	
	
	

	
	
	
	

	26.5 Cabin door windows for condition, crazing and security. Replace if required.
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	C 1000.27 57 – WING – LH 

	
	
	
	

	27.1 All accessible electrical wiring for deterioration, chafing, bonding wire for fraying, corrosion and security of attachment, connector for cleanliness and security.
	
	
	

	
	
	
	

	27.2 Outboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
	
	
	

	
	
	
	

	27.3 Inboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
	
	
	

	
	
	
	

	27.4 Outboard foreflap pushrod fork attachment for corrosion and security of attachment.
	
	
	

	
	
	
	

	27.5 Inboard foreflap pushrod fork attachment for corrosion and security of attachment.
	
	
	

	
	
	
	

	27.6 Do a detailed visual inspection of the ailerons as follows;
	

	
	

	27.6.1 Nose and tail skins for condition, dents, scores, abrasions and fasteners for security.
	
	
	

	
	
	
	

	27.6.2 Trim and gear tab hinge adapter for corrosion, wear, security and freedom of movement. Lubricate.
	
	
	

	
	
	
	

	27.6.3 Bellcrank structure channels for condition, fasteners for security, bearings for freedom of operation and security.
	
	
	

	
	
	
	

	27.6.4 Aileron trim and gear tab skins for condition, buckling and fasteners for security.
	
	
	

	
	
	
	

	27.6.5 Hing arms for condition, corrosion and security.
	
	
	

	
	
	
	

	27.6.6 Trim tab hinge for condition, corrosion, wear and freedom of movement. Lubricate.
	
	
	

	
	
	
	

	C 1000.28 57 – WING – RH 

	
	
	
	

	28.1 All accessible electrical wiring for deterioration, chafing, bonding wire for fraying, corrosion and security of attachment, connector for cleanliness and security.
	
	
	

	
	
	
	

	28.2 Outboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
	
	
	

	
	
	
	

	28.3 Inboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
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	28.4 Outboard foreflap pushrod fork attachment for corrosion and security of attachment.
	
	
	

	
	
	
	

	28.5 Inboard foreflap pushrod fork attachment for corrosion and security of attachment.
	
	
	

	
	
	
	

	28.6 Do a detailed visual inspection of the aileron as follows;
	

	
	

	28.6.1 Nose and tail skins for condition, dents, scores, abrasions and fasteners for security.
	
	
	

	
	
	
	

	28.6.2 Trim and gear tab hinge adapter for corrosion, wear, security and freedom of movement. Lubricate.
	
	
	

	
	
	
	

	28.6.3 Bellcrank structure channels for condition, fasteners for security, bearings for freedom of operation and security.
	
	
	

	
	
	
	

	28.6.4 Aileron trim and gear tab skins for condition, buckling and fasteners for security.
	
	
	

	
	
	
	

	28.6.5 Hing arms for condition, corrosion and security.
	
	
	

	
	
	
	

	28.6.6 Trim tab hinge for condition, corrosion, wear and freedom of movement. Lubricate.
	
	
	

	
	
	
	

	C 1000.29 61 – PROPELLERS – LH 

	
	
	
	

	29.1 Stall warning cam limit microswitch mechanism and propeller reset limit switch for condition and security, connect for security.
	
	
	

	
	
	
	

	C 1000.30 61 – PROPELLERS – RH 

	
	
	
	

	30.1 Stall warning cam limit microswitch mechanism and propeller reset limit switch for condition and security, connect for security.
	
	
	

	
	
	
	

	C 1000.31 71 – POWERPLANT - LH

	
	
	
	

	31.1 Remove intake deflector air line filters at inlet and return ports of air control valves.
	
	
	

	
	
	
	

	31.2 Inspect intake deflector air line filters at inlet and return ports of air control valves.
	
	
	

	
	
	
	

	31.3 Install intake deflector air line filters at inlet and return ports of air control valves.
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	C 1000.32 71 – POWERPLANT - RH

	
	
	
	

	32.1 Remove intake deflector air line filters at inlet and return ports of air control valves.
	
	
	

	
	
	
	

	32.2 Inspect intake deflector air line filters at inlet and return ports of air control valves.
	
	
	

	
	
	
	

	32.3 Install intake deflector air line filters at inlet and return ports of air control valves.
	
	
	

	
	
	
	

	C 1000.33 76 – ENGINE CONTROLS 

	
	
	
	

	33.1 Overhead console flight control and flap selector aluminum quadrants for condition and security, freedom of movement, cable attachment for security.
	
	
	

	
	
	
	

	33.2 Overhead console flight control and flap selector pulleys for smoothness and freedom of operation.
	
	
	

	
	
	
	

	C 1000.34 OPERATIONAL CHECKS

	
	

	34.1 Perform the following Operational Checks;
	

	
	

	34.1.1 Instrument pneumatic system for correct vacuum and/or pressure, as applicable.
	
	
	

	
	
	
	

	34.1.2 Bleed air shutoff valves.
	
	
	

	
	
	
	

	34.1.3 Wing tank fuel system (SOO 6095 and 6247). Power On.
	
	
	

	
	
	
	

	34.1.4 ECTM/FOQA (IONode) (SOO 6288) Data Capture System. Power on.
	
	
	

	
	
	
	

	34.1.5 QAR (SOO 6356). Power on.
	
	
	

	
	
	
	

	34.1.6 STA 111 Cabin Fans (SOO 6378). Power on.
	
	
	

	
	
	
	

	34.1.7 STA 332 Blower (SOO 6379). Power on.
	
	
	

	
	
	
	

	34.2 Leak check the following items, as applicable, after installation;
	

	
	

	34.2.1 Instrument pneumatic system (bleed air) filters.
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	C 1000.35 POST INSPECTION

	
	
	
	

	35.1 Inspect for operation and leaks.
	
	
	

	
	
	
	

	35.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	35.3 Clean aircraft and engine once maintenance is completed.
	
	
	

	
	
	
	

	35.4 Perform Functional Check Flight if required per DHC-6 Maintenance Manual or AFM as appropriate.
	
	
	

	
	
	
	

	35.5 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	

	
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6 – C 1000RT – 1000 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


