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Reference:  DHC-6 Maintenance Program, Viking PSM Maintenance Manual

	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	C 1500.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	DHC-6
MP
	
	

	
	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	DHC-6

MP
	
	

	
	
	
	

	C 1500.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	
	
	
	

	C 1500.3  CORROSION CONTROL

	
	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	Appendix

B
	
	

	
	
	
	

	C 1500.4 PREPARATION

	
	
	
	

	4.1 Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	C 1500.5 21 – AIR CONDITIONING 

	
	
	
	

	5.1 Heater ejector for condition and security.
	
	
	

	
	
	
	

	5.2 Heater silencer for condition and security, insulation for condition and security.
	
	
	

	
	
	
	

	5.3 Ram air and cabin air control valves operating mechanism for ease of operation and security; flexible cable, clamps and brackets for condition and security.
	
	
	

	
	
	
	

	5.4 Duct temperature sensor and duct overheat switch for security.
	
	
	

	
	
	
	

	5.5 Outside air temperature sensor for security.
	
	
	

	
	
	
	

	5.6 Cabin temperature sensor for condition and security.
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	5.7 Heating system hot air valve for security.
	
	
	

	
	
	
	

	5.8 Ram air screens scoop and duct for condition.
	
	
	

	Effectivity: Pre Mod 6/1070
	
	
	

	5.9 Main ram air duct ground operable fan for security.
	
	
	

	
	
	
	

	5.10 Flight compartment and cabin heater ducts for condition and evidence of overheat, connections for security. Ducts for condition and delamination, supporting structure for condition and security.
	
	
	

	
	
	
	

	5.11 L/H nacelle bleed air shut off valve for condition and security.
	
	
	

	
	
	
	

	5.12 R/H nacelle bleed air shut off valve for condition and security.
	
	
	

	
	
	
	

	5.13 Electrical wiring and connectors forward of instrument panel for condition and security, bonding wires for condition.
	
	
	

	
	
	
	

	C 1500.6 23 – COMMUNICATIONS

	
	
	
	

	6.1 VHF/FM unit for condition and security of mounting, electrical cables for condition and connector for security. Clean as required.
	
	
	

	
	
	
	

	6.2 Radio navigation equipment shock mounts for condition, cracks, corrosion and security, vibration isolators for condition, bonding wire for condition and security.
	
	
	

	
	
	
	

	C 1500.7 24 – ELECTRICAL POWER

	
	
	
	

	7.1 Circuit breaker panels for condition and security
	
	
	

	Note: Refer to A.D. 70-22-04, if applicable.
	
	
	

	7.2 Nose electrical wiring and connectors forward of instrument panel for condition and security, bonding wires for condition.
	
	
	

	
	
	
	

	7.3 Electrical wiring and connectors under flight compartment floor for condition and security, bonding wires for condition.
	
	
	

	
	
	
	

	7.4 Electrical wiring in flight compartment for condition and connectors for security.
	
	
	

	
	
	
	

	7.5 Electrical wiring and connectors in empennage for condition and security, bonding wires for condition.
	
	
	

	
	
	
	

	7.6 External power for condition and security, bus bars for condition.
	
	
	

	
	
	
	

	7.7 Battery relays for condition and security, bus bars for condition.
	
	
	

	Effectivity: SOO 6371
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	C 1500.8 25 - EQUIPMENT/FURNISHINGS 

	
	
	
	

	8.1 First aid kit for required content, proper stowage and security.
	
	
	

	
	
	
	

	8.2 14-volt outlet for condition and security, bonding wires for condition and security of attachment.
	
	
	

	Effectivity: Mod 6/2028
	
	
	

	8.3 28-volt outlet for condition and security, bonding wires for condition and security of attachment.
	
	
	

	Effectivity: Mod 6/2028
	
	
	

	8.4 Flight compartment axe and axe stowage for condition and security of axe stowage structure. Condition and security of axe cutting edge and pie to axe handle.
	
	
	

	Effectivity: SOO 6376
	
	
	

	C 1500.9 26 – FIRE PROTECTION 

	
	
	
	

	9.1 L/H engine fire protection wiring and connectors for condition and security, clips for security.  Clean as required.
	
	
	

	
	
	
	

	9.2 R/H engine fire protection wiring and connectors for condition and security, clips for security.  Clean as required.
	
	
	

	
	
	
	

	C 1500.10 27 – FLIGHT CONTROLS 

	
	
	
	

	10.1 Flap selector lever for condition, proper detent action of movement and security.  Lubricate.
	
	
	

	
	
	
	

	C 1500.11 28 – FUEL

	
	
	
	

	11.1 Fuel system position indicator for condition and security.
	
	
	

	Effectivity: SOO 6235 Pre Mod 6/2009
	
	
	

	11.2 Capacitance tank units for corrosion, security and leakage.
	
	
	

	
	
	
	

	11.3 Fuel quantity signal conditioner for corrosion, security of wiring and connectors.
	
	
	

	Effectivity: Mod 6/2046
	
	
	

	11.4 Fuel cells for security and leakage, cell vent necks and vent lines for condition and leakage.
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	C 1500.12 29 – HYDRAULIC POWER  

	
	
	
	

	12.1 Hydraulic and brake system pressure indicators for condition, security and leakage.
	
	
	

	Effectivity: Pre Mod 6/2002
	
	
	

	12.2 Hydraulic and brake system pressure sensors for condition, security and leakage.
	
	
	

	Effectivity: Pre Mod 6/2002
	
	
	

	C 1500.13 30 – ICE AND RAIN PROTECTION

	
	
	
	

	13.1 Heated windscreen temperature controllers for condition and security, connectors for security.
	
	
	

	
	
	
	

	13.2 Windshield heat relay box for damage and security, connectors for security.
	
	
	

	
	
	
	

	13.3 L/H propeller blade deicing electrical harness for security of connections.
	
	
	

	
	
	
	

	13.4 R/H propeller blade deicing electrical harness for security of connections.
	
	
	

	
	
	
	

	13.5 Inspect the windshield wiper system as follows;
	

	
	

	13.5.1 Wiper motor for security of attachment.
	
	
	

	
	
	
	

	13.5.2 Converters for condition and freedom of movement
	
	
	

	
	
	
	

	13.5.3 Flexible drives for condition, security and freedom of operation, evidence of water ingress.
	
	
	

	
	
	
	

	13.5.4 Wiring and connectors for condition and security.
	
	
	

	
	
	
	

	C 1500.14 31 – INSTRUMENTS

	
	
	
	

	14.1 Instrument panels for condition and security, bonding wires for condition and security.
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	C 1500.15 32 – LANDING GEAR 

	
	
	
	

	15.1 Nose landing gear torque arms, bushing and pip-pin for wear, condition, corrosion and security, pip-pin chain for security.
	
	
	

	
	
	
	

	15.2 Nose gear attachment fittings for corrosion and cracks, pre-load bolt torque marks for proper alignment.
	
	
	

	
	
	
	

	15.3 Inspect the main landing gear shock absorbing blocks as follows.
	
	

	Note: Refer to Maintenance Manual.
	
	

	15.3.1 Permanent set and gaps between compression blocks and separator plates.
	
	
	

	
	
	
	

	15.3.2 Upper to lower platen and preload bolt dimension.
	
	
	

	Effectivity: Pre-Mod and Mod 6/1469 standard compression blocks
	
	
	

	15.3.3 Rebound block and plate for condition, corrosion and separation.
	
	
	

	
	
	
	

	15.4 Landing gear stay struts for cracks, corrosion and security.
	
	
	

	
	
	
	

	C 1500.16 33 – LIGHTS

	
	
	
	

	16.1 Anti-collision (Beacon) light for condition and operation.
	
	
	

	Effectivity: Pre Mod 6/2028 A.D 67-33-01, if applicable
	
	
	

	16.2 Strobe light flasher unit (if installed) for condition, connector for security.
	
	
	

	Effectivity: Pre Mod 6/2028
	
	
	

	16.3 R/H wing position light power supply (if installed) for condition and security.
	
	
	

	Effectivity: Pre Mod 6/2447 and Mod 6/2028
	
	
	

	16.4 Cabin interior passenger warning lights for condition and security.
	
	
	

	Effectivity: Pre Mod 6/2028
	
	
	

	16.5 Cabin interior passenger lights for condition and security.
	
	
	

	Effectivity: Pre Mod 6/2028
	
	
	

	16.6 Nose baggage compartment lights for condition and security.
	
	
	

	
	
	
	

	16.7 Aft baggage compartment lights for condition and security.
	
	
	

	
	
	
	

	16.8 Door unlocked warning system for condition and security, limit switches and actuator mechanisms for condition and security. Operate each door separately.
	
	
	

	
	
	
	

	16.9 Flight and cabin electrical wiring in ceiling area for condition, connectors and security. Clean and required.
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	C 1500.17 34 – NAVIGATION

	
	
	
	

	17.1 Pitot static systems selector valve for security and smooth operation, pipes for condition and connections for security.
	
	
	

	
	
	
	

	C 1500.18 36 – PNEUMATIC 

	
	

	18.1 Inspect the instrument pneumatic system nose baggage compartment bleed air, vacuum or engine driven pump installation as follows;
	

	Effectivity: Mods 6/1077, 6/1166
	

	18.1.1 L/H engine pressure regulators for damage and security.
	
	
	

	
	
	
	

	18.1.2 L/H engine pressure relief valves for damage and security.
	
	
	

	
	
	
	

	18.1.3 L/H engine mounting plates for cracks, damage and security.
	
	
	

	
	
	
	

	18.1.4 L/H Automatic water drain for security
	
	
	

	
	
	
	

	18.1.5 R/H Automatic water drain for security
	
	
	

	
	
	
	

	18.1.6 R/H engine pressure regulators for damage and security.
	
	
	

	
	
	
	

	18.1.7 R/H engine pressure relief valves for damage and security.
	
	
	

	
	
	
	

	18.1.8 R/H engine mounting plates for cracks, damage and security.
	
	
	

	
	
	
	

	18.1.9 All pipes for condition, connections for security, flexible hoses for condition.
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	C 1500.19 52 – DOORS

	
	
	
	

	19.1 L/H flight compartment door for condition, corrosion and security, seals for condition and security.
	
	
	

	
	
	
	

	19.2 R/H flight compartment door for condition, corrosion and security, seals for condition and security
	
	
	

	19.3 L/H cabin doors for condition, corrosion and security, seals for condition and security
	
	
	

	
	
	
	

	19.4 R/H cabin doors for condition, corrosion and security, seals for condition and security
	
	
	

	
	
	
	

	19.5 Inspect the airstair door as follows (If installed):
	

	19.5.1 Condition and security, seals for condition and security.
	
	
	

	
	
	
	

	19.5.2 Handrail and springs for condition and security including proper stowage.
	
	
	

	
	
	
	

	19.5.3 Springs for security and operation.
	
	
	

	
	
	
	

	19.5.4 Cables for condition and security of attachment, protective cable covers for tears and deterioration.
	
	
	

	
	
	
	

	19.5.5 Restraint unit, if installed, for corrosion, security of attachment and smooth movement of operation.
	
	
	

	Effectivity: Mod 6/2326 & 6/2386
	
	
	

	19.6 Rear baggage compartment doors for condition and security, seals for condition, door handle and lock for condition and proper operation. Clean as required.
	
	
	

	
	
	
	

	19.7 Nose baggage compartment doors latches for condition, security, and proper operation.
	
	
	

	
	
	
	

	19.8 L/H cabin doors for condition, corrosion and security, seals for condition and security
	
	
	

	
	
	
	

	19.9 R/H cabin doors for condition, corrosion and security, seals for condition and security
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	C 1500.20 53 – FUSELAGE

	
	
	
	

	20.1 L/H fuselage frame wing attach lugs @ Sta. 239.88 for condition, cracking, corrosion and fasteners for security.
	
	
	

	Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges. Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required.
	
	

	20.2 R/H fuselage frame wing attach lugs @ Sta. 239.88 for condition, cracking, corrosion and fasteners for security.
	
	
	

	Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges.  Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required.


	
	

	20.3 Elevator Bellcrank and Hyd. Hand pump attaching structure for condition, cracking and security of fasteners.
	
	
	

	Note:  Refer to Service Bulletin N. 6/348 and AD 77-03-07 & 93-09-04 if applicable. 
	
	
	

	C 1500.21 54 – LH NACELLE

	21.1 Internal structure of wing and nacelle, where accessible, for condition, cracks, buckling and corrosion.  Waste fuel return pipes (if installed for condition, connections for leakage and security.
	
	
	

	
	
	
	

	C 1500.22 54 – RH NACELLE

	
	
	
	

	22.1 Internal structure of wing and nacelle, where accessible, for condition, cracks, buckling and corrosion.  Waste fuel return pipes (if installed for condition, connections for leakage and security.
	
	
	

	
	
	
	

	C 1500.23 55 – STABILIZERS

	
	

	23.1 Inspect the horizontal stabilizer as follows;
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	23.1.1 Accessible internal structure of for corrosion, cracks, buckling and security.
	
	
	

	Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges.  Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required. Corrosion around bonding jumpers where fitted, will necessitate cleaning and re-priming of effected areas, as applicable.
	
	

	23.1.2 Top upper skin, skin doubler beneath center pickup fitting for cracking.
	
	
	

	
	
	
	

	23.1.3 Lower skin between Stations 30.00 and 35.00 for condition, cracks, distortion and fasteners for security.
	
	
	

	
	
	
	

	23.1.4 Leading edge skins for condition, dents, scores and fastener security. Aft of deicing boots for surface corrosion.
	
	
	

	Effectivity: SOO 6004
	
	
	

	23.1.5 Fwd and Aft spar webs between attachment brackets and center line for condition, cracks and fasteners for security.
	
	
	

	Note:  Refer to Service Bulletin No. 6/310 and A.D. 74-22-06, if applicable.
	
	
	

	23.1.6 External skin structure for dents, scores, abrasions corrosion, cracks and buckling and fasteners for security.
	
	
	

	.
	
	
	

	23.1.7 Fwd and Aft spar webs between attachment brackets and center line for condition, cracks and fasteners for security.
	
	
	

	Note:  Refer to Service Bulletin No. 6/310 and A.D. 74-22-06, if applicable.
	
	
	

	23.1.8 External skin structure for dents, scores, abrasions corrosion, cracks and buckling and fasteners for security.
	
	
	

	.
	
	
	

	23.2 Inspect the vertical stabilizer as follows;
	

	Effectivity: Mod 6/2417
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	23.2.1 Accessible internal structure for corrosion, cracks, buckling and security.
	
	
	

	Note:  Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges.  Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required. Corrosion around bonding jumpers where fitted, will necessitate cleaning and re-priming of effected areas, as applicable.
	
	

	23.2.2 Top hinge arm adapter fitting for condition, corrosion and security.
	
	
	

	Effectivity: Pre Mod 6/1339
	
	
	

	23.2.3 Mid hinge arm adapter fitting for condition, fretting, corrosion and security.
	
	
	

	Effectivity: Pre Mod 6/1340
	
	
	

	23.2.4 External skin structure for dents, scores, abrasions corrosion, cracks and buckling and fasteners for security.
	
	
	

	.
	
	
	

	23.3 Inspect the rudder as follows;
	

	
	

	23.3.1 Skins for condition, dents, scores, buckles, leading edge silicon aerodynamic seal for adhesion and security, fasteners for security.
	
	
	

	
	
	
	

	23.3.2 Lower hinge arm for condition, corrosion, fasteners for security and bearing for condition.
	
	
	

	Note:  As bearing deterioration results in rudder drop this bearing should be replaced when wear is noted. A gap dimension between the lower hinge arm housing and the rudder hinge arm bearing support plate of 0.058 inch (1.47 mm) will indicate that the bearing manufacture's axial service limit has been reached. A smaller gap dimension requires the bearing to be replaced at the earliest opportunity available.

Effectivity:  Pre Mod and Post Mod 6/1340
	
	

	23.3.3 Mid and upper hinge arm adapter fitting for condition corrosion and fasteners for security.
	
	
	

	Effectivity: Pre Mod 6/1339


	
	
	

	23.3.4 Mid and upper hinge arms for condition corrosion and fasteners for security.
	
	
	

	Effectivity: Pre Mod 6/1339
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	23.3.5 Mass balance weight for condition and security. Move rudder vigorously to detect movement of internal weights.
	
	
	

	
	
	
	

	23.3.6 Rudder trim and gear tabs skins for condition, dents, scores, buckles and fasteners for security, hinge arms for condition, hinges for condition, corrosion, security and freedom of movement.  Lubricate.
	
	
	

	
	
	
	

	23.3.7 Rear spar tab hinge for condition, corrosion and freedom of movement.  Lubricate.
	
	
	

	
	
	
	

	23.4 Inspect the elevator as follows;
	

	
	

	23.4.1 Skins for condition, dents, scores, buckles, leading edge silicon aerodynamic seal for adhesion and security, fasteners for security.
	
	
	

	
	
	
	

	23.4.2 Mid and upper hinge arm adapter fitting for condition corrosion and fasteners for security.
	
	
	

	Effectivity: Pre Mod 6/1342
	
	
	

	23.4.3 Mid hinge arm adapter fitting for condition, fretting, corrosion and security.
	
	
	

	Effectivity: Pre Mod 6/1342
	
	
	

	23.4.4 Trim and interconnect tab skins for condition, dents, scores, buckles. Fasteners for security, hinge arms for condition, hinges for condition, corrosion, security and freedom of movement.  Lubricate
	
	
	

	
	
	
	

	23.4.5 Torque tube for condition, corrosion, security and freedom of movement.  
	
	
	

	
	
	
	

	23.4.6 Trim and interconnect tab hinge adapter for condition, corrosion, security and freedom of movement.  Lubricate
	
	
	

	
	
	
	

	23.4.7 Mass balance weights for condition, carrion and security.
	
	
	

	
	
	
	

	23.5 Electrical wiring and connectors in empennage for condition and security, bonding wires for condition and security.
	
	
	

	
	
	
	

	C 1500.24 57 – LH WING

	
	
	
	

	24.1 Wing lower skin between station 97.00 and 235.00 (wing pick-up fitting) for cracks, buckling and fasteners for security.
	
	
	

	
	
	
	

	24.2 Wing upper skin between station 147.00 and 210.00 (wing pick-up fitting) for cracks, buckling and fasteners for security.
	
	
	

	
	
	
	

	24.3 Wing main spar (strut link) lug for condition, corrosion and bush for security.
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	24.4 Nose spar adapter D nose section for condition, corrosion and fasteners for security, leading edge skin for condition, corrosion and security, hinges for condition and smooth operation of D nose leading edge cover, stay bar for condition and security of stowage.
	
	
	

	24.5 Wing tip fairing for cracks, delamination and security.
	
	
	

	
	
	
	

	24.6 Wing strut skins condition, dents, scores and fasteners for security.
	
	
	

	Note:  Refer to Service Bulletin N. 6/342 and A.D. 97-07-10, if applicable.
	
	
	

	24.7 Wing strut link for condition, corrosion and bush for security.
	
	
	

	Effectivity:  Pre Mod 6/1174
	
	
	

	24.8 Internal structure of wing, where accessible, for condition, cracks, buckling and corrosion. Waste fuel return pipes (if installed) for condition, connections for leakage and security.
	
	
	

	
	
	
	

	24.9 Internal structure of nacelle, where accessible, for condition, cracks, buckling and corrosion.
	
	
	

	
	
	
	

	24.10 Aileron bellcranks for corrosion and security, bearings for condition. Clean as required. 
	
	
	

	
	
	
	

	24.11 Flap bellcranks for corrosion and security, bearings for condition. Clean as required. 
	
	
	

	
	
	
	

	C 1500.25 57 – RH WING

	
	
	
	

	25.1 Wing lower skin between station 97.00 and 235.00 (wing pick-up fitting) for cracks, buckling and fasteners for security.
	
	
	

	
	
	
	

	25.2 Wing upper skin between station 147.00 and 210.00 (wing pick-up fitting) for cracks, buckling and fasteners for security.
	
	
	

	
	
	
	

	25.3 Wing main spar (strut link) lug for condition, corrosion and bush for security.
	
	
	

	
	
	
	

	25.4 Nose spar adapter D nose section for condition, corrosion and fasteners for security, leading edge skin for condition, corrosion and security, hinges for condition and smooth operation of D nose leading edge cover, stay bar for condition and security of stowage.
	
	
	

	25.5 Wing tip fairing for cracks, delamination and security.
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	25.6 Wing strut skins condition, dents, scores and fasteners for security.
	
	
	

	Note:  Refer to Service Bulletin N. 6/342 and A.D. 97-07-10, if applicable.
	
	
	

	25.7 Wing strut link for condition, corrosion and bush for security.
	
	
	

	Effectivity:  Pre Mod 6/1174
	
	
	

	25.8 Internal structure of wing, where accessible, for condition, cracks, buckling and corrosion. Waste fuel return pipes (if installed) for condition, connections for leakage and security.
	
	
	

	
	
	
	

	25.9 Internal structure of nacelle, where accessible, for condition, cracks, buckling and corrosion.
	
	
	

	
	
	
	

	25.10 Wing main hinge arms for corrosion, cracks and wear.
	
	
	

	Effectivity:  Pre Mod 6/1334
	
	
	

	25.11 Flap hinge arm attachments for condition, cracking, corrosion and jo-bolts for security.
	
	
	

	Effectivity:  Pre Mod 6/1335
	
	
	

	25.12 Inboard and outboard foreflap hinge arms for condition, corrosion, security and bearings for security.
	
	
	

	Effectivity:  Pre Mod 6/1336 and 6/1349
	
	
	

	25.13 Wing inboard trailing flap hinge arms for condition, corrosion, security and bearings for security.
	
	
	

	Effectivity:  Pre Mod 6/1337
	
	
	

	25.14 Aileron hinge arms for condition, corrosion, security and bearings for security.
	
	
	

	Effectivity:  Pre Mod 6/1338
	
	
	

	25.15 Aileron bellcranks for corrosion and security, bearings for condition. Clean as required. 
	
	
	

	
	
	
	

	25.16 Flap bellcranks for corrosion and security, bearings for condition. Clean as required. 
	
	
	

	
	
	
	

	C 1500.26 61 – L/H PROPELLER

	
	

	26.1 Inspect the propeller controls as follows;
	

	
	

	26.1.1 Pulleys for condition, freedom of operation and security.
	
	
	

	26.1.2 Levers, pushrods and reversing linkage for security, springs for condition and security, stops for security.
	
	
	

	
	
	
	

	26.1.3 Teleflex control to reverse valve for condition, kinks, smooth operation and security.
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	26.1.4 Constant speed governor, speed adjusting lever proper attachment to shaft.
	
	
	

	Note:  Refer to TAB 635/4
	
	
	

	26.1.5 Linkages for condition and security.
	
	
	

	
	
	
	

	26.2 Do a detailed visual inspection of cable terminals as follows;
	

	26.2.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	26.2.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	26.2.3 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	26.2.4 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	26.2.5 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 26.2.1, rig the control system.
	
	
	

	
	
	
	

	26.2.6 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	26.3 Tachometer for condition and security of installation.
	
	
	

	
	
	
	

	C 1500.27 61 – R/H PROPELLER

	
	

	27.1 Inspect the propeller controls as follows;
	

	
	

	27.1.1 Pulleys for condition, freedom of operation and security.
	
	
	

	27.1.2 Levers, pushrods and reversing linkage for security, springs for condition and security, stops for security.
	
	
	

	
	
	
	

	27.1.3 Teleflex control to reverse valve for condition, kinks, smooth operation and security.
	
	
	

	
	
	
	

	27.1.4 Constant speed governor, speed adjusting lever proper attachment to shaft.
	
	
	

	Note:  Refer to TAB 635/4
	
	
	

	27.1.5 Linkages for condition and security.
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	27.2 Do a detailed visual inspection of cable terminals as follows;
	
	

	27.2.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	27.2.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	27.2.3 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	27.2.4 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	27.2.5 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 26.2.1, rig the control system.
	
	
	

	
	
	
	

	27.2.6 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	27.3 Tachometer for condition and security of installation.
	
	
	

	
	
	
	

	C 1500.28 71 – L/H POWERPLANT

	
	
	
	

	28.1 Intake deflector plate and exit door hinges for condition, corrosion, cracks and security. Clean as required.
	
	
	

	
	
	
	

	28.2 Intake deflector for condition and security, electrical wiring for condition, connectors for security.  Clean as required.
	
	
	

	
	
	
	

	28.3 Air intake duct for condition and security.
	
	
	

	
	
	
	

	28.4 Upper engine cowling for condition, lower cowling hinge for condition and latch mechanism for condition and proper operation.
	
	
	

	
	
	
	

	28.5 Engine compressor wash spray ring for condition and security.
	
	
	

	
	
	
	

	28.6 Engine nacelle fuel drain lines for condition, security and leakage.
	
	
	

	Effectivity:  Pre Mod 6/1583
	
	
	

	28.7 Engine nacelle mounts for condition, corrosion, cracking and security.
	
	
	

	
	
	
	

	28.8 Engine vibration isolators for condition, separation, corrosion, cracking and security.  Conduct inspection for separations between metal plate and elastomer; must not exceed 1-inch length or 1/16th inch in depth. Pay particular attention to corrosion and cracks at the base of the housing (P/N 7351256-2) right next to the edge of the cores (pucks).
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	28.9 Bonding wires for condition and security.
	
	
	

	
	
	
	

	C 1500.29 71 – R/H POWERPLANT

	
	
	
	

	29.1 Intake deflector plate and exit door hinges for condition, corrosion, cracks and security. Clean as required.
	
	
	

	
	
	
	

	29.2 Intake deflector for condition and security, electrical wiring for condition, connectors for security.  Clean as required.
	
	
	

	
	
	
	

	29.3 Air intake duct for condition and security.
	
	
	

	
	
	
	

	29.4 Upper engine cowling for condition, lower cowling hinge for condition and latch mechanism for condition and proper operation.
	
	
	

	
	
	
	

	29.5 Engine compressor wash spray ring for condition and security.
	
	
	

	
	
	
	

	29.6 Engine nacelle fuel drain lines for condition, security and leakage.
	
	
	

	Effectivity:  Pre Mod 6/1583
	
	
	

	29.7 Engine nacelle mounts for condition, corrosion, cracking and security.
	
	
	

	
	
	
	

	29.8 Engine vibration isolators for condition, separation, corrosion, cracking and security.  Conduct inspection for separations between metal plate and elastomer; must not exceed 1-inch length or 1/16th inch in depth. Pay particular attention to corrosion and cracks at the base of the housing (P/N 7351256-2) right next to the edge of the cores (pucks).
	
	
	

	
	
	
	

	29.9 Bonding wires for condition and security.
	
	
	

	
	
	
	

	C 1500.30 73 – L/H ENGINE FUEL AND CONTROL

	
	
	
	

	30.1 Fuel heater for condition, security and leakage.
	
	
	

	
	
	
	

	30.2 Fuel flow transmitters for condition, leakage and security.
	
	
	

	
	
	
	

	C 1500.31 73 – R/H ENGINE FUEL AND CONTROL

	
	
	
	

	31.1 Fuel heater for condition, security and leakage.
	
	
	

	
	
	
	

	31.2 Fuel flow transmitter for condition, leakage and security.
	
	
	

	
	
	
	


	
	
	MECH
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	C 1500.32 76 – L/H ENGINE CONTROLS

	
	
	
	

	32.1 Cable pulleys for condition, freedom of operation and security.
	
	
	

	32.2 Do a detailed visual inspection of engine cable terminals as follows;

Note:  Refer to A.D. 68-05-03, if applicable.
	

	32.2.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	32.2.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	32.2.3 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	32.2.4 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	32.2.5 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 32.2.1, rig the control system.
	
	
	

	
	
	
	

	32.2.6 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	C 1500.33 76 – R/H ENGINE CONTROLS

	
	
	
	

	33.1 Cable pulleys for condition, freedom of operation and security.
	
	
	

	33.2 Do a detailed visual inspection of engine cable terminals as follows;

Note:  Refer to A.D. 68-05-03, if applicable.
	

	33.2.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	33.2.2 Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	33.2.3 Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	33.2.4 If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
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	33.2.5 If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 33.2.1, rig the control system.
	
	
	

	
	
	
	

	33.2.6 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	
	
	
	

	C 1500.34 79 – L/H OIL 

	
	
	
	

	34.1 Power plant oil pipes, hoses and connections for condition and security.
	
	
	

	
	
	
	

	34.2 Oil cooler mounting for condition and security.
	
	
	

	
	
	
	

	C 1500.35 79 – R/H OIL 

	
	
	
	

	35.1 Power plant oil pipes, hoses and connections for condition and security.
	
	
	

	
	
	
	

	35.2 Oil cooler mounting for condition and security.
	
	
	

	
	
	
	

	C 1500.36 80 – OPERATIONAL CHECKS

	
	

	36.1 Perform the following Operational Checks;
	

	
	

	36.1.1 Cabin temperature sensor blower. Power On
	
	
	

	
	
	
	

	36.1.2 Hot air valve (travel time from open to closed position). Power on.
	
	
	

	
	
	
	

	36.1.3 Airframe deicing system. Power on.
	
	
	

	
	
	
	

	36.1.4 Engine intake anti-icing system. Power on.
	
	
	

	
	
	
	

	36.1.5 Propeller deicing system. Power on.
	
	
	

	
	
	
	

	36.1.6 Ram air valve.
	
	
	

	
	
	
	

	36.1.7 Cabin air control valve.
	
	
	

	
	
	
	

	36.1.8 Brake system.
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	C 1500.37 POST INSPECTION

	
	
	
	

	37.1 Inspect for operation and leaks.
	
	
	

	
	
	
	

	37.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	37.3 Clean aircraft and engine once maintenance is completed.
	
	
	

	
	
	
	

	37.4 Perform Functional Check Flight if required per DHC-6-400 Maintenance Manual or AFM as appropriate.
	
	
	

	
	
	
	

	37.5 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	

	
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6 – C 1500RT – 1500 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


