A0125
On signoff page in the signoff paragraph, change “DHC-6-400” to just DHC-6


B0250
10.1 – Fuel filter should have open RII box. – Pilot and Mech can leak check
11.1 – Fuel Filter should have open RII box. – Pilot and Mech can leak check
Add under 10.1 and 11.1, “Strainer body for condition and security of attachment, and security of drain valve”.
19.2 – Spelling error on the word Hinge.
26.7 – Remove Deceleration check. Per SB1568 our engine model serial number is not affected. See snip attached for serial numbers.
26.2 – lift detectors and stall warning are the same. We can remove 26.10 and add to 26.2 “Function test light and horn (power on) flaps must be at a minimum of 10dreeges to check both switches.
26.10 – Removed. See above.
On signoff page in the signoff, change “DHC-6-400” to DHC-6. 

C0500
This inspection is labeled incorrectly. It’s labeled as B0500 and should be C0500. Mislabeled on header of every page. 
7.1.3 – Change “Chock cords” to Return Spring Assembly. 
8.1 – Spelling correction, change “Graying” to Fraying.
14.15 – Remove. Not installed. Only one upper TCAS antenna. 
14.18 – Remove. Only one ADF antenna installed. 
Signoff page, in the signoff change B0500 to C0500.
