	MARITIME HELICOPTERS
	DHC-6 MAINTENANCE MANUAL

	
	

	Page No:
	1

	Revision:
	Original

	Issue Date:
	05/01/21

	CHECK:
	
	B 0250 – BASIC INSPECTION

	FREQUENCY:
	
	Every 250 Hours

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  Viking PSM 1-64-2 Maintenance Manual, Pratt & Whitney PT6A-34 Maintenance Manual
	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	B 0250.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	DHC-6-400
MP
	
	

	
	PT6A MM
	
	

	1.4 Overhaul all components that have completed published operating limits.
	DHC-6-400

MP
	
	

	
	PT6A MM
	
	

	B 0250.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	
	
	
	

	B 0250.3  CORROSION CONTROL

	
	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	Appendix

B
	
	

	
	
	
	

	B 0250.4  PREPARATION

	
	
	
	

	4.1 Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	B 0250.5 23 - COMMUNICATIONS

	
	
	
	

	5.1 Pilot and Co-pilots head sets for condition and security.
	
	
	

	
	
	
	

	5.2 Nose cap lightning rod for condition and security.
	
	
	

	
	
	
	

	B 0250.6 24 – ELECTRICAL POWER

	
	
	
	

	6.1 Avionics Start Battery for condition and security.
	
	
	

	Effectivity: Mod 6/2315
	
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	B 0250.7 26 – FIRE PROTECTION - LH

	
	
	
	

	7.1 Fire detection thermal units and wire loops for condition and security.
	
	
	

	
	
	
	

	7.2 Engine fire extinguisher bottle for condition and security, correct pressure, pipes for condition and security, electrical wiring for condition and connectors for security.
	
	
	

	
	
	
	

	B 0250.8 26 – FIRE PROTECTION - RH

	
	
	
	

	8.1 Fire detection thermal units and wire loops for condition and security.
	
	
	

	
	
	
	

	8.2 Engine fire extinguisher bottle for condition and security, correct pressure, pipes for condition and security, electrical wiring for condition and connectors for security.
	
	
	

	
	
	
	

	B 0250.9 27 – FLIGHT CONTROLS - LH

	
	
	
	

	9.1 Flap actuator for condition and security of mounting and leakage, selector valve for condition, security of mounting and leakage.
	
	
	

	
	
	
	

	9.2 Selector pulleys properly secured to spindle.
	
	
	

	
	
	
	

	9.3 Drip trays for condition, security and fluid content. Remove, dry out and install pads as required.
	
	
	

	
	
	
	

	B 0250.10 27 – FLIGHT CONTROLS - RH

	
	
	
	

	10.1 Flap actuator for condition and security of mounting and leakage, selector valve for condition, security of mounting and leakage.
	
	
	

	
	
	
	

	10.2 Selector pulleys properly secured to spindle.
	
	
	

	
	
	
	

	10.3 Drip trays for condition, security and fluid content. Remove, dry out and install pads as required.
	
	
	

	
	
	
	

	B 0250.11 29 – HYDRAULIC POWER

	
	
	
	

	11.1 Hydraulic reservoir filler neck for condition and contamination, fluid leakage, end of vent clear of power package tray. Dip stick for seal deterioration.
	
	
	

	
	
	
	

	B 0250.12 30 – ICE AND RAIN PROTECTION

	
	
	
	

	12.1 Propeller deicing boots for cuts, tears, burns, deterioration and proper adhesion.
	
	
	

	
	
	
	

	12.2 Propeller deicing brush block and back plate slip ring for condition and security.
	
	
	

	
	
	
	


	
	
	MECH

INITIALS
	RII

INTIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	B 0250.13 32 – LANDING GEAR NOSE

	
	
	
	

	13.1 Nose gear shock strut for correct extension as given on date plate.  Fork retaining nut properly secured.
	
	
	

	
	
	
	

	13.2 Nosewheel steering actuator for condition and leakage, hydraulic pipes and input swivel lever for condition, connections for security and leakage.
	
	
	

	
	
	
	

	13.3 Steering cables where visible, for condition, corrosion, kinks, flattening, proper attachment and security; pulleys for condition, freedom of operation and security.
	
	
	

	13.4 Pulleys for condition, freedom of operation and security, turnbuckles for security.
	
	
	

	13.5 Perform a detail visual inspection of cable terminals as follows;
	
	

	
	
	

	13.5.1 Remove and discard the lockwire from the cable terminals.
	
	
	

	Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	13.5.2 Do a detailed visual inspection of cable terminals excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	
	
	
	

	13.5.3 Do a detailed visual inspection of cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	
	
	
	

	13.5.4 If corrosion pits and/or cracks are found on any cable terminal, remove the applicable cable assembly and replace with new cable assembly.
	
	
	

	
	
	
	

	13.5.5 In a new cable assembly is install or if the rigging was disturbed when the lockwire was removed in step 15.5.1, rig the control system.
	
	
	

	
	
	
	

	13.5.6 If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	Note: Refer to Service bulletin No. 6/453.
	
	
	

	13.6 Steering actuator linkage for condition, corrosion and security, fouling of linkage on shock struct cylinder body.
	
	
	

	
	
	
	

	13.7 Remove nose wheel and clean as required.  
	
	
	

	
	
	
	

	13.8 Inspect as follows;
	
	

	
	
	

	13.8.1 Wheel for abrasions, cracks, chipped rims.
	
	
	

	
	
	
	

	13.8.2 Bearings for signs of wear, corrosion, fretting and blueing; lubricate.
	
	
	

	
	
	
	

	13.8.3 Bushings for signs of wear.
	
	
	

	
	
	
	

	13.8.4 Seals for distortion, fit, deterioration and security.
	
	
	

	
	
	
	

	13.9 Install nose wheel assembly.
	
	
	

	
	
	
	

	
	
	MECH

INITIALS
	RII

INTIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	B 0250.14 32 – LANDING GEAR MAIN

	
	
	
	

	14.1 Remove and clean main wheels.
	
	
	

	
	
	
	

	14.2 Inspect as follows;
	

	
	

	14.2.1 Wheels for abrasions, cracks, chipped rims, brake drive signs of wear.
	
	
	

	
	
	
	

	14.2.2 Wheel bearings for signs for wear corrosion, fretting and blueing. lubricate.
	
	
	

	
	
	
	

	14.2.3 Brake housing for evidence of overheating.
	
	
	

	
	
	
	

	14.2.4 Brake discs for scoring, distortion, evidence of overheating.
	
	
	

	
	
	
	

	14.2.5 Brake disk guides (when installed) for condition and security.
	
	
	

	
	
	
	

	14.2.6 Brake linings for wear and within limits.
	
	
	

	
	
	
	

	14.3 Reinstall main wheels.
	
	
	

	B 0250.15 52 – DOORS

	
	
	
	

	15.1 Cabin escape hatch door release mechanisms for proper operation, seals for deterioration and security.
	
	
	

	
	
	
	

	B 0250.16 53 – FUSELAGE 

	
	
	
	

	16.1 Cabin floor panes for condition, delamination, corrosion and security. Clean as required.
	
	
	

	
	
	
	

	16.2 Cargo tie-down rings for condition and security.
	
	
	

	Note: if cabin floor panes are severely damaged, removed panels and inspect supporting structure for damage, buckling and cracks.
	
	
	

	B 0250.17 55 - STABILIZERS

	
	
	
	

	17.1 Elevator and rudder including tab hinge arms for condition and security.
	
	
	

	
	
	
	

	17.2 Hing arm attachment bolts for safety and security.
	
	
	

	
	
	
	


	
	
	MECH

INITIALS
	RII

INTIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	B 0250.18 57 – WING – LH  

	
	
	
	

	18.1 Wing root rib forward aluminum adapter (Pre-Mod 6/1887 and EO69080) for condition, cracks, corrosion and security.
	
	
	

	Note: Refer to Service Bulletin Nos. 6/174 and 6/476 and A.D. 94-04-01 if applicable.
	
	
	

	18.2 Wing exterior upper surfaces for dents, scores, abrasions and corrosion.
	
	
	

	
	
	
	

	18.3 Inboard trailing flap for condition skins for cracks and fastener for security.
	
	
	

	Note: Refer to Service Bulletin No. 6/174 and 6/345 
	
	
	

	18.4 Wing flap, aileron hinge arms and connecting link attachment bolts for safety and security.
	
	
	

	
	
	
	

	18.5 Main wing hinge arms, bonding wire, bearings for condition and security and attachment bolts for safety and security.
	
	
	

	Note: Includes inboard hinge location mounted to the fuselage side at STA 248.41.
	
	
	

	B 0250.19 57 – WING – RH  

	
	
	
	

	19.1 Wing root rib forward aluminum adapter (Pre-Mod 6/1887 and EO69080) for condition, cracks, corrosion and security.
	
	
	

	Note: Refer to Service Bulletin Nos. 6/174 and 6/476 and A.D. 94-04-01 if applicable.
	
	
	

	19.2 Wing exterior upper surfaces for dents, scores, abrasions and corrosion.
	
	
	

	
	
	
	

	19.3 Inboard trailing flap for condition skins for cracks and fastener for security.
	
	
	

	Note: Refer to Service Bulletin No. 6/174 and 6/345 
	
	
	

	19.4 Wing flap, aileron hinge arms and connecting link attachment bolts for safety and security.
	
	
	

	
	
	
	

	19.5 Main wing hinge arms, bonding wire, bearings for condition and security and attachment bolts for safety and security.
	
	
	

	Note: Includes inboard hinge location mounted at the fuselage side at STA 248.41.
	
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	B 0250.20 80 – STARTING - LH

	
	
	
	

	20.1 Remove spark igniters for operational test. 
	
	
	

	
	
	
	

	20.2 Clean as required and install serviceable spark igniters.
	
	
	

	
	
	
	

	20.3 Examine the ignition cables for chafing, wear and installation.
	
	
	

	
	
	
	

	20.4 Examine the spark igniters for cleanliness and erosion.
	74-20-00
	
	

	
	
	
	

	20.4.1 Perform a functional check.
	Cables &
Spark Ignig
	
	

	
	Maint Pract
	
	

	B 0250.21 80 – STARTING - RH

	
	
	
	

	21.1 Remove spark igniters for operational test. 
	
	
	

	
	
	
	

	21.2 Clean as required and install serviceable spark igniters.
	
	
	

	
	
	
	

	21.3 Examine the ignition cables for chafing, wear and installation.
	
	
	

	
	
	
	

	21.4 Examine the spark igniters for cleanliness and erosion.
	74-20-00
	
	

	21.4.1 Perform a functional check.
	Cables &

Spark Ignig
	
	

	
	Maint Pract
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	B 0250.22 OPERATIONAL CHECKS

	
	

	22.1 Perform the following Operational Checks;
	

	NOTE

Electrical power for the following tests is obtained by

connecting a ground power source or by running the

engines, whichever is more convenient
	

	22.2 Lift Detector Vanes (WINGS) for freedom of movement, condition, corrosion and security. Function test (Power on).
	
	
	

	
	
	
	

	22.3 All communications and navigation systems.
	
	
	

	
	
	
	

	22.4 Weather radar.
	
	
	

	
	
	
	

	22.5 Wing flaps in normal and emergency.
	
	
	

	
	
	
	

	22.6 Fuel booster pumps, check for evidence of rough running.
	
	
	

	
	
	
	

	22.7 Fuel system strainers for leak check under system pressure after installation.
	
	
	

	
	
	
	

	
	
	
	

	22.8 Flight controls, including trim tabs for full and free movement of all controls.
	
	
	

	
	
	
	

	22.9 Stall warning light and horn system (Pre Mod and Mod 6/2028) by actuating detecting vane.
	
	
	

	
	
	
	

	22.10 Master warning and caution indication and control (Mod 6/2028) function test. (Power on).
	
	
	

	
	
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	B 0250.23 POST INSPECTION

	
	
	
	

	23.1 Inspect for operation and leaks.
	
	
	

	
	
	
	

	23.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	23.3 Clean aircraft and engine once maintenance is completed.
	
	
	

	
	
	
	

	23.4 Perform Functional Check Flight if required per DHC-6-400 Maintenance Manual or AFM as appropriate.
	
	
	

	
	
	
	

	23.5 Perform a deceleration check on L/H engine.
	71-00-00

Power Plant
Adj Test
	
	

	23.6 Perform a deceleration check on R/H engine.
	71-00-00

Power Plant
Adj Test
	
	

	23.7 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	

	
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6-400 – B 0250 – 250 Hour Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


