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	Page No:
	1

	Revision:
	Original

	Issue Date:
	05/01/20

	CHECK:
	
	R E007 – ROUTINE E INSPECTION

	FREQUENCY:
	
	Every 7 Days

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  DHC-6 Maintenance Program, Viking PSM 1-64-2 Maintenance Manual 
	
	
	MECH

INITIALS
	RII

INTIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	R E007.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	DHC-6

MP
	
	

	
	
	
	

	1.4 Open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	DHC-6

 MP
	
	

	R E007.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	R E007.3  CORROSION CONTROL

	
	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	Appendix

C
	
	

	R E007.4 INSPECTIONS

	
	
	
	

	4.1 Propeller shaft seal for evidence of oil leakage.
	
	
	

	
	
	
	

	4.2 Propeller deicing boots for condition and security.
	
	
	

	4.3 Engine intake deflector. Clean as required.
	
	
	

	4.4 Compressor inlet screen. Clean as required.
	
	
	

	Note: If dirty screen warrants removal for cleaning, clean inlet as required.
	
	
	

	4.5 Check for correct oil level. Oil filter cap for condition and proper locking.
	
	
	

	Note: If level indication is low when checking oil quantity after engine has been shut down for more than 30 minutes, or after an oil change, then start the engine and run at ground-idle for minimum five minutes, feather the propeller, shutdown the engine, and recheck the oil quantity.
	
	
	

	4.6 Fuel, oil and bleed air pipes leakage.
	
	
	

	
	
	
	

	4.7 Remove, clean and install engine driven air pump intake filter.
	
	
	

	
	
	
	

	4.8 Oil coolers and pressure transmitters for security and leakage.
	
	
	

	
	
	
	

	4.9 Wing deiced bonded stall bar for condition and proper adhesion.
	
	
	

	
	
	
	


	
	
	MECH

INITIALS
	RII

INTIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	R E007.5 FINAL CLOSE UP

	
	
	
	

	5.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	R E007.6 POST INSPECTION

	
	
	
	

	6.1 Perform Functional Check Flight if required per DHC - 6 Maintenance Manual or AFM as appropriate.
	
	
	

	
	
	
	

	6.2 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	

	
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC- 6 – R E007 – 7 day Routine E Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	



