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	12/30/21

	CHECK:
	
	R 0007 – ROUTINE INSPECTION

	FREQUENCY:
	
	Every 7 Days

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  DHC-6 Maintenance Program, Viking PSM 1-64-2 maintenance Manual 

	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	R 0007.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	DHC-6

MP
	
	

	
	
	
	

	1.4 Open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	DHC-6

 MP
	
	

	R 0007.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	R 0007.3  CORROSION CONTROL

	
	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	Appendix

B
	
	

	R 0007.4  INTERNAL

	
	
	
	

	4.1 Cargo nets for condition and security, if installed.
	
	
	

	Effectivity: Mod SOO 6274 & Mod 6389
	
	
	

	4.2 Window escape hatches for condition and security.
	
	
	

	4.3 Heated windshields for condition, discoloration, delamination and security.
	
	
	

	4.4 Emergency hand pump handle for security in stowed position
	
	
	

	4.5 Portable fire extinguisher(s) for condition and evidence of leakage, security in stowed position.
	
	
	

	Note: Refer to manufacturer’s instructions and local regulatory authority approval.
	
	
	

	4.6 Flight compartment axe and axe stowage for condition and security of axe stowage structure. Condition and security of axe cutting edge and pike to axe handle.
	
	
	

	Effectivity: Mod SOO 6376
	
	
	



	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	
	
	

	4.7 Crew seats and seat belts for condition and security. Seat belt buckles for proper operations.
	
	
	

	
	
	
	

	4.8 Utility seats and seat belts for condition and security. Seat belt buckles for proper operations.
	
	
	

	Effectivity: IKHANA STC SA02556LA, I.C.A Doc SU-6-11 Para 8.2
	
	
	

	4.9 Nose baggage compartment verity the HIRF covers are installed. All fasteners must be engaged.  Replace if damaged.
	
	
	

	Effectivity: Mod SOO 6/2024
	
	
	

	R 0007.5 EXTERNAL

	
	
	
	

	5.1 Fire extinguisher indicator discs for evidence of extinguisher discharge.
	
	
	

	
	
	
	

	5.2 Elevator, aileron and all flap skins for condition, drain holes for obstruction and wing tip fairings for condition.


	
	
	

	5.3 Stall warning lift detector vanes for condition, free movement and security.
	
	
	

	
	
	
	

	5.4 External surfaces of fuselage, nacelles, wings and stabilizers for condition, drains holes for obstruction, wing fences for condition and security, deicing boots for condition.
	
	
	

	5.5 Wing strut skins (where visible) for condition and fasteners for security.
	
	
	

	
	
	
	

	5.6 Water contamination in fuel system at water drain and fuel strainer drain points.
	
	
	

	
	
	
	

	5.7 Evidence of fuel leaks on underside of fuselage, drain valves for leakage and security.
	
	
	

	
	
	
	

	5.8 Fuel vent outlets for obstructions.
	
	
	

	
	
	
	

	5.9 Fuel for water content, drain valves for condition and security, bent outlets for obstruction, evidence of fuel leaks from wing tank area, filler cap for proper fit and seal condition, filler necks for condition.
	
	
	

	
	
	
	

	5.10 Depressurize hydraulic system and check gas pressure in accumulators.
	
	
	

	
	
	
	

	5.11 Hydraulic reservoir for correct fluid level.
	
	
	

	
	
	
	

	5.12 Pitot heads and static vents for obstructions.
	
	
	

	
	
	
	

	5.13 Windshield for signs of leakage. Clean as required.
	
	
	

	
	
	
	

	5.14 Cabin, cabin door and escape hatch windows. Clean as required.
	
	
	

	
	
	
	



	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	
	
	

	5.15 Nose and main wheels for cuts, wear, deterioration and inflation.
	
	
	

	
	
	
	

	5.16 Main and nose wheels for condition.
	
	
	

	
	
	
	

	5.17 Tail bumper for condition and security.
	
	
	

	
	
	
	

	R 0007.6 WING - LH

	
	
	
	

	6.1 Propeller shaft seal for evidence of oil leakage.
	
	
	

	
	
	
	

	6.2 Propeller deicing boots for condition and security.
	
	
	

	
	
	
	

	6.3 Engine intake deflector. Clean as required.
	
	
	

	
	
	
	

	6.4 Compressor inlet screen. Clean as required.
	
	
	

	Note: If dirty screen warrants removal for cleaning, clean inlet as required.
	
	
	

	6.5 Check for correct oil level. Oil filter cap for condition and proper locking.
	
	
	

	Note: If level indication is low when checking oil quantity after engine has been shut down for more than 30 minutes, or after an oil change, then start the engine and run at ground-idle for minimum five minutes, feather the propeller, shutdown the engine, and recheck the oil quantity.
	
	
	

	6.6 Fuel, oil and bleed air pipes leakage.
	
	
	

	
	
	
	

	6.7 Oil coolers and pressure transmitters for security and leakage.
	
	
	

	
	
	
	

	6.8 Wing deiced bonded stall bar for condition and proper adhesion.
	
	
	

	
	
	
	

	R 0007.7 WING - RH

	
	
	
	

	7.1 Propeller shaft seal for evidence of oil leakage.
	
	
	

	
	
	
	

	7.2 Propeller deicing boots for condition and security.
	
	
	

	
	
	
	

	7.3 Engine intake deflector. Clean as required.

	
	
	

	
	
	
	



	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	
	
	

	7.4 Compressor inlet screen. Clean as required.
	
	
	

	Note: If dirty screen warrants removal for cleaning, clean inlet as required.
	
	
	

	7.5 Check for correct oil level. Oil filter cap for condition and proper locking.
	
	
	

	Note: If level indication is low when checking oil quantity after engine has been shut down for more than 30 minutes, or after an oil change, then start the engine and run at ground-idle for minimum five minutes, feather the propeller, shutdown the engine, and recheck the oil quantity.
	
	
	

	7.6 Fuel, oil and bleed air pipes leakage.
	
	
	

	
	
	
	

	7.7 Oil coolers and pressure transmitters for security and leakage.
	
	
	

	
	
	
	

	7.8 Wing deiced bonded stall bar for condition and proper adhesion.
	
	
	

	
	
	
	

	R 0007.8 FUNCTIONAL CHECKS

	
	
	
	

	8.1 Position, anti-collision, cabin and landing lights.
	
	
	

	
	
	
	

	8.2 Taxi, wing inspection lights and instrument panel lights.
	
	
	

	Note: Refer also to Special Inspection cards when operating under abnormal environmental conditions.
	
	
	

	8.3 Pitot system head heaters.
	
	
	

	
	
	
	

	8.4 Flood lights.
	
	
	

	Effectivity: Mod 6/2028
	
	
	

	8.5 Caution lights dimming and dome lights.
	
	
	

	Effectivity: Mod 6/2028
	
	
	

	8.6 ESIS Operational test.
	
	
	

	Effectivity: Mod SOO 6209 & Mod 6/2049
	
	
	

	R 0007.9 FINAL CLOSE UP

	
	
	
	

	9.1 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	R 0007.10 POST INSPECTION

	
	
	
	

	10.1 Perform Functional Check Flight if required per DHC - 6 Maintenance Manual or AFM as appropriate.
	
	
	

	
	
	
	

	10.2 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	

	
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC - 6 – R 0007 – 7 day Routine Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


