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	CHECK:
	
	CT 6000NT – COMPONENT TEST

	FREQUENCY:
	
	Every 6000 Hours

	NOTE:
	
	Bench Test – Component removed from aircraft. No Tolerance



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  DHC-6 Controlled Inspection Program, Viking PSM 1-64-2 Maintenance Manual 
	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	CT 6000.1 26 – FIRE PROTECTION

	
	
	
	

	1.1 Fire detecting thermal units.
	
	
	

	
	
	
	

	CT 6000.2 27 – FLIGHT CONTROLS 

	
	
	
	

	2.1 Flap actuator (pressure test).
	
	
	

	
	
	
	

	2.2 Flap selector valve (pressure test).
	
	
	

	
	
	
	

	CT 6000.3  29 – HYDRAULIC POWER

	
	
	
	

	3.1 Hydraulic system accumulators.
	
	
	

	
	
	
	

	3.2 Hydraulic (electric-driven) pump.
	
	
	

	
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection/test form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have tested all the items initialed by me in accordance with Maritime Helicopters DHC - 6 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC - 6 – CT 6000NT – 6000 Hour Inspection/Test and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


