	MARITIME HELICOPTERS
	DCH-6 CONTINUOUS AIRWORTHINESS MAINTENANCE PROGRAM

	
	

	Page No:
	1

	Revision:
	2

	Issue Date:
	12/30/21

	CHECK:
	
	F 3000NT – FUNCTIONAL CHECKS

	FREQUENCY:
	
	EVERY 3000 HOURS

	NOTE:
	
	No Tolerance



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  DHC-6 Maintenance Program, Viking PSM 1-64-2 Maintenance Manual 
	
	
	MECH

INITIALS
	RII

INTIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	F 3000.1 21 – AIR CONDITIONING

	
	
	
	

	1.1 Bleed air heating system. Power on.
	
	
	

	
	
	
	

	F 3000.2 27 – FLIGHT CONTROLS

	
	
	
	

	2.1 Flight control surfaces for alignment with external rigging marks; for rudder check dimension ‘L’.
	
	
	

	
	
	
	

	2.2 All trim and gear tabs for free play.
	
	
	

	
	
	
	

	2.3 Rudder gear box for play.
	
	
	

	
	
	
	

	F 3000.3   28 – FUEL

	
	
	
	

	3.1 Fuel forward and aft low-level warning system. Adjust tank levels to obtain indication. Power on.
	
	
	

	
	
	
	

	3.2 Main fuel quantity indicating system (calibration).
	
	
	

	
	
	
	

	F 3000.4 30 – ICE AND RAIN PROTECTION

	
	
	
	

	4.1 Propeller deicing timer.
	
	
	

	
	
	
	

	F 3000.5 34 - NAVIGATION

	
	
	
	

	5.1 Pitot system.
	
	
	

	
	
	
	

	F 3000.6 36 - PNEUMATIC

	
	
	
	

	6.1 Pneumatic system pressure test.
	
	
	

	
	
	
	

	F 3000.7 71 – POWERPLANT - LH

	
	
	
	

	7.1 Intake deflector system. Power on.
	
	
	

	
	
	
	

	F 3000.8 71 – POWERPLANT - RH

	
	
	
	

	8.1 Intake deflector system. Power on.
	
	
	

	
	
	
	


Upon satisfactory completion of each test item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each function test, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have function tested all the items initialed by me in accordance with Maritime Helicopters DHC - 6 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this function tests form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft components have been tested in accordance with Maritime Helicopters’ DHC - 6 – F 3000NT – 3000 Hour Functional Tests and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	


