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MANUAL CONTROL

The Director of Maintenance shall initiate the necessary revision(s). Each revision, in its final form, shall be submitted to the FAA. A cover letter and individual copies shall be submitted to the FAA assigned Principal Maintenance Inspector at the FAA District Office having authority. The FAA representative shall signify approval by signing and dating the bottom of the Log of Effective Pages and returning one original copy to the Director of Maintenance. Upon approval by the Director of Maintenance, an electronic copy shall be posted on the Maritime web portal and made available to all necessary personnel.

Field Bases Distribution

All field bases will have access to this Maintenance Manual and any subsequent revisions, on the Maritimes web portal.

Corporate Office Distribution

All applicable corporate office personnel will have access to this Maintenance Manual and any subsequent revisions, on the Maritimes web portal.
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1	INTRODUCTION

Aircraft operated by Maritime Helicopters Inc., type certificated for a passenger seating capacity, excluding any pilot seat, of ten or more seats are maintained in accordance with a Continuous Airworthiness Maintenance Program (CAMP). Under this program, Maritime Helicopters Inc. is primarily responsible for the airworthiness of its aircraft and the performance of all the inspection, maintenance or alterations.

The purpose of this CAMP Maintenance Manual is to establish “What” and “When” to inspect and conditions to be sought. In general, the objective of the requirements is to direct the attention of maintenance personnel to components and areas where defects may result from normal usage. The requirements are not designed to lead to the detection of isolated discrepancies that may occur on a one-time basis, nor discrepancies resulting from abuse or poor maintenance practices.

This CAMP Maintenance Manual is based on the manufacturers' recommended maintenance program. All items pertinent to the continued airworthiness of this aircraft make andmodel are included, though possibly rearranged.

Maritime Helicopters Inc CAMP program is complied with using both the CAMP General Manual and this aircraft specific CAMP Maintenance Manual herby referred to as the Maintenance Manual.

1.1	INSPECTIONS/TESTS

Basic Inspections
·	R Checks ·	A Checks ·	B Checks ·	C Checks
Special Condition Inspections (Tracked on CALM Program) Functional Tests
Component Tests Powerplant
Propeller (Incorporated into Basic Inspections) Corrosion Control


1.2	MAINTENANCE

This Maintenance Manual is broken down into two inspection sections that address overall maintenance of the DHC-6-400 aircraft;


Airframe – DHC-6-400 ·	Scheduled
·	Preventative ·	Alterations
·	Unscheduled
Powerplant – Pratt & Whitney Canada PT6A-34 ·	Normal
·        Preventative ·        Unscheduled


Scheduled and Preventative Maintenance are complied with thru inspection work cards with published intervals. Unscheduled maintenance must be rectified on a case-by-case basis depending on the discrepancy. Due to the numerous possibilities of unscheduled maintenance, no attempt has been made to list them all and each technician must use the appropriate manufacturer trouble shooting procedure. Alterations will be tracked on Maritimes CALM program for any required recurring inspection intervals.

All inspection series are independent (stand-alone) of one another. They may be performed in conjunction with one another or independently. Because of their individuality, the Maintenance Manual inspection series shall be tracked independently on the aircraft “status sheet.” They also provide additional flexibility and availability of Maritime aircraft and provide a schedule suitable to the environment in which the aircraft operates.
.

NOTE:
On new aircraft only, the date the entry issuing the airworthiness certificate was made in the aircraft logbook is to be used as the basis for all (calendar related) time limited items.
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1.3	REFERENCE DOCUMENTS

The following information shall be used as reference material in conjunction with this DHC-6-400Maintenance Manual:

·	MHI Continuous airworthiness Maintenance Program (CAMP) ·	Code of Federal Regulations (14 CFR)
·	Airworthiness Directives
·	Aircraft Specifications or Type Certificate Datasheets for Aircraft, Engines, Propellers ·	Maritime Operations Manual
·	Maritime Aircraft “Status Report” ·	Aircraft Log Books
·	Technical Advisory Bulletins ·	DHC-6 Series
Maintenance Manual –PSM 1-64-2 Mechanical Repair Manual – PSM 1-6-3 Structural Repair Manual –PSM 1-6-3
Corrosion Prevention and Control Manual –PSM 1-6-5 Hartzell Propeller Manual No. 139
Airframe Airworthiness Limitations Manual, DHC-6 – PSM 1-6-11 Service Bulletins
·	Pratt and Whitney PT6A-34 Series Engine Maintenance Manual Service Bulletins
·	FAA Form 337’s documenting major alterations to DHC-6 Series aircrafts operated by Maritime Helicopters. ·	National Fire Protection Association, NFPA 10
·	Concord Battery Corporation Battery Products Instruction Manual. ·	Additional references, as required

Any appliance or emergency equipment installed in the aircraft in accordance with the manufacturer's instructions and have maintenance/inspection requirements, which are not contained in the airframe manufactures’ Maintenance Manual, shall be a part of Maritime Helicopters’ Continuous Airworthiness Maintenance Program and tracked on Maritime Helicopters “Status Report”. All appliances or emergency equipment installed on the aircraft having inspection and maintenance requirements not contained in the airframe manufactures’ Maintenance Manual shall cause Maritime Maintenance Manual to be amended to incorporate those items.
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2	SCOPE OF INSPECTION


2.1	PROGRAM RESPONSIBILITY AND REVIEW

The Director of Maintenance is responsible for this inspection and maintenance program. The maintenance manual forms will be reviewed by the Director of Maintenance (or designee) for abnormalities. The Director of Maintenance or the mechanic shall insure that special tools, equipment, and parts needed are available.

2.2	MAINTENANCE AND SERVICING

All maintenance and servicing described in the Continuous Airworthiness Maintenance Program Maintenance Manual shall be performed in accordance with the appropriate manufacturer's maintenance manual or other data acceptable to the administrator.


2.3	AIRWORTHINESS LIMITATIONS (LIFE LIMITS)

No airworthiness limitation items may be exceeded. These are mandatory limitations of hours, calendar time, or cycles, as specified by Type Certificate Data Sheet andthe manufacturer's retirement schedule. Items with airworthiness limitations are listed in Appendix A.

2.4	OVERHAUL TIME LIMITS

Manufacturer's time limits for overhaul requirements shall be adhered to and may only be altered provided the manufacturer allows an extension to the overhaul time/calendar and, if applicable, local authority (FAA) approval requirements are met. The overhaul time limited items are specified and tracked on the Maritime Helicopters Aircraft “CALM Report” and are not a part of this Maintenance Manual.

2.5	INSPECTIONTYPES

The objective of the inspection types is to direct maintenance personnel to components and areas where defect may result from normal usage. The main inspection types are as follows:

2.5.1	BASIC INSPECTIONS

Basic inspection requirements are for normal operations for paved runways under moderate climatic conditions and provide a series of routine visual inspection checks on a 6000 hours cycle.

In addition to the visual inspections, this maintenance manual prescribes the following tests;

· Operational – Can be performed on aircraft

· Functional – May require supplemental ground support or test equipment

· Bench – This requires removal of the item from the aircraft


2.5.2	SPECIAL CONDITIONAL INSPECTIONS

Special conditional inspection are inspection requirements which supplement the Basic Inspections and provides coverage for special operating and environmental conditions, calendar timed inspections, heavy landing inspection, wing structural integrity check, hot end, and lightning strike.

2.5.3	STRUCTURAL COMPONENTS SERVICE LIFE LIMITS/INSPECTION

PSM 1-6-7 PART 3 contains the manufacturer’s background information on how the service life limits of structural components contained are determined and compliments the approved Service Life limits in Appendix A. A procedure is included for the wing main spar Fail-Safe inspection, with some illustration provided for crack detection on critical fittings which have been subject to abnormal conditions.

2.5.4	CORROSIONPREVENTION AND CONTROL

The Corrosion Prevention and Control provides mandatory supplementary inspections that are required to maintain the integrity of an ageing aircraft. Corrosion Prevention compliance intervals are listed in Appendix B.

The relationship between the Inspections Requirements and Corrosion Prevention is the inspections provide overall coverage to the corrosion prevention program considered necessary to maintain the aircraft in a continuous state of airworthiness. The corrosion prevention program provides supplementary structural inspection that may be required to maintain the integrity of structures of the aircraft approaching their originally intended economic design life.
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2.6	LUBRICATION

All Lubrication items described in the Continuous Airworthiness Maintenance Program shall be performed in accordance with the PSM 1-64-2 Chapter 12-20 Scheduled Servicing and appropriate Manufacturer's Maintenance Manual or other data acceptable to the administrator.

2.7	UNSCHEDULED AND CONDITIONAL INSPECTIONS/MAINTENANCE

The Special, Unscheduled, and Conditional Inspections/Maintenance are defined, depending on the airframe and engine manufacturer or modifier, as inspections and maintenance required by an unusual event or required at other than the normal time intervals. Both inspections and required maintenance are listed in this Maintenance Manual and shall be accomplished in accordance with the appropriate Manufacturer's Maintenance Manual.

2.8	FAA AIRWORTHINESS DIRECTIVES AND MANDATORY BULLETINS

Maritime Helicopters shall comply with all FAA Airworthiness Directives. The Maritime Helicopters Director of Maintenance shall evaluate all Airframe and Engine Service Bulletins and the mechanics will be notified of the requirements for all Service Bulletins selected for compliance. Recurring bulletins that Maritime Helicopters Director of Maintenance chooses to comply with will be incorporated into the Maintenance Manual at the next major revision. (Ref: CAMP General Manual Page 7)

2.9	INSTRUCTIONS FOR CONTINUED AIRWORTHINESS (ICA) OF ITEMS INSTALLED UNDER FAA FORM 337

ICA items shall be entered and tracked by Maritime Helicopters CALM system and complied with at the scheduled interval. When Major Alterations are made to the aircraft and the manufacturer does not provide a checklist or inspection procedures and signature sheet one shall be developed by Maritime Helicopters must be used. These check list/signature sheets will be retained as part of the historical records.

NOTE:
Other reference material may be required to maintain aircraft equipment. Approved data acceptable to the administrator and standard aviation practices may be used.

2.10	CONTRACT MAINTENANCE

All inspections performed on aircraft that are being operated under Maritime Helicopters' CAMP by maintenance facilities other than Maritime Helicopters’ shall be done in accordance with Maritime Helicopters’ CAMP and Maritime Helicopters’ Operations Manual. A copy of the CAMP General and Maintenance Manual shall be provided and appropriate training for the particular job to be performed. (Ref: CAMP General Manual Page 19)


2.11	MANUAL REVISIONS

Changes to any portion of Maritime’s Maintenance Manual shall not be made unless the responsible FAA district office first approves them. The program shall be amended whenever the following occurs:

·	The issuance of changes to FAR’s that affect and pertain to this company's manual, operations, equipment, personnel, or facility. ·	Major changes to Manufacturer's inspection methods, limits, and procedures.
·	Whenever the administrator of the FAA finds that it is necessary.

NOTE:
Inspection requirements associated with the installation of new equipment on an aircraft shall be monitored via the computerized tracking system as a separate inspection until the CAMP Maintenance Manual is revised and FAA approved.

A vertical bar (change bar) in the right margin indicates a change, addition, or deletion in the adjacent text for the current revision of that page only. The change bar is dropped at the next revision of that page. Fleetwide changes to the preamble or Maintenance Manual inspections that are common to multiple aircraft may omit the change bars as they may not accurately indicate all changes.

Revisions to paragraphs in the Preamble will not have a change bar in Table of Contents unless the title of the paragraph has changed. Only changes to the Table of Contents itself will have a vertical bar. The Log of Effective Pages will not have any change bars due to changes already indicated by referencing Issue Dates.
.
Once the Maritime Helicopters’ Maintenance Manual is approved by the responsible FAA district office, the Maintenance Manual shall be posted, within 5 working day, on the Maintenance Portal, accessible to Maritime Helicopters’ personnel through the internet. To allow continuation of work in progress, both revisions, the previous revision and the superseding revision, shall be posted together on the portal for a period of 5 days. Once posted, inspections shall be printed from the newly posted revision.
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If the overlap has expired, comply of one of the following steps.

1	 If all initialing mechanic(s) is (are) present, print new form and review both forms. Initial all identical items that have been complied with. Perform all additional work added during the revision. Discard the old inspection form.

2	 If initialing mechanic(s) is (are) not available, print new inspection form and review both forms. Initial all identical items that have been complied with by mechanics that are available. For identical items complied with by mechanics that are not available, the signing mechanic will initial the block on the new inspection form, with a note to see the item (listed by item number) on the old inspection form and attach that page to the end of the new inspection form. Perform all additional work added during the revision. Discard all other pages of the old inspection form.

When printed from the Portal, a footer comes printed at the bottom of all Maintenance Manual Inspection forms. The footer will include the aircraft model, Maintenance Manual revision number, and Maintenance Manual revision date. It is the responsibility of the signing mechanic to verify that the form used is the current Maintenance Manual inspection form posted on the Portal.


2.12	ABBREVIATIONS:

The following abbreviations may be used in Maritime Helicopters’ paperwork procedures:
NOTE: Abbreviations need not be case sensitive as depicted in the listing below. Additional abbreviations may be used if legible and standard to the industry. A/C - Aircraft	NT	No Tolerance
AC - Alternating Current	NFPA - National Fire Protection Association ACFT - Aircraft                                                                                                          No.	Number
ACTT - Aircraft Total Time	NT	No Tolerance AD - Airworthiness Directive                                                                                  OC - On Condition A/F - Airframe                                                                                                        OH - Overhaul
AFM - Aircraft Flight Manual	OPS CK - Operational Check AFTT - Airframe Total Time                                                                       OPS CK FLT - Operational Check Flight
AFMS - Aircraft Flight Manual Supplement	PARA	Paragraph AHRS - Attitude and Heading Reference System                                                    P&W	Pratt & Whitney
ALF	After Last Flight	P/C/W - Previously Complied With MHI - Maritime Helicopters, Inc.                                                                            PMA - Parts Manufacturer Approval A/P - Auto Pilot                                                                                                      P/N - Part Number
A & P - Airframe & Powerplant Mechanic	RT	Restricted Tolerance ASB	Alert Service Bulletin                                                                                    REF - Reference
C1	Compressor Turbine (Speed, Cycle count, etc.)	RIN - Retirement Index Number C2	Power Turbine (Speed, Cycle count, etc.)	R/H - Right Hand
CAMP	Continuous Airworthiness Maintenance Program	RII	Required Inspection Items CASS	Continuing Analysis and surveillance System                                                 RT	Restricted Tolerance
CEB - Commercial Engine Bulletin	SB - Service Bulletin CH - Chapter                                                                                                       SLL	Service Life Limit CL - Calendar                                                                                                      S/N - Serial Number
CAN	Compliance Action Notice	SRM	Structural Repair Manual CFR	Code of Federal Regulations                                                                       STD - Standard
CMM	Component Maintenance Manual	SI - Service Instruction
CRO	Component Overhaul and Repair Manual	STC - Supplemental Type Certificate CSL - Commercial Service Letter                                                                             TB - Technical Bulletin
C/W - Complied With	TCU - Torque Control Unit CYL - Cycle                                                                                                            TSI - Time Since Inspection
DC - Direct Current	TSO - Time Since Overhaul ELT - Emergency Locator Transmitter                                                                   TSN - Time Since New
EMER - Emergency	TSR	Time Since Repair ENG - Engine                                                                                                           TT - Total Time
ENGTT - Engine Total Time	VFR - Visual Flight Rules FAA - Federal Aviation Administration                                                                   HRS - Hours
CFR - Code of Federal Regulations – Title 14	IA - Inspection Authorization FOD - Foreign Object Damage                                                                             I/A/W	In Accordance With
GOV - Governor	ICA	Instructions for Continued airworthiness GMM	General Maintenance Manual                                                                       IFR - Instrument Flight Rules
ACFT        Aircraft                                                                                                       INSP - Inspection MOC - Maintenance Operational Check                                                                   L/H - Left Hand MM - Maintenance Manual                                                                                  MON        Months
N1	Compressor Turbine (Speed, Cycle count, etc.)	MEL - Minimum Equipment List N2	Power Turbine (Speed, Cycle count, etc.)                                                    YRS	Years
N/A - Not Applicable	W&B - Weight and Balance Ng	Compressor Turbine (Speed, Cyclecount, etc.)
Np	Power Turbine (Speed, Cycle count, etc.)
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2.13	DEFINITIONS

For definitions not inthis paragraph, refer to 14 CFR Part 1.



AIRWORTHY:




CHECK:


DAILY:


INSPECTION DESIGNATOR:


EXAMINE:





FILL:


FUNCTIONAL TEST:


“HOME BASE” OF OPERATION


INCLUDES:

INSPECTION:


INSTALL:

LOANER PART:


LONG TERM MAINTENANCE:

LUBRICATE:

MAINTENANCE:


MAY:

REMOVE:

NEED NOT:

NO TOLERANCE INSPECTION:

Two conditions must be met for an aircraft to be considered “airworthy.”
1)	The aircraft must conform to its typecertificate (design) or properly altered state. 2)	The aircraft must be in condition for safe operation.
NOTE: IF EITHER OF THESE CONDITIONS ARE NOT MET, THE AIRCRAFT WOULD BE CONSIDERED  UNAIRWORTHY.

Examinations in the form of comparisons with stated standards for the purpose of verifying condition, accuracy, and tolerance.

A 24-hour period of time beginning at midnight;
(0000 through 2359 military time or 12:00.00 a.m. through 11:59.59 p.m.)

The inspection designator in the Maritime CAMP Inspectionshall indicate:
1)	NT: No Tolerance allowed in this inspection; no overflight available.
2)	RT: Restricted Tolerance, must comply with this inspection within the tolerances allowed.

Look at the condition of an item for the following:
Chafing	Distortion	Contamination	Fractures	Cracks Corrosion	Fraying	Leaks	Scoring	Deterioration Wear	Loose or missing	Insecurity of	Faulty / broken locking devices
rivets	attachment
Loose clips orfasteners	Discoloration due to overheating

Fill to the correct level, pressure, or quantity. This also includes where necessary the following: 1)	Remove caps or covers,	2)	Examine caps, covers, gaskets, seals,
3) Install caps, covers,	4)	Install locking devices if appropriate.

This test is used to ascertain that a system orcomponent is functioning properly in all aspects in conformance with minimum acceptable design specifications. This test may require the use of supplemental groundsupport equipment or bench test equipment.

Is an Maritime maintenance station where:
1)	The subject aircraft is normally located, and
2)	Maritimemaintenance personnel are normally on duty.

Means “includes but is not limited to.”

Utilizing acceptable methods, techniques, and practices to determine physical condition and detect defects.

Put a component in the correct position and attach it correctly.

A part (refer to definition) temporarily being utilized as a replacement forsome other original part being repaired.

Maintenance that requires the aircraft is taken out of service and relocated to a repair station.

Apply lubricant.

Inspections, overhaul, repair, preservation, and the replacement of parts, but excludes preventative maintenance.

Has been used only when application of a procedure is optional.

Disconnect a component or system and move it from its correct position.

Has been used only when application of a procedure is optional.

A CAMP Inspectionthat has no overfly, the inspection must be performed on or before to the due time.
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2.13	DEFINITIONS (Continued)

OPERATIONAL TEST:


PART(s):


PORTAL:



Operation of aircraft components, appliances, or systems to evaluate functional performance while installed in the aircraft.

Is defined as a “Product” whichmeans an aircraft, aircraft engine, or propeller. It includes components and parts of aircraft, of aircraft engines, and of propellers (rotors); also parts, materials, and appliances.

Maritime Helicopters’ intranet, accessible by Maritime Helicopters’ personnel through the internet.



PREVENTATIVE MAINTENANCE:


RESTRICTED TOLERANCE INSPECTION:

REPLACE:

SERVICEABILITY:


SHALL:

SHOULD:

STANDARD PARTS:


TEST:

TRACEABILITY:


WILL:

Simple or minor preservation operations and the replacement of small standard parts not involving complex assembly operations.

A CAMP Inspectionthat has a tolerance less than 10%, the inspectionmust be performed prior to the due time plus the allowed overflight.

Remove an item and install a new or serviceable item in its place.

Documentation that a part: a) has been manufactured or, b) is (or has been maintained) in an airworthy condition, according to the FAR’s.

Has been used only when application of a procedure is mandatory.

Has been used only when application of a procedure is recommended.

Parts conforming to established industry or United States specifications (such as bolts and nuts) (refer to 14 CFR Part 21 Subpart K).

Operation of aircraft components, appliances, or systems to evaluate functional performance.

Historical evidence that shall include the requirements of 14 CFR Part 21, 14 CFR Part 91.417 (Maintenance Records), and 14 CFR Part 43.

Has been used only to indicate futurity, never to indicate mandatory procedure.

MARITIME HELICOPTERS	DHC-6 MAINTENANCE MANUAL

Page No:	3-1 Revision:	Orig
Issue Date:	5/1/20


3	IMPLEMENTATION OF THIS INSPECTION PROGRAM

3.1	AIRCRAFT ELIGIBLE FOR CONTINUOUS AIRWORTHINESS MAINTENANCE PROGRAM

Each additional aircraft and/or engine being placed on or removed from a Continuous Airworthiness Maintenance Program will have a complete record audit to ensure that all required inspections, applicable mandatory service bulletins, Airworthiness Directives and aircraft servicing arecurrent prior tobeing placed on the CAMP. Thetime inservice calendar orcycles of operation accumulated under the previous program will be applied to determine inspection due time under the new program (14 CFR 91.409). This "phase in" must be approved by the Director of Maintenance.

Except for new aircraft (less than 50 hours total time) being introduced to this CAMP that are not operating on a Part 135 Program or Manufactures Program, a determination shall be made by the Director of Maintenance as to what inspections must be complied with prior to putting the aircraft on to the CAMP program. A bridging document determining which inspections must be complied with before bringing the aircraft onto the program will be created and remain on file for 1 year.


3.2	PROCEDURE FOR ENTERING PROGRAM

The following procedures shall be used when entering an aircraft on Maritime Helicopters’ Continuous Airworthiness Maintenance Program (CAMP).

·	The aircraft registration number, make, model, and serial number shall be on the Operations Specification List of Approved Aircraft.
·	The requirements of paragraph 3.1(Aircraft  Eligiblefor Continuous Airworthiness Maintenance Program) have been complied with.
·	 A bridging document will be created and remain on file for 1 year. The document shall determine by outline which inspections must be complied with before bringing the aircraft onto the CAMP. These inspections shall be entered on to the aircraft logbook and signed off before the aircraft entered onto the program.
·	 Once the bridging requirement inspections have been complied with, the Aircraft and Engine Log Book shall have an entry made stating that the aircraft and engine are now being inspected in accordance with Maritime Helicopters Model DHC- 6 Series Continuous Airworthiness Maintenance Program

3.3	PROCEDURE FOR LEAVING PROGRAM

When an aircraft is removed from the Continuous Airworthiness Maintenance Program, it shall be the responsibility of the new owner/operatorto assume the responsibility for the safe operation and airworthiness of that aircraft. Maritime Helicopters shall make a logbook entry stating that the aircraft is no longer beingmaintained on the Maritime Helicopters’ Approved Continuous Airworthiness Maintenance Program.

3.4	PROCEDURE FOR INSTALLATION OF REPLACEMENT PARTS

The following procedure shall be used when replacement parts (not maintained under Maritime Helicopters Continuous Airworthiness Maintenance Program) are installed.

·	Inspection of new replacement parts or overhauled parts (TSO 0.0) shall be at the next normally scheduled Maintenance Manual Inspection following installation.
·	Inspection of “loaner part(s)” shall be maintained in accordance with Maritime Helicopters Continuous Airworthiness MaintenanceProgram.

It shall be the installing mechanic’s responsibility to determine the “status” of operation accumulated on the part under previous inspection programs prior to installation of the serviceable replacement part. If the “status” of operation accumulated on the part under previous inspection programs cannot be determined, the serviceable part shall be inspected to all previous Maintenance Manual Inspection allowing it to coincide with the next normally scheduled Maintenance Manual Inspection.


3.5	PROCEDURE FOR NEWLY INSTALLED KITS (ACCESSORIES) NOT COVERED BY THIS CAMP

If the manufacturer of a kit (accessory), appliance or product newly installed on the aircraft supplies instructions for continued airworthiness, Maritime Helicopters Continuous Airworthiness Maintenance Program aircraft status sheet (CALM) shall be revised to incorporate the new instructions for continued airworthiness. Maintenance Manual Inspection requirements associated with the installation of new equipment on an aircraft shall be monitored via the computerized tracking system as a separate inspection until the Maintenance Manual is revised and FAA approved.
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4	PROGRAM OPERATION

4.1	PERFORMANCE INSTRUCTIONS

A Maintenance Manual inspection may be started at any point. Inspection’s due times may be exceeded as allowed by the Maintenance Manual inspection’s interval. NOTE:See Paragraph 4.2.1 for limitations of tolerances and calculation of time to nextMaintenance Manual inspection due.


LEGEND CAMP Inspection Form – Inspection Item Numbering - A 0305.3.1.2

A	030	5.	3.	1.	2

Denotes Sequential Inspection Steps Within a “Single” InspectionItem

Denotes a “Single” Inspection Item Within The Segment (All sequential inspection items shall be performed)

Denotes Inspection Segment
(Inspection items may be performed individually)

Denotes Inspection Sequence Number for Inspections of the same frequency requiring separation.

Denotes Inspection Section Number


Denotes Inspection Section

4.2	INSPECTION DUE TIMES

The Maintenance Manual has been developed into inspection series and are independent (stand-alone) of one another. They may be performed in conjunction with one another or independently.

Airframe inspectionseries shall be tracked on the aircraft “status sheet” based on airframe total time.
Powerplant inspectionseries applies to engine inspections and shall be tracked on the engine “status sheet” based on engine total time. .

4.2.1	INSPECTIONTOLERANCE

Inspection tolerances in this Maintenance Manual are controlled by the manufacture’s requirements. If the manufacturer has no tolerance allowed for an inspection item, the inspection item will be found in a No Tolerance (NT) Inspection or placed in a convenient lower frequency inspection. If the manufacturer has a tolerance for an inspection item and the tolerance is less than 10% or restricted to 100 hours and/or 30 days, the inspection item will be found in a restricted Tolerance (RT) Inspection or placed in a convenient lower frequency inspection. If the tolerance is at least 10%, the inspection will be placed in an inspection without designators. A statement of “No Tolerances,” or “This Inspection is Restricted to (XX Hours or XX Days),” as required, shall be placed in the notesection of the header on the Maintenance Manual Inspection form.

·	Use of the Inspection tolerances are to be considered as non-routine maintenance practice, not standard operating procedure.
·	Each inspection without a designator may be exceeded by 10% of theMaintenance Manual inspection’s most restrictive interval.
·	Each inspection with a designated NT or No Tolerance shall not exceed any interval.

·	Each inspection with a designated RT or Restricted Tolerance may be exceeded by the stated tolerance in the NOTE section of the work card.
·	 If the Maintenance Manual inspection was completed prior to the scheduled due time, the time to the next inspection due shall be calculated from the time the inspection was completed.
·	 If the Maintenance Manual Series A inspection was started after the scheduled due time, the time to the next inspection due shall be calculated from the time it was completed. Series B will also be figured from when the inspection was completed. Inspections are not to exceed the stated tolerance of the Maintenance Manual inspection’s interval (the standard 10% tolerance or stated restriction).
For aircraft repositioned for long term maintenance; calendar Maintenance Manual inspection intervals performed during the long-term maintenance will start from the date the aircraft is returned to service for all Maintenance Manual inspections completed.
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4.3	SCHEDULE OF INSPECTIONS

4.3.1	BASIC INSPECTIONS: Basic Inspections Applicable to DHC-6 Series Aircraft

	SECTION
	
	TYPE
	
	FREQUENCY

	
R 007	Routine 	Every 7 Days

REMOVED	

A 0125	Basic	Every 125 Hours

B 0250	Basic	Every 250 Hours

C 0500	Basic	Every 500 Hours

C 1000RT	Basic	Every 1000 Hours

C 1500RT	Basic	Every 1500 Hours

C 1700NT	Basic	Every 12 Months

C 3000RT	Basic	Every 3000 Hours



4.3.2	POWERPLANT INSPECTIONS: Powerplant Inspections Applicable to Pratt & Whitney PT6B-34 Series Powerplant

	SECTION
	
	TYPE
	
	FREQUENCY

	
 REMOVED 

REMOVED




4.3.3	FUNCTIONAL INSPECTIONS: Functional Inspections Applicable to DHC-6 Series Aircraft

	SECTION
	
	TYPE
	
	FREQUENCY

	
F 3000NT	Functional	Every 3000 Hours




4.3.4	COMPONENT TESTS: Component Tests Applicable to DHC-6 Series Aircraft performed Off Wing

	SECTION
	
	TYPE
	
	FREQUENCY

	
CT 6000NT	Component Test	Every 6000 Hours
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4.4	UNSCHEDULED INSPECTIONS

4.4.1	POWERPLANT - Unscheduled inspections are done when the engine is subjected to unusual stress or operating conditions, or exceeds operating limitations or gives unsatisfactory performance/handling. Unscheduled Powerplant inspections are to be performed I/A/W the Pratt & Whitney PT6A-34 MM 72-00-00 ENGINE INSPECTION Chapter 12.

4.4.2	AIRFRAME - Unscheduled inspections are to be completed I/A/W the appropriate section of the Viking PSM 1-6-7 Maintenance Manual as required.

Unscheduled inspection shall be entered into the either the Work Order or Aircraft Log Book. These discrepancies must be rectified prior to release of aircraft for flight.

4.5	SPECIFIC CONDITION INSPECTIONS

Specific Conditional inspections are to be performed I/A/W;
1) Pratt & Whitney PT6T MM 72-00-00 ENGINE - INSPECTION/CHECK 2) Viking PSM 1-6-7 Part 2

4.6	OPERATIONAL CHECKS AND OPERATIONAL CHECK FLIGHTS

See the "Maritime Helicopters Operations Manual,” and “General Maintenance Manual” as revised, for complete instructions concerning operational checks and flights.

4.7	INSPECTIONS AWAY FROM HOME BASE

Inspections away from home base shall be conducted in accordance with the Continuous Airworthiness Maintenance Program and the Maritime Helicopters General MaintenanceManual, as revised.

4.8	OVERHAUL SCHEDULE

Overhauls are tracked on Maritime Aircraft’s computer aircraft status CALM sheets.

MARITIME HELICOPTERS	DHC-6 MAINTENANCE MANUAL

Page No:	5-1 Revision:	Orig
Issue Date:	5/1/20



5	PAPERWORK

The basic guide to record keeping concerning maintenance, preventative maintenance, rebuilding, and alterations is contained in 14 CFRPart 43.

5.1	PAPERWORK DISTRIBUTION

Completed inspection forms along with the aircraft records shall be returned WEEKLY to the Homer or Fairbanks office, in accordance with the "Maritime Helicopters General Maintenance Manual,” as revised.

5.2	DEFERRED DISCREPANCY LOG

See “Section B – Maintenance and Mechanical Discrepancies” of the "Maritime Helicopters General Maintenance Manual,” as revised, for complete instructions concerning deferredmaintenance.

5.3	DOCUMENTING DISCREPANCIES

All discrepancies discovered during the course of, or in between, scheduled inspections will be entered in the aircraft logbook. When the inspections are being performed by acertified repair station, the RepairStation personnel will enter the discrepancies on the Repair Station Work Order.

All discrepancies affecting airworthiness will be corrected before approving the aircraft for return to service. Repairs will be accomplished using data that is acceptable to the FAA. For major repairs, data that is approved by the FAA will be used. The corrective action taken for each discrepancy will be entered in the aircraft logbook or on the RepairStation Work Order when the inspectionis being performed by acertified repairstation.

5.4	AIRWORTHINESS RELEASE ORINSPECTIONLOG ENTRY

An airworthiness release or an appropriate entry in the Aircraft Logbook shall be made by an authorized mechanic (as defined in paragraph 2.3) after inspections have been performed on an aircraft.

A.	Inspections performed by a FAA Repair Station shall have an airworthiness release signed by a certified and authorized mechanic or inspector. B.	A Maritime Helicopters mechanic shall make an appropriate entry in the Aircraft Logbook and Maintenance Discrepancy worksheet as follows:
1.	A description of work performed.
2.	Date of completion of work performed.
3.	Type of Certificate and Certificate Number of person approving work performed. 4.	Signature of person approving work performed.
C.	Inspections completed in accordance with Maritime Helicopters’ CAMP Maintenance Manual shall be made as described in the individual inspectionforms.
D.	Completion of C above certifies the following:
1.	The entries required by Paragraph C were prepared in accordance with the procedure in Maritime Helicopters’ CAMP.
2.	All work was performed in accordance with the requirements of Maritime Helicopters’ Continuous Airworthiness Maintenance Program. 3.	All required items were inspected by an authorized mechanic who determined that the work was satisfactorily completed.
4.	So far as the work performed is concerned, the aircraft is in acondition for safe operation.
5.	The signature of the authorized person constitutes the approval for return to service only forthe work performed.
E.	All components removed or installed that have a time, cycle, RIN, or calendar life limit shall have the total time, time since inspection, time since overhaul, total cycles, total flights/landings, and calendar date, of both the removed and installed items, as applicable. This information will be entered in the Aircraft Logbook, Engine Logbook (s), andMaintenance Discrepancy worksheet as required.
F.	Recurring Airworthiness Directives shall require the time and/or date and when the next action is due, to be entered in the Aircraft Logbook, Engine Logbook (s), and Maintenance Discrepancy worksheet as required.
G.	All discrepancies noted during Maintenance Manual inspection(s) shall be recorded and rectified in the aircrafts logbook before approval to return to service.

5.5	AIRCRAFT “STATUS REPORT”

The Aircraft “Status Report” (CALM) is designedto be used as a tracking aid for aircraft inspections, component overhauls, airworthiness limitations, AD's, ASB's, FAR requirements, and lubrication intervals. All data is supported by a component recordcard or a logbook entry.

A.	The report breakdown consists of:
1.	Aircraft ID - Registration Number 2.	Model -Of Aircraft
3.	Serial Number - Of Aircraft
4.	Current hours -As of date of last update
5.	Task Code Number – Identification of individual line item
6.	Part Number - Identifies manufacturer's approved part number 7.	Nomenclature - For identification of each line item
8.	Serial Number - Of Component
9.	TSN/TSO at install - Total time of component when installed 10.	Remains -Time before overhaul, retire, or inspection.
11.	Current TSN/TSO - Current time on an item as of last revised status sheet date 12.	Service Life -Manufacturer's assigned service life
13.	 The status of all applicable airworthiness directives and recurring manufacturer's alert service bulletins are listed as to next compliance and next due.
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B.	 The Aircraft “Status Report” shall be used as a guide to ensure that time or calendar-controlled components, inspections, airworthiness directives and manufacturer's alert service bulletins shall be removed or inspected by the time or date indicated.
C.	The Aircraft “Status Report” shall be updated by using the actual aircraft total time logged inthe aircraft Logbook. D.	The Director of Maintenance (or designee) will verify all changes to the Aircraft “Status Report” are true and correct.
E.	Changes to the Aircraft “Status Report” involving component changes or maintenance complied with shall be submitted by the mechanic and verified for true and correct updates.
F.	The Aircraft “Status Report” also includes the cycle of Maintenance Manual inspections for upcoming and completed inspections

5.6	INSPECTION FORMS

Maritime Helicopters Continuous Airworthiness Maintenance Program Maintenance Manual inspection forms provide the necessary instructions and procedures to conduct aircraft (airframe, engines, rotors, and appliances, including emergency equipment) inspections. Completed Inspection forms will remain on record for each inspection until superseded by the next same inspection.


5.7	INSPECTION ITEMS

Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for assuring the inspection form is current with the Maintenance Manual published on the MHI Portal and making the logbook entry shown at the conclusion of this inspection.

NOTE:
If a manufacturer extends (escalates) the recommended inspection interval, Maritime shall request FAA approval for the new manufacturer inspection interval usingthe Temporary Revision process (2.14)to facilitate compliance until the Maintenance Manual has been revised. The request shall be accompanied by a copy of the manufacturer’s recommendation.

5.8	REQUIRED INSPECTION ITEMS (RII)

Maintenance performed, scheduled or unscheduled, to these components or systems require inspection by properly authorized RII inspectors.

• Flight Controls • Landing Gear • Propellers
• Engine Installation • Engine Controls

Component and system possible inspection items are described in detail in this manual.


5.9	REQUIRED INSPECTION METHODS

RII function shall be performed I/A/W Maritime Helicopters Maintenance Manual using the RII Management Process. RII inspectors are the final authority as to the status of all maintenance, preventive maintenance, and alterations functions performed that require a RII approval. The approved RII Inspector list is maintained by the DOM

The authorized inspector’s signature or affixed stamp constitutes the approval for return to service. If the stamp is used it shall be affixed to both copies of the aircraft maintenance logbook sheets.

If an RII inspection is required, it will be entered in the work order or aircraft logbook as aseparate entry.

If a pilot operational check is required it shall also be entered inthe aircraft logbook as being due, as a separate entry. The pilot’s signature at the completion of the maintenance operational check returns the aircraft to service.

The technician performing the work shall have a company authorized inspector perform the inspection of the required inspection item. The technician performing the work may not perform the required inspection.

Required inspection items shall be inspected by designated inspection personnel using manufacturer’s manuals. The method of performing these inspections constitutes a visual inspection at critical steps of the work in process and upon completion of the work. The technician performing the work has the responsibility to have his work inspected by an RII inspector at critical stages.

An RII Inspector must:
a. Verify all critical processes
b. Verify all rigging dimensions and adjustments c. Verify all hidden torques and safeties
d. Ensure the use of: i. Proper parts
ii. Proper materials iii. Proper procedures
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In all cases, required inspection items will be inspected to ensuresaid items are in an airworthy and safe condition.

In the event that the inspector does not approve the item of work, he will not sign off the required inspection, and will advise the technician who accomplished the item of work of the discrepancies found. The technician will then remedy the discrepancies and the inspector will repeat his inspection function. This procedure will be referred to as the “Buy-Back” procedure, and will be repeated until the item of work has been satisfactorily accomplished.

Discrepancies found by the RII Inspector must be entered in the aircraft logbook, if that inspector cannot ensure he will see the “Buy-Back” procedure through to completion.

In the event that any required inspection is not completed as a result of work interruptions, the RII Inspector will make an entry on the appropriate form (logbook, etc.), stating the required inspection is incomplete, and a brief description of the reason why it is incomplete.

If any company authorized inspector finds an item which is questionable, the Chief Inspector or Director of Maintenance shall be consulted and shall have final authority to approve the aircraft for return to service or take other necessary action.

Questions concerning any decisions of any required inspection personnel will be made to the Chief Inspector. In the case that the Chief Inspector is not available, the decision of the required inspection personnel will stand until the Chief Inspector is available to make the final decision.

The Required Inspection Items are inspected by a designated RII Inspector at any time a component of one of the items is removed and a like item is installed, or when any part of one of the items is disconnected and reconnectedfor any reason.

It is the responsibility of the maintenance technician performing the work to have that work inspected priorto approving the aircraft for return to service.


5.9.1	REQUIRED INSPECTION ITEMS STANDARDS

Maritime Helicopters Inc. will utilize the following RII task card whenever perform RII inspections.


	Acceptance
	Task & JASC 6200 Series Code:

	
	1. Verify the maintenance manual revision is up to date.

	
	2. Verify date of calibration of special tools utilized.

	
	3. Verify the maintenance manual procedure is followed for this installation.

	
	4. Verify the applicability of Alert Service Bulletins and Technical Bulletins to this installation.

	
	5. Visually inspect installation for attachment, security, proper installation, and system integrity.

	
	6. Verify all torques, final closures, and verify all safeties.

	
	7. Apply torque seal to all safeties.

	
	8. Review logbook and record entries for accuracy and completion.
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6 WEIGHT AND BALANCE CONTROL


6.1	INDIVIDUAL AIRCRAFT WEIGHT AND BALANCE CONTROL

The individual weight and balance of each aircraft will be re-established at the specified reweighing periods. It will also be re-established whenever the cumulative changes to the empty weight exceed plus or minus one-half of one percent of the maximum landing weight or the cumulative change in C/G position exceeds one-half of one percent of the C/G range. Weight and Balance shall be carried out I/A/WViking PSM 1-64-8 WEIGHT & BALANCE Manual.

6.2	RESPONSIBILITY

The Chief Inspector has the responsibility for current empty aircraft weight and balance. Prior to release of an aircraft which has undergone a repair or alteration effectingthe weight and balance of the aircraft, the Chief Inspector will accomplish the following as applicable:

If the cumulative weight change is less than plus or minus one half of one percent of the C.G. range, the cumulative change in weight and balance will be recorded on the Aircraft Basic Weight andBalance Form.

When the cumulative weight changes to the empty weight, exceeds plus or minus one half of one percent of the maximum landing weight, re-compute the empty weight.

When the cumulativechange in the C.G. position exceeds plus orminus one half of one percent of the C.G. Range, re-compute the empty weight C.G.

The re-computed aircraft empty weight and balance will be forwarded with a revision control sheet to the Director of Maintenance. The signed revision control sheet must be returned to the Chief Inspector's office prior to release of the aircraft.

Changes to the aircraft C.G., empty weight, or cumulative change to the aircraft weight and balance, their effect on the current loading schedule is the responsibility of the Director of Maintenance.

6.3	WEIGHT AND BALANCE FORMS


6.3.1	AIRPLANE WEIGHT AND BALANCE RECORD

This form is intended to serve as a ready reference to show the current empty and/or weighed weight and index for each Maritime Helicopters, Inc. aircraft. The master copy of this form will be retained in the Aircraft Weight and Balance files. This report is completed by the Company Chief Inspector each time a change is made to any aircraft weight. The information for this report will be gained from data supplied by the Assistant Chief Pilot-Fixed Wing and filed in each aircraft permanent Weight and Balance file. The permanent records will be checked at the end of each calendar month and the Aircraft Weight and Balance Status Report will be reviewed for accuracy. The Chief Inspector will compute the aircraft index and provide it tothe Operations Department.

6.3.2	PRE-WEIGHING CHECK LIST

This report is used and completed prior to the actual weighing of the aircraft and is attached to the actual Weight and Balance Form for filing. This form is to establish that the aircraft is in proper condition to be weighed.

6.3.3	AIRCRAFT EQUIPMENT LIST

This form is used to record all permanent equipment installed in the aircraft at the time of weighing. The Chief Inspector is responsible for the accuracy and completeness of this form. It is attached to the actual Weight and Balance Form for retentionin the aircraft records.

6.3.4	AIRCRAFT WEIGHT AND BALANCE MANIFEST

This form will be used for computation of operational index units and per cent C.G. and provides the data required by the flight crews to compute the weight and balancefor each flight.

6.3.5	BASIC WEIGHT CHANGE RECORD

This form will be used between aircraft weighing to compute the change in C.G. cause by any removed or installed equipment, or major repairs which will affect the weight and balance of the aircraft. Weight changes totaled on this sheet may not exceed one-half of 1.0% of the maximum landing weight of the aircraft without recomputing the weight and balance. Any of the Accumulative Weight and Change Records sheet accumulated between weighing may be discarded at weighting.

NOTE: Any other forms that provide equivalent information may be used if this companies name is placed on the form in a conspicuous place.

Specific Weight andBalance figures are from the Viking PSM 1-64-8 WEIGHT & BALANCE Manual
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6.4	WEIGHT AND BALANCE FORMS


[image: ]6.4.1	MARITIME HELICOPTERS WEIGHT AND BALANCE FORM PRE-WEIGHING CHECK LIST
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7	AIRFRAME INSPECTIONS







The following airframe inspections shall be performedin conjunction with Maritime Helicopters CAMP General Manual and applicable VikingMaintenance Manuals as listed.
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7.1	ROUTINE INSPECTION


Registration No.:     N                                         Start Aircraft S/N:                                                Date:

Aircraft Start Total Time: Aircraft Start Total Cycles:


Reference: DHC-6 Maintenance Program, Viking PSM 1-64-2 Maintenance Manual

	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INTIALS

	R 007.1	GENERAL

	
1.1	Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	1.2	Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3	Replace all life limited components that have completed published operating limits.
	DHC-6 MP
	
	

	1.4	Open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	DHC-6 MP
	
	

	R 007.2	PLACARDS AND MARKINGS

	
2.1	Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	R 007.3	CORROSION CONTROL

	
3.1	Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	
Appendix C
	
	

	R 007.4	INTERNAL

	
4.1	 Cargo nets for condition and security, if installed. Effectivity: Mod SOO 6274& Mod 6389
	
	
	

	4.2	Removed N/A with our aircraft.
	
	
	

	4.3	Heated windshields for condition, discoloration, delamination and security.
	
	
	

	4.4	Emergency hand pump handle for security in stowed position
	
	
	

	4.5	Portable fire extinguisher(s) for condition and evidence of leakage, security in stowed position.
Note: Refer to manufacturer’s instructions and local regulatory authority approval.
	
	
	

	4.6	Flight compartment axe and axe stowage forcondition and security of axe stowagestructure. Condition and security of axe cutting edge and pike to axe handle.
Effectivity: Mod SOO 6376
	
	
	

	4.7	Pilot and Copilot seats, seat belts for condition and security, seat belt buckles for proper operation.
	
	
	

	4.8	Utility Seats and Seat Belts for condition and security; Seat Belt Buckles for proper operation. 
                 I.A.W IKHANA STC SA02556LA, I.C.A Doc SU-6-11 Para 8.2

	
	
	

	4.9	Removed, not installed.
	
	
	

	4.10	Nose baggage compartment verity the HIRF covers are installed. All fasteners must be engaged. Replace if damaged.
Effectivity: Mod 6/2024
	
	
	



MARITIME HELICOPTERS	DCH-6 MAINTENANCE MANUAL




CHECK: FREQUENCY: NOTE::




R 007 – ROUTINE INSPECTION Every 7 Days

Page No: Revision: Issue Date:

7-3 Original 05/01/20


	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INTIALS

	R 007.5	EXTERNAL

	
5.1	Fire extinguisher indicator discs for evidence of extinguisher discharge.
	
	
	

	5.2	Elevator, aileron and all flap skins for condition, drain holes for obstruction and wingtip fairings for condition.
Note: Removed, N/A with our aircraft.
	
	
	

	5.3	Stall warning lift detector vanes for condition, free movement and security.
	
	
	

	5.4	External surfaces of fuselage, nacelles, wings and stabilizers for condition, drains holes for obstruction, wing fences for condition and security, deicing boots for condition.
	
	
	

	5.5	Wing strut skins (where visible) for condition and fasteners for security.
Note: Removed, N/A with our aircraft.
	
	
	

	5.6	Water contamination in fuel system at water drain and fuel strainer drain points.
	
	
	

	5.7	Evidence of fuel leaks on underside of fuselage, drain valves for leakage andsecurity.
	
	
	

	5.8	Fuel vent outlets for obstructions.
	
	
	

	5.9	Fuel for water content, drain valves for condition and security, bent outlets for obstruction, fillercap for proper fit and seal condition, filler necks for condition.
Effectivity: Mod SOO 6095& Mod 6247 edit, removed wing tank.
	
	
	

	5.10	Depressurize hydraulic system and check gas pressure in accumulators.
	
	
	

	5.11	Hydraulic reservoir for correct fluid level.
	
	
	

	5.12	Pitot heads andStatic vents for obstructions.
	
	
	

	5.13	Windshieldforsigns of leakage. Clean as required.
	
	
	

	5.14	Cabin, cabin doors and escape hatch windows. Clean as required.
	
	
	

	5.15	Nose and main wheels for cuts, wear, deterioration and inflation.
	
	
	

	5.16	Main and nose wheels forcondition.
	
	
	

	5.17	Tail bumper for condition and security.
	
	
	

	5.18	Removed. See 5.9.
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MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INTIALS

	R 007.6	FUNCTIONAL CHECKS

	
6.1	Position, anti-collision, cabin and landing lights.
	
	
	

	6.2	Taxi, wing inspection lights and instrument panel lights.

	
	
	

	6.3	Pitot system head heaters.
	
	
	

	6.4	Flood lights.

Effectivity: Mod 6/2028
	
	
	

	6.5	Caution lights dimming and dome lights. Effectivity: Mod 6/2028
	
	
	

	6.6	ESIS Operational test.

Effectivity: Mod SOO 6209 & Mod 6/2049
	
	
	

	R A007.7	FINAL CLOSE UP

	
7.1	Removed, carry over.
	
	
	

	R A007.8	POST INSPECTION

	
8.1	Removed. If anything requires a check flight we can put that check flight in the log book.
	
	
	

	8.2	Removed and carry over to next inspection. Plan is to combine the Routine inspections. No need for two weekly inspections.
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6 (Removed -400) Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may benoted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC- 6 – R 007 – 7 day Routine A Inspection and was determined to be in an airworthy condition. (Can we remove this and sign inspections off with, “Completed Routine Insp IAW MHI DHC-6 CAMP”?) This comes off to me as a Part 91 sign off.


Registration No.:	N	End Aircraft S/N:                                               Date:

Aircraft Ending Total Time: Aircraft Ending Total Cycles:


Signature:	Certificate Type & No:
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MAINTENANCE ACTION
	
REF
	L/H
MECH INITIALS
	R/H
MECH
INITIALS
	
RII INTIALS

	
	R 007.1	GENERAL

	
1.1	Remove.
	
	
	
	

	1.2	Remove
	
	
	
	

	1.3	Remove
	DHC-6 MP
	
	
	

	1.4	Remove
	DHC-6 MP
	
	
	

	
	R 007.2	PLACARDS AND MARKINGS

	
2.1	Remove
	
	
	
	

	
	R 007.3	CORROSION CONTROL

	
3.1	Remove
	
Appendix C
	
	
	

	
	R 007.4	INSPECTIONS

	
4.1	Propellershaft seal for evidence of oil leakage.
	
	
	
	

	4.2	Propeller deicing boots for condition and security.
	
	
	
	

	4.3	Engine intake deflector. Clean as required.
	
	
	
	

	4.4	Compressor inlet screen. Clean as required.
Note: If dirty screen warrants removal for cleaning, clean inlet as required.
	
	
	
	

	4.5	Check for correct oil level. Oil filtercap forcondition and proper locking.
Note: If level indication is low when checking oil quantity after engine has been shut down for more than 30 minutes, or after an oil change, then start the engine and run at ground-idle for minimum five minutes, feather the propeller, shutdown the engine, and recheck the oil quantity.
	
	
	
	

	4.6	Fuel, oil and bleed air pipes leakage.
	
	
	
	

	4.7	Removed, not installed on our Aircraft.
	
	
	
	

	
	
	

	4.8	Oil coolers and pressure transmitters for security and leakage.
	
	
	
	

	4.9	Wing deiced bonded stall bar for condition and proper adhesion.
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MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INTIALS

	R E007.5	FINAL CLOSE UP

	
5.1	Replace orclose all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	R E007.6	POST INSPECTION

	
6.1	Removed.
	
	
	

	6.2	Make an entry in the appropriate logbook (referto the following page forwording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be notedin the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

Completed Routine inspection IAW M.H.I DHC-6 CAMP.



Registration No.:	N	End Aircraft S/N:                                               Date:



Aircraft Ending Total Time: Aircraft EndingTotal Cycles:


Signature:	Certificate Type & No:
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7.3	BASIC INSPECTIONS Need to add AFTT, Start Date, A/C SN# and Cycles.

Reference: DHC-6 Maintenance Program, PSM 1-64-2 Maintenance Manual

	

MAINTENANCE ACTION
	

REF
	
MECH INITIALS
	
RII INITIALS

	
	A 0125.1	GENERAL

	
1.1	Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	1.2	Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3	Replace all life limited components that have completed published operating limits.
	DHC-6-400 MP
	
	

	1.4	Overhaul all components that have completed published operating limits.
	DHC-6-400 MP
	
	

	A 0125.2	PLACARDS AND MARKINGS

	
2.1	Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	A 0125.3	CORROSION CONTROL

	
3.1	Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	
Appendix C
	
	

	A 0125.4	PREPARATION

	
4.1.	Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
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MAINTENANCE ACTION
	

REF
	
MECH INITIALS
	
RII INITIALS

	A 0125.5	61 - PROPELLERS -RH

	
5.1.	Bata backup carbon block retaining pin for free movement. Lubricate
	
	
	

	5.2.	Overspeed governor for condition, security and leakage.

Removed AD Note, not our model.
	
	
	

	
5.3.	Propeller governor for condition, security and leakage.
	
	
	

	5.4.	 Propeller blades for condition, nicks, cracks, blades for freedom of movement on hub pitot tubes by rocking slightly using counterweights as levers; grease blade clamps.
	
	
	

	5.5.	Propeller tachometer generator for condition and security of installation.
	
	
	

	
5.6.	Propeller shaft seal for oil leaks.
	
	
	

	A 0125.6	61 - PROPELLERS -LH

	
6.1	Bata backup carbon block retaining pin for free movement. Lubricate
	
	
	

	6.2	Overspeed governor for condition, security and leakage.

Removed AD note, not our model.
	
	
	

	
6.3	Propeller governor for condition, security and leakage.
	
	
	

	6.4	Propeller blades for condition, nicks, cracks, blades for freedom of movement on hub pitot tubes by rocking slightly using counterweights as levers; grease blade clamps.
	
	
	

	6.5	Propeller tachometer generator for condition and security of installation.
	
	
	

	
6.6	Propeller shaft seal for oil leaks.
	
	
	

	A 0125.7	71 - POWEPLANT -LH

	
7.1.	Engine cowling fire seals for condition and security
	
	
	

	7.2.	Engine pipes, insulated air tubes, leads and controls; pipes for condition, security and leakage, controls for security and operation, clamps, and brackets for condition, leads for condition and security. Lockwire for security and installation. Clean as required.
	
	
	

	A 0125.8	71 - POWEPLANT -RH

	
8.1.	Engine cowling fire seals for condition and security
	
	
	

	8.2.	Engine pipes, insulated air tubes, leads and controls; pipes for condition, security and leakage, controls for security and operation, clamps, and brackets for condition, leads for condition and security. Lockwire for security and installation. Clean as required.
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MAINTENANCE ACTION
	

REF
	
MECH INITIALS
	
RII INITIALS

	A 0125.9	72 - ENGINE - LH

	9.1.	 Engine external tubing for condition, cracks bulges and evidence of fuel and oil leakage.
	
	
	

	                     Engine gas generator case for condition, cracks, bulges and evidence of hot spots
  9.2.           Cleanliness of air inlet screen.
	
	
	

	
9.3.	Power section and turbine exhaust for duct for condition, cracks and distortion.
	
	
	

	
   9.4           Check scavenge oil pump housing for leaks. 
	
	
	

	A 0125.10	72 - ENGINE - RH

	10.1.	Engine external tubing for condition, cracks bulges and evidence of fuel and oil leakage.
	
	
	

	                     Engine gas generator case for condition, cracks, bulges and evidence of hot spots. 
10.2.       Cleanliness of air inlet screen.
	
	
	

	
10.3.	Power section and turbine exhaust for duct for condition, cracks and distortion.
	
	
	

	
   10.4.         Check scavenge oil pump housing for leaks.
	
	
	

	A 0125.11	73 - ENGINE FUEL AND CONTROL - LH

	
11.1.	Fuel pump for security and evidence of leakage. 
               Removed AD note, N/A.
	
	
	

	11.2.	Fuel pump filter screen (inlet). Remove, inspect and install. Clean or replace as required and leak check (power on).
CAUTION: Whenever any component upstream of the filter is replaced, check screen after run up or first flight.
	
	
	

	11.3.	Fuel pump filter screen (outlet). Remove, inspect and install. Clean or replace as required and leak check (power on).
Note: Refer to PWC Service Bulletin No. 1155
	
	
	

	11.4.	 Fuel control unit for condition, security, linkages, sense lines and heaters for condition, security, and leakage. Examine FCU for bearing washout, shown by blue dye at FCU vent.
Removed AD note, N/A
	
	
	

	11.5.	 Remove and Replace High Pressure fuel filter element. Clean filter bowl. Reinstall assembly, torque to 100-150 in-lbs., and lockwire.
	
	
	

	
11.6.	Disconnect rod-ends and clean with solvent. Examine rod-ends for corrosion,  
                 roughness, and side play. Lubricate with MIL-PRF-7870E. 
	
	
	

	 
   11.7.        Check free movement of linkage.
	
	
	

	
11.8.	Compressor discharge P3 filter – clean filter element ultrasonically. Reinstall and safety.  Effectivity: Mod SOO 6177
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MAINTENANCE ACTION
	

REF
	
MECH INITIALS
	
RII INITIALS

	A 0125.12	73 - ENGINE FUEL AND CONTROL - RH

	
12.1.	Fuel pump for security and evidence of leakage. Note: Removed AD, N/A
	
	
	

	12.2.	Fuel pump filter screen (inlet). Remove, inspect and install. Clean or replace as required and leak check (power on).
CAUTION: Whenever any component upstream of the filter is replaced, check screen after run up or first flight.
	
	
	

	12.3.	Fuel pump filter screen (outlet). Remove, inspect and install. Clean or replace as required and leak check (power on).
Note: Refer to PWC Service Bulletin No. 1155
	
	
	

	12.4.	Fuel control unit for condition, security, linkages, sense lines and heaters for condition, security and leakage. Examine FCU for bearing washout, shown by blue dye at FCU vent.
Removed AD note, N/A
	
	
	

	12.5.	Remove and Replace High Pressure fuel filter element. Clean filter bowl. Reinstall assembly, torque to 100-150 in-lbs., and lockwire.
	
	
	

	
12.6.	Disconnect rod-ends and clean with solvent. Examine rod-ends for corrosion,  
                 roughness, and side play. Lubricate with MIL-PRF-7870E.
	
	
	

	
   12.7.        Check free movement of linkage.
	
	
	

	12.8.	Compressor discharge P3 filter – clean filter element ultrasonically. Reinstall and safety.  Effectivity: Mod SOO 6177
	
	
	

	A 0125.13	76 – ENGINE CONTROLS - LH

	
13.1.	Lubricate power control mechanism, Cambox, and linkage interconnecting rod - ends.

Removed AD and SIL note, not our model engine.
	
	
	

	A 0125.14	76 – ENGINE CONTROLS - RH

	
14.1.	Lubricate power control mechanism, Cambox, and linkage interconnecting rod - ends.

Removed AD and SIL note, not our model engine.
	
	
	

	A 0125.15	77 – ENGINE INDICATING - LH

	
15.1.	Torque pressure transmitter for condition and security.
	
77-02
	
	

	
15.2.	Gas generator tachometer for condition and security of installation. Removed prop tach gen. See 6.5
	
61-07 7-705
	
	

	A 0125.16	77 – ENGINE INDICATING - RH

	
16.1.	Torque pressure transmitter for condition and security
	
77-02
	
	

	
16.2.	 Gas generator tachometer for condition and security of installation. Removed prop tach gen. See 5.5.
	
61-07 7-705
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MAINTENANCE ACTION
	

REF
	
MECH INITIALS
	
RII INITIALS

	A 0125.17	79 - OIL - LH

	
17.1.	Engine oil filter remove and check for foreign matter. Install a serviceable filter.

Note: Clean or renew filter according to instruction in the Engine Maintenance Manual. Change oil I/A/W UACL Service Bulletin No. 1001.
	
79-01
	
	

	
	
	
	

	17.2.	Test magnetic chip detector in reduction gearbox for electrical continuity.
	79-03a
	
	

	
17.3.	Check oil level and condition, security of oil filler cap.
	
79-03
	
	

	A 0125.18	79 - OIL - RH

	
18.1.	Engine oil filter remove and check for foreign matter. Install a serviceable filter.

Note: Clean or renew filter according to instruction in the Engine Maintenance Manual. Change oil I/A/W UACL Service Bulletin No. 1001.
	
79-01
	
	

	
	
	
	

	3.2	Test magnetic chip detector in reduction gearbox for electrical continuity.
	79-03a
	
	

	
18.1.	Check oil level and condition, security of oil filler cap.
	
79-03
	
	

	A 0125.19	80 - STARTING - LH

	
19.1.	Starter generator for security of installation, electrical connectors for security. Clean as required
	
80-01-1
	
	

	19.2.	Ignition exciter and ignition leads for security and condition. 
	
	
	

	A 0125.20	80 - STARTING - RH

	
20.1.	Starter generator for security of installation, electrical connectors for security. Clean as required
	
80-01-1
	
	

	20.2.	Ignition exciter and ignition leads for security and condition.
	80-03
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MAINTENANCE ACTION
	

REF
	
MECH INITIALS
	
RII INITIALS

	A 0125.21	OPERATIONAL CHECKS

	
21.1	Perform the following Operational Checks;

NOTE
Electrical power for the following tests is obtained by connecting a ground power source or by running the engines, whichever is more convenient
	

	21.1.1	Fuel emergency shutoff valve - Return switches to NORMAL after test. Power on.
	
28-06-2
	
	

	
21.1.2	Fuel crossfeed valve and (if installed), position indicator (Pre Mod 6/2009).
	28-07-2 28-07a-2
	
	

	
21.1.3	HP fuel filter for leaks after element installation.
	
73-06-1
	
	

	
21.1.4	Fuel pump for leaks after inlet filter screen and outlet filter installation.

Note: Refer to PWC Service Bulletin No. 155
	
73-01a

73-01b
	
	

	
21.1.5	Oil filter for leaks after installation.
	
79-03
	
	

	
21.1.6	Fwd avionics compartment cooling fans (Mod 6/2045). (Power on).
	
21-20-2
	
	

	
21.1.7	DAU cooling fans (Mod 6/2045). (Power on).
	
21-21-2
	
	

	
21.1.8	Reversion control panel (Mod 6/2049) switch.
	
31-06-3
	
	

	
21.1.9	ADAHRS #1 and #2 (Mod 6/2049) reversion switches. (
	34-22-4 34-22a-4
	
	

	A 0125.22	POST INSPECTION

	
21.1	Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	21.2	Clean aircraft and engine once maintenance is completed.
	
	
	

	21.3	Removed, N/A
	
	
	

	
21.4	Check oil levels of hydraulic tank, engine prior to running aircraft.
	
	
	

	
21.5	Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters Viking DHC-6 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

Completed A0125 inspection IAW M.H.I DHC-6 CAMP.




Registration No.: N	End Aircraft S/N:                                     Date:

Aircraft Ending Total Time: Aircraft Ending Total Cycles:


Signature:	Certificate Type & No:
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Registration No.: N                                Start Aircraft S/N:                                      Date:

Aircraft Start Total Time: Aircraft Start Total Cycles:


Reference: DHC-6 Maintenance Program

	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	B 0250.1	GENERAL

	
1.1	Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	1.2	Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3	Replace all life limited components that have completed published operating limits.
	DHC-6-400 MP
	
	

	1.4	Overhaul all components that have completed published operating limits.
	DHC-6-400 MP
	
	

	B 0250.2	PLACARDS AND MARKINGS

	
2.1	Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	B 0250.3	CORROSION CONTROL

	
3.1	Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	
Appendix C
	
	

	B 0250.4	PREPARATION

	
4.1	Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	B 0250.5	21- AIRCONDITIONING

	
5.1	Removed, not installed.
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MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	B 0250.6	23 - COMMUNICATIONS

	
6.1	Pilot and Co-pilots head sets for condition and security.
	
	
	

	6.2	Nose cap lightning rod for condition and security.
	
	
	

	B 0250.7	24 – ELECTRICAL POWER

	
7.1	Removed, Not installed.
	
	
	

	7.2	Avionics Start Battery for condition and security.
Effectivity: Mod 6/2315
	
	
	

	B 0250.8	26 – FIRE PROTECTION - LH

	
8.1	Fire detection thermal units and wire loops for condition and security.
	
	
	

	8.2	Engine fire extinguisher bottle for condition and security, correct pressure, pipes for condition and security, electrical wiring for condition and connectors for security.
	
	
	

	B 0250.9	26 – FIRE PROTECTION - RH

	
9.1	Fire detection thermal units and wire loops for condition and security.
	
	
	

	9.2	Engine fire extinguisher bottle for condition and security, correct pressure, pipes for condition and security, electrical wiring for condition and connectors for security.
	
	
	

	B 0250.10	27 – FLIGHT CONTROLS - LH

	
10.1	Flap actuator for condition and security of mounting and leakage, selector valve for condition, security of mounting and leakage.
	
	
	

	10.2	Selector pulleys properly secured to spindle.
	
	
	

	10.3	Drip trays for condition, security and fluid content. Remove, dry out and install pads as required.
	
	
	

	B 0250.11	27 – FLIGHT CONTROLS - RH

	
11.1	Flap actuator for condition and security of mounting and leakage, selector valve for condition, security of mounting and leakage.
	
	
	

	11.2	Selector pulleys properly secured to spindle.
	
	
	

	11.3	Drip trays for condition, security and fluid content. Remove, dry out and install pads as required.
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MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	B 0250.12	28 – FUEL - LH

	
12.1	Removed, not installed.
	
	
	

	
	
	
	

	12.2	Removed, this is on the A0125 insp.
	
	
	

	12.3	Removed, not installed.
	
	
	

	12.4	Removed, not installed.
	
	
	

	12.4.1	Removed, not installed.
	
	
	

	12.4.2	Removed.
	
	
	

	B 0250.13	28 – FUEL - RH

	
13.1	Removed, not installed.
	
	
	

	13.2	Removed, this is on the A0125.
	
	
	

	13.3	Removed, not installed.
	
	
	

	13.4	Removed, not installed.
	
	
	

	13.4.1	Removed, not installed.
	
	
	

	13.4.2	Removed, not installed.
	
	
	

	B 0250.14	29 – HYDRAULIC POWER

	
14.1	Hydraulic reservoir filler neck for condition and contamination, fluid leakage, end of vent clear of power package tray. Dip stick for seal deterioration.
	
	
	

	B 0250.15	30 – ICE AND RAIN PROTECTION

	
15.1	Propeller deicing boots for cuts, tears, burns, deterioration and proper adhesion.
	
	
	

	15.2	Propeller deicing brush block and back plate slip ring for condition and security.
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MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	B 0250.16	32 – LANDING GEAR NOSE

	
16.1	Nose gear shock strut for correct extension as given on date plate. Fork retaining nut properly secured.
	
	
	

	16.2	Nosewheel steering actuator for condition and leakage, hydraulic pipes and input swivel lever for condition, connections for security and leakage.
	
	
	

	16.3	Steering cables where visible, for condition, corrosion, kinks, flattening, proper attachment and security; pulleys for condition, freedom of operation and security.
	
	
	

	16.4	Pulleys for condition, freedom of operation and security, turnbuckles for security.
	
	
	

	16.5	Perform a detail visual inspection of cable terminals as follows;
	
	

	16.5.1	Remove and discard the lockwire from the cable terminals.
Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	16.5.2	Do a detailed visual inspection of cable terminals excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	16.5.3	Do a detailed visual inspection of cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	16.5.4	If corrosion pits and/or cracks are found on any cable terminal, remove the applicable cable assembly and replace with new cable assembly.
	
	
	

	16.5.5            In a new cable assembly is install or if the rigging was disturbed when the lockwire was removed in step 15.5.1, rig the control system.
	
	
	

	16.5.6	If the lockwire was removed, secure the cable terminals with lockwire.
Note: Refer to Service bulletin No. 6/453.
	
	
	

	16.6	Steering actuator linkage for condition, corrosion and security, fouling of linkage on shock struct cylinder body.
	
	
	

	16.7	Remove nose wheel and clean as required.
	
	
	

	16.8	Inspect as follows;
	
	

	16.8.1	Wheel for abrasions, cracks, chipped rims.
	
	
	

	16.8.2	Bearings for signs of wear, corrosion, fretting and blueing; lubricate.
	
	
	

	16.8.3	Bushings for signs of wear.
	
	
	

	16.8.4	Seals for distortion, fit, deterioration and security.
	
	
	

	16.9	Install nose wheel assembly.
	
	
	



MARITIME HELICOPTERS	DCH-6 MAINTENANCE MANUAL




CHECK: FREQUENCY: NOTE::




B 0250 – BASIC INSPECTION Every 250 Hours

Page No: Revision: Issue Date:

7-20 Original 05/01/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	B 0250.17	32 – LANDING GEAR MAIN

	
17.1	Remove and clean main wheels.
	
	
	

	17.2	Inspect as follows;
	

	17.2.1	Wheels for abrasions, cracks, chipped rims, brake drive signs of wear.
	
	
	

	17.2.2	Wheel bearings for signs for wear corrosion, fretting and blueing.
	
	
	

	17.2.3	Brake housing for evidence of overheating.
	
	
	

	17.2.4	Brake discs for scoring, distortion, evidence of overheating.
	
	
	

	17.2.5	Brake disk guides (when installed) for condition and security.
	
	
	

	17.2.6	Brake linings for wear and within limits.
	
	
	

	17.3	Reinstall main wheels.
	
	
	

	B 0250.18	52 – DOORS

	
18.1	Cabin escape hatch door release mechanisms for proper operation, seals for deterioration and security.
	
	
	

	B 0250.19	53 – FUSELAGE

	
19.1	Cabin floor panes for condition, delamination, corrosion and security. Clean as required.
	
	
	

	19.2	Cargo tie-down rings for condition and security.

Note: if cabin floor panes are severely damaged, removed panels and inspect supporting structure for damage, buckling and cracks.
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MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	B 0250.20	55 - STABILIZERS

	
20.1	Elevator and rudder including tab hinge arms for condition and security.
	
	
	

	20.2	Hing arm attachment bolts for safety and security.
	
	
	

	B 0250.21	57 – WING – LH

	
21.1	Wing root rib forward aluminum adapter (Pre Mod 6/1887 and EO69080) for condition, cracks, corrosion and security.
Note: Refer to Service Bulletin Nos. 6/174 and 6/476 and A.D. 94-04-01 if applicable.
	
	
	

	21.2	Wing exterior upper surfaces for dents, scores, abrasions and corrosion.
	
	
	

	21.3	Inboard trailing flap for condition skins for cracks and fastener for security.

Note: Refer to Service Bulletin No. 6/174 and 6/345
	
	
	

	21.4	Wing flap, aileron hinge arms and connecting link attachment bolts for safety and security.
	
	
	

	21.5	Main wing hinge arms, bonding wire, bearings for condition and security and attachment bolts for safety and security.
Note: Includes inboard hinge location mounted ot the fuselage side at STA 248.41.
	
	
	

	B 0250.22	57 – WING – RH

	
22.1	Wing root rib forward aluminum adapter (Pre Mod 6/1887 and EO69080) for condition, cracks, corrosion and security.

Note: Refer to Service Bulletin Nos. 6/174 and 6/476 and A.D. 94-04-01 if applicable.
	
	
	

	22.2	Wing exterior upper surfaces for dents, scores, abrasions and corrosion.
	
	
	

	22.3	 Inboard trailing flap for condition skins for cracks and fastener for security. Note: Refer to Service Bulletin No. 6/174 and 6/345
	
	
	

	22.4	Wing flap, aileron hinge arms and connecting link attachment bolts for safety and security.
	
	
	

	22.5	Main wing hinge arms, bonding wire, bearings for condition and security and attachment bolts for safety and security.

Note: Includes inboard hinge location mounted at the fuselage side at STA 248.41.
	
	
	

	B 0250.23	61- PROPELLERS - LH

	
23.1	Removed, on A0125 insp.
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MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	B 0250.24	61- PROPELLERS - RH

	
24.1	Removed, on A0125 insp.
	
	
	

	
	
	
	

	B 0250.25	72 – ENGINE - LH

	
25.1	Exhaust duct for condition, defector vanes for cracks, erosion and security.
	
	
	

	
  25.2        Check Flow Divider/Dump Valve for installation and leaks.
	
	
	

	
  25.3         Check drain valves for installation and leaks.
	
	
	

	
  25.4         Check oil-to-fuel heater for installation and leaks.
	
	
	

	
  25.5         Inspect pneumatic tubes and lines for cracks and damages especially at the 
                 fittings and joints.
	
	
	

	
  25.6        Perform a visual inspection with a mirror or a borescope of the first stage
                compressor rotor.

                NOTE: If any FOD has caused the engine to become prone to engine surges or 
                causes unusual compressor whining, the large bent airfoil will make the whining 
                sound, remove the engine immediately.
	
	
	

	
	

	B 0250.26	72 – ENGINE - RH

	
26.1	Exhaust duct for condition, defector vanes for cracks, erosion and security.
	
	
	

	
   26.2       Check Flow Divider/Dump Valve for installation and leaks.
	
	
	

	
   26.3       Check drain valves for installation and leaks.
	
	
	

	
   26.4       Check oil-to-fuel heater for installation and leaks.
	
	
	

	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII      INITIALS

	
   26.5       Inspect pneumatic tubes and lines for cracks and damages especially at the 
                 fillings and joints.
	
	
	

	

   26.6      Perform a visual inspection with a mirror or a borescope of the fist stage 
                compressor rotor.

                NOTE: If any FOD has caused the engine to become prone to enine surges or
                causes unusual compressor whining, the large bent airfoil will make the whining 
                sound, remove the engine immediately.
	
	
	

	
	
	
	

	B 0250.27	80 – STARTING - LH

	
27.1	Remove spark igniters for operational test.
	
	
	

	27.2	Clean as required and install serviceable spark igniters.
	
	
	

	27.3	Install spark igniters.
	
	
	

	B 0250.28	80 – STARTING - RH

	
28.1	Remove spark igniters for operational test.
	
	
	

	28.2	Clean as required and install serviceable spark igniters.
	
	
	

	28.3	Install spark igniters.
	
	
	

	B 0250.29	OPERATIONAL CHECKS

	
29.1	Perform the following Operational Checks; NOTE
Electrical power for the following tests is obtained by connecting a ground power source or by running the engines, whichever is more convenient
	

	29.2	Lift Detector Vanes (WINGS) for freedom of movement, condition, corrosion and security. Function test (Power on).
	
	
	

	29.3	All communications and navigation systems.
	
	
	

	29.4	Weather radar.
	
	
	

	29.5	Wing flaps in normal and emergency.
	
	
	

	29.6	Fuel booster pumps, check for evidence of rough running.
	
	
	

	29.7	Fuel system strainers for leak check under system pressure after installation.
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MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
29.8	Flight controls, including trim tabs for full and free movement of all controls.
	
27-16-1
	
	

	29.9	Stall warning light and horn system (Pre Mod and Mod 6/2028) by actuating detecting vane.
	27-15a-2

27-15b-2
	
	

	29.10	Master warning and caution indication and control (Mod 6/2028) function test. (Power on).
	31-13-2
	
	

	B 0250.30	POST INSPECTION

	
30.1	Inspect for operation and leaks.
	
	
	

	30.2	Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	30.3	Clean aircraft and engine once maintenance is completed.
	
	
	

	30.4	Perform Functional Check Flight if required per DHC-6-400 Maintenance Manual or AFM as appropriate.
	
	
	

	30.5	Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

Completed B0250 inspection IAW M.H.I DHC-6 CAMP.



Registration No.: N	End Aircraft S/N:                                     Date:

Aircraft Ending Total Time: Aircraft Ending Total Cycles:


Signature:	Certificate Type & No:
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Registration No.: N                                Start Aircraft S/N:                                      Date:

Aircraft Start Total Time: Aircraft Start Total Cycles:


Reference: DHC-6 Maintenance Program

	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	C 0500.1	GENERAL

	
1.1	Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	1.2	Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3	Replace all life limited components that have completed published operating limits.
	DHC-6-400 MP
	
	

	1.4	Overhaul all components that have completed published operating limits.
	DHC-6-400 MP
	
	

	C 0500.2	PLACARDS AND MARKINGS

	
2.1	Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	C 0500.3	CORROSION CONTROL

	
3.1	Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection
	
Appendix C
	
	

	C 0500.4	PREPARATION

	
4.1	Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	C 0500.5	21 – AIR CONDITIONING

	
5.1	Cabin exhaust outlet or, if pneumatic package is installed, heat exchange for condition and clear of obstructions.
	
	
	

	5.2	Cabin exhaust outlet vent for condition and obstruction.
	
	
	

	5.3	STA 111 Cabin fans for condition and security, standoff mounting brackets for security.
Effectivity: SOO 6378
	
	
	

	5.4	 STA 332 Blower for condition and security, standoff mounting brackets for security. Effectivity: SOO 6379
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MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	C 0500.6	22 – AUTO FLIGHT

	
6.1	Autopilot (all models) for condition and security of mounting, altitude hold or controller for condition, static line for condition and security, attitude heading selector and turn and slip sensor (if installed) for condition and security. Clean as required.
	
	
	

	6.2	Autopilot (all models) aileron servo cable for fraying, kinks, flattening, proper attachment and security, turnbuckles for security. Pulleys and cable drum for condition, freedom of operation and security. Clamps for security and no evidence of movement on main aileron control cable clamp.
	
	
	

	6.3	Autopilot rudder (all models) servo cable for fraying, kinks, flattening, proper attachment and security, turnbuckles for security. Pulleys and cable drum for condition, freedom of operation and security. Clamps for security and no evidence of movement on main aileron control cable clamp.
	
	
	

	6.4	Rudder (all models) autopilot servo for condition and security of mounting.
	
	
	

	6.5	Autopilot elevator (all models) servo cable for fraying, kinks, flattening, proper attachment and security, turnbuckles for security. Pulleys and cable drum for condition, freedom of operation and security. Clamps for security and no evidence of movement on main aileron control cable clamp.
	
	
	

	6.6	Elevator (all models) autopilot servo for condition and security of mounting.
	
	
	

	6.7	Removed, No VOR duel selector relay.
	
	
	

	6.8	Automatic pitch trim (all models) system cables for fraying, kinks, flattening, proper attachment and security, turnbuckles for security. Pulleys and cable drive for condition, security and freedom of operation. Clamps for security and no evidence of movement on elevator flight control cable clamp.
	
	
	

	6.9	Autopilot (all models) electrical wiring for condition and connectors for security, bonding wires for condition and security. Clean as required.
	
	
	



MARITIME HELICOPTERS	DCH-6 MAINTENANCE MANUAL




CHECK: FREQUENCY: NOTE::




C 0500 – BASIC INSPECTION Every 500 Hours

Page No: Revision: Issue Date:

7-27 Original 05/01/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
6.10	AFCS (autopilot) system, inspect as follows;
Effectivity: Mod 6/2302, SOO6221
	

	6.10.1	Pilot and co-pilot Go Around (G/A) and Touch Control Switches for security and clean as required. Function test.
	
	
	

	6.10.2	Pilot and Co-Pilot; AP Disconnect (AP DISC) Switch for security and clean as required
	
	
	

	6.10.3	Perform ground Function Test
	
	
	

	6.10.4	Autopilot aileron servo for condition and security.
	
	
	

	6.10.5	Autopilot pitch trim servo actuator for condition and security. Clean as required.
	
	
	

	6.10.6	Autopilot pitch trim servo system pitch trim switch. Inspect for condition and security. Clean as required.
	
	
	

	C 0500.7	23 – COMMUNICATIONS

	
7.1	Audio system control units and power panels for condition and security of mounting. Flight compartment speakers and speaker panel assembly for condition and security.
	
	
	

	7.2	VHF upper aft antenna for condition and security, control and indicators for condition, wiring and connector for security. Clean as required.
Effectivity: Mod 6/2003
	
	
	

	7.3          VHF forward antenna for condition and security, control and indicators for condition, wiring and connector for security. Clean as required.
Effectivity: Mod 6/2003
	
	
	

	

	7.4	VHF lower aft antenna for condition and security, control and indicators for condition, wiring and connector for security. Clean as required.
Effectivity: Mod 6/2003, SOO6231
	
	
	

	7.5	VHF-FM antenna for condition and security, control and indicators for condition, wiring and connector for security. Clean as required.
Effectivity: Mod SOO 6296
	
	
	

	

	7.6	VHF and VHF standby antennas for loose connections, fiberglass cover for cracks and deterioration, wire whip for bending or misalignment.
Effectivity: Pre Mod 6/2003
	
	
	

	

	7.7	Removed. No HF radio installed. 
	
	
	

	7.8	Removed. No HF radio installed.
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MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
7.9	Power distribution and generator control box for condition and security; terminals, connectors and relays for condition and security, signs of overheat, arcing, torque of large terminal posts. Clean as required. Current Limiters (Mod 6/1651) for condition and serviceability.
	
	
	

	7.10	Removed. No HF radio installed.
	
	
	

	7.11	Static discharge wicks for condition and security, minimum length of one-inch wick extension from sheath.
	
	
	

	7.12	GPS/IRIDIUM/WiFi antenna for condition, security and corrosion, condition of external fillet seal, condition of coaxial cables and connectors and security of attachment of coaxial cables.
	
	
	

	7.13	Diodes CR 141 thru CR 146 – check diodes. Replace if required.
	
	
	

	7.14	Removed. No inverters installed in aircraft. This was for a -300 model.
	
	
	

	7.15	All aircraft accessible wiring and connectors for condition and security.
	
	
	

	7.16	Check condition and security of main Battery cables at Main Battery and Power Distribution control box.

	
	
	

	C 0500.8	25 - EQUIPMENT/FURNISHINGS

	
8.1	Inspect pilots and co-pilots seats as follows;
	

	8.1.1	Seat structure and seat pan for condition and security, freedom of movement.
	
	
	

	8.1.2	Seat rails for condition and security of stops.
	
	
	

	8.1.3	Chock cords for condition and security.
	
	
	

	8.1.4	Safety harness for condition and security, quick release for proper operation. Clean as required.
	
	
	

	8.1.5	Inertia reel for condition and security, proper operation.
	
	
	

	8.1.6	Inspect ELT mounting provision for security, condition, and retention. 
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8.2	Cabin side rail and floor for condition and security.

Removed SB and AD note. Not our SN Aircraft.
	
	
	

	8.3	Removed. Not installed in our aircraft.
	
	
	

	C 0500.9	27 – FLIGHT CONTROLS

	
9.1	Trim cables for condition, graying, corrosion, flattening, proper attachment and security.
	
	
	

	9.2	Control column boot for condition and security.
	
	
	

	9.3	Nylon cable jacket for condition, cracking and necking down in diameter.
	
	
	

	9.4	Pulleys (bulkhead and elevator torque tube) for condition and freedom of movement, pulley brackets for condition and security.
	
	
	

	9.5	Lubricate pulley bracket bushings at elevator torque tube.
	
	
	

	9.6	Rudder and elevator trim screw jacks for condition of cable drum grooves, freedom of operation and security. Lubricate.
	
	
	

	9.7	Flap selector valve and follow-up cables for condition, corrosion, fraying, flattening and security of attachment, turnbuckles for security, pulleys for condition and freedom of operation.
	
	
	

	9.8	Do a detailed visual inspection of cable terminals as follows;
	
	

	9.8.1	Remove and discard the lockwire from the cable terminals.

Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	9.8.2	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	9.8.3	Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	9.8.4	If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	9.8.5	If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 9.7.1, rig the control system.
	
	
	

	9.8.6	If the lockwire was removed, secure the cable terminals with lockwire.
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9.9	Flap/elevator interconnect ball screw jack for condition of cable drum grooves, freedom of operation and security. Lubricate
	
	
	

	9.10	Elevator flap interconnect screw jack for condition of cable drum grooves, freedom of operation and security. Lubricate.
	
	
	

	9.11	Aft fuselage elevator quadrant for condition, distortion, loose toque tube bolts, freedom of movement and mounting brackets for condition, cracks and security.
Note: Refer to Service Bulletins S.B. 6/379 & 6/511 and A.D.’s 79-14-01 & 89-24-06 if applicable.
WARNING: Inspect within 25 flight hours if parked aircraft subjected to ground winds with a mean velocity of 35 MPH or greater. Mean wind speeds of 35 MPH will generate wind gusts up to 65 MPH.
	
	
	

	
9.12	Stall warning light for condition and security.
	
	
	

	9.13	Stall warning horn for condition and security.

Effectivity: Pre Mod 6/2028
	
	
	

	C 0500.10	28 – FUEL

	
10.1	L/H Wing fuel emergency shutoff valve for leakage and security.
	
	
	

	10.2	R/R Wing fuel emergency shutoff valve for leakage and security.
	
	
	

	10.3	Remove and inspect motive line check valve strainer for contamination. Clean as required and install serviceable unit. Leak check.
Note: Drain fuel before removing strainers.
	
	
	

	10.4	 Removed. No wing fuel tanks.
	
	
	

	10.5	 Removed. No wing fuel tanks.
	
	
	

	C 0500.11	29 – HYDRAULIC POWER

	
11.1	Accumulator air charging valves for condition and security. Clean as required.
	
	
	

	11.2	Hydraulic pump (electric motor driven) for security and leakage.
	
	
	

	11.3	Hydraulic pressure switch security and leakage.
	
	
	

	11.4	Drain holes in hydraulic power package tray clear of obstruction. Clean as required.
	
	
	

	11.5	Emergency hydraulic hand pump for security and leakage.
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11.6	Hydraulic pipes and connections for condition, connections for security.
	
	
	

	11.7	Remove hydraulic filter element and replace with new element. Leak check.
	
	
	

	C 0500.12	30 – ICE AND RAIN PROTECTION

	
12.1	Horizontal stabilizer deicing boots for cuts, tears, deterioration and proper adhesion.
	
	
	

	12.2	L/H Wing deicing boots for cuts, tears, deterioration and proper adhesion.
	
	
	

	12.3	R/H Wing deicing boots for cuts, tears, deterioration and proper adhesion.
	
	
	

	12.4	Horizontal stabilizer deicing system water separator drain holes and lines for obstruction and security. Water separator filter for condition and replace as necessary.
	
	
	

	12.5	L/H Wing deicing system water separator drain holes and lines for obstruction and security. Airframe deicing water separator filter for condition and replace as necessary.
	
	
	

	12.6	R/H Wing deicing system water separator drain holes and lines for obstruction and security. Airframe deicing water separator filter for condition and replace as necessary.
	
	
	

	12.7	Windshield wiper blades for condition and security, drive arms for tension, tie rods for wear, distortion and security.
	
	
	

	12.8	Removed. No windshield washer system installed.
	
	
	

	12.9	Removed. No windshield washer system installed.

	
	
	

	12.10	Removed. No anti ice or deice system on outer engine outlet.
	
	
	

	

	12.11	Removed. No anti ice or deice system on outer engine outlet.
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	C 0500.13	32 – LANDING GEAR

	
13.1	Nose Gear
	

	13.1.1	Thoroughly clean nose gear shock strut and inspect for condition, security and leakage, service as necessary.
	
	
	

	13.1.2	Remove steering actuator external filter, clean and reinstall.
	
	
	

	13.1.3	Lubricate nose gear torque arms.
Effectivity: Mod 6/1377
	
	
	

	13.1.4	Nose leg taxi light for condition and security, electrical connection for security.
	
	
	

	13.2	Wheel brake pedal linkage, springs, levers and linkage for condition, wear and security.
	
	
	

	C 0500.14	33 - LIGHTS

	
14.1	Taxi light for condition and security, electrical connection for security.
	
	
	

	C 0500.15	34 - NAVIGATION

	
15.1	Pitot heads for security and corrosion.
	
	
	

	15.2	Drain the pitot static moister traps at the following locations:
	
	

	15.2.1	Adjacent to pitot masts.
	
	
	

	15.2.2	Below static valve on center pylon
	
	
	

	15.2.3	Autopilot computer static line.
	
	
	

	15.3	Pitot head heat electrical wiring for condition and connections for security.
	
	
	

	15.4	Lower transponder antenna #1 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
Effectivity: Mod SOO 6388, 6381 and Mod 6/2003
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15.5	Lower transponder antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
Effectivity: Mod SOO 6388, 6381 and Mod 6/2003
	
	
	

	15.6	Upper transponder antenna #1 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
Effectivity: Mod SOO 6388, 6381 & 6/2003
	
	
	

	15.7	Upper transponder antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
Effectivity: Mod SOO 6388, 6381 & 6/2003
	
	
	

	15.8	GPS antenna #1 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.

Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.9	GPS antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.

Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.10	DME center fuselage antenna for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.11	DME antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.

Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.12	Radar altimeter antenna #1 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.13	Radar altimeter antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
Effectivity: Mod SOO 6388, 6/2003
	
	
	

	15.14	TCAS upper antenna #1 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.

Effectivity: Mod SOO 6382, 6/2003
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15.15	TCAS upper antenna #2 for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
Effectivity: Mod SOO 6219, 6/2003
	
	
	

	15.16	TCAS lower antenna for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.

Effectivity: Mod SOO 6382, 6/2003
	
	
	

	15.17	ADF antenna #1 covers for condition, moisture ingress, cracks deterioration and security, connectors and insulators for security, masts for cracks and security. Clean as required.
Effectivity: Mod SOO 6209, 6/2003
	
	
	

	15.18	ADF antenna #2 covers for condition, moisture ingress, cracks deterioration and security, connectors and insulators for security, masts for cracks and security. Clean as required.
Effectivity: Mod SOO 6209, 6/2003
	
	
	

	
	
	

	C 0500.16	36 - PNEUMATIC

	
16.1	Cabin exhaust outlet or, if pneumatic package is installed, heat exchange for condition and clear of obstruction.
	
	
	

	16.2	Remove pneumatic system strainer element, clean and install. Leak check.
	
	
	

	16.3	 Removed. Not installed in our Aircraft.
	
	
	

	C 0500.17	44 – CABIN SYSTEMS

	
17.1	 Condition and security of mounting, cabin speakers for condition and security. Effectivity: Mod SOO 6/2049
	
	
	

	C 0500.18	52 – DOORS

	
18.1	Flight compartment door hinges and locks for condition and security, freedom of operation and proper locking. Lubricate and clean as required.
	
	
	

	18.2	Inspect the cabin doors as follows:
	
	
	

	18.2.1	Hinges and lock for condition, security, freedom of operation and proper locking
	
	
	

	18.2.2	Close cabin LH rear cargo door and position both lower and upper latches in the locked condition. Make sure each latch pin makes positive engagement with door frame and holes.
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18.2.3	Make sure the lower latch pin remains positively engaged when the locked latch is lifted to the top of its vertical play.
	
	
	

	18.2.4	Clean as required.
	
	
	

	18.3	Inspect the IKHANA fwd cargo door as follows:
	
	

	18.3.1	Hinge and lock for condition, security, corrosion, freedom of operation and proper locking, Lubricate.
	
	
	

	18.3.2	Inward opening cargo door for condition and security, hinges for condition and freedom of operation. Lubricate.
	
	
	

	18.3.3	Retention strap for condition.
	
	
	

	18.3.4	Clean as required.
	
	
	

	18.3.5	Door guard assembly for condition, check spring engagement against inner handle, ensure the guard assembly is in contact with the handle. Replace damaged springs as required.
Effectivity: Mod 6/2326 & 6/2386
	
	
	

	18.4	Inspect rear baggage compartment door as follows;
	
	

	18.4.1	Hinge for condition, freedom of operation.
	
	
	

	18.4.2	Stay bar for condition of fastener and security in stowed position.
	
	
	

	18.4.3	Door handle and lock for condition and proper operation.
	
	
	

	18.4.4	Lubricate.
	
	
	

	18.5	Inspect nose compartment door as follows
	
	

	18.5.1	Hinges for condition and freedom of operation.
	
	
	

	18.5.2	Stay bar for condition of fastener and security in stowed position.
	
	
	

	18.5.3	Latches for proper operation.
	
	
	

	18.5.4	Lubricate.
	
	
	

	18.6	Removed. Not installed our aircraft.
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	C 0500.19	54 – NACELLE - LH

	
19.1	Inspect lower longeron for condition, buckling, cracking, corrosion and fasteners for security at the following locations;
CAUTION: INSPECTION APPLIES TO ALL AIRCRAFT CONFIGURATIONS AND MUST BE CARRIED OUT PRIOR TO NEXT FLIGHT, IF AIRCRAFT HAS ENCOUNTERED HARD LANDING CONDITION.
	
	
	

	19.1.1	Forward engine mount fittings.
	
	
	

	19.1.2	Forward and at intersection with the wing.
	
	
	

	C 0500.20	54 – NACELLE - RH

	
20.1	Inspect lower longeron for condition, buckling, cracking, corrosion and fasteners for security at the following locations;
CAUTION: INSPECTION APPLIES TO ALL AIRCRAFT CONFIGURATIONS AND MUST BE CARRIED OUT PRIOR TO NEXT FLIGHT, IF AIRCRAFT HAS ENCOUNTERED HARD LANDING CONDITION.
	
	
	

	20.1.1	Forward engine mount fittings.
	
	
	

	20.1.2	Forward and at intersection with the wing.
	
	
	

	C 0500.21	57 – WING – LH

	
21.1	Wing exterior upper surfaces for dents, scores, abrasions and corrosion.
	
	
	

	21.2	Wing leading edge and shroud skins for condition, dents, scores, fasteners for security
Note: Refer to Service Bulletin Nos. 6/517.
	
	
	

	21.3	Electrical wiring and where visible, for condition, connectors for security.
	
	
	

	C 0500.22	57 – WING – RH

	
22.1	Wing exterior upper surfaces for dents, scores, abrasions and corrosion.
	
	
	

	22.2	Wing leading edge and shroud skins for condition, dents, scores, fasteners for security
Note: Refer to Service Bulletin Nos. 6/517.
	
	
	

	22.3	Electrical wiring and where visible, for condition, connectors for security.
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	C 0500.23	61 – PROPELLERS – LH

	
23.1	Autofeather limit switches and slide mechanisms for condition and security, wiring for condition and connectors security. Clean as required.
	
	
	

	23.2	Beta range backup system limit switch and mechanism for condition and security, wiring for condition and connectors for security. Clean as required.
	
	
	

	23.3	Propeller spinner for dents and security, hub for grease or oil leakage and attach bolts for condition and security.
Removed AD note. Not applicable.
	
	
	

	23.4	Removed. Was repeated from 23.1.
	
	
	

	23.5	Removed. Not installed.
	

	23.5.1	Speed setting actuator.
	
	
	

	23.5.2	Rod end trimmer.
	
	
	

	23.5.3	Flexible shaft.
	
	
	

	23.5.4	Electrical wiring for condition and connectors for security.
	
	
	

	C 0500.24	61 – PROPELLERS – RH

	
24.1	Autofeather limit switches and slide mechanisms for condition and security, wiring for condition and connectors security. Clean as required.
	
	
	

	24.2	Beta range backup system limit switch and mechanism for condition and security, wiring for condition and connectors for security. Clean as required.
	
	
	

	24.3	Propeller spinner for dents and security, hub for grease or oil leakage and attach bolts for condition and security.
Removed. Not applicable.
	
	
	

	24.4	Removed. Repeated from 24.1
	
	
	

	24.5	Removed. Not installed.
	

	24.5.1	Speed setting actuator.
	
	
	

	24.5.2	Rod end trimmer.
	
	
	

	24.5.3	Flexible shaft.
	
	
	

	24.5.4	Electrical wiring for condition and connectors for security.
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	C 0500.25	71 – POWERPLANT - LH

	
25.1	Inspect intake deflector system as follows;
	

	25.1.1	Exit door for condition and security.
	
	
	

	25.1.2	Actuators for condition security and leakage.
	
	
	

	25.1.3	Locking and release levers for condition, security and leakage, pipes for condition and leakage.
	
	
	

	25.1.4	Air control valves for condition, security and leakage, pipes for condition and leakage.
	
	
	

	25.1.5	Cables for fraying, kinks and wear, connectors for security, rod ends and bearings for condition and security, linkage for condition. Brackets for condition.
	
	
	

	25.2	Perform a detailed visual inspection of cable terminals as follows;
Note: If corrosion pits and/or cracks are found on any cable terminal, remove the applicable cable assembly and replace with a new cable assembly.
	
	

	25.2.1	Remove and discard the lockwire from cable terminals. If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed, rig the control system.
Note: If safety clip is installed, do not remove the safety clip. If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	25.2.2	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	25.2.3	Cable terminals for signs of cracks in all expose parts of the terminals.
	
	
	

	C 0500.26	71 – POWERPLANT - RH

	
26.1	Inspect intake deflector system as follows;
	

	26.1.1	Exit door for condition and security.
	
	
	

	26.1.2	Actuators for condition security and leakage.
	
	
	

	26.1.3	Locking and release levers for condition, security and leakage, pipes for condition and leakage.
	
	
	

	26.1.4	Air control valves for condition, security and leakage, pipes for condition and leakage.
	
	
	

	26.1.5	Cables for fraying, kinks and wear, connectors for security, rod ends and bearings for condition and security, linkage for condition. Brackets for condition.
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26.2	Perform a detailed visual inspection of cable terminals as follows;
Note: If corrosion pits and/or cracks are found on any cable terminal, remove the applicable cable assembly and replace with a new cable assembly.
	

	26.2.1	Remove and discard the lockwire from cable terminals. If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed, rig the control system.
Note: If safety clip is installed, do not remove the safety clip. If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	26.2.2	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	26.2.3	Cable terminals for signs of cracks in all expose parts of the terminals.
	
	
	

	C 0500.27	73 – ENGINE FUEL AND CONTROL – LH

	
27.1	These can all be removed. These are all on the A0125 inspection which is due at 
               The same time as this inspection.
	
	
	

	27.2	
	
	
	

	27.3	

	
	
	

	27.4	
	
	
	

	C 0500.28	73 – ENGINE FUEL AND CONTROL – RH

	
28.1	These can all be removed. These are all on the A0125 inspection which is due at 
               The same time as this inspection.

	
	
	

	28.2	
	
	
	

	28.3	

	
	
	

	28.4	
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	C 0500.29	76 – ENGINE CONTROLS

	
CAUTION

With engine stopped 1) DO NOT move power lever in either direction if blades latches are engaged. 2) DO NOT select reverse power if power if propeller is at feather.
	

	29.1	Power control mechanisms and linkages, including beta backup for condition, chafing, fouling and security.
	
	
	

	29.2	Inspect overhead console power controls follows;
Removed SB note. Not applicable to our aircraft.
	
	
	

	29.2.1	Mechanism and linkages for condition and freedom of movement.
	
	
	

	29.2.2	Power and propeller levers for smooth operation and propeller/power lever interlock mechanism for operation.
	
	
	

	29.2.3	Fuel shutoff control lever for smooth operation and proper detent action.
	
	
	

	29.2.4	Friction damper for operation, power lever Beta arming switch condition.
	
	
	

	C 0500.30	77 – ENGINE INDICATING - LH

	
30.1	Engine indicating instrument wiring for condition, connectors for security. Clean as required.
	
	
	

	C 0500.31	79 – ENGINE INDICATING - RH

	
31.1	Engine indicating instrument wiring for condition, connectors for security. Clean as required.
	
	
	

	C 0500.32	79 – OIL - LH

	
32.1	Oil temperature bulb for leakage and security, Connection for security.
	
	
	

	C 0500.33	79 – OIL - RH

	
33.1	Oil temperature bulb for leakage and security, Connection for security.
	
	
	

	C 0500.34	80 – STARTING – LH

	
34.1	Starter generator brushes for condition and wear.
	
	
	

	34.2	Drive splines for wear. Lubricate
	
	
	

	34.3	Removed. This check is on the A0125 inspection.
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34.4	Removed. This check is on the A0125 and B0250.
	
	
	

	34.5	Starter generator electrical wiring for condition, insulation for deterioration and connectors for security. Clean as required.
	
	
	

	C 0500.35	80 – STARTING – LH

	
35.1	Starter generator brushes for condition and wear.
	
	
	

	35.2	Drive splines for wear. Lubricate
	
	
	

	35.3	Removed. This check in on the A0125.
	
	
	

	35.4	Removed. This check is on the A0125 and B0250.
	
	
	

	35.5	Starter generator electrical wiring for condition, insulation for deterioration and connectors for security. Clean as required.
	
	
	

	C 0500.36	OPERATIONAL CHECKS

	
36.1	Perform the following Operational Checks;

NOTE
Electrical power for the following tests is obtained by connecting a ground power source or by running the engines, whichever is more convenient
	

	36.1.1	Oil pressure indicator, oil temperature indicator (Pre Mod 6/2012)
	
	
	

	36.1.2	Autopilot system
	
	
	

	36.1.3	Doors unlocked warning lights, including limit switch operation
	
	
	

	36.1.4	Fuel leak check after installation of motive line check valve strainers
	
	
	

	36.1.5	Run engine(s) and check the following;
	

	36.1.5.1	Autofeather system
	
	
	

	36.1.5.2	Beta backup system
	
	
	

	36.1.5.3	Propeller/power interlock
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36.1.5.4	Removed. Not installed.
	
	
	

	36.1.5.5	Removed. Not installed.
	
	
	

	36.1.6	Emergency cabin lights (Mod SOO 6098, 6179 and 6208).
	
	
	

	36.1.7	Windshield wipers

CAUTION: DO NOT OPERATE WIPERS ON DRY WINDSHIELD SURFACE
	
	
	

	36.1.8	The following items, as applicable, for leaks after installation.
	

	36.1.8.1	Hydraulic filter unit Leak check 
	
	
	

	36.1.8.2	Removed. Not installed.
	
	
	

	36.1.8.3	Pneumatic package strainer
	
	
	

	36.1.8.4	Steering actuator filter Leak Check.
	
	
	

	36.1.8.5	Removed. On A0125 check.
	
	
	

	36.1.9	Heated windscreen
	
	
	

	36.1.10	Aileron trim tab position indicator (Pre Mod 6/2047).
	
	
	

	36.1.11	Position indication (Mod 6/2047), do a display indication function test, neutral and full range of travel.
	
	
	

	36.1.12	Alignment of mechanical rudder trim pointer and EFIS rudder trim display (Mod 6/2047).
	
	
	

	36.1.13	Alignment of mechanical pitch trim pointer and EFIS pitch trim display (Mod 6/2047).
	
	
	

	36.1.14	AFCS (Autopilot) (Mod SOO 6221) - KS 272A Pitch trim servo system.
	
	
	



MARITIME HELICOPTERS	DCH-6 MAINTENANCE MANUAL




CHECK: FREQUENCY: NOTE::




C 0500 – BASIC INSPECTION Every 500 Hours

Page No: Revision: Issue Date:

7-43 Original 05/01/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	C 0500.37	POST INSPECTION

	
37.1	Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	37.2	Clean aircraft and engine once maintenance is completed.
	
	
	

	37.3	Perform Functional Check Flight if required per DHC-6-400 Maintenance Manual or AFM as appropriate.
	
	
	

	37.4	Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

[bookmark: _Hlk64725406]Completed C0500 inspection IAW M.H.I DHC-6 CAMP.



Registration No.: N	End Aircraft S/N:                                     Date:

Aircraft Ending Total Time: Aircraft Ending Total Cycles:


Signature:	Certificate Type & No:
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Registration No.: N                                Start Aircraft S/N:                                      Date:

Aircraft Start Total Time: Aircraft Start Total Cycles:


Reference: DHC-6 Maintenance Program

	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	C 1000.1	GENERAL

	
1.1	Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	1.2	Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3	Replace all life limited components that have completed published operating limits.
	DHC-6-400 MP
	
	

	1.4	Overhaul all components that have completed published operating limits.
	DHC-6-400 MP
	
	

	C 1000.2	PLACARDS AND MARKINGS

	
2.1	Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	C 1000.3	CORROSION CONTROL

	
3.1	Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	
Appendix C
	
	

	C 1000.4	PREPARATION

	
4.1	Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	C 1000.5	21 – AIR CONDITIONING

	
5.1	Forward avionics compartment air filter for condition, security and free of obstruction. Clean as required.
Effectivity: Mod C10-06/2014
	
	
	

	5.2	DAU cooling fan for condition and security, bonding wires for condition, security and security of attachment.
Effectivity: Mod 6/2049
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	C 1000.6	22 – AUTO FLIGHT

	
6.1	REMOVE. NOT INSTALLED ON OUR SERIES.
Radio magnetic indicator and annunciator (if fitted) for condition and security, electrical connection for security and hoses, if required, for condition and security. Clean as required.
Note: Refer to Service Bulletin No. 6/349 and A.D. 76-07-09 if applicable.
	
	
	

	6.2	SM3000 Aileron servo for grounding of unit wiring bundle shield braid to airframe structure (<7.5 milliohms) .
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6221
	
	
	

	6.3	SM3000 Aileron servo for bonding of the mating surfaces between servo mount and airframe structure (<2.5 milliohms) .
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6221
	
	
	

	6.4	AFCS (Autopilot) SM3000 aileron system servo. Check bridle cable tensions and verify no slippage of clamps has occurred.
	
	
	

	6.5	AFCS (Autopilot) SM3000 elevator system servo. Check bridle cable tensions and verify no slippage of clamps has occurred.
	
	
	

	6.6	AFCS (Autopilot) SM3000 rudder system servo. Check bridle cable tensions and verify no slippage of clamps has occurred.
	
	
	

	6.7	SM3000 rudder servo for grounding of unit wiring bundle shield braid to airframe structure (<7.5 milliohms) .
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6221
	
	
	

	6.8	SM3000 Aileron servo for bonding of the mating surfaces between servo mount and airframe structure (<2.5 milliohms) .
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6221
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6.9	KS 272A pitch trim servo for grounding of unit wiring bundle shield braid to airframe structure (<7.5 milliohms) .
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6221
	
	
	

	6.10	KS 272A pitch trim servo for bonding of the mating surfaces between servo mount and airframe structure (<2.5 milliohms) .
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6221
	
	
	

	6.11	KS 272A pitch trim system servo. Check bridle cable tensions and verify no slippage of clamps has occurred.
	
	
	

	C 1000.7	23 – COMMUNICATIONS

	
7.1	VHF upper antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003
	
	
	

	7.2	VHF upper aft antenna for condition and security, control and indicators for condition, wiring and connector for security. Clean as required.
Effectivity: Mod 6/2003
	
	
	

	7.3	VHF forward antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003
	
	
	

	7.4	VHF lower aft antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003 & Mod 6231
	
	
	

	7.5	VHF lower aft antenna for condition and security, control and indicators for condition, wiring and connector for security. Clean as required.

Effectivity: Mod 6/2003, SOO6231
	
	
	

	7.6	VHF-FM antenna for condition and security, control and indicators for condition, wiring and connector for security. Clean as required.
Effectivity: Mod SOO 6296
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7.7	VHF-FM antenna for bonding of the mating surfaces between antenna and airframe (<3 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6296
	
	
	

	7.8	Pilots audio panel (KMA 29), for condition and security, bonding wires for condition and security.

Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.9	Pilots audio panel (KMA 29), inspect bonding of the mating surfaces between the mounting tray and the airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6209, Mod 6/2049
	
	
	

	7.10	Co-Pilots audio panel (KMA 29), for condition and security, bonding wires for condition and security.
Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.11	Co-Pilots audio panel (KMA 29), inspect bonding of the mating surfaces between the mounting tray and the airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6209, Mod 6/2049
	
	
	

	7.12	Pilot audio panel (KMA 29), emergency switch operational test.
Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	

	7.13	Co-Pilot audio panel (KMA 29), emergency switch operational test.
Effectivity: SOO 6209 & Mod 6/2049
	
	
	

	7.14	Audio system (NAT 247) isolation amplifier for bonding of the mating surfaces between antenna and airframe (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	

	
	
	
	

	7.15	Audio system (NAT 247) isolation amplifier for condition and security, bonding wires for condition and security.
Effectivity: Mod 6/2049
	
	
	

	

	7.16	MMDR #1 for bonding of the mating surfaces between antenna and airframe (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	
	



MARITIME HELICOPTERS	DCH-6 MAINTENANCE MANUAL




CHECK: FREQUENCY: NOTE::




C 1000RT – BASIC INSPECTION Every 1000 Hours
This inspection is restricted to 50 hours

Page No: Revision: Issue Date:

7-49 Original 5/01/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
7.17	MMDR #2 for condition and security, bonding wires for condition and security.

Effectivity: Mod SOO 6209, Mod 6/2049
	
	
	

	
	

	7.18	MMDR #2 for bonding of the mating surfaces between antenna and airframe (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6209, Mod 6/2049
	
	
	

	7.19	MMDR #1 for condition and security, bonding wires for condition and security.

Effectivity: Mod 6/2049
	
	
	

	7.20	Emergency frequency com tuning switch operational test.
	
	
	

	7.21	GPS/IRIDIUM/WiFi Antenna for condition, security and corrosion, condition of external fillet seal, condition of coaxial cables and connectors and security of attachment of coaxial cables.
	
	
	

	7.22	GPS/IRIDIUM/WiFi Antenna for bonding of the mating surfaces between antenna baseplate and airframe (<3 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: SOO 6288 or 6298
	
	
	

	7.23	SkyNode SAT COM Panel/Dialer (RC6000/A), for condition, security and corrosion; electrical wires and connectors for condition and security of attachment.

Effectivity: SOO 6298
	
	
	

	C 1000.8	24 – ELECTRICAL POWER

	
8.1	External power receptacle for condition and security. Clean as required.
	
	
	

	8.2	Grounding and bonding wires for condition and security. Clean as required.
	
	
	

	8.3	Voltage regulators for condition and security. Clean as required.
	
	
	

	C 1000.9	25 - EQUIPMENT/FURNISHINGS

	
9.1	ELT for bonding of the mating surfaces between the backshell and airframe (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
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9.2	ELT Antenna bonding of the mating surfaces between the antenna and airframe (<3 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	
	

	9.3	Flight compartment axe and axe storage;
	

	9.3.1	Axe handle retention strap and elastic webbing for damage or deterioration (loss of elastic properties). Replace on condition.
	
	
	

	9.3.2	Condition and security of axe stowage structure. Condition and security of axe cutting edge and pike to axe handle.
	
	
	

	C 1000.10	27 – FLIGHT CONTROLS

	10.1	Inspect control column (Mod 6/1433) as follows;
	

	10.1.1	Condition, security and full and free movement.
	
	
	

	
	

	10.1.2	Brackets for condition and security, centering strut for condition, proper operation and security.
	
	
	

	10.1.3	Remove covers.
	
	
	

	10.1.4	Check for evidence of binding, chain alignment with control wheel sprockets, sprockets for condition, security and teeth wear, turnbuckles for safety.
	
	

	
	
	
	

	10.1.5	Control column floor boot for condition and security.
	
	
	

	10.1.6	Lubricate.
	
	
	

	10.1.7	Reinstall covers (OK to close).
	
	
	

	10.2	Rudder torque tube and quadrats for condition and security, linkage and push rod installation for security.
	
	
	

	10.3	Gust lock control for condition and proper operation, brackets and connecting rods for cracks, buckling and security.
Note: Refer to Service Bulletin N. 6/508, if applicable.
	
	
	

	10.4	Rudder pedal support assembly, push rods, levers and linkage for condition and security; pedals for full and free movement; condition and security; pedals for cracking as shown in PSM 1-6-7, Part 1 Figure 2. Replace if cracked.
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10.5	Inspect rudder, elevator and aileron primary control cables as follows;

Note 1: Refer to Service Bulletin N. 6/523, if applicable.
Note 2: Ensure adequate clearance with adjacent electrical conduits, structure and other systems, making allowance for vibratory motion of cable under tension.
Note 3: In the event of early or abnormal cable wear at pulley(s), replace the worn cable(s) and the corresponding pulley(s).
	

	10.5.1	Cables (from beneath flight compartment) floor to wings and empennage) for fraying corrosion, flattening, proper attachment and security.
	
	
	

	10.5.2	Pulleys for condition and freedom of movement, pulley brackets and guides for condition and security, turnbuckles for security.
	
	
	

	10.5.3	Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	10.6	Inspect rudder flight control cables as follows
	

	
	

	10.6.1            Control and tab cables, flap/elevator interconnect and elevator trim cables for fraying kinks, flattening, corrosion and security of attachments.
	
	
	

	10.6.2	Cable ends with nylon sheathing, (where applicable) for condition.
	
	
	

	10.6.3	Turnbuckles for security. Replace cable where evidence of damage is found.
	
	
	

	10.6.4	Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	10.7	Inspect aileron L/H wing flight control cables as follows
	

	10.7.1	Fraying, flattening, corrosion, proper attachment and security.
	
	
	

	10.7.2	Pulleys for condition and freedom of movement, pulley brackets and guides for condition and security, turnbuckles for security.
	
	
	

	10.7.3	Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	10.8	Inspect aileron R/H wing flight control cables as follows
	

	
	

	10.8.1	Fraying, flattening, corrosion, proper attachment and security.
	
	
	

	10.8.2	Pulleys for condition and freedom of movement, pulley brackets and guides for condition and security, turnbuckles for security.
	
	
	



MARITIME HELICOPTERS	DCH-6 MAINTENANCE MANUAL




CHECK: FREQUENCY: NOTE::




C 1000RT – BASIC INSPECTION Every 1000 Hours
This inspection is restricted to 50 hours

Page No: Revision: Issue Date:

7-52 Original 5/01/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	
	
	

	
10.8.3	Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	10.9	Inspect rudder and elevator trim tab controls as follows;
	

	
	

	10.9.1	Full and freedom of movement, cables for fraying, kinks, flattening, proper attachment and security.
	
	
	

	10.9.2	Pulleys for freedom of operation and pulley brackets for condition and security.
	
	
	

	10.10	Do a detailed visual inspection of cable terminals as follows;
	
	

	10.10.1	 Remove and discard the lockwire from the cable terminals. Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	10.10.2	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	10.10.3	Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	10.10.4	If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	10.10.5	If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.1.15.1, rig the control system.
	
	
	

	10.10.6	If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	10.11	Inspect rudder gear tab mechanism as follows;
	

	10.11.1	Gearbox for condition and security of mounting plate installation and cover, tab pushrod for security and evidence of irregular operation during rudder movement.
	
	
	

	10.11.2	Gearbox to rudder linkage for condition and security, pushrod for security of attachments.
	
	
	

	10.12	Inspect L/H aileron trim tab actuator as follows;
	

	10.12.1	Smooth operation and security.
	
	
	

	10.12.2	Electrical wiring and connections for security.
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10.12.3	Linkages for damage, safety and security.
	
	
	

	10.12.4	Position transmitter for cleanliness, loose connections and security of mounting.
	
	
	

	10.13	Inspect R/H aileron trim tab actuator as follows;
	

	10.13.1	Smooth operation and security.
	
	
	

	10.13.2	Electrical wiring and connections for security.
	
	
	

	10.13.3	Linkages for damage, safety and security.
	
	
	

	10.13.4	Position transmitter for cleanliness, loose connections and security of mounting.
	
	
	

	10.14	Aileron trim tab position indicator for condition and security, wiring and connectors for condition and security.
Effectivity: Mod 6/2047
	
	
	

	10.15	Rubber, elevator and aileron position voltage check.

Effectivity: Mod 6/2047
	
	
	

	10.16	Position transmitter, inspect for security of mounting and brackets, wiring and connections for security. Clean as required.
Effectivity: Mod 6/2047
	
	
	

	10.17	Flap position cable for fraying, flattening, corrosion and security of attachment, spring for condition, tension and security.
	
	
	

	10.18	 Flap position indicator for smooth operation. Effectivity: Mod 6/2048
	
	
	

	10.19	Flap position dracon cable cord at window frame small pulley locations for condition.
	
	
	

	10.20	Flap/elevator interconnect, elevator trim cables and flap indicator cables for condition, fraying, corrosion, flattening and security of attachment, turnbuckles for security, pulleys for condition, security and freedom of operation.
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10.21	Do a detailed visual inspection as follows;
	
	

	
	
	

	10.21.1	Fuselage aileron, elevator and rudder flight control cables.
	
	
	

	10.21.2	Flap to elevator interconnect tab cables
	
	
	

	10.21.3	Flap selector valve and follow up cables.
	
	
	

	10.22	Do a detailed visual inspection of cable terminals as follows;
	
	

	10.22.1	Remove and discard the lockwire from the cable terminals.

Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	10.22.2	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	10.22.3	Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	10.22.4	If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	10.22.5          If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.18.1, rig the control system.
	
	
	

	10.22.6	If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	10.23	Inspect rudder flight control cables as follows;

Note 1: Refer to Service Bulletin N. 6/523, if applicable.
Note 2: Ensure adequate clearance with adjacent electrical conduits, structure and other systems, making allowance for vibratory motion of cable under tension.
Note 3: In the event of early or abnormal cable wear at pulley(s), replace the worn cable(s) and the corresponding pulley(s).
	

	
	

	10.23.1	Cables and tab cables, flap/interconnect and elevator trim cables for fraying corrosion, kinks, flattening, proper attachment and security.
	
	
	

	10.23.2	Cable ends with nylon sheathing, (where applicable), for condition.
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10.23.3	Turnbuckles for security. Replace cable where evidence of damage is found.
	
	
	

	10.23.4	Perform a detailed visual inspection of cable terminals for signs of corrosion pits or cracks.
	
	
	

	10.24	Overhead console flight control and flap selector (Mod 6/1895) aluminum quadrants for condition and security, freedom of movement, cable attachment for security, pulley for smooth and freedom of operation.
	
	
	

	10.25      Aileron flight control cable quadrants in cabin roof for condition and security, bearings for condition, cable guides for security. Clean as required.
	
	
	

	10.26	Elevator control quadrants for cleanliness, damage, corrosion and security; bearings for corrosion, cleanliness and security; stops for damage.
	
	
	

	10.27	Elevator control lever and connecting rod for full and free movement, attaching brackets for cracks and distortion.
	
	
	

	10.28	L/H wing root rib/flap pushrod support rollers for condition, wear and security, proper clearance between rod surface and roller and freedom of operation. Lubricate inside of spacer and bolt.
Effectivity: Post Mod 6/1707
	
	
	

	10.29	R/H wing root rib/flap pushrod support rollers for condition, wear and security, proper clearance between rod surface and roller and freedom of operation. Lubricate inside of spacer and bolt.

Effectivity: Post Mod 6/1707
	
	
	

	10.30	Stall warning cam limit microswitch mechanism and propeller reset limit switch for condition and security, connector for security.

Effectivity: Post Mod 6/1701
	
	
	

	10.31	Rudder position transmitter, inspect for security of mounting and brackets, wiring and connections for security. Clean as required.

Effectivity: Mod 6/2047
	
	
	

	10.32	Elevator position transmitter, inspect for security of mounting and brackets, wiring and connections for security. Clean as required.

Effectivity: Mod 6/2047
	
	
	

	10.33	Inspect CVR; Remove, inspections can be found on 14.25, and 14.26.

Effectivity: Mod 6/2049
	

	10.33.1	Removed due to repeated on 14.25
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10.33.2	Removed due to inspection repeated on 14.26

	
	
	

	10.34	Inspect FDR; Remove this inspection. Can be found repeated on 14.27 and 14.28.

Effectivity: Mod 6/2049
	

	10.34.1	Removed. Inspection was repeated on 14.27.
	
	
	

	10.34.2	Removed. Inspection was repeated on 14.28.

	
	
	

	C 1000.11	28 – FUEL

	
11.1	Fuel system pipes for condition, connections and hoses for security and leakage, sump plates for corrosion and leakage. Clean as required
Note: Refer to Service Bulletin No. 6/269 and A.D. 71-16-01, if applicable.
	
	
	

	11.2	 Do a detailed visual inspection of the fuel manifold as follows; Effectivity: Mod 6/2389
	
	

	11.2.1	Bonding clamp sealant and terminal lug sealant for condition and integrity, peeling, cracking or evidence of corrosion.
	
	
	

	11.2.2	Inspect bonding jumpers for condition, security, integrity and corrosion.
	
	
	

	11.2.3	If damaged, replace component, re-apply sealant.
	
	
	

	11.3	Do a detailed visual inspection of the booster pumps as follows;
	
	

	11.3.1	Condition, security, corrosion and cleanliness.
	
	
	

	11.3.2	Wiring for condition, corrosion, signs of overheat or arcing.
	
	
	

	11.3.3	 Radio noise filters for security, condition and corrosion. Effectivity: Pre Mod 6/2267
	
	
	

	11.3.4	Electrical terminals for condition and deterioration of sealant.
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11.3.5	Electronic EMI noise filters for condition, security, sign of overheat. Resistance check and condition of electrical termination.
Effectivity: Pre Mod 6/2267
	
	
	

	11.3.6	Bleed resistors for condition, security, sign of overheat. Resistance check and condition of electrical termination.
Effectivity: Pre Mod 6/2267
	
	
	

	11.4	Fuel ejectors for condition and security.
	
	
	

	11.5	Crossfeed valve for corrosion, security and evidence of leakage.
	
	
	

	11.6	Fuel system pipes for condition, connections and hoses for security and leakage, sump plates for corrosion and leakage. Clean as required.
Note: Refer to Service Bulletin No. 6/269 and A.D. 71-16-01, if applicable.
	
	
	

	11.7	Fuel low pressure switches for condition, leakage and security, electrical connector for security.
	
	
	

	11.8	Coaxial electrical wiring in fuel gallery for condition, connectors for condition and security. Clean as required.
For Mod 6/2390, do a detailed visual inspection of the environmental wrap for condition, integrity (split, tear or removal etc.). If deterioration is evident, remove the environmental wrap and inspect underlying components for general condition, corrosion,	wiring,	terminations,	shield	terminations.	Replace	damaged components and install new environmental wrap (refer to PSM1-64-2, Chapter 20-50-03).

For Mod 6/2395, do a detailed visual inspection of the backshell and backshell sealant for deterioration in the seal cavities. If deterioration is evident, clean and reseal backshell. Replace if deterioration is severe.
	
	
	

	11.9	Grounding and bounding leads for fraying, broken wires, loose connections, cleanliness.
For Mod 6/2390, do a detailed visual inspection of the environmental wrap for condition, integrity (split, tear or removal etc.). If deterioration is evident, remove the environmental wrap and inspect underlying components for general condition, corrosion,	wiring,	terminations,	shield	terminations.	Replace	damaged components and install new environmental wrap (refer to PSM1-64-2, Chapter 20-50-03).

For Mod 6/2395, do a detailed visual inspection of the backshell and backshell sealant for deterioration in the seal cavities. If deterioration is evident, clean and reseal backshell. Replace if deterioration is severe.
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11.10	Removed. Wing Fuel Tanks not installed.
	
	

	Effectivity: SOO 6095 and 6247
	
	

	11.10.1	NOT INSTALLED ON AIRCRAFT. 
	
	
	

	11.10.2	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.10.3	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.10.4	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.10.5	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.10.6	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.10.7	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.10.8	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.11	NOT INSTALLED ON AIRCRAFT.
	
	

	Effectivity: SOO 6095 and 6247
	
	

	11.11.1	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.11.2	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.11.3	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.11.4	NOT INSTALLED ON AIRCRAFT.
Effectivity: Pre Mod 6/2046
	
	
	

	11.11.5	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.11.6	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.11.7	NOT INSTALLED ON AIRCRAFT.
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11.11.8	NOT INSTALLED ON AIRCRAFT.
	
	
	

	11.11.9	NOT INSTALLED ON AIRCRAFT.
	
	
	

	C 1000.12	29 – HYDRAULIC POWER

	
12.1	Hydraulic accumulators for leakage and security.
	
	
	

	12.2	Hydraulic brake system pressure relief valve for leakage and security.
	
	
	

	12.3	Hydraulic system pressure relief valve for leakage and security.
	
	
	

	12.4	Flap system thermal relief valves for leakage and security.
	
	
	

	12.5	Main leg hydraulic lines for condition, leakage, loose clamps and connections for security.
	
	
	

	12.6	Main leg flexible hoses for condition, leakage and connections for security.
	
	
	

	C 1000.13	30 – ICE AND RAIN PROTECTION

	
13.1	Heated windshield elements and wiring for condition and security.
	
	
	

	13.2	Airframe deicing timer and connectors for condition and security.
	
	
	

	13.3	Do a detailed visual inspection of the horizontal stabilizer deicing system as follows;
	

	13.3.1	Ejector for condition and security, clear of obstruction. Clean as required.
	
	
	

	13.3.2	Distributor valve for condition, security and leakage.
	
	
	

	13.3.3	Distributor valve heating jacket for security, electrical connections for corrosion and security.
	
	
	

	13.3.4	Horizontal stabilizer pressure system indicating switches for security, electrical connections for security.
	
	
	

	13.3.5	Pipe for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
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13.4	Do a detailed visual inspection of the L/H wing deicing system as follows;
	

	13.4.1	Distributor valves for leaks and security.
	
	
	

	13.4.2	Distributor valves heater jackets for security, electrical connections for corrosion and security.
	
	
	

	13.4.3	Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	
	
	

	13.5	Do a detailed visual inspection of the R/H wing deicing system as follows;
	

	13.5.1	Distributor valves for leaks and security.
	
	
	

	13.5.2	Distributor valves heater jackets for security, electrical connections for corrosion and security.
	
	
	

	13.5.3	Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	
	
	

	13.6	Do a detailed visual inspection of the horizontal stabilizer deicing system as follows;
	

	
	

	13.6.1	Ejector for condition and security, clear of obstructions. Clean s required.
	
	
	

	13.6.2	Distributor valves for leaks and security.
	
	
	

	13.6.3	Distributor valves heater jackets for security, electrical connections for corrosion and security.
	
	
	

	13.6.4	Pressure system indicating switches for security, electrical connections for security.
	
	
	

	13.6.5	Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	
	
	

	13.6.6	Caution light panel and cockpit dome light for condition and security.
	
	
	

	13.6.7	Deicing boot pressure warning lights for condition and security.

Effectivity: Pre Mod 6/2028
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13.7	Do a detailed visual inspection of the airframe deicing system as follows;
	

	13.7.1	Timer and connectors for condition and security
	
	
	

	13.7.2	Distributor valves for leaks and security.
	
	
	

	13.7.3	Distributor valves heater jackets for security, electrical connections for corrosion and security.
	
	
	

	13.7.4	Pipes for condition, chafing, loose clamps and connections, flexible hoses for deterioration, chafing and security.
	
	
	

	13.7.5	Pressure system indicating switches for security, electrical connections for security.
	
	
	

	13.7.6	Ejector for condition and security, clear of obstructions. Clean s required.
	
	
	

	13.7.7	Deicing pressure and suction indicator for condition, leakage and security.
	
	
	

	C 1000.14	31 – INSTRUMENTS

	
14.1	Primary flight display unit KDU 1080 or KDU 1080-2 for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2049
	
	
	

	14.2	Primary flight display unit KDU 1080 or KDU 1080-2, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	
	

	14.3	Primary flight display controller KMC2210 for condition and security, bonding wires for condition and security of attachment.

Effectivity: Mod 6/2049
	
	
	

	14.4	Primary flight controller KMC2210, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	
	

	14.5	Multi-function display unit KDU 1080 or KDU 1080-2 for condition and security, bonding wires for condition and security of attachment
Effectivity: Mod 6/2049
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14.6	Multi-function display controller KMC2220, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	
	

	14.7	Multi-function display controller KMC2220 for condition and security, bonding wires for condition and security of attachment
Effectivity: Mod 6/2049
	
	
	

	14.8	Flight controller KMC9200 for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2049
	
	
	

	14.9	Flight controller KMC9200, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	
	

	14.10	Reversion control panel for displays, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	
	

	14.11	Reversion control panel for displays for condition and security, bonding wires for condition and security of attachment.
	
	
	

	14.12	ESIS display for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2049, Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.13	ESIS display, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.14	ESIS battery for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2049, Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
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14.15	ESIS battery, inspect grounding of unit wiring bundle shield braid to airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.16	ESIS magnetometer for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2049 & Mod SOO 6209
	
	
	

	14.17	ESIS magnetometer, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.18	ESIS magnetometer, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.19	MAU for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2049
	
	
	

	14.20	MAU, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	
	

	14.21	MAU, verify ferrite beads are installed on the LAN wires inside the backshells of all the NIC’s (bead P/N is a Ferronics 21-727-B).
Effectivity: Mod 6/2049
	
	
	

	14.22	MAU, visually inspect the mesh covering the air intake for dust and debris. Clean as required.
Effectivity: Mod 6/2049
	
	
	

	14.23	MAU power supplies, inspect bonding of mating surfaces between mounting feet and airframe structure (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.24	MAU power supplies for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2049
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14.25	CVR for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2049 & Mod SOO 6384
	
	
	

	14.26	CVR, inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Pre Mod 6/2170, Post Mod 6/2170, Mod SOO 6209
	
	
	

	14.27	FDR for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod SOO 6385 Mod 6/2049 & Mod SOO 6385
	
	
	

	14.28	FDR, inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6385 Mod 6/2049 & Mod SOO 6385
	
	
	

	14.29	DAU #1 & #2 for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2049
	
	
	

	14.30	DAU #1 & #2, inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	
	

	14.31	Master warning and caution indication and control inspect for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2028
	
	
	

	14.32	ECTM/FOQA (IONode 100) (SOO 6288) for condition, security and corrosion; electrical wires and connectors for security of attachment.
	
	
	

	14.33	Inspect FDR (Mod SOO 6385) (Mod 6/2049) (Post Mod 6/2332) for;
	

	
	

	14.33.1	Condition and security; bonding wires for condition and security of attachment.
	
	
	

	14.33.2	Bonding of the mating surfaces between the unit and airframe (< 2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
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	C 1000.15	32 – LANDING GEAR

	
15.1	Inspect the nosewheel steering cables forward of Sta. 60 and beneath cockpit floor as follows;
Effectivity: Mod 6/1800
	
	

	15.1.1	Condition, kinks, flattening, proper attachment and security.
	
	
	

	15.1.2	Pulleys for condition, freedom of operation and security.
	
	
	

	15.1.3	Turnbuckles for security.
	
	
	

	15.1.4	Do a detailed visual inspection of nosewheel cable terminals as follows;
	

	15.1.5	Remove and discard the lockwire from the cable terminals.

Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	15.1.6	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	15.1.7	Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	15.1.8	If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	15.1.9	If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.1.15.1, rig the control system.
	
	
	

	15.1.10	If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	15.2	Inspect the nosewheel steering lever as follows;

Effectivity: Mod 6/1800
	
	

	15.2.1	Remove control column cover.
	
	
	

	15.2.2	Cables for condition, kinks, flattening, proper attachment and security.
	
	
	

	15.2.3	Pulleys for condition, freedom of operation and security.
	
	
	

	15.2.4	Turnbuckles for security.
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15.2.5	Do a detailed visual inspection of nosewheel cable terminals as follows;
	

	
	

	15.2.6	Remove and discard the lockwire from the cable terminals.

Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	15.2.7	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	15.2.8	Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	15.2.9	If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	15.2.10	If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 10.1.15.1, rig the control system.
	
	
	

	15.2.11	If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	15.2.12	Steering cables for tension.
	
	
	

	15.2.13	Install control column cover (OK to close).
	
	
	

	15.3	Remove nose wheel.

Note: Refer also to Special Inspection Card SP1 if applicable.
	
	
	

	15.3.1	Remove tire from wheel and examine for visible cracks or chipping on rims.
	
	
	

	15.3.2	Lubricate bearings as required.
	
	
	

	15.3.3	Install serviceable tire on wheel.
	
	
	

	15.3.4	Install serviceable nose wheel.
	
	
	

	15.4	Remove L/H main wheel.

Note: Refer also to Special Inspection Card SP1 if applicable.
	
	
	

	15.4.1	Remove tire from wheel and examine for visible cracks or chipping on rims.
	
	
	

	15.4.2	Lubricate bearings as required.
	
	
	

	15.4.3	Install serviceable tire on wheel.
	
	
	

	15.4.4	Install serviceable L/H main wheel.
	
	
	

	15.5	Remove R/H main wheel.

Note: Refer also to Special Inspection Card SP if applicable.
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15.5.1	Remove tire from wheel and examine for visible cracks or chipping on rims.
	
	
	

	15.5.2	Lubricate bearings as required.
	
	
	

	15.5.3	Install serviceable tire on wheel.
	
	
	

	15.5.4	Install serviceable R/H main wheel.
	
	
	

	15.6	Do a detailed visual inspection of L/H brake system as follows;
	
	

	15.6.1	Remove console cover.
	
	
	

	15.6.2	Parking brake rods and linkage for signs of wear and security.
	
	
	

	15.6.3	Lubricate cams.
	
	
	

	15.6.4	Wheel brake valve for leakage and security.
	
	
	

	15.6.5	Clean as required.
	
	
	

	15.6.6	Reinstall console cover (OK to close).
	
	
	

	15.7	Do a detailed visual inspection of R/H brake system as follows;
	
	

	15.7.1	Remove console cover.
	
	
	

	15.7.2	Parking brake rods and linkage for signs of wear and security.
	
	
	

	15.7.3	Lubricate cams.
	
	
	

	15.7.4	Wheel brake valve for leakage and security.
	
	
	

	15.7.5	Clean as required.
	
	
	

	15.7.6	Reinstall console cover (OK to close).
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15.8	Do a detailed visual inspection of main gear fairings as follows;
	
	

	15.8.1	Remove center fairings.
	
	
	

	15.8.2	Cracks, delamination and security.
	
	
	

	15.8.3	Seals for tears, deterioration and security.
	
	
	

	15.8.4	Fairing supporting structure for cracks, corrosion, buckling and loose anchor nuts.
	
	
	

	15.8.5	Roller blind assembly for adequate spring tension, blind for fraying, tears and security.
	
	
	

	15.8.6	Roller for free running and security.
	
	
	

	15.8.7	Welds for cracks at tubes, lugs, pivot fittings and brake flange ale housing.
Note: Refer to PSM1-6-7 Part 3, Figure 8 for leg weld locations.
	
	
	

	15.8.8	Reinstall center fairings.
	
	
	

	15.9	Inspect shock absorber blocks for condition, free from oil, grease, deterioration, splitting on surface adjacent to bolt holes and displacement of blocks. Discard blocks that have sustained permanent set due to displacement beyond edge of scuff plate. Clean as required.

Note: Displacement within boundaries of scuff plate edge is allowable and not detrimental to aircraft safety. Inspect for bubbles close to vertical surface of block by smearing surface with water and using a strong light viewed from opposite side of block. For bubble criteria, refer to Maintenance Manual.
	
	
	

	15.10	Main landing gear upper and lower fuselage attachment fittings for condition and security.
	
	
	

	C 1000.16	33 – LIGHTS

	
16.1	Caution light panel and cockpit dome light for condition and security.
	
	
	

	16.2	Horizontal stabilizer deicing boot pressure warning lights for condition and security.

Effectivity: Pre Mod 6/2028
	
	
	

	16.3	Co-pilot dimming control rheostat for condition and clear from cable routing

Effectivity: Pre Mod 6/2028
Note: Refer to Service Bulletin No. 6/401, if applicable.
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16.4	Do a visual inspection of the following lights for condition and security, bonding wires for condition and security of attachment;
Effectivity: Mod 6/2028
	

	16.4.1	Instrument panel, panel overlay and compass
	
	
	

	16.4.2	Flight compartment flood lights, aisle, eye reference, avionics CB post, instrument panel and visor lights.
	
	
	

	16.4.3	Flight compartment instrument panel, trim panel static valve post and selector lights.
	
	
	

	16.4.4	Flight compartment dome
	
	
	

	16.4.5	Map lights
	
	
	

	16.4.6	Caution dimming lights
	
	
	

	16.5	Do a visual inspection of the following exterior lights for condition and security, bonding wires for condition and security of attachment;
Effectivity: Mod 6/2028
	

	16.5.1	Position and strobe
	
	
	

	16.5.2	Aircraft exterior position and strobe
	
	
	

	16.5.3	Aircraft exterior beacons
	
	
	

	16.5.4	Aircraft exterior landing

Effectivity: Mod 6/2028, 6/2285, 6/2407
	
	
	

	16.5.5	Aircraft exterior wing inspection lights
	
	
	

	16.5.6	Position, anti-collision and strobe for condition and security.

Effectivity: Pre Mod 6/1513 AND 6/2028
Note: Refer to Service Bulletin No. 6/57 and A.D 67-33-01 (Pre Mod 6/116), if applicable (Pre Mod 6/2028)
	
	
	

	16.6	Passenger Warning and passenger lights for condition and security.
Effectivity: Pre Mod 6/2028
	
	
	

	16.7	 Cabin interior boarding lights Effectivity: Mod 6/2028
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16.8	 Cabin interior lighting Effectivity: Mod 6/2028, 6/2427
	
	
	

	C 1000.17	34 - NAVIGATION

	
17.1	#1 VOR antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003
	
	
	

	17.2	#2 VOR antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003
	
	
	

	17.3	#1 Glide Slope antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003
	
	
	

	17.4	#2 Glide Slope antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003
	
	
	

	17.5	Marker beacon antenna for condition, loose connections, entry of moisture and security.
	
	
	

	17.6	Marker beacon antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003
	
	
	

	17.7	Weather radar transmitter and receiver (RDR2000) inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2049
	
	
	

	17.8	Nav systems grounding and bonding wires for condition and security. Clean as required.
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17.9	Transponders; KXP 2290 or 2290A;
	

	
	

	
	

	17.9.1	Condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.9.2	Perform a power on operational test (Power On).
	
	
	

	17.9.3	Inspect bonding of mating surfaces between mounting tray and the nearest airframe ground. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.9.4	Inspect grounding of unit wiring bundle shield brain to airframe structure. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.9.5	#1 lower antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.9.6	#2 lower antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.9.7	#1 upper antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.9.8	#2 upper antenna inspect bonding of mating surfaces between unit and airframe. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003, Mod SOO 6388 & 6381
	
	
	

	17.10	#1 GPS (KGS 200)
	

	
	

	Effectivity: Mod 6/2049, Post Mod 6/2304 & Mod SOO 6388
	

	17.10.1	Inspect for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.10.2	Perform a power on operational test (Power On).
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17.10.3	Inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.10.4	Inspect antenna bonding of mating surfaces between mounting tray and the nearest airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.10.5	Antenna for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
Effectivity: Mod SOO 6388 and Mod 6/2003
	
	
	

	17.11	#2 GPS (KGS 200)
Effectivity: Mod 6/2049, Post Mod 6/2304 & Mod SOO 6388
	

	17.11.1	Inspect for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.11.2	Perform a power on operational test.
	
	
	

	17.11.3	Inspect antenna bonding of mating surfaces between mounting tray and the nearest airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.11.4	Inspect bonding of mating surfaces between unit and airframe. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.11.5	Antenna for condition and security, control and indicators for condition, bonding wires for condition and security of attachment. Clean as required.
Effectivity: Mod SOO 6388 and Mod 6/2003
	
	
	

	17.12	#1 DME (KN63)

Effectivity: Mod 6/2049 & Mod SOO 6388
	

	17.12.1	Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.12.2	Perform power on operational test of transceiver unit.
	
	
	

	17.12.3	Inspect transceiver unit bonding of mating surfaces between mounting tray and the nearest airframe ground. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
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17.12.4	Inspect center fuselage antenna bonding of mating surfaces between mounting tray and the nearest airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.13	#2 DME (KN63)
	

	Effectivity: Mod 6/2049 & Mod SOO 6388
	

	17.13.1	Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.13.2	Perform power on operational test of transceiver unit.
	
	
	

	17.13.3	Inspect transceiver unit bonding of mating surfaces between mounting tray and the nearest airframe ground. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.13.4	Inspect antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.14	Inspect center fuselage antenna bonding of mating surfaces between antenna and airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.15	#1 Radar Altimeter Unit

Effectivity: Mod 6/2049 & Mod SOO 6388
	

	17.15.1	Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.15.2	Perform power on operational test of radar altimeter unit.
	
	
	

	17.15.3	Inspect bonding of mating surfaces between mounting tray airframe ground. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.15.4	Inspect antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003 & Mod SOO 6388
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17.16	#2 Radar Altimeter Unit
	

	
	

	Effectivity: Mod 6/2049 & Mod SOO 6218
	

	17.16.1	Inspect transceiver unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.16.2	Perform power on operational test of radar altimeter unit.
	
	
	

	17.16.3	Inspect bonding of mating surfaces between mounting tray and airframe ground. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.16.4	Inspect antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003 & Mod SOO 6388
	
	
	

	17.17	Inspect Radar Altimeter unit antenna’s #3 & #4 bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003 & Mod SOO 6388
	
	
	

	17.18	#1 TCAS I Processor Unit (KTA 970)

Effectivity: Mod 6/2049 & Mod SOO 6382
	

	17.18.1	Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.18.2	Perform power on operational test of processor unit (Power On).
	
	
	

	17.18.3	Inspect bonding of mating surfaces between mounting tray airframe ground. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.18.4	Inspect upper antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003 & Mod SOO 6382
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17.18.5	Inspect lower antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003 & Mod SOO 6382
	
	
	

	17.19	#2 TCAS II Processor Unit (KTA 970)

Effectivity: Mod 6/2049 & Mod SOO 6219
	

	17.19.1	Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.19.2	Perform power on operational test of processor unit.
	
	
	

	17.19.3	Inspect bonding of mating surfaces between mounting tray and airframe ground. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.19.4	Inspect upper antenna bonding of mating surfaces between antennas and airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003 & Mod SOO 6219
	
	
	

	17.20	EGPWS (MK VI)

Effectivity: Mod 6/2049 & Mod SOO 6387
	

	17.20.1	Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.20.2	Perform power on operational test of EGPWS unit.
	
	
	

	17.20.3	Inspect bonding of mating surfaces between mounting tray and airframe ground. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.21	#1 ADAHRS (KSG 7200)
	

	Effectivity: Mod 6/2049
	

	17.21.1	Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.21.2	Perform power on operational test of EGPWS unit.
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17.21.3	Inspect bonding of mating surfaces between mounting tray and airframe ground. (<1.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.22	#2 ADAHRS (KSG 7200)
	

	Effectivity: Mod 6/2049 & Mod SOO 6209
	

	17.22.1	Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.22.2	Perform power on operational test of EGPWS unit.
	
	
	

	17.22.3	Inspect bonding of mating surfaces between mounting tray and airframe ground. (<1.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.23	ADAHRS - Magnetometer (KSG 7210)
	

	Effectivity: Mod 6/2049 & Mod SOO 6209 and Pre Mod 6/2171
	

	17.23.1	Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.23.2	Inspect bonding of mating surfaces between mounting feet and airframe structure. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.24	#1 ADF Antenna
	

	Effectivity: Mod 6/2003 & Mod SOO 6209
	

	17.25	ADAHRS - Magnetometer (KSG 7210)
	

	Effectivity: Mod 6/2049 & Mod SOO 6209 and Post Mod 6/2171
	

	17.25.1	Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	17.25.2	Inspect bonding of mating surfaces between mounting feet and airframe structure. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.26	#1 ADF Antenna
	

	Effectivity: Mod 6/2003 & Mod SOO 6209
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17.26.1	Inspect bonding of mating surfaces between the antenna and the airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.27	#2 ADF Antenna

Effectivity: Mod 6/2003 & Mod SOO 6209
	

	17.27.1	Inspect bonding of mating surfaces between the antenna and the airframe ground. (<3.0 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	17.28	XM antenna - Inspect bonding of mating surfaces between the antenna and the airframe ground. (<2.5 milliohms).

Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2003
	
	
	

	C 1000.18	36 - PNEUMATIC

	
18.1	Instrument pneumatic system filter for long nose aircraft with (Mod 6/1046) bleed air or (Mod 6/1166) engine driven pump systems.
	
	
	

	18.2	Remove and install new filters and leak check.
	
	
	

	
	

	C 1000.19	44 – CABIN SYSTEMS

	
19.1.1	Inspect grounding of cabin speakers and airframe structure. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod SOO 6/221 & Mod 6/2049
	
	
	

	19.2	NAT 245 PA Amplifier
Effectivity: Mod SOO 6/2010 & Mod 6/2049
	

	19.2.1	Inspect unit for condition and security, bonding wires for condition and security of attachment.
	
	
	

	19.2.2	Inspect grounding of unit wire bundle shield braid to airframe structure. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
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	C 1000.20	52 – DOORS

	
20.1	Flight compartment LH and RH doors to airframe for bonding. (<10 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2024
	
	
	

	20.2	Cabin LH and RH doors to airframe for bonding. (<10 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2024
	
	
	

	20.3	Airstair door to airframe for bonding. (<10 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2024
	
	
	

	20.4	Aft baggage compartment door to airframe for bonding. (<10 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2024
	
	
	

	20.5	Fwd baggage compartment door to airframe for bonding. (<10 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2020 & Mod 6/2161
	
	
	

	C 1000.21	53 – FUSELAGE

	
21.1	External structure for dents, scores, fretting and cracks, fasteners for security.
	
	
	

	21.2	Radome for condition, cracks, delamination and security.
	
	
	

	21.3	Nose baggage compartment to radome joint diverter strip (qty 4) for electrical bonding. (<10 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
	
	
	

	21.4	Radio equipment racks for cracks, buckling and corrosion. Vibration isolators for deterioration. Clean as required.
	
	
	

	21.5	Rear baggage compartment for condition. Equipment shelves for cracks, buckling and corrosion. Clean as required.
Note: In addition, when Mod 6/2020 or Mod 6/2160 is installed at STA 44.0 nose attachment, pay particular attention for the corrosion to the exterior aluminum joint straps and fasteners common to the carbon nose.
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21.6	Fuel gallery structure for corrosion.
	
	
	

	21.7	Inspect fuel gallery access panels and seals for damage. Repair or replace as required.

Effectivity: Mod 6/2408
	
	
	

	21.8	Nose baggage bulkhead at STA 15.45 for condition, security and corrosion between aluminum brackets and fasteners attached to the carbon nose.
	
	
	

	21.9	Cargo tie-downs located on STA 15.45 bulkhead for condition and security.
	
	
	

	21.10	Inspect the nose baggage compartment weather radar wiring metal conduit to airframe for electrical bonding. (<10 milliohms).

Effectivity: Mod 6/2020 & 6/2160
	
	
	

	21.11	Inspect the nose baggage compartment fuselage circumferential aluminum strap joint for electrical bonding. (<10 milliohms).
Effectivity: Mod 6/2020 & 6/2160
	
	
	

	21.12	Ensure bonding jumpers in nose baggage compartment have no sign of corrosion, braid damage such as kinks, fretting or fraying, cracked or broken terminal ends.
	
	
	

	21.13	Inspect forward avionics compartment shelves to airframe for bonding. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2005
	
	
	

	21.14	Inspect forward avionics compartment shelves bonding jumpers have no sign of corrosion, braid damage such as kinks, fretting or fraying, cracked or broken terminal ends.
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2005
	
	
	

	21.15	Inspect aft avionics compartment shelves to airframe for bonding. (<2.5 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2028
	
	
	

	21.16	Ensure aft avionics equipment shelves bonding jumpers have no sign of corrosion, braid damage such as kinks, fretting or fraying, cracked or broken terminal ends.

Effectivity: Mod 6/2028
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	C 1000.22	54 – NACELLE - LH

	
22.1	Nacelle fairing to airframe for bonding. (<10 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2021
	
	
	

	C 1000.23	54 – NACELLE - RH

	
23.1	Nacelle fairing to airframe for bonding. (<10 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6/2021
	
	
	

	C 1000.24	55 – STABILIZER - LH

	
24.1	Mid hinge arm adapter place for condition, corrosion, fasteners for security and bearings for condition
Effectivity: Pre Mod 6/1341
	
	
	

	C 1000.25	55 – STABILIZER - RH

	
25.1	Mid hinge arm adapter place for condition, corrosion, fasteners for security and bearings for condition
Effectivity: Pre Mod 6/1341
	
	
	

	C 1000.26	56 – WINDOWS

	
26.1	Flight compartment windshield and door windows for condition, crazing and security, retaining strips for condition and security of attachment. For SOO 6320 or 6321, if installed, inspect vent for condition and security of attachment. Replace as required.
	
	
	

	26.2	Flight compartment LH and RH doors to airframe for bonding. (<10 milliohms).
Note: HIRF/IEL/DEL inspection. Refer to Inspection Requirements Page 7, Para 12 for details.
Effectivity: Mod 6024
	
	
	

	26.3	Cabin windows for condition, crazing and security. Inspect vents (SOO 6368) for condition and security of attachment. Replace if required.
	
	
	

	26.4	Cabin side escape hatch windows for condition, crazing and security. Replace if required.
	
	
	

	26.5	Cabin door windows for condition, crazing and security. Replace if required.
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	C 1000.27	57 – WING – LH

	
27.1	All accessible electrical wiring for deterioration, chafing, bonding wire for fraying, corrosion and security of attachment, connector for cleanliness and security.
	
	
	

	27.2	Outboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
	
	
	

	27.3	Inboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
	
	
	

	27.4	Outboard foreflap pushrod fork attachment for corrosion and security of attachment.
	
	
	

	27.5	Inboard foreflap pushrod fork attachment for corrosion and security of attachment.
	
	
	

	27.6	Do a detailed visual inspection of the ailerons as follows;
	

	27.6.1	Nose and tail skins for condition, dents, scores, abrasions and fasteners for security.
	
	
	

	27.6.2	Trim and gear tab hinge adapter for corrosion, wear, security and freedom of movement. Lubricate.
	
	
	

	27.6.3	Bellcrank structure channels for condition, fasteners for security, bearings for freedom of operation and security.
	
	
	

	27.6.4	Aileron trim and gear tab skins for condition, buckling and fasteners for security.
	
	
	

	27.6.5	Hing arms for condition, corrosion and security.
	
	
	

	27.6.6	Trim tab hinge for condition, corrosion, wear and freedom of movement. Lubricate.
	
	
	

	C 1000.28	57 – WING – RH

	
28.1	All accessible electrical wiring for deterioration, chafing, bonding wire for fraying, corrosion and security of attachment, connector for cleanliness and security.
	
	
	

	28.2	Outboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
	
	
	

	28.3	Inboard foreflaps for condition, drain holes for obstruction, skins for dents, scores, corrosion, cracks and fasteners for security.
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28.4	Outboard foreflap pushrod fork attachment for corrosion and security of attachment.
	
	
	

	28.5	Inboard foreflap pushrod fork attachment for corrosion and security of attachment.
	
	
	

	28.6	Do a detailed visual inspection of the aileron as follows;
	

	28.6.1	Nose and tail skins for condition, dents, scores, abrasions and fasteners for security.
	
	
	

	28.6.2	Trim and gear tab hinge adapter for corrosion, wear, security and freedom of movement. Lubricate.
	
	
	

	28.6.3	Bellcrank structure channels for condition, fasteners for security, bearings for freedom of operation and security.
	
	
	

	28.6.4	Aileron trim and gear tab skins for condition, buckling and fasteners for security.
	
	
	

	28.6.5	Hing arms for condition, corrosion and security.
	
	
	

	28.6.6	Trim tab hinge for condition, corrosion, wear and freedom of movement. Lubricate.
	
	
	

	C 1000.29	61 – PROPELLERS – LH

	
29.1	Stall warning cam limit microswitch mechanism and propeller reset limit switch for condition and security, connect for security.
	
	
	

	C 1000.30	61 – PROPELLERS – RH

	
30.1	Stall warning cam limit microswitch mechanism and propeller reset limit switch for condition and security, connect for security.
	
	
	

	C 1000.31	71 – POWERPLANT - LH

	
31.1	Remove intake deflector air line filters at inlet and return ports of air control valves.
	
	
	

	31.2	Inspect intake deflector air line filters at inlet and return ports of air control valves.
	
	
	

	31.3	Install intake deflector air line filters at inlet and return ports of air control valves.
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	C 1000.32	71 – POWERPLANT - RH

	
32.1	Remove intake deflector air line filters at inlet and return ports of air control valves.
	
	
	

	32.2	Inspect intake deflector air line filters at inlet and return ports of air control valves.
	
	
	

	32.3	Install intake deflector air line filters at inlet and return ports of air control valves.
	
	
	

	C 1000.33	73 – ENGINE FUEL AND CONTROL – LH

	
33.1	Move to CALM
	
	
	

	33.2	Move to CALM
	
	
	

	C 1000.34	73 – ENGINE FUEL AND CONTROL – RH

	
34.1	Move to CALM
	
	
	

	34.2	Move to CALM
	
	
	

	C 1000.35	76 – ENGINE CONTROLS

	
35.1	Overhead console flight control and flap selector aluminum quadrants for condition and security, freedom of movement, cable attachment for security.
	
	
	

	35.2	Overhead console flight control and flap selector pulleys for smoothness and freedom of operation.
	
	
	

	C 1000.36	OPERATIONAL CHECKS

	
36.1	Perform the following Operational Checks;
	

	36.1.1	Instrument pneumatic system for correct vacuum and/or pressure, as applicable.
	
	
	

	36.1.2	Bleed air shutoff valves.
	
	
	

	36.1.3	Wing tank fuel system (SOO 6095 and 6247). Power On.
	
	
	

	36.1.4	ECTM/FOQA (IONode) (SOO 6288) Data Capture System. Power on.
	
	
	

	36.1.5	QAR (SOO 6356). Power on.
	
	
	

	36.1.6	STA 111 Cabin Fans (SOO 6378). Power on.
	
	
	

	36.1.7	STA 332 Blower (SOO 6379). Power on.
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36.2	Leak check the following items, as applicable, after installation;
	

	36.2.1	Instrument pneumatic system (bleed air) filters.
	
	
	

	36.2.2	Not installed on aircraft.
	
	
	

	36.2.3	Not installed on aircraft.
	
	
	

	C 1000.37	POST INSPECTION

	
37.1	Inspect for operation and leaks.
	
	
	

	37.2	Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	37.3	Clean aircraft and engine once maintenance is completed.
	
	
	

	37.4	Perform Functional Check Flight if required per DHC-6-400 Maintenance Manual or AFM as appropriate.
	
	
	

	37.5	Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6-400 – C 1000RT – 1000 Hour Inspection and was determined to be in an airworthy condition.


Registration No.: N	End Aircraft S/N:                                     Date:

Aircraft Ending Total Time: Aircraft Ending Total Cycles:


Signature:	Certificate Type & No:

MARITIME HELICOPTERS	DCH-6 MAINTENANCE MANUAL




CHECK: FREQUENCY: NOTE::




C 1500RT – BASIC INSPECTION Every 1500 Hours
This inspection is restricted to 50 hours

Page No: Revision: Issue Date:

7-86 Original 5/01/20



Registration No.: N                                Start Aircraft S/N:                                      Date:
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Reference: DHC-6 Maintenance Program, Viking PSM Maintenance Manuals
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	C 1500.1	GENERAL

	
1.1	Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	1.2	Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3	Replace all life limited components that have completed published operating limits.
	DHC-6-400 MP
	
	

	1.4	Overhaul all components that have completed published operating limits.
	DHC-6-400 MP
	
	

	C 1500.2	PLACARDS AND MARKINGS

	
2.1	Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	C 1500.3	CORROSION CONTROL

	
3.1	Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	
Appendix C
	
	

	C 1500.4	PREPARATION

	
4.1	Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	C 1500.5	21 – AIR CONDITIONING

	
5.1	Heater ejector for condition and security.
	
	
	

	5.2	Heater silencer for condition and security, insulation for condition and security.
	
	
	

	5.3	Ram air and cabin air control valves operating mechanism for ease of operation and security; flexible cable, clamps and brackets for condition and security.
	
	
	

	5.4	Duct temperature sensor and duct overheat switch for security.
	
	
	

	5.5	Outside air temperature sensor for security.
	
	
	

	5.6	Cabin temperature sensor for condition and security.
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5.7	Heating system hot air valve for security.
	
	
	

	5.8	 Ram air screens scoop and duct for condition. Effectivity: Pre Mod 6/1070
	
	
	

	5.9	Main ram air duct ground operable fan for security.
	
	
	

	5.10	Flight compartment and cabin heater ducts for condition and evidence of overheat, connections for security. Ducts for condition and delamination, supporting structure for condition and security.
	
	
	

	5.11	L/H nacelle bleed air shut off valve for condition and security.
	
	
	

	5.12	R/H nacelle bleed air shut off valve for condition and security.
	
	
	

	5.13	Removed. Not installed on our aircraft.
	
	
	

	5.14	Electrical wiring and connectors forward of instrument panel for condition and security, bonding wires for condition.
	
	
	

	C 1500.6	23 – COMMUNICATIONS

	
6.1	VHF/FM unit for condition and security of mounting, electrical cables for condition and connector for security. Clean as required.
	
	
	

	6.2	Radio navigation equipment shock mounts for condition, cracks, corrosion and security, vibration isolators for condition, bonding wire for condition and security.
	
	
	

	C 1500.7	24 – ELECTRICAL POWER

	
7.1	 Circuit breaker panels for condition and security Note: Refer to A.D. 70-22-04, if applicable.
	
	
	

	7.2	Removed. Not installed on our aircraft.

	
	
	

	  7.3	Removed. Not installed on our aircraft.
	
	
	

	7.4	Nose electrical wiring and connectors forward of instrument panel for condition and security, bonding wires for condition.
	
	
	

	7.5	Electrical wiring and connectors under flight compartment floor for condition and security, bonding wires for condition.
	
	
	

	7.6	Electrical wiring in flight compartment for condition and connectors for security.
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7.7	Electrical wiring and connectors in empennage for condition and security, bonding wires for condition.
	
	
	

	7.8	External power for condition and security, bus bars for condition.
	
	
	

	7.9	Battery relays for condition and security, bus bars for condition.

Effectivity: SOO 6371
	
	
	

	C 1500.8	25 - EQUIPMENT/FURNISHINGS

	
8.1	First aid kit for required content, proper stowage and security.
	
	
	

	8.2	14-volt outlet for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2028
	
	
	

	
	

	8.3	28-volt outlet for condition and security, bonding wires for condition and security of attachment.
Effectivity: Mod 6/2028
	
	
	

	8.4	Flight compartment axe and axe stowage for condition and security of axe stowage structure. Condition and security of axe cutting edge and pie to axe handle.


Effectivity: SOO 6376
	
	
	

	C 1500.9	26 – FIRE PROTECTION

	
9.1	L/H engine fire protection wiring and connectors for condition and security, clips for security. Clean as required.
	
	
	

	9.2	R/H engine fire protection wiring and connectors for condition and security, clips for security. Clean as required.
	
	
	

	C 1500.10	27 – FLIGHT CONTROLS

	
10.1	Flap selector lever for condition, proper detent action of movement and security. Lubricate.
	
	
	

	C 1500.11	28 – FUEL

	
11.1	Fuel system position indicator for condition and security.
Effectivity: SOO 6235 Pre Mod 6/2009
	
	
	

	11.2	Capacitance tank units for corrosion, security and leakage.
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11.3	Fuel quantity signal conditioner for corrosion, security of wiring and connectors.
Effectivity: Mod 6/2046
	
	
	

	11.4	Fuel cells for security and leakage, cell vent necks and vent lines for condition and leakage.
	
	
	

	  11.5	Removed. Not installed on our aircraft.
	
	
	

	  11.6        Removed. Not installed on our aircraft.
	
	
	

	C 1500.12	29 – HYDRAULIC POWER

	
12.1	Hydraulic and brake system pressure indicators for condition, security and leakage.
Effectivity: Pre Mod 6/2002
	
	
	

	12.2	Hydraulic and brake system pressure sensors for condition, security and leakage.

Effectivity: Pre Mod 6/2002
	
	
	

	
	

	C 1500.13	30 – ICE AND RAIN PROTECTION

	
13.1	Heated windscreen temperature controllers for condition and security, connectors for security.
	
	
	

	13.2	Windshield heat relay box for damage and security, connectors for security.
	
	
	

	13.3	L/H propeller blade deicing electrical harness for security of connections.
	
	
	

	13.4	R/H propeller blade deicing electrical harness for security of connections.
	
	
	

	13.5	Inspect the windshield wiper system as follows;
	

	13.5.1	Wiper motor for security of attachment.
	
	
	

	13.5.2	Converters for condition and freedom of movement
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13.5.3	Flexible drives for condition, security and freedom of operation, evidence of water ingress.
	
	
	

	13.5.4	Wiring and connectors for condition and security.
	
	
	

	C 1500.14	31 – INSTRUMENTS

	
14.1	Instrument panels for condition and security, bonding wires for condition and security.
	
	
	

	C 1500.15	32 – LANDING GEAR

	
15.1	Nose landing gear torque arms, bushing and pip-pin for wear, condition, corrosion and security, pip-pin chain for security.
	
	
	

	15.2	Nose gear attachment fittings for corrosion and cracks, pre load bolt torque arks for proper alignment.
	
	
	

	15.3	 Inspect the main landing gear shock absorbing blocks as follows. Note: Refer to Maintenance Manual.
	
	

	15.3.1	Permanent set and gaps between compression blocks and separator plates.
	
	
	

	15.3.2	Upper to lower platen and preload bolt dimension.
Effectivity: Pre-Mod and Mod 6/1469 standard compression blocks
	
	
	

	15.3.3	Rebound block and plate for condition, corrosion and separation.
	
	
	

	15.4	Landing gear stay struts for cracks, corrosion and security.
	
	
	

	C 1500.16	33 – LIGHTS

	
16.1	Inspect Anti-collision (Beacon) light for condition and operation.

	
	
	

	  16.2	  Removed. Not installed on our aircraft.
	
	
	

	16.3	Strobe light flasher unit (if installed) for condition, connector for security.

Effectivity: Pre Mod 6/2028
	
	
	

	16.4	L/H wing tip fairing for cracks, delamination and security. Strobe light power supply (if installed) for condition and security.
Effectivity: Pre Mod 6/2028 and Mod 6/1513
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16.5	L/H wing position light power supply (if installed) for condition and security.

Effectivity: Pre Mod 6/2447 and Mod 6/2028
	
	
	

	
	

	16.6	R/H wing tip fairing for cracks, delamination and security. Strobe light power supply (if installed) for condition and security.
Effectivity: Pre Mod 6/2028 and Mod 6/1513
	
	
	

	16.7	R/H wing position light power supply (if installed) for condition and security.

Effectivity: Pre Mod 6/2447 and Mod 6/2028
	
	
	

	16.8	 Cabin interior passenger warning lights for condition and security. Effectivity: Pre Mod 6/2028
	
	

	
	
	
	

	16.9	 Cabin interior passenger lights for condition and security. Effectivity: Pre Mod 6/2028
	
	
	

	16.10	Nose baggage compartment lights for condition and security.
	
	
	

	16.11	Aft baggage compartment lights for condition and security.
	
	
	

	16.12	Door unlocked warning system for condition and security, limit switches and actuator mechanisms for condition and security. Operate each door separately.
	
	
	

	16.13	Flight and cabin electrical wiring in ceiling area for condition, connectors and security. Clean and required.
	
	
	

	C 1500.17	34 – NAVIGATION

	
  17.1        Removed. Inspection is a duplicate. See 6.2.
	
	
	

	17.2	Pitot static systems selector valve for security and smooth operation, pipes for condition and connections for security.
	
	
	

	C 1500.18	36 – PNEUMATIC

	
18.1	Inspect the instrument pneumatic system nose baggage compartment bleed air, vacuum or engine driven pump installation as follows;

Effectivity: Mods 6/1077, 6/1166
	

	18.1.1	L/H engine pressure regulators for damage and security.
	
	
	

	18.1.2	L/H engine pressure relief valves for damage and security.
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18.1.3	L/H engine mounting plates for cracks, damage and security.
	
	
	

	18.1.4	Removed. No engine pressure indicators installed. System pressure is identified by low or loss of pressure through the CAS System.
	
	
	

	18.1.5	Removed. No engine driven air pumps installed.
Effectivity: Mod 6/1166
	
	
	

	18.1.6	Removed. No engine driven air pumps installed. System works off Bleed air, w/ Bleed air valve controlled from cockpit by switch.
	
	
	

	18.1.7	L/H Automatic water drain for security
	
	
	

	18.1.8	L/H Automatic water drain for security
	
	
	

	18.1.9	R/H engine pressure regulators for damage and security.
	
	
	

	18.1.10	R/H engine pressure relief valves for damage and security.
	
	
	

	18.1.11	R/H engine mounting plates for cracks, damage and security.
	
	
	

	18.1.12	Removed. No engine pressure indicators installed. System pressure is identified by low or loss of pressure through the CAS System.
	
	
	

	18.1.13	Removed. No engine driven air pumps installed.
Effectivity: Mod 6/1166
	
	
	

	18.1.14	Removed. No engine driven air pumps installed. System works off Bleed air, w/ Bleed air valve controlled from cockpit by switch.
	
	
	

	18.1.15	Removed. There is no Emergency Instrument Vacuum Valve installed on the 400 series.
	
	
	

	18.1.16	Removed. There are not pressure and suction indicators installed on the 400 series.
	
	
	

	18.1.17	All pipes for condition, connections for security, flexible hoses for condition.
	
	
	

	C 1500.19	52 – DOORS

	
19.1	L/H flight compartment door for condition, corrosion and security, seals for condition and security.
	
	
	

	19.2	R/H flight compartment door for condition, corrosion and security, seals for condition and security
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19.3	L/H cabin doors for condition, corrosion and security, seals for condition and security
	
	
	

	19.4	R/H cabin door for condition, corrosion and security, seals for condition and security
	
	
	

	19.5	Inspect the airstair door (if installed) as follows:
	
	

	19.5.1	Condition and security, seals for condition and security.
	
	
	

	19.5.2	Handrail and springs for condition and security including proper stowage.
	
	
	

	19.5.3	Springs for security and operation.
	
	
	

	19.5.4	Cables for condition and security of attachment, protective cable covers for tears and deterioration.
	
	
	

	19.5.5	Restraint unit, if installed, for corrosion, security of attachment and smooth movement of operation.
Effectivity: Mod 6/2326 & 6/2386
	
	
	

	19.6	Rear baggage compartment doors for condition and security, seals for condition, door handle and lock for condition and proper operation. Clean as required.
	
	
	

	19.7	Nose baggage compartment doors latches for condition, security, and proper operation
	
	
	

	C 1500.20	53 – FUSELAGE

	
20.1	L/H fuselage frame wing attach lugs @ Sta. 239.88 for condition, cracking, corrosion and fasteners for security.
Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges. Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required.
	
	
	

	
	
	
	

	20.2	R/H fuselage frame wing attach lugs @ Sta. 239.88 for condition, cracking, corrosion and fasteners for security.
Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges. Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required.
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20.3	Elevator Bellcrank and Hyd. Hand pump attaching structure for condition, cracking and security of fasteners.
Note: Refer to Service Bulletin N. 6/348 and AD 77-03-07 & 93-09-04 if applicable.
	
	
	

	C 1500.21	54 – LH NACELLE

	
21.1	Internal structure of wing and nacelle, where accessible, for condition, cracks, buckling and corrosion. Waste fuel return pipes (if installed for condition, connections for leakage and security.
	
	
	

	C 1500.22	54 – RH NACELLE

	
22.1	Internal structure of wing and nacelle, where accessible, for condition, cracks, buckling and corrosion. Waste fuel return pipes (if installed for condition, connections for leakage and security.
	
	
	

	C 1500.23	55 – STABILIZERS

	
23.1	Inspect the horizontal stabilizer as follows;
	

	23.1.1	Accessible internal structure of for corrosion, cracks, buckling and security.

Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges. Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required. Corrosion around bonding jumpers where fitted, will necessitate cleaning and re-priming of effected areas, as applicable.
	
	
	

	
	

	23.1.2	Top upper skin, skin doubler beneath center pickup fitting for cracking.
	
	
	

	23.1.3	Lower skin between Stations 30.00 and 35.00 for condition, cracks, distortion and fasteners for security.
	
	
	

	23.1.4	Leading edge skins for condition, dents, scores and fastener security. Aft of deicing boots for surface corrosion.
Effectivity: SOO 6004
	
	
	

	23.1.5	Fwd and Aft spar webs between attachment brackets and center line for condition, cracks and fasteners for security.

Note: Refer to Service Bulletin No. 6/310 and A.D. 74-22-06, if applicable.
	
	
	

	23.1.6	External skin structure for dents, scores, abrasions corrosion, cracks and buckling and fasteners for security.
.
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23.2	Inspect the vertical stabilizer as follows;

Effectivity: Mod 6/2417
	

	23.2.1	Accessible internal structure for corrosion, cracks, buckling and security.

Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges.	Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required. Corrosion around bonding jumpers where fitted, will necessitate cleaning and re-priming of effected areas, as applicable.
	
	
	

	
	
	
	

	23.2.2	Top hinge arm adapter fitting for condition, corrosion and security.

Effectivity: Pre Mod 6/1339
	
	
	

	23.2.3	 Mid hinge arm adapter fitting for condition, fretting, corrosion and security. Effectivity: Pre Mod 6/1340
	
	
	

	23.2.4	External skin structure for dents, scores, abrasions corrosion, cracks and buckling and fasteners for security.
.
	
	
	

	23.3	Inspect the rudder as follows;
	

	23.3.1	Skins for condition, dents, scores, buckles, leading edge silicon aerodynamic seal for adhesion and security, fasteners for security.
	
	
	

	23.3.2	Lower hinge arm for condition, corrosion, fasteners for security and bearing for condition.

Note: As bearing deterioration results in rudder drop this bearing should be replaced when wear is noted. A gap dimension between the lower hinge arm housing and the rudder hinge arm bearing support plate of 0.058 inch (1.47 mm) will indicate that the bearing manufacture's axial service limit has been reached. A smaller gap dimension requires the bearing to be replaced at the earliest opportunity available.
Effectivity: Pre Mod and Post Mod 6/1340
	
	
	

	
	
	
	

	23.3.3	Mid and upper hinge arm adapter fitting for condition corrosion and fasteners for security.
Effectivity: Pre Mod 6/1339
	
	
	

	23.3.4	Mid and upper hinge arms for condition corrosion and fasteners for security.

Effectivity: Pre Mod 6/1339
	
	
	



MARITIME HELICOPTERS	DCH-6 MAINTENANCE MANUAL




CHECK: FREQUENCY: NOTE::




C 1500RT – BASIC INSPECTION Every 1500 Hours
This inspection is restricted to 50 hours

Page No: Revision: Issue Date:

7-96 Original 5/01/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
23.3.5	Mass balance weight for condition and security. Move rudder vigorously to detect movement of internal weights.
	
	
	

	23.3.6	Rudder trim and gear tabs skins for condition, dents, scores, buckles and fasteners for security, hinge arms for condition, hinges for condition, corrosion, security and freedom of movement. Lubricate.
	
	
	

	23.3.7	Rear spar tab hinge for condition, corrosion and freedom of movement. Lubricate.
	
	
	

	23.4	Inspect the elevator as follows;
	

	23.4.1	Skins for condition, dents, scores, buckles, leading edge silicon aerodynamic seal for adhesion and security, fasteners for security.
	
	
	

	23.4.2	Mid and upper hinge arm adapter fitting for condition corrosion and fasteners for security.
Effectivity: Pre Mod 6/1342
	
	
	

	23.4.3	 Mid hinge arm adapter fitting for condition, fretting, corrosion and security. Effectivity: Pre Mod 6/1342
	
	
	

	23.4.4	Trim and interconnect tab skins for condition, dents, scores, buckles. Fasteners for security, hinge arms for condition, hinges for condition, corrosion, security and freedom of movement. Lubricate
	
	
	

	23.4.5	Torque tube for condition, corrosion, security and freedom of movement.
	
	
	

	23.4.6	Trim and interconnect tab hinge adapter for condition, corrosion, security and freedom of movement. Lubricate
	
	
	

	23.4.7	Mass balance weights for condition, carrion and security.
	
	
	

	23.5	Electrical wiring and connectors in empennage for condition and security, bonding wires for condition and security.
	
	
	

	C 1500.24	57 – LH WING

	
24.1	Wing lower skin between station 97.00 and 235.00 (wing pick-up fitting) for cracks, buckling and fasteners for security.
	
	
	

	24.2	Wing upper skin between station 147.00 and 210.00 (wing pick-up fitting) for cracks, buckling and fasteners for security.
	
	
	

	24.3	Wing main spar (strut link) lug for condition, corrosion and bush for security.
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24.4	Nose spar adapter D nose section for condition, corrosion and fasteners for security, leading edge skin for condition, corrosion and security, hinges for condition and smooth operation of D nose leading edge cover, stay bar for condition and security of stowage.
	
	
	

	24.5	Wing tip fairing for cracks, delamination, and security.
	
	
	

	
	

	24.6	Removed. This inspection is already accomplished on 16.5.
	
	
	

	24.7	 Wing strut skins condition, dents, scores, and fasteners for security. Note: Refer to Service Bulletin N. 6/342 and A.D. 97-07-10, if applicable.
	
	
	

	24.8	Wing strut link for condition, corrosion, and bush for security.

Effectivity: Pre Mod 6/1174
	
	
	

	24.9	Internal structure of wing, where accessible, for condition, cracks, buckling and corrosion. Waste fuel return pipes (if installed) for condition, connections for leakage and security.
	
	
	

	24.10	Internal structure of nacelle, where accessible, for condition, cracks, buckling and corrosion.
	
	
	

	24.11	Aileron bellcranks for corrosion and security, bearings for condition. Clean as required.
	
	
	

	24.12	Flap bellcranks for corrosion and security, bearings for condition. Clean as required.
	
	
	

	C 1500.25	57 – RH WING

	
25.1	Wing lower skin between station 97.00 and 235.00 (wing pick-up fitting) for cracks, buckling and fasteners for security.
	
	
	

	25.2	Wing upper skin between station 147.00 and 210.00 (wing pick-up fitting) for cracks, buckling and fasteners for security.
	
	
	

	25.3	Wing main spar (strut link) lug for condition, corrosion, and bush for security.
	
	
	

	25.4	Nose spar adapter D nose section for condition, corrosion and fasteners for security, leading edge skin for condition, corrosion and security, hinges for condition and smooth operation of D nose leading edge cover, stay bar for condition and security of stowage.
	
	
	

	25.5	Wing tip fairing for cracks, delamination, and security.
	
	
	

	25.6	Removed. This inspection is already accomplished on 16.7.
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25.7	 Wing strut skins condition, dents, scores and fasteners for security. Note: Refer to Service Bulletin N. 6/342 and A.D. 97-07-10, if applicable.
	
	
	

	25.8	Wing strut link for condition, corrosion and bush for security.

Effectivity: Pre Mod 6/1174
	
	
	

	25.9	Internal structure of wing, where accessible, for condition, cracks, buckling and corrosion. Waste fuel return pipes (if installed) for condition, connections for leakage and security.
	
	
	

	25.10	Internal structure of nacelle, where accessible, for condition, cracks, buckling and corrosion.
	
	
	

	25.11	Wing main hinge arms for corrosion, cracks and wear.
Effectivity: Pre Mod 6/1334
	
	
	

	25.12	Flap hinge arm attachments for condition, cracking, corrosion and jo-bolts for security.
Effectivity: Pre Mod 6/1335
	
	
	

	25.13	Inboard and outboard foreflap hinge arms for condition, corrosion, security and bearings for security.
Effectivity: Pre Mod 6/1336 and 6/1349
	
	
	

	25.14	Wing inboard trailing flap hinge arms for condition, corrosion, security and bearings for security.
Effectivity: Pre Mod 6/1337
	
	
	

	25.15	Aileron hinge arms for condition, corrosion, security and bearings for security.

Effectivity: Pre Mod 6/1338
	
	
	

	25.16	Aileron bellcranks for corrosion and security, bearings for condition. Clean as required.
	
	
	

	25.17	Flap bellcranks for corrosion and security, bearings for condition. Clean as required.
	
	
	

	C 1500.26	61 – L/H PROPELLER

	
26.1	Inspect the propeller controls as follows;
	

	26.1.1	Pulleys for condition, freedom of operation and security.
	
	
	

	26.1.2	Levers, pushrods and reversing linkage for security, springs for condition and security, stops for security.
	
	
	

	26.1.3	Teleflex control to reverse valve for condition, kinks, smooth operation and security.
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26.1.4	Constant speed governor, speed adjusting lever proper attachment to shaft.
Note: Refer to TAB 635/4
	
	
	

	26.1.5	Linkages for condition and security.
	
	
	

	26.2	Do a detailed visual inspection of cable terminals as follows;
	

	26.2.1	Remove and discard the lockwire from the cable terminals.
Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	26.2.2	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	26.2.3	Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	26.2.4	If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	26.2.5	If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 26.2.1, rig the control system.
	
	
	

	26.2.6	If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	26.3	Tachometer for condition and security of installation.
	
	
	

	C 1500.27	61 – R/H PROPELLER

	
27.1	Inspect the propeller controls as follows;
	

	27.1.1	Pulleys for condition, freedom of operation and security.
	
	
	

	27.1.2	Levers, pushrods and reversing linkage for security, springs for condition and security, stops for security.
	
	
	

	27.1.3	Teleflex control to reverse valve for condition, kinks, smooth operation and security.
	
	
	

	27.1.4	 Constant speed governor, speed adjusting lever proper attachment to shaft. Note: Refer to TAB 635/4
	
	
	

	27.1.5	Linkages for condition and security.
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27.2	Do a detailed visual inspection of cable terminals as follows;
	
	

	27.2.1	Remove and discard the lockwire from the cable terminals.

Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	27.2.2	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	27.2.3	Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	27.2.4	If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	27.2.5	If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 26.2.1, rig the control system.
	
	
	

	27.2.6	If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	27.3	Tachometer for condition and security of installation.
	
	
	

	
	

	C 1500.28	71 – L/H POWERPLANT

	
28.1	Intake deflector plate and exit door hinges for condition, corrosion, cracks and security. Clean as required.
	
	
	

	28.2	Intake deflector for condition and security, electrical wiring for condition, connectors for security. Clean as required.
	
	
	

	28.3	Air intake duct for condition and security.
	
	
	

	28.4	Upper engine cowling for condition, lower cowling hinge for condition and latch mechanism for condition and proper operation.
	
	
	

	28.5	Engine compressor wash spray ring for condition and security.
	
	
	

	28.6	Engine nacelle fuel drain lines for condition, security and leakage.

Effectivity: Pre Mod 6/1583
	
	
	

	28.7	Engine nacelle mounts for condition, corrosion, cracking and security.
	
	
	

	28.8	Engine vibration isolators for condition, separation, corrosion, cracking and security. Conduct inspection for separations between metal plate and elastomer; must not exceed 1-inch length or 1/16th inch in depth. Pay particular attention to corrosion and cracks at the base of the housing (P/N 7351256-2) right next to the edge of the cores (pucks).
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28.9	Bonding wires for condition and security.
	
	
	

	28.10	 Removed, due to change on 28.6. 
	
	
	

	28.11	Removed. Not installed on our aircraft.
	
	
	

	C 1500.29	71 – R/H POWERPLANT

	
29.1	Intake deflector plate and exit door hinges for condition, corrosion, cracks and security. Clean as required.
	
	
	

	29.2	Intake deflector for condition and security, electrical wiring for condition, connectors for security. Clean as required.
	
	
	

	29.3	Air intake duct for condition and security.
	
	
	

	29.4	Upper engine cowling for condition, lower cowling hinge for condition and latch mechanism for condition and proper operation.
	
	
	

	29.5	Engine compressor wash spray ring for condition and security.
	
	
	

	29.6	Engine nacelle fuel drain Lines for condition, security and leakage.

Effectivity: Pre Mod 6/1583
	
	
	

	29.7	Engine nacelle mounts for condition, corrosion, cracking and security.
	
	
	

	29.8	Engine vibration isolators for condition, separation, corrosion, cracking and security. Conduct inspection for separations between metal plate and elastomer; must not exceed 1-inch length or 1/16th inch in depth. Pay particular attention to corrosion and cracks at the base of the housing (P/N 7351256-2) right next to the edge of the cores (pucks).
	
	
	

	29.9	Bonding wires for condition and security.
	
	
	

	29.10	Removed due to change on 29.6.
	
	
	

	29.11	Removed. Not installed on our aircraft.
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	C 1500.30	73 – L/H ENGINE FUEL AND CONTROL

	
30.1	Fuel heater for condition, security and leakage.
	
	
	

	30.2	Fuel flow transmitters for condition, leakage and security.
	
	
	

	C 1500.31	73 – R/H ENGINE FUEL AND CONTROL

	
31.1	Fuel heater for condition, security and leakage.
	
	
	

	31.2	Fuel flow transmitter for condition, leakage and security.
	
	
	

	C 1500.32	76 – L/H ENGINE CONTROLS

	
32.1	Cable pulleys for condition, freedom of operation and security.
	
	
	

	32.2	Do a detailed visual inspection of engine cable terminals as follows;

Note: Refer to A.D. 68-05-03, if applicable.
	
	

	32.2.1	Remove and discard the lockwire from the cable terminals.
Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	32.2.2	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
	
	
	

	32.2.3	Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	32.2.4	If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	32.2.5	If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 32.2.1, rig the control system.
	
	
	

	32.2.6	If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	C 1500.33	76 – R/H ENGINE CONTROLS

	
33.1	Cable pulleys for condition, freedom of operation and security.
	
	
	

	33.2	Do a detailed visual inspection of engine cable terminals as follows;

Note: Refer to A.D. 68-05-03, if applicable.
	
	

	33.2.1	Remove and discard the lockwire from the cable terminals.
Note: If safety clip is installed, do not remove the safety clip.
	
	
	

	33.2.2	Cable terminals (excluding the hexagonal wrench flat area) for signs of corrosion pits.
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33.2.3	Cable terminals for signs of cracks in all exposed parts of the terminals.
	
	
	

	33.2.4	If corrosion pits and/or cracks are found on any cable terminal, remove and applicable cable assembly and replace with new cable assembly.
	
	
	

	33.2.5	If a new cable assembly is installed or if the rigging was disturbed when the lockwire was removed in step 32.2.1, rig the control system.
	
	
	

	33.2.6	If the lockwire was removed, secure the cable terminals with lockwire.
	
	
	

	C 1500.34	79 – L/H OIL

	
34.1	Power plant oil pipes, hoses and connections for condition and security.
	
	
	

	34.2	Oil cooler mounting for condition and security.
	
	
	

	C 1500.35	79 – R/H OIL

	
35.1	Power plant oil pipes, hoses and connections for condition and security.
	
	
	

	35.2	Oil cooler mounting for condition and security.
	
	
	

	C 1500.36	80 – OPERATIONAL CHECKS

	
36.1	Perform the following Operational Checks;
	

	36.1.1	Cabin temperature sensor blower. Power On
	
	
	

	36.1.2	Hot air valve (travel time from open to closed position). Power on.
	
	
	

	36.1.3	Airframe deicing system. Power on.
	
	
	

	36.1.4	Engine intake anti-icing system. Power on.
	
	
	

	36.1.5	Propeller deicing system. Power on.
	
	
	

	36.1.6	Ram air valve.
	
	
	

	36.1.7	Cabin air control valve.
	
	
	

	36.1.8	Brake system.
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	C 1500.37	POST INSPECTION

	
37.1	Inspect for operation and leaks.
	
	
	

	37.2	Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	37.3	Clean aircraft and engine once maintenance is completed.
	
	
	

	37.4	Perform Functional Check Flight if required per DHC-6-400 Maintenance Manual or AFM as appropriate.
	
	
	

	37.5	Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6-400 – C 1500RT – 1500 Hour Inspection and was determined to be in an airworthy condition.


Registration No.: N	End Aircraft S/N:                                     Date:

Aircraft Ending Total Time: Aircraft Ending Total Cycles:


Signature:	Certificate Type & No:
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Reference: DHC-6 Maintenance Program, Viking PSM Maintenance Manual
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	C 1700.1	GENERAL

	
1.1	Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	1.2	Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3	Replace all life limited components that have completed published operating limits.
	DHC-6-400 MP
	
	

	1.4	Overhaul all components that have completed published operating limits.
	DHC-6-400 MP
	
	

	C 1700.2	PLACARDS AND MARKINGS

	
2.1	Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	
	
	
	

	
	
	
	

	C 1700.3	CORROSION CONTROL

	
3.1	Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection
	
Appendix C
	
	

	
	
	
	

	
	
	
	

	C 1700.4	PREPARATION

	
4.1	Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	
	
	
	

	C 1700.5	22 – AUTO FLIGHT

	
5.1	Perform the following inspections on the SM3000 aileron servo cables;
	
	

	5.1.1	No fraying, kinks, flattening, proper attachment and security.
	
	
	

	5.1.2	Turnbuckles for security, freedom of operation.
	
	
	

	5.1.3	Clamps for security and no evidence of movement on main flight control cable.
	
	
	

	5.1.4	Bridle cable tensions. (15lbs +2lbs -0lbs. Ref Viking DHC-6-400 Maintenance                   manual, 22-10-12, Table 1) 
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5.2	Perform the following inspections on the SM3000 elevator servo cables;
	
	

	5.2.1	No fraying, kinks, flattening, proper attachment and security.
	
	
	

	5.2.2	Turnbuckles for security, freedom of operation.
	
	
	

	5.2.3	Clamps for security and no evidence of movement on main flight control cable.
	
	
	

	5.2.4	Clamps for security and no evidence of movement on main flight control cable.
	
	
	

	5.2.5	Bridle cable tensions. (25lbs +5lbs -0lbs, Ref Viking DHC-6-400 Maintenance Manual, 22-10-12 table 1)
	
	
	

	5.3	Perform the following inspections on the SM3000 rudder servo cables;
	
	

	5.3.1	No fraying, kinks, flattening, proper attachment and security.
	
	
	

	5.3.2	Turnbuckles for security, freedom of operation.
	
	
	

	5.3.3	Clamps for security and no evidence of movement on main flight control cable.
	
	
	

	5.3.4	Bridle cable tensions. (25lbs +5lbs -0lbs, Ref Viking DHC-6-400 Maintenance Manual, 22-10-12 table 1)
	
	
	

	5.4	Perform the following inspections on the KS 272A pitch trim servo cables;
	
	

	5.4.1	No fraying, kinks, flattening, proper attachment and security.
	
	
	

	5.4.2	Turnbuckles for security, freedom of operation.
	
	
	

	5.4.3	Clamps for security and no evidence of movement on main flight control cable.
	
	
	

	5.4.4	Bridle cable tensions. (15lbs +2lbs -0lbs, Ref Viking DHC-6-400 Maintenance Manual, 22-10-12 table 1)
	
	
	

	C 1700.6	23 – COMMUNICATIONS

	
6.1	Removed. We do not have a High Frequency Radio installed.

Effectivity: Mod SOO 6215, Mod 6/2049
NOTE: Refer to PSM 1-64-2, Maintenance Manual.
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	C 1700.7	24 – ELECTRICAL POWER

	
7.1	Perform the following inspections on the power distribution box;
	
	

	7.1.1	Condition and security
	
	
	

	7.1.2	Terminals, connectors and relays for condition and security
	
	
	

	7.1.3	Signs of overheat, arching
	
	
	

	7.1.4	Torque on large terminal posts
	
	
	

	7.1.5	Clean as required
	
	
	

	7.1.6	Current limiters (Mod 6/1651) for condition and serviceability.
	
	
	

	7.2	Perform the following inspections on generator control box;
	
	

	7.2.1	Condition and security
	
	
	

	7.2.2	Terminals, connectors and relays for condition and security
	
	
	

	7.2.3	Signs of overheat, arching
	
	
	

	7.2.4	Torque on large terminal posts
	
	
	

	7.2.5	Clean as required
	
	
	

	7.2.6	Current limiters (Mod 6/1651) for condition and serviceability.
	
	
	

	C 1700.8	27 – FLIGHT CONTROLS

	
8.1	Elevator control quadrants for cleanliness, damage, corrosion and security, bearings for corrosion, cleanliness and security, stops for damage.
	
	
	

	8.2	Rudder trim tab controls for full and free movement, security of attachment at rudder and elevator trim control console.
	
	
	

	8.3	Elevator trim tab controls for full and free movement, security of attachment at rudder and elevator trim control console.
	
	
	

	8.4	Perform the following inspections on flap position cable;
	
	

	8.4.1	Corrosion fraying, kinks, flattening, proper attachment and security.
	
	
	

	8.4.2	Spring for condition, tension and security.
	
	
	

	8.4.3	Indicator for smooth operation.
	
	
	

	8.4.4	Dracon cable cord at window frame.
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8.4.5	Small pulley locations for condition.
	
	
	

	8.5	Perform the following inspections on flap/elevator interconnect trim tab and flap indicator cables;
	
	

	
	
	

	8.5.1	No fraying, condition, corrosion, flattening and security of attachment.
	
	
	

	8.5.2	Pulleys for condition, security and freedom of operation.
	
	
	

	8.5.3	Turnbuckles for security.
	
	
	

	8.6	Perform the following inspections on rudder flight control cables (flight compartment to empennage);

NOTE: In the event of early or abnormal cable wear at pulley(s), replace the worn cable(s) and the corresponding pulley(s).
	
	

	8.6.1	No fraying, corrosion, flattening, proper attachment and security.
	
	
	

	8.6.2	Pulleys for condition and freedom of movement.
	
	
	

	8.6.3	Pulley brackets and guides for condition and security.
	
	
	

	8.6.4	Turnbuckles for security.
	
	
	

	8.7	Perform the following inspections on elevator flight control cables (flight compartment to empennage);

NOTE: In the event of early or abnormal cable wear at pulley(s), replace the worn cable(s) and the corresponding pulley(s).
	
	

	8.7.1	No fraying, corrosion, flattening, proper attachment and security.
	
	
	

	8.7.2	Pulleys for condition and freedom of movement.
	
	
	

	8.7.3	Pulley brackets and guides for condition and security.
	
	
	

	8.7.4	Turnbuckles for security.
	
	
	

	8.8	Perform the following inspections on aileron flight control cables (flight compartment to empennage);

NOTE: In the event of early or abnormal cable wear at pulley(s), replace the worn cable(s) and the corresponding pulley(s).
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8.8.1	No fraying, corrosion, flattening, proper attachment and security.
	
	
	

	8.8.2	Pulleys for condition and freedom of movement.
	
	
	

	8.8.3	Pulley brackets and guides for condition and security.
	
	
	

	8.8.4	Turnbuckles for security.
	
	
	

	8.9	Perform the following inspections on rudder trim tab controls (flight compartment to empennage);
	
	

	8.9.1	Full and free movement.
	
	
	

	8.9.2	Cables for fraying, kinks, corrosion, flattening, proper attachment and security.
	
	
	

	8.9.3	Pulleys for condition and freedom of movement.
	
	
	

	8.9.4	Pulley brackets and guides for condition and security.
	
	
	

	8.9.5	Turnbuckles for security.
	
	
	

	8.10	Perform the following inspections on elevator trim tab controls (flight compartment to empennage);
	
	

	8.10.1	Full and free movement.
	
	
	

	8.10.2	Cables for fraying, kinks, corrosion, flattening, proper attachment and security.
	
	
	

	8.10.3	Pulleys for condition and freedom of movement.
	
	
	

	8.10.4	Pulley brackets and guides for condition and security.
	
	
	

	8.10.5	Turnbuckles for security.
	
	
	

	8.11	Fuselage aileron, elevator and rudder flight control cables.
	
	
	

	8.12	Flap to elevator interconnect tab cables.
	
	
	

	8.13	Flap selector valve and follow up cables
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8.14	All trim tab cables for tensions.
	
	
	

	8.15	Wing root rib/flap pushrod support rollers, lubricate inside of space and bolt.
	
	
	

	C 1700.9	28 – FUEL

	
9.1	Fuel manifold bonding clamp and terminal lug sealant for condition and integrity, peeling, cracking or evidence of corrosion. Inspect bonding jumpers for condition, security, integrity, and corrosion. If damaged, replace component, re-apply sealant.

Effectivity: Mod 6/2389
	
	
	

	
	
	
	

	C 1700.10	32 – LANDING GEAR

	
10.1	Main gear fairings for cracks, delamination and security, seals for tears, deterioration, and security.
	
	
	

	10.2	Nose gear attachment fittings for corrosion and cracks.
Note: Preload bolt torque marks for proper alignment.
	
	
	

	10.3	Landing gear stay struts for cracks, corrosion and security.
	
	
	

	10.4	Main landing gear upper and lower fuselage attachment fittings for condition and security.
	
	
	

	C 1700.11	34 - NAVIGATIONS

	
11.1	Removed. This is on the CALM for the same time frequency.
	
	
	

	C 1700.12	54 – RH NACELLE

	
12.1	Internal structure of wing and nacelle, where accessible, condition, cracks, buckling and corrosion.
	
	
	

	C 1700.13	54 – LH NACELLE

	
13.1	Internal structure of wing and nacelle, where accessible, condition, cracks, buckling and corrosion.
	
	
	

	C 1700.14	55 – LH STABILIZER

	
14.1	Accessible internal structure of horizontal and vertical stabilizer for corrosion, cracks, buckling and security.
	
	
	

	14.2	Horizontal stabilizer outboard hinge arm adapter plate for condition, if applicable.

Effectivity: Pre and Post Mod 6/1799
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14.3	Horizontal stabilizer leading edge skin for condition; dents scores and fasteners for security; and aft of deicing boots, if installed, for surface corrosion.
	
	
	

	14.4	Rudder skin for condition, dents, scores, buckling; leading edge silicon aerodynamic seal for adhesion and security.
	
	
	

	14.5	Rudder lower hinge arm for condition; corrosion and bearing for wear.
Note: As bearing deterioration results in rudder drop this bearing should be replaced when wear is noted. A gap dimension between the lower hinge arm housing and the rudder hinge arm bearing support plate of 0.058 inch (1.47 mm) will indicate that the bearing manufacture's axial service limit has been reached. A smaller gap dimension requires the bearing to be replaced at the earliest opportunity available.

Effectivity: Pre Mod and Mod 6/1340
	
	
	

	
	

	14.6	Elevator skin for condition, dents, scores, buckling; leading edge silicon aerodynamic seal for adhesion and security.
	
	
	

	14.7	Elevator torque tube for condition, corrosion and security of fasteners.
	
	
	

	C 1700.15	57 – WING – LH

	
15.1	Nose spar adapter D nose section for condition; corrosion and fasteners for security; leading edge skin for condition, corrosion and security; hinges for condition and smooth operation of D nose leading edge cover; stay bar for condition and security of stowage.
	
	
	

	15.2	Aileron and flap bellcranks for corrosion and security; bearings for condition. Clean as required.
	
	
	

	C 1700.16	57 – WING – RH

	
16.1	Nose spar adapter D nose section for condition; corrosion and fasteners for security; leading edge skin for condition, corrosion and security; hinges for condition and smooth operation of D nose leading edge cover; stay bar for condition and security of stowage.
	
	
	

	16.2	Aileron and flap bellcranks for corrosion and security; bearings for condition. Clean as required.
	
	
	

	C 1700.17	POST INSPECTION

	
17.1	Inspect for operation and leaks.
	
	
	

	17.2	Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
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17.3	Clean aircraft and engine once maintenance is completed.
	
	
	

	17.4	Perform Functional Check Flight if required per DHC-6-400 Maintenance Manual or AFM as appropriate.
	
	
	

	17.5	Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6 – C 1700NT – 12 Month Inspection and was determined to be in an airworthy condition.


Registration No.: N	End Aircraft S/N:                                     Date:

Aircraft Ending Total Time: Aircraft Ending Total Cycles:


Signature:	Certificate Type & No:
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Registration No.: N                                Start Aircraft S/N:                                      Date:

Aircraft Start Total Time: Aircraft Start Total Cycles:


Reference: DHC-6 Maintenance Program, Viking PSM 1-64-2 Maintenance Manual

	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INTIALS

	
	C 3000.1	GENERAL

	
1.1	Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	1.2	Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3	Replace all life limited components that have completed published operating limits.
	DHC-6-400 MP
	
	

	1.4	Overhaul all components that have completed published operating limits.
	DHC-6-400 MP
	
	

	C 3000.2	PLACARDS AND MARKINGS

	
2.1	Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your airframe.
	
	
	

	C 3000.3	CORROSION CONTROL

	
3.1	Perform corrosion inspection in accordance with the Corrosion Guide PSM 1-6-5, Part 3 on any area’s accessed during this CAMP inspection.
	
Appendix C
	
	

	C 3000.4	PREPARATION

	
4.1	Remove or open all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	C 3000.5	21 – AIR CONDITIONING

	
5.1	Cabin exhaust outlet scoop (on fuselage roof) for condition and security. Clean as required.
	
	
	

	5.2	Heater system outlets for condition and security. Clean as required.
	
	
	

	5.3	Cabin ventilating ducts for condition and security, louvers for proper operation.
	
	
	

	5.4	Flight compartment ventilating ducts for condition and security, louvers for proper operation.
	
	
	

	5.5	Recirculated air flap mechanism for condition and security.
	
	
	



MARITIME HELICOPTERS	DCH-6 MAINTENANCE MANUAL




CHECK: FREQUENCY: NOTE::




C 3000RT – BASIC INSPECTION Every 3000 Hours
This inspection is restricted 50 hours

Page No: Revision: Issue Date:

7-116 Original 05/01/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
5.6	Outside air temperature sensor for security.
	
	
	

	5.7	Bleed air pipes below cockpit floor for condition and security; clamps and brackets for condition, insulation for condition.
	
	
	

	5.8	Bleed air pipes for condition and security; clamps and brackets for condition, insulation for condition.
	
	
	

	5.9	Duct temperature sensor and duct overhead switch for security.
	
	
	

	5.10	Automatic temperature controller for condition and security; mounting brackets for security.
	
	
	

	C 3000.6	22 – AUTO FLIGHT

	
6.1	Autopilot mounting and brackets for condition and security. Clean as required.
	
	
	

	6.2	Pipes for condition and connections for security from solenoid valve to rudder, elevator and pitch trim servo units.
	
	
	

	6.3	HF and VHF transceivers and control units for condition and security of mounting
	
	
	

	6.4	Aileron autopilot servo mounting brackets for condition and security.
	
	
	

	6.5	Autopilot pitch trim servo mounting brackets for condition and security.
	
	
	

	6.6	Elevator servo actuator mounting bracket for condition and security.
	
	
	

	C 3000.7	23 – COMMUNICATIONS

	
7.1	Communication unit cables for condition, connections for security, bonding wire for condition and security. Clean as required.
	
	
	

	C 3000.8	24 – ELECTRICAL POWER

	
8.1	Circuit breaker panel assembly condition and security. Pull out panels and check wiring connection for security. Clean as required.
Note: Refer to A.D. 70-22-04, if applicable.
	
	
	

	8.2	Main distribution box for condition and security, terminals, connectors and relays for condition and security. Clean as required.
	
	
	

	8.3	Overvoltage relay for condition and security. Clean as required.
Effectivity: Pre Mod 6/1590 or 6/1636
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8.4	Generator field control relay for condition and security. Clean as required.

Effectivity: Pre Mod 6/1590 or 6/1636
	
	
	

	
	

	C 3000.9	27 – FLIGHT CONTROLS
	

	
9.1	Remove clevis pin and upper bolts from rudder pedal push rod ends and wheel brake rod ends.
	
	
	

	9.2	Inspect pins, bearings and rod ends for wear.
	
	
	

	9.3	Reinstall clevis pin and upper bolts from rudder pedal push rod ends and wheel brake rod ends.
	
	
	

	C 3000.10	28 – L/H FUEL

	
10.1	Capacitance tank unit inspect for condition and security, wiring connections and leakage.
	
	
	

	C 3000.11	28 – R/H FUEL

	
11.1	Capacitance tank unit inspect for condition and security, wiring connections and leakage.
	
	
	

	C 3000.12	30 – ICE AND RAIN PROTECTION

	
12.1	Propeller deicing timer and for condition and security, connectors for security.
	
	
	

	12.2	Control box for condition and security, connectors for security.
	
	
	

	C 3000.13	31 – INSTRUMENTS

	
13.1	Instrument panel vibration isolators for security.
	
	
	

	C 3000.14	32 – LANDING GEAR

	
14.1	Tail bumper axle and attachments for security, shock absorber pad for deterioration and security of bonding.
	
	
	

	C 3000.15	36 - PNEUMATIC

	
15.1	Removed. No Automatic water drain installed. 
	
	
	

	15.2	Inspect the following pneumatic package system components for condition and security. 
	

	15.2.1	Heat Exchanger.
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REF
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RII INITIALS

	
15.2.2	Pressure Regulator. 
	
	
	

	15.2.3	Service Strainer. (Ref Viking Maintenance Manual 36-10-00 (2) )
	
	
	

	15.2.4	Low pressure warning switch
	
	
	

	C 3000.16	52 – DOORS

	
16.1	Removed, Not installed.
	
	
	

	16.2	 Removed, Not installed.
	
	
	

	C 3000.17	53 - FUSELAGE

	
17.1        Access and inspection panels for condition and security; fasteners for condition and proper operation. Fiberglass panels for cracks and delamination.

NOTE: Does not include MLG leg fairings
	
	
	

	17.2	Hockey stick frames Station 239.88 at cabin floor level for condition, corrosion and fasteners for condition and security. Clean area as required.
	
	
	

	17.3	Cabin and flight compartment bulkheads for condition, equipment stowage and brackets for condition and security.
	
	
	

	17.4	Nose leg lower attachment fittings for condition, corrosion and cracks, fasteners for security.
Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges. Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required.
	
	
	

	17.5	Nose cap back-up structure for condition, corrosion and cracks, fasteners for security.
Effectivity: Pre Mod 6/2020
	
	
	

	17.6	Where accessible, examine aft fuselage horizontal and vertical stabilizer attach frame adapter plates and adjacent structure in the upper frame area for condition and corrosion.
Effectivity: Pre Mods 6/1843, 6/1844, 6/1845 and 6/1846
	
	
	

	17.7	Where accessible, examine aft fuselage horizontal and vertical stabilizer adapter plates and adjacent structure in the upper frame area for condition and corrosion.
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17.8	Inspect the following for cracks, corrosion and security;
Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges. Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required. Corrosion around bonding wires, where fitted, will necessitate cleaning and priming of effected area.
NOTE: Also see figures in PSM 1-6-7, Part 3
	

	17.8.1	Fuselage frame lug Station 219 at wing strut lower attachment area.

NOTE: Also see figures in PSM 1-6-7, Part 3, Figure 9
	
	
	

	17.8.2	Wing strut upper and lower beam area and strut link.

NOTE: Also see figures in PSM 1-6-7, Part 3, Figure 10
	
	
	

	17.8.3	Fuselage forward spar beam Station 200.00 and box structure, fasteners for security.
	
	
	

	17.8.4	Fuselage forward spar Station 200.00 adapters.
	
	
	

	17.9	Remove cabin floor panels
	
	
	

	17.10	Inspect sub floors (Fuel Cells) for condition and security.
	
	
	

	17.11	Reinstall cabin floor panels (OK to close)
	
	
	

	17.12	Removed, not installed.
	
	
	

	17.13	Removed, inspection duplicated. See 17.2
	
	
	

	C 3000.18	54 – L/H NACELLE

	
18.1	Firewall for condition, buckling and cracks and fasteners for security.
	
	
	

	C 3000.19	54 – R/H NACELLE

	
19.1	Firewall for condition, buckling and cracks and fasteners for security.
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	C 3000.20	55 – STABILIZERS

	
20.1	Inspect the vertical stabilizer as follows;
	

	20.2	Mid hinge arm adapter fitting for condition, corrosion and security.
Effectivity: Mod 6/1339
	
	
	

	20.3	Top hinge arm adapter fitting for condition, corrosion and security.
Effectivity: Mod 6/1339
	
	
	

	20.4	Where accessible, examine the vertical stabilizer forward and aft spar lower adapter plates (Mods 6/1841 and 6/1842) and adjacent structure for condition, corrosion, and fasteners for security. Check bolt torque.
Effectivity: Mod 6/1840 and 6/1842
	
	
	

	20.5	Inspect the rudder as follows for condition, corrosion and security;
	

	20.5.1	Mid hinge arm
Effectivity: Mod 6/1340
	
	
	

	
	

	20.5.2	Upper hinge arm
	
	
	

	20.5.3	Mid hinge arm adapter fitting
	
	
	

	20.5.4	Upper hinge arm adapter fitting
	
	
	

	20.6	Inspect the elevator as follows for condition, corrosion and security, bearings for condition;
	

	20.6.1	Mid hinge arm adapter fitting
Effectivity: Mod 6/1342
	
	
	

	
	

	20.6.2	Outer hinge arm adapter fitting
Effectivity: Mod 6/1342
	
	
	

	20.6.3	Root rib
Effectivity: Mod 6/1769
	
	
	

	
	

	20.6.4	Mid hinge arm
Effectivity: Mod 6/1342
	
	
	

	
	

	20.6.5	Outer hinge arm
NOTE: All hinge arms for evidence of corrosion around bolt holes requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required.
Effectivity: Mod 6/1342 and 6/1799
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20.7	Fairings, access covers, inspection panels for proper fit, damage and security, fasteners for damage and proper operation and security, fiberglass panes for cracks and delamination.
	
	
	

	C 3000.21	57 – L/H WING

	
21.1	Wing fairings and access panels for proper fit, damage and security, fasteners for damage and proper operation and security, fiberglass panes for cracks and delamination.
	
	
	

	21.2	Wing rear spar cap for condition, cracking, bush and fasteners for security.

Effectivity: Mod 6/1301
	
	
	

	21.3	Wing to fuselage forward steel adapters for condition and security.

Effectivity: Mod 6/1887 AMD EO69080-1/2
NOTE: Refer to TAB 678/6
	
	

	
	
	
	

	21.4	Wing main hinge arms for cracks, wear and corrosion.

Effectivity: Mod 6/1334
Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges. Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required. Corrosion around bonding wires, where fitted, will necessitate cleaning and priming of effected area.
	
	
	

	21.5	Flap hinge arm attachment for condition, corrosion and security.
Effectivity: Mod 6/1335
	
	
	

	
	

	21.6	Inboard and outboard foreflap hinge arms for condition, corrosion and security and bearing for security.
Effectivity: Mod 6/1336 and 6/1349
	
	
	

	
	

	21.7	Inboard trailing flap hinge arms for condition, corrosion and security and bearing for security.
Effectivity: Mod 6/1337
	
	
	

	21.8	 Wing strut link for condition, corrosion, bush for security. Effectivity: Mod 6/1174
	
	
	

	C 3000.22	57 – R/H WING

	
22.1	Wing fairings and access panels for proper fit, damage and security, fasteners for damage and proper operation and security, fiberglass panes for cracks and delamination.
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22.2	Wing rear spar cap for condition, cracking, bush and fasteners for security.

Effectivity: Mod 6/1301
	
	
	

	
	

	22.3	Wing to fuselage forward steel adapters for condition and security.

Effectivity: Mod 6/1887 AMD EO69080-1/2 NOTE: Refer to TAB 678/6
	
	
	

	22.4	Wing main hinge arms for cracks, wear and corrosion.

Effectivity: Mod 6/1334
Note: Pay particular attention to immediate area around bolt holes and bearings, where visible, and along attachment and pickup fittings mating edges. Evidence of corrosion at areas indicated above requires removal of bolts for internal examination of holes and condition of bolts. Evidence of internal corrosion will necessitate disengaging fitting for further inspection and treatment as required. Corrosion around bonding wires, where fitted, will necessitate cleaning and priming of effected area.
	
	
	

	22.5	Flap hinge arm attachment for condition, corrosion and security.
Effectivity: Mod 6/1335
	
	
	

	
	

	22.6	Inboard and outboard foreflap hinge arms for condition, corrosion and security and bearing for security.
Effectivity: Mod 6/1336 and 6/1349
	
	
	

	22.7	Inboard trailing flap hinge arms for condition, corrosion and security and bearing for security.
Effectivity: Mod 6/1337
	
	
	

	
	

	C 3000.23	61 -L/H PROPELLERS

	
23.1	Propeller Auto Feather system relay box for security of mounting, bonding wire for security. Clean as required.
NOTE: Refer to Service Bulletin No. 6/297 and A.D. 73-19-01, if applicable
	
	
	

	23.2	Removed, not installed on 400 series.
Effectivity: Pre Mod 6/2014
	
	
	

	C 3000.24	61 -R/H PROPELLERS

	
24.1	Propeller Auto Feather system relay box for security of mounting, bonding wire for security. Clean as required.
NOTE: Refer to Service Bulletin No. 6/297 and A.D. 73-19-01, if applicable
	
	
	

	24.2	Removed, not installed on 400 series.
Effectivity: Pre Mod 6/2014
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	C 3000.25	71 – L/H POWER PLANT

	
25.1	Generator cooling duct for condition and security.
	
	
	

	C 3000.26	76 – R/H POWER PLANT

	
26.1	Generator cooling duct for condition and security.
	
	
	

	C 3000.27	76 – L/H ENGINE CONTROLS

	
27.1	Engine control pulley brackets for condition and security.
	
	
	

	C 3000.28	76 – R/H ENGINE CONTROLS

	
28.1	Engine control pulley brackets for condition and security.
	
	
	

	C 3000.29	79 – L/H OIL

	
29.1	Remove oil cooler
	
	
	

	29.2	Pressure test.
	
	
	

	29.3	Reinstalled oil cooler
	
	
	

	C 3000.30	79 – R/H OIL

	
30.1	Remove oil cooler
	
	
	

	30.2	Pressure test.
	
	
	

	30.3	Reinstalled oil cooler
	
	
	

	C 3000.31	OPERATIONAL CHECKS

	
31.1	Bleed air heating system. Power on.
	
	
	

	31.2	Pitot system.
	
	
	

	31.3	Flight control surfaces for alignment with external rigging marks; for rudder check dimension ‘L’.
	
	
	

	31.4	All trim and gear tabs for free play.
	
	
	

	31.5	Fuel forward and aft low level warning system. Adjust tank levels to obtain indication. Power on.
	
	
	

	31.6	Rudder gear box for play.
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31.7	Intake deflector system. Power on.
	
	
	

	31.8	Main fuel quantity indicating system (calibration).
	
	
	

	31.9	Propeller deicing timer.
	
	
	

	31.10	Pneumatic system pressure test.
	
	
	

	C 3000.32	POST INSPECTION

	
32.1	Inspect for operation and leaks.
	
	
	

	32.2	Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	32.3	Clean aircraft and engine once maintenance is completed.
	
	
	

	32.4	Perform Functional Check Flight if required per DHC-6-400 Maintenance Manual or AFM as appropriate.
	
	
	

	32.5	Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-6-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC-6-400 – C 3000RT – 3000 Hour Inspection and was determined to be in an airworthy condition.


Registration No.: N	End Aircraft S/N:                                     Date:

Aircraft Ending Total Time: Aircraft Ending Total Cycles:


Signature:	Certificate Type & No:
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Registration No.: N                                Start Aircraft S/N:                                      Date:

Aircraft Start Total Time: Aircraft Start Total Cycles:


Reference: DHC-6 Controlled Inspection Program

	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INTIALS

	
	CT 6000.1	26 – FIRE PROTECTION

	
1.1	Fire detecting thermal units.
	
	
	

	CT 6000.2	27 – FLIGHT CONTROLS

	
2.1	Flap actuator (pressure test).
	
	
	

	2.2	Flap selector valve (pressure test).
	
	
	

	CT 6000.3	29 – HYDRAULIC POWER

	
3.1	Hydraulic system accumulators.
	
	
	

	3.2	Hydraulic (electric-driven) pump.
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Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection/test form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have tested all the items initialed by me in accordance with Maritime Helicopters DHC-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC- 6 – CT 6000NT – 6000 Hour Inspection/Test and was determined to be in an airworthy condition.


Registration No.: N	End Aircraft S/N:                                     Date:

Aircraft Ending Total Time: Aircraft Ending Total Cycles:


Signature:	Certificate Type & No:
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CHECK: FREQUENCY: NOTE::


7.5	FUNCTIONAL CHECKS

Page No: Revision: Issue Date:
F 3000NT – FUNCTIONAL CHECKS Every 3000 Hours
Bench Test – Component removed from aircraft. No Tolerance

7-128 Original 05/01/20



Registration No.: N                                Start Aircraft S/N:                                      Date:

Aircraft Start Total Time: Aircraft Start Total Cycles:


Reference: DHC-6 Maintenance Program

	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INTIALS

	
	F 3000.1	21 – AIR CONDITIONING

	
1.1	Bleed air heating system. Power on.
	
	
	

	F 3000.2	27 – FLIGHT CONTROLS

	
2.1	Flight control surfaces for alignment with external rigging marks; for rudder check dimension ‘L’.
	
	
	

	2.2	All trim and gear tabs for free play.
	
	
	

	2.3	Rudder gear box for play.
	
	
	

	F 3000.3	28 – FUEL

	
3.1	Fuel forward and aft low-level warning system. Adjust tank levels to obtain indication. Power on.
	
	
	

	3.2	Main fuel quantity indicating system (calibration).
	
	
	

	F 3000.4	30 – ICE AND RAIN PROTECTION

	
4.1	Propeller deicing timer.
	
	
	

	F 3000.5	34 - NAVIGATION

	
5.1	Pitot system.
	
	
	

	F 3000.6	36 - PNEUMATIC

	
6.1	Pneumatic system pressure test.
	
	
	

	F 3000.7	71 – POWERPLANT - LH

	
7.1	Intake deflector system. Power on.
	
	
	

	F 3000.8	71 – POWERPLANT - RH

	
8.1	Intake deflector system. Power on.
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Page No: Revision: Issue Date:
F 3000NT – FUNCTIONAL CHECKS Every 3000 Hours
Bench Test – Component removed from aircraft. No Tolerance

7-129 Original 05/01/20


Upon satisfactory completion of each test item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each function test, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have function tested all the items initialed by me in accordance with Maritime Helicopters DHC-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this function tests form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft components have been tested in accordance with Maritime Helicopters’ DHC- 6 – F 3000NT – 3000 Hour Functional Tests and was determined to be in an airworthy condition.


Registration No.: N	End Aircraft S/N:                                     Date:

Aircraft Ending Total Time: Aircraft Ending Total Cycles:


Signature:	Certificate Type & No:
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8	POWERPLANT INSPECTIONS


The followingPowerplant inspections shall be performed in conjunctionwith Maritime Helicopters CAMP General Manual and applicable Pratt & Whitney Maintenance Manuals as listed.
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CHECK: FREQUENCY: NOTE::


8.1	INSPECTIONS



P 0100 – ENGINE INSPECTION EVERY 100 HOURS   

Page No: Revision: Issue Date:

8-2 Original 05/01/20



Registration No.: N Aircraft S/N: Engine S/N:

Start                             Aircraft Start Total Time: Date:                             Engine Start Total Time: Engine Start Total Cycles:

	         	

Reference: DHC - 6 PSM 1-65-2 MM, Pratt & Whitney PT6A-34 MM

	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	P 0100.1	GENERAL

	
1.1	Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	1.2	Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3	Replace all life limited components that have completed published operating limits.
	Pratt & Whitney PT6A MM
	
	

	1.4	Overhaul all components that have completed published operating limits.
	Pratt & Whitney PT6A MM
	
	

	P 0100.2	PLACARDS AND MARKINGS

	
2.1	Examine the placards, decals, and markings in engine area. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your aircraft.
	
	
	

	P 0100.3	CORROSION CONTROL

	
3.1	Perform a visual corrosion inspection on any area’s access during this CAMP inspection.
	
	
	

	P 0100.4	ENGINE EXTERNALS

	
4.1	Inspect the following on all tubing, wiring, control linkages, hoses assemblies;
NOTE: Pay particular attention to rear linkage cam box, fuel control unit arm, telescopic rod and rod end fittings.
	
	
	

	4.1.1	All accessible connections, clamps and brackets for attachment.
	
	
	

	4.1.2	Accessible lockwire and safety cable for security and installation.
	
	
	

	4.1.3	Wear, chafing, cracks and corrosion.
	
	
	

	4.1.4	Fuel and oil lines for leaks.
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CHECK: FREQUENCY: NOTE::




P 0100 – ENGINE INSPECTION EVERY 100 HOURS

Page No: Revision: Issue Date:

8-3 Original 05/01/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
4.1.5	All insulated air tubes for sign of swelling, cracking, bulging of rubber sheath material. Refer to repair section and SB1687. Replace as necessary.
	
	
	

	4.1.6	Disconnect rod ends and clean using solvent (PWC11-027) or (PWC11-031).
	
	
	

	4.1.7	Examine rod end for corrosion, roughness in rotation, side play and radial play.
	
	
	

	4.1.8	Lubricate with light grease (PWC04-001) after engine external wash.
	
	
	

	4.1.9	After lubrication reinstall rod ends and torque to specified value.
	76-10-00
	
	

	4.1.10	Check free movement of linkage.
	
	
	

	4.1.11	Cleanliness of air inlet screen.
	72-20-00
	
	

	4.1.12	Gas generator case external surfaces and fire seal mount ring brackets for cracks, distortion and corrosion
	72-30-04
	
	

	4.1.13	Fire seal mount rings for cracks and attachment of brackets and seals.
	72-30-01/-02
	
	

	4.1.14	Exhaust duct for cracks and distortion.
	72-50-05 Maintenance Practices
	
	

	4.1.15	Propeller shaft seal for oil leaks.
	72-10-00
	
	

	4.1.16	Accessories attachment and linkages, air, oil and fuel lines.
	73-10-07/ -08
	
	

	P 0100.5	ENGINE INTERNALS

	
5.1	Perform a visual inspection with a mirror or a borescope of the first stage compressor rotor.
NOTE: If any FOD has caused the engine to become prone to engine surges or causes unusual compressor whining, the large bent airfoil will make the whining sound, remove the engine immediately. Fig 602
	
Para. 9.D.
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Revision: Issue Date:

TEMP REV #1 07/13/20



TEMPORARY REVISION #1

INSTRUCTIONS

1. This Temporary Revision #1 updates the P 0100 inspection.
2. Place this instruction page front of Page 8-4 of the current A P 0100 inspection. 3. Replace Page 8-4 with Temp Rev #1 page revision attached.
4. Comply with all other inspections of the P 0100 inspection as required.

CAUTION: DO NOT REMOVE THIS TEMPORARY UPDATE UNTIL INSTRUCTED TO DO SO AS PART OF:

- A NORMAL UPDATE
- A NEW TEMPORARY REVISION UPDATE SUPERSEDING THIS ONE

DESCRIPTION

1.	This revision updates the P 0100 inspection item 6.3 by removing the oil filter requirement as it is already C/W in A 0125.17 – L/H and A 0125.18 – R/H.

INCORPORATION

Temporary Revision #1 to the P 0100 Power Plant inspection. Inspection Page 8-4, item 6.3 will be removed in the CAMP as part of the next normal revision.
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P 0100 – ENGINE INSPECTION EVERY 100 HOURS

Page No: Revision: Issue Date:

8-4
Temp Rev #1 07/13/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	P 0100.6	SYSTEMS

	
6.1	Check oil level.
	
SERVICING
	
	

	6.2	Check condition and locking of oil filler cap.
	72-60-00
	
	

	6.3	Perform a visual inspection of the fuel pump


NOTE: If airframe fuel boost pump fails or is inadvertently left off for an accumulative time in excess of 10 hours, the engine driven fuel pump must be removed and replaced. The removed pump should be sent to an approved overhaul facility.
	
	
	

	
	
	
	

	6.4	Check scavenge oil pump housing for leaks
	
	
	

	6.5	Perform a visual inspection of the fuel pump for installation and leakage.
	72-10-02 Fuel Pump
Maint Pract
	
	

	6.6	Inspect outlet filter for foreign matter or distortion.
	73-10-02
	
	

	6.7	Check drain valve for installation and leaks.
	73-10-06
	
	

	6.8	Inspect FCU for installation, linkages and pneumatic tubes.
	73-20-00
	
	

	6.9	 Examine the FCU for bearing washout, shown by blue dye (grease and fuel mixed) at FCU vent.
	Fault Iso Operating Problems
	
	

	6.10	Check starting flow control/flow divider for installation and leaks.
	73-10-04
	
	

	6.11	Check oil-to-fuel heater installation.
	73-10-00 Ign Exciter Maint Pract
	
	

	6.12	Check P3 filter for installation.

NOTE: Visually inspect the P3 filter for corrosion. If the filter shows presence of corrosion, discard the filter and replace with a new filter.
	

73-10-07
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CHECK: FREQUENCY: NOTE::




P 0100 – ENGINE INSPECTION EVERY 100 HOURS

Page No: Revision: Issue Date:

8-5 Original 05/01/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
6.14	Inspect pneumatic tubes and lines for cracks and damages especially at the end fittings and joints.
	
	
	

	6.15	Redundant, see 6.12
	
	
	

	6.16	Not installed.
	
	
	

	P 0100.7	POST INSPECTION

	
7.1	Inspect for operation and leaks.
	
	
	

	7.2	Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	7.3	Perform Functional Check Flight if required per PT6A Maintenance Manual or AFM as appropriate.
	
	
	

	7.4	Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	



MARITIME HELICOPTERS	DCH-6 MAINTENANCE MANUAL




CHECK: FREQUENCY: NOTE::




P 0100 – ENGINE INSPECTION EVERY 100 HOURS

Page No: Revision: Issue Date:

8-6 Original 05/01/20


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC- 6 – P 0100 – 100 Hour Powerplant Inspection and was determined to be in an airworthy condition.


Registration No.: N Aircraft S/N: Engine S/N:

Start                             Aircraft Start Total Time: Date:                             Engine Start Total Time: Engine Start Total Cycles:


Signature:	Certificate Type & No:
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CHECK: FREQUENCY: NOTE::




P 0400 – ENGINE INSPECTION EVERY 400 HOURS

Page No: Revision: Issue Date:

8-7 Original 5/1/20



Registration No.: N Aircraft S/N: Engine S/N:

Start                             Aircraft Start Total Time: Date:                             Engine Start Total Time: Engine Start Total Cycles:


Reference: DHC - 6 PSM 1-65-2 MM, Pratt & Whitney PT6A-34 MM

	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
	P 0400.1	GENERAL

	
1.1	Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	1.2	Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	1.3	Replace all life limited components that have completed published operating limits.
	Pratt & Whitney PT6A MM
	
	

	1.4	Overhaul all components that have completed published operating limits.
	Pratt & Whitney PT6A MM
	
	

	P 0400.2	PLACARDS AND MARKINGS

	
2.1	Examine the placards, decals, and markings in engine area. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your aircraft.
	
	
	

	P 0400.3	CORROSION CONTROL

	
3.1	Perform a visual corrosion inspection on any area’s access during this CAMP inspection.
	
	
	

	P 0400.4	INSPECTIONS

	
4.1	Check magnetic chip detector(s) for continuity, open circuit must exist indicating no contamination at pole tips. If continuity is there, remove and examine for contamination. Any foreign material found on the chip detector or in the main oil filter must be identified before further inspection/operation.
	
79-20-02 Oil Filter Housing and Check Valve NOTE 3
	
	

	4.2	Perform a deceleration check.

Effectivity: Post-SB1568
	71-00-00 Power Plant
Adj Test
	
	

	4.3	Examine the ignition exciter/current regulator for installation and condition.
	74-10-00

Ign/Exciter Maintenance Practices
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CHECK: FREQUENCY: NOTE::




P 0400 – ENGINE INSPECTION EVERY 400 HOURS

Page No: Revision: Issue Date:

8-8 Original 5/1/20



	
MAINTENANCE ACTION
	
REF
	
MECH INITIALS
	
RII INITIALS

	
4.4	Examine the ignition cables for chafing, wear and installation.
	
	
	

	4.5	Examine the spark igniters for cleanliness and erosion.
	74-20-00
	
	

	4.5.1	Perform a functional check.
	Cables & Spark Ignig Maint Pract
	
	

	P 0400.5	POST INSPECTION

	
5.1	Inspect for operation and leaks.
	
	
	

	5.2	Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	5.3	Perform Functional Check Flight if required per Pratt & Whitney PT6A Maintenance Manual or AFM as appropriate.
	
	
	

	5.4	Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
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P 0400 – ENGINE INSPECTION EVERY 400 HOURS

Page No: Revision: Issue Date:

8-9 Original 5/1/20


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided. All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form. The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
INITIALS
	
SIGNATURE
	
CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC- 6 – P 0400 – 400 Hour Powerplant Inspection and was determined to be in an airworthy condition.


Registration No.: N Aircraft S/N: Engine S/N:

Start                             Aircraft Start Total Time: Date:                             Engine Start Total Time: Engine Start Total Cycles:


Signature:	Certificate Type & No:
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A	AIRWORTHINESS LIMITATIONS

NOTE: The entire airframe must be removed from service at or before the end of the validated life at 66,000 flight Hours, or 312,000 Flight Cycles, whichever occurs first.

AIRFRAME

A.1 Compliance of all Airworthiness Inspections must be completed by the limits specified in the below table. Each inspection shall be entered either in a work order orthe aircraft log book as appropriate and remaina permanent record until repeated.

A.2 The appropriate maintenance manual shall be referenced when performing each event.

	

TASK
	
ITEM

DESCRIPTION
	
EFFECTIVITY/

CONFIGURATION
	AIRWORTHINESS LIMITATIONS
	
ACTION

NOTES

	
	
	
	SAFE LIFE LIMIT EXCEPTIONS FROM AIRFRAME LIMIT
	

MODIFICATION LIMIT
	INSPECTION OR OVERHAUL
	

	
	
	
	
	
	

INITIAL
	

REPEAT
	



	
32 – FLIGHT CONTROLS

	
27-002
	Elevator and Rudder Primary Flight Control Cables
	
Landplanes
	
60 Months
	
-
	
-
	
-
	
Replace

	

27-004
	Elevator and Rudder Primary Flight Control Cables below Baggage Floor
	
All Configurations If spillage occurs when operating with
corrosive cargo
	
Within 2 Months of spillage
	

-
	

-
	

-
	

Replace

	
27-006
	
Aileron Primary Flight
Control Cables
	
All Configurations
	
60 Months
	
-
	
-
	
-
	
Replace

	
27-007
	Elevator and Rudder
Cable Pulleys at Sta 270.3
	
All Configurations
	
60 Months
	
-
	
-
	
-
	
Replace

	32 – LANDING GEAR

	

32-001
	

Main Landing Gear Leg
	All Configurations with New Main Landing Gear Leg with No Previous Overhaul and No Previous Repair
	

Safe Life Limit Not Applicable
	

-
	24,000 Landings or 120 Months whichever occurs first
	

-
	Remove Overhaul in accordance with TB V6/00063 Rev. NC or later

	

32-002
	

Main Landing Gear Leg
	
All Configurations with Previous Overhaul or Previous Repair
	

Safe Life Limit Not Applicable
	

-
	
	7,000 Landings or 60 Months whichever occurs first
	Remove Overhaul in accordance with TB V6/00063 Rev. NC or later
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TASK
	
ITEM

DESCRIPTION
	
EFFECTIVITY/

CONFIGURATION
	AIRWORTHINESS LIMITATIONS
	
ACTION

NOTES

	
	
	
	SAFE LIFE LIMIT EXCEPTIONS FROM AIRFRAME LIMIT
	

MODIFICATION LIMIT
	INSPECTION OR OVERHAUL
	

	
	
	
	
	
	

INITIAL
	

REPEAT
	

	
53 – FUSELAGE

	




53-005
	


Fuselage Frame Assembly, Sta. 218.8, Part No.
C6FSM2582–1
	




Post Mod 6/1173
	




-
	


39,000 Flight Hours or 78,000 Flight Cycles whichever occurs first
	




-
	




-
	Remove this frame assembly from service and replace with a new assembly
C6MK1553–1 or –3 Incorporating Mod 6/1553 (Refer to SB 6/354)

	
53 – FUSELAGE (Cont’d)

	




53-006
	



Fuselage Frame Assembly, Sta. 239
	




All Configurations
	




-
	




-
	



1,200 Flight Hours or 12 Months whichever occurs first
	


Every 1,200 Flight Hours or
12 Months whichever occurs first
	If cracks are within limits in accordance withSB 6/521 Rev. C or later, inspect
every 600 Flight Hours or 6 Months whichever
occurs first. Replace or repair if cracks are out of limits.

	
54 – NACELLES

	

54-002
	

Engine Nacelle Structure
	

All Configurations
	

-
	

-
	
3,000 Flight Hours or 6,000 Flight Cycles whichever occurs first
	Every 3,000 Flight Hours or
6,000 Flight Cycles whichever occurs first
	Inspect the left side of each nacelle structure (Referto PSM 1-6-7 Part 3)

	

54-009
	

Engine Nacelle Lower Longerons
	
Aircraft that are not addressed by 54-003 through 54-008
	

-
	

-
	

400 Flight Hours
	

Every 400 Flight Hours
	Inspect lower longerons for buckles or cracks on each nacelle structure (Refer to SB 6/509)

	

54-010
	

Engine Nacelle Lower Longerons
	

All Configurations After Hard Landing
	

-
	

-
	

Immediate
	

Immediate
	Inspect lower longerons for buckles or cracks on each nacelle structure (Refer to SB 6/509)
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TASK
	
ITEM

DESCRIPTION
	
EFFECTIVITY/

CONFIGURATION
	AIRWORTHINESS LIMITATIONS
	
ACTION

NOTES

	
	
	
	SAFE LIFE LIMIT EXCEPTIONS FROM AIRFRAME LIMIT
	

MODIFICATION LIMIT
	INSPECTION OR OVERHAUL
	

	
	
	
	
	
	

INITIAL
	

REPEAT
	

	
57 – WINGS

	

57-026
	Wing Assembly C6W1001–33, –35, & subsequent Wing Box C6W1002–67, –69, & subsequent
	Post Mod 6/1117 and
Pre Mod 6/1630 and
Pre Mod 6/1318
	

-
	
12,000 Flight Hours or 24,000 Flight Cycles
	

-
	

-
	
Incorporate Mod 6/1318 (Refer to SB 6/268)

	

57-027
	Wing Assembly C6W1001–33, –35, & subsequent Wing Box C6W1002–67, –69, & subsequent
	
Post Mod 6/1117 and
Pre Mod 6/1630 and
Pre Mod 6/1318
	

-
	

-
	12,000 Flight Hours or 24,000 Flight Cycles whichever occurs first
	Every 1,200 Flight Hours or
2,400 Flight Cycles whichever occurs first
	Inspect Main Spar at Station 152.8 (Refer to PSM 1-6-7 Part 3)

	
57 – WINGS (Cont’d)

	

57-029
	Wing Assembly C6W1001–33, –35, & subsequent Wing Box C6W1002–67, –69, & subsequent
	
Post Mod 6/1117 and
Pre Mod 6/1630
	33,000 Flight Hours or 66,000 Flight Cycles whichever occurs first
	

-
	

-
	

-
	Incorporate Mod 6/1630 to extend service life (Refer to SB 6/362)

	

57-030
	
C6W1002– Replacement Box (Replaces 67, –69, & subsequent
	Post Mod 6/1117 and when installed into C6W1001 as part of Mod 6/1630 and
Pre Mod 6/1318
	

-
	
12,000 Flight Hours or 24,000 Flight Cycles
	

-
	

-
	
Incorporate Mod 6/1318 (Refer to SB 6/268)

	

57-031
	
C6W1002– Replacement Box (Replaces 67, –69, & subsequent
	
Post Mod 6/1117 and when installed into C6W1001 as part of Mod 6/1630
	

-
	

-
	12,000 Flight Hours or 24,000 Flight Cycles whichever occurs first
	Every 1,200 Flight Hours or
2,400 Flight Cycles whichever occurs first
	Inspect Main Spar at Sta. 152.8 (Refer to PSM 1-6-7 Part 3)

	



57-032
	


C6W1002– Replacement Box (Replaces 67, –69, & subsequent
	


Post Mod 6/1117 and when installed into C6W1001 as part of Mod 6/1630
	



-
	



-
	

24,000 Flight Hours or 48,000 Flight Cycles whichever occurs first
	

Every 1,200 Flight Hours or
2,400 Flight Cycles whichever occurs first
	Inspect Lwr Skin at WS185, Lwr Wing Skin, Stringers and Aft Spar Lwr Flange from WS122 to WS263
(ribs 8 to 20) (Refer to PSM 1-6-7 Part 3)

	

57-033
	

Wing Assembly C6W1001–33, –35 & subsequent
	

Post Mod 6/1117 and
Post Mod 6/1630
	66,000 Flight Hours or 132,000 Flight Cycles whichever occurs first
	

-
	

-
	

-
	

-
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TASK
	
ITEM

DESCRIPTION
	
EFFECTIVITY/

CONFIGURATION
	AIRWORTHINESS LIMITATIONS
	
ACTION

NOTES

	
	
	
	SAFE LIFE LIMIT EXCEPTIONS FROM AIRFRAME LIMIT
	

MODIFICATION LIMIT
	INSPECTION OR OVERHAUL
	

	
	
	
	
	
	

INITIAL
	

REPEAT
	

	
57 – WINGS (Cont’d)

	






57-037
	





Wing Strut Assembly C6W1005–9, –10 Link Assembly C6WM1409–1, –3
	





Post Mod 6/1172 and
Post Mod 6/1174
	




36,000 Flight Hours or 72,000 Flight Cycles whichever occurs first
	






-
	






-
	






-
	Remove these wing strut and link assemblies, including all attachment bolts,
from service and replace with new parts C6W1005–9, and –10 (strut), C6WM1409–3 (link), and attachment bolts C6WM1411–27 (one per strut) and –29
(two per strut)

	

57-038
	
Wing Flap Hinge Arm
Attachment Fittings at
Wing Sta. 97.5
	
Landplanes and Floatplanes that have been used in Landplane configuration
	

-
	

-
	
31,800 Flight Hours or 63,600 Flight Cycles whichever occurs first
	Every 2,400 Flight Hours or
4,800 Flight Cycles whichever occurs first
	Inspections of the lower attachment fittings C6W1045 (Refer to PSM 1-6-7)

	
57-041
	Wing Upper Surface Inspection for Disbonding
	
All Configurations
	
-
	
-
	
20 years
	
Every 5 years
	
As per SB V6/0018
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POWERPLANT


	
PT6A-34

	
Part Number
	
ITEM DESCRIPTION
	
Time Before Overhaul (TBO)
	
Service Life Limit Cycles
	
Notes

	
3031700
	
Hot End Inspection HSI
	
2000 Hours*
	
	
*Inspection Only

	
3031700
	
Hot End Inspection HSI
	
4000 Hours
	
	

	
3019712
	
Power Turbine Disk
	
	
20000
	

	
3013111
	
Compressor Hub (1st Stage)
	
	
19000
	

	
3013712
	
Compressor Disk (2nd Stage)
	
	
24000
	

	
3011713
	
Compressor Disk (3rd Stage)
	
	
25000
	

	
3033292
	
Impeller
	
	
19000
	

	
3013411
	
CompressorTurbine Disk
	
	
16000
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POWERPLANT (Cont’d)

	
PT6A-34

	
	
ITEM DESCRIPTION
	
Time Before Overhaul (TBO)
	
	

	
	
Fuel Control Unit (FCU)
	
4500
	
	

	
	
Fuel Heather
	
4500
	
	

	
	
PropellerGovernor
	
4500
	
	

	
	
Ignition Exciter
	
4500
	
	

	
	
Compressor Bleed Valve
	
4500
	
	

	
	
Flow Divider/Starting Control Installation
	
4500
	
	

	
	
Fuel Pump (Argo-Tech only)
	
4500
	
	

	
	
Fuel Pump (Hamilton Sundstrand)
	
4000
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AVIONICS

Table 1 identifies Airworthiness Limitations (AWL’s) based on associated Critical Design Configuration Control Limitations (CDCCL’s) for the Avionics Systems of the DHC-6 Series 400 aircraft with the Phase 2 Avionics Upgrade.

Note; Phase 2 aircraft (including Super-Lite aircraft) must embody MOD 6/2303 (refer to Table 1 and Table 2). Irrespective of other Apex and avionics options and installations, any aircraft with Apex Load 4.4 software is a “Phase 2” aircraft and any aircraft with S.O.O. 6388 is a Super-Lite aircraft.

Note; Compliance with Airworthiness Limitations is mandatory.

Table 1 – Phase 2 Airworthiness Limitations Including Conditions of Design Approval
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B	CORROSION CONTROL

B.1	This corrosion control program to fulfill PSM 1-6-5, Part 3, CorrosionManual requirements over a 5-year period

[image: ]B.2	Inspections shall be entered in theWork Order or aircraft log book as applicable when each even is complied with. Each inspection year will be tracked under the aircraft maintenance CALM program.
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Identifier

‘Affected System

Description

Remarks

General

GEN-DD1

“All Avirics
Systems.

For purposes of the
avionics uparades, the
DHC'6 Series 400
Class IV aicraftin the
meaning of FAA Advisory
Circular (AC) 23.1309-1E.
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Identifier ‘Affected System Description Remarks
AFCS008 Gear Configuration | FD and AP use has been | The Amphibious Float and Seaplane
evalusted on Wigine Float STC hoiders are responsble for
Model 13000 Amphibious | ensuring that STC documents are:
Float airraft modified i | updated to reflect operating
‘accordance with TCCA | procedures and imitations
STC SAT1.7 or SAS3-103 | appropriate o FD and AP use with
of FAASTC SAZCH_FD | Amphibious Floats or Seaplane
and AP have been Floats installed
determined o be
‘compatibie with s gear
configuration and with
‘Seaplane Floals subject o
‘approprate operating
procedures and imitations.
Transponders and ADS-B Out
TRE001 Transponder | Transponders mustbe | Honeywell KXP 2280 and
Configuration | KXP 22904 f ADS-B Out | KXP 2290 fransponders are elgibe
functionalfy s enabled on | for Phase 2 and Super Lie afcraft
Apex. instalation. Installation of the ADS-B
Out enabled KXP 2290A
ransponders s thiough MOD
612354, The enabiing of ADS-5 Out
functonaity through Apex is
controlled thiough S.0.0. 6347.
For Phase 2 afcraft and for Super-
Lie aifcraft wih two transponders,
both nstaled transponder LRU's
must be KXP 22904 for ADS-B Out
functonaity. Ming IO 2290 and
1OXP 22904 configuration &
protibited
For Super.Lite airraft with just one
transponder, the nstalied
transponder LRU must be XP
'2290A i ADS™B Out functionly s
enabled.
Teasn
TeAs 001 TCASIRA | Phase 2 aircraftand Phase 1 aircraft with Apex Load 13
Configuration | Super e airraft ‘equipped with TCAS Il had only

‘quipped with optonal
TCAS Il musthave the
TCAS Il Resolution
‘Advisory (RA)functionaity
enabed

Phase 2 aircraft TCAS Il
hardware instalation with
only TCAS | functionality
enabled is prohibited.

‘Trafic Advisory (TA) functoniy
‘enabled, RA functionaity was
disabled
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‘Affected System

Description

Remarks

General

GEN-DD1

“All Avirics
Systems.

For purposes of the
avionics uparades, the
DHC'6 Series 400
Class IV aicraftin the
meaning of FAA Advisory
Circular (AC) 23.1309-1E.
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Identifier ‘Affected System Description Remarks
AFCS008 Gear Configuration | FD and AP use has been | The Amphibious Float and Seaplane
evalusted on Wigine Float STC hoiders are responsble for
Model 13000 Amphibious | ensuring that STC documents are:
Float airraft modified i | updated to reflect operating
‘accordance with TCCA | procedures and imitations
STC SAT1.7 or SAS3-103 | appropriate o FD and AP use with
of FAASTC SAZCH_FD | Amphibious Floats or Seaplane
and AP have been Floats installed
determined o be
‘compatibie with s gear
configuration and with
‘Seaplane Floals subject o
‘approprate operating
procedures and imitations.
Transponders and ADS-B Out
TRE001 Transponder | Transponders mustbe | Honeywell KXP 2280 and
Configuration | KXP 22904 f ADS-B Out | KXP 2290 fransponders are elgibe
functionalfy s enabled on | for Phase 2 and Super Lie afcraft
Apex. instalation. Installation of the ADS-B
Out enabled KXP 2290A
ransponders s thiough MOD
612354, The enabiing of ADS-5 Out
functonaity through Apex is
controlled thiough S.0.0. 6347.
For Phase 2 afcraft and for Super-
Lie aifcraft wih two transponders,
both nstaled transponder LRU's
must be KXP 22904 for ADS-B Out
functonaity. Ming IO 2290 and
1OXP 22904 configuration &
protibited
For Super.Lite airraft with just one
transponder, the nstalied
transponder LRU must be XP
'2290A i ADS™B Out functionly s
enabled.
Teasn
TeAs 001 TCASIRA | Phase 2 aircraftand Phase 1 aircraft with Apex Load 13
Configuration | Super e airraft ‘equipped with TCAS Il had only

‘quipped with optonal
TCAS Il musthave the
TCAS Il Resolution
‘Advisory (RA)functionaity
enabed

Phase 2 aircraft TCAS Il
hardware instalation with
only TCAS | functionality
enabled is prohibited.

‘Trafic Advisory (TA) functoniy
‘enabled, RA functionaity was
disabled
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Identiier

‘Affected System

Description

Remarks,

“Apex Configuration and Options

ERs 001

‘Apex Software

Phase 2 and SuperLite
aircraft must use Apex 12
Siot Software Configuration
Load 4.4 (Part Number
EBB002734.0104)

Inespecive of oher Apex and
avionics iniallations and optons,
any airraf wih Apex Load 4.4
Software s a Phase 2" afcraft. The
instalation of Apex Load 4.4 software:
is by incorporation of MOD 6/2303.

EFis002

‘Apex Options.

The folouing Apex option
s prohibied on the DHC-6
‘Series 400: dual charts.

EFis 003

Elecironic Check
List(ECL)

Use of a ECL is approved
for Normal Procedures
oniy. Use of ECL for
‘Abnormal and Emergency
procedures is prohibited

EFis 004

EcL

‘Approved content of ECL s
controled through Viking
50.0.6213.

EFiS 005

Engine Displays

US-regtered (AA)
aircrat must be confiured
for norma conditons.
engine display n green in
accordance wih'S.0.0.
G260

Engine display configuraion s
establshed wih an Apex Optons File
parameter.

EFiS 006

Dispiay Units

‘Al our display units (DU')
must be the same model
type either KDU 1080 or
KDU 1080-2, mived
configuratons are.
prokibited

KDU 1060-2 display unis are
incorporated by bod 62450.

Fiight Management System (FMS)

Fus-001

ESIS/ Apex
Navigation Iterface

Navigation (SRN or LRN)

frfacing of Apex with L3
‘Avionics GH-3100 or
GH302ESISIs
proibited

FuS002

SBAS Based
‘Approaches.

With ihe Apex options fle
setlo SBAS based
navigation including LPV.
‘approaches predicated on
'SBAS GPS capabilty
nabed, for Phase 2
airraf (wo GPS unis
requird) or with Superdite
aircraft with two GPS unts,
both GPS LRU's must be.
066.01201.0105 KGS 200
(GPS receivers. For Super-
Lite airraft with one GPS
LRU instaled, it mustbe &
066.01201.0105 KGS 200
GPS receiver.

nstalation s based on MOD 612304
and $.0.0. 6225,
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Identifier

Affected System

Description

Remarks|

FMS-003

S Arcral
Database (ACDB)

‘Apex must use FMS
'ACDB's identied by
Honeywell PN
'MMB0000461-002 (12,500
pounds) or Honeywell PN
60000461-004 (14,000
pounds). Use of the.
14,000 pound ACD does
ot consitufe a design
approvalfor operations
over 12,500 pounds.

“The 14,000 pound ACDB is dentified
by Honeywel PIN 50000461.004 as
called Up n 5.0.0. 6224,

GPS Receivers

GPs001

GPS Installation

‘Apex on Phase 2 arcrat s
‘approved for use with non-
'SBAS or SBAS-enabled
KGS 200 GPS receivers.
Only Phase 2 airraft may
be equipped with cither the
non-SBAS Honeywel

KGS 200 (PIN 066.01201-
0101) GPS receiver (two
for Phase 2 airraf) or the.
‘SBAS enabled KGS 200
(PIN 086-01201.0105)
(GPS recevers (two for
Phase 2 aircaft and one or
w0 for Super-Lite aircraf).

GPs002

GPS Instalations

Phase 2 arcrat with two
‘GPS receivers must have
cither two 066.01201-0101
‘GPS receivers or two 086-
01201.0105 GPS.
receivers, mbed
configuratons are.
profibited. Super-Lite
airraft must have one or
w0 066-01201-0105 GPS

GPS003

GPS Instalations

With the Apex options fle
setlo SBAS based
navigation including LPV.
‘approaches disabled, the.
(GPS receivers for Phase 2
aircraft mustbe cither the
066.01201.0101 or 066~
01201.0105 receivers.

“The one or two GPS.
receivers on Super-Lte
aircraft must always be the
066.01201.0105 GPS.
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Identiier ‘Affected System Description Remarks,

GPS 004 GPS Installaions | Installation of SBAS- ‘SBAS-enabled KGS 200 receivers
enabled are incompatible with Apex Phase 1
066.01201.0105 GPS (Load 1.3) software. MOD 62303 s a

receivers (two for Phase 2 | prerequisie modification
airraftand one or wofor | MOD 612305,

Super-Lie aircraf) must

oniy be accomplshed on
airraft with Apex Load 4.4
(ako see Anwortiness.
Limiation EFIS001)

GPS005 GPS Instalaions | Installation of the
Honeywell
066.01201.0102, 0103,
and 0104 KGS 200 GPS
receivers in iew o ciher
the 0101 or 0105 GPS
receiver s prohibied.

‘Automatic Flight Control System (AFCS)

AFcs 001 Flight Director | Fight Diector enabled is | For aicraf without Fight Director
type design standard for | enabled (i may arise for special
Phase 2 and Super-Lite | mission or for ofher operational and
airraftsubject o operating | certficaton reasons), contact Vking
Iimitaions in Supplement.

50 (Phase 2 airraft),
‘Supplement 55 (SuperLite:
aircraf)or i ofher
approved supplements.

AFcs 002 ‘Autopiot ‘Winimum Use Height Use of the AP at ower MUH (for
(MUH)ofthe AP 15200 | example for CAT Il approaches or at
foet AGL. Minimum lower MEH is prohibited (aso refer to

Engage Height (MEH) of | Supplement 50 for Phase 2 aircaft
the AP s 400 feet AGL. | and Supplement 55 for Super.Lite

sircratt),

AFcs 003 ‘Autopiot Disengage ofhe AP on | AP use during Go-Around (GA) 18
GAis controlled at an prohibited (aiso refer o Supplement
aircraftlevel, the Apex | 50 for Phase 2 arcraft and

options fle parameter for | Supplement 55 or Super-Lite
“afcsCpGaEnable” must | aircraft) On the DHC.6 Series 400
be setfo Enable” ‘automaic disengage of he AP on

‘GAis implemented at an airraft
level

AFCS 004 ‘Apex Option | Phase 2 and Super Lite:
Fiyaway Parameter | airraft must have Apex
Optons Fie.
“afcsFlyAway” must be set
to"Disable.

AFCS005 | Gear Configuraions | Flight Director (FD) and

‘Autopilt (4P) use are-
‘approved on Standard
Gear Wheels (SGW),
Intemediate Floatation
Gear (IFG), and wheel sk
aircratt
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Identifier ‘Affected System Description Remarks.
AFCS 006 Gear Configuration | D and AP use has been | The Amphbious Fioat and Seaplane
evalusted on Wipline Float STC holders are responsible for
Model 13000 Amphibious | ensuring that STC documents are
Floataicraft modified in | updated to reflect operating
accordance wi TCCA | procedures and imitatons.
STC SAT17 or SAS3-103 | approprite fo FD and AP use with
o FAA STC SADCH. FD | Amptibious Floats or Seaplane
and AP have been Floats nstaled.
detemined to be
‘compatible wit tis gear
configuration and with
‘Seaplane Floats subject o
‘appropriate operating
procedures and imitatons.
Transponders and ADS 5 Out
TRP001 Transponder | Transponders mustbe | Honeywell P 2290 and
Configuration | KXP 2290A If ADS-B Out | KXP 22904 transponders are eigibie
functionalfy s enabled on | for Phase 2 and Super-Lie aircraft
Apex. instalation. Instalaion o the ADS-B
‘Out enabled KXP 22504
ransponders i through MOD
612354, The enabiing of ADS-B Out
functionalty through Apex s
controlled through 5.0.0. 6347,
For Phase 2 airraft and for Super-
Lite aifcraft with two ransponders,
both nstaled transponder LRU's
‘must be KXP 22904 for ADS.B Out
functionalty. Mixing KOXP 2290 and
10 22904 confguration s
prohibied.
For Superte afcrat with just one:
ransponder, he installed
transponder LRU must be K
‘22904 f ADS.B Out unctionaify i
enabed
TeAs T
TeAs 001 TCASIRA | Phase 2 arcraftand Phase 1 aircraf wih Apex Load 13
Configuration | SuperLte arcrat ‘equipped ith TCAS Il had oy

equipped wih optional
TCAS Il must have the
TCAS Il Resolution
‘Advisory (RA) functionaity
enabed.

Phase 2 ircrat CAS I
hardware instalation with
only TCAS | functionalty
enabled s prohibted.

Traffc Advisory (TA) functionalfy
enabled, RA functionaty was.
disabied
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Identifier ‘Affected System Description Remarks.
Super-Lite,
SUPER-001 | Minimum Number of | The minimum number of | A 2070 DV configuration s
DME 'DME on Super-Lie arcraft | incompatiie with Apex.
SUPER-002 | inimum Number of | The minimum number of | A zero radar altmeter configuration s
Radar Alimeters | radar afimeters on Super- | incompatitie with Apex.
Lite airraft s one.
SUPER-003 | Minimum Number of | The minimum number of | A zero ransponder configuration i
Transponders | Mode S transponders s | incompatibe with Apex.
SUPER-004 | Minimum Number of | The minimum number of | Three DU configurations (one
Display Units | display uns (DU's) s four. | Primary Fliht Display [PFD] and two.
Mt Functon Displays (VFD's] or
two PFD's and one MFD) are not
approved.
SUPER005 | Minimum Number of | The minimumm number of
"Audio Control | Audio Control Panls
Pancls (ACP3) i two.
SUPER006 | Minimum Number of | The minimum number of
Mult-Mode Digtal | MultMode Digital Racios.

Radios

s two.
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AIRCRAFT CORROSION

CARD No. CORR

AREA: TRADE:
EXTERNAL and INTERNAL

AIRFRAME

MANHOURS: PREP
TOTAL:

‘An equalized corrosion inspection program to fulfill PSM 1-6-5, Part 3, Corrosion Manual requirements over a 5 year period. The equalized
inspection should commence after the aircraft has previously undergone the initial 5 year corrosion inspection specified in Transport Canada

Ainworthiness Directive CF-94-12 when approval has been received from your Local Regulatory Authority. The periods of inspection are based
on a typical annual operation of 1200 flight hours accumulating 6000 flight hours over a 5 year period. The five yearly EMMA Cards identify the

inspections for that particular year

CORROSION INDEX

Airworthiness

Directives
Corrosion Description and service
Task Bulletins

Inspection
Access

Access

Timeand | Inspect | Total

Reinstall | Time Time | Inspection
(mins) | (mins) | (mins) Year

28-00 FUEL GALLERY

C28-00-00 | Fuel structure, piping. booster pumps. fuel

Remove panel

strainer, crossfeed valve, sump plates and F13, Fi4and
electrical wiring and connections. F17
32-10 MAINLEG
C32-10-01 | Main landing gear leg upper platen Remove 1
o e fairing, and
C32-10-02 | Main landing gear leg upper platen links, ige‘ ‘zuzgM panek 4 F5 1
F8,F9.F18
C32-10-03 | Main landing gear leg lower platen and F20 1
C32-10-04 | Main landing gear leg rebound block base 1
plates
C32-10-05 | Main landing gear leg axle Jack aircraft 1
remove wheel
32-15 FLOAT  NOT APPLICABLE AT THIS TIME

C32-15-01 | Float installation - Front spreader bar, tie
rod lugs, tie rod, vertical strut and
hardware.

Beach aircraft
In situ

12,3,
4and5
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Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year

3215 FLOAT (CONT'D) NOT APPLICABLE AT THIS TIME

C32-15:02 | Float installation - Top front strut bracket, When beached 123
front strut and hardware. In situ 4and5

C32-15-03 | Float installation - Bottom front strut lug. en beached 123
front strut and hardware. In situ 4and5

C32-15:04 | Float installation - Rear spreader bar, When beached 123
support strut bracket, rear support struts, In situ 4and5
swivel end fittings, main leg pivot lug and
hardware.

C32-15-05 | Float installation - Main strut, drag strut, RemoveTairing 123
fuselage lug, wing strut attachment and F4,F5, F8and 4and5
hardware. F9, remove

strut fairings

C32-15-06 | Float installation - Main strut, drag strut Remove strut 123
and hardware at float fairings panel 4and5

C32-15:07 | Float installation - Internal and external Remove 123
structure areas panels and 4and5

internal
bulkhead
panels

32-20 NOSELEG

C32-20-01 | Noseleg upper and lower forque finks, Insitu 1
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
32-20 NOSELEG (CONT’D)
C32-20-02 | Noseleg steering actuator lever. Open F1 or F2 1
door and
removeavionic
shields
C32-20-03 | Noseleg cylinder lower bearing assembly. During 1
overhaul
C32-20-04 | Noseleg fork where locknut bears against During 1
lower surface of fork overhaul
52-00 DOOR
C52-00-01 | Airstair door outer skin, adjacent fo hinge: Insitu 1
C52-00-02 | Airstair door hinge. Lower door 1
C52-00-03 | Cabin door RH, Upper and lower hinges. Insitu 1
Open doors
C52-00-04 | Nose baggage compartment door hinge in situ 1
Open F1 nose
cap or F2 door
53-11 FUSELAGE FORWARD
C53-11-01 | Noseleg lower attachment adapter fiting. in situ 5
Station 60
C53-11-02 | Noseleg upper mounting block, Station Open panels 5
60 F3and F10
C53-11-03 | Pilot door hinge, upper and lower In'situ 5

attachment plates, station 73.
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
53-11 FUSELAGE FORWARD (CONT'D)
C53-11-04 | Co-pilot door hinge, upper and lower In'situ 5
attachment plates, Station 73
C53-11-05 | Nose Attachment, exterior aluminum joint n'situ 5
straps and fasteners common to the nose.
station 44.
C53-11-06 | Battery tray structure, interior surface of Open nose 5
nose luggage compartment near battery luggage door
tray, fasteners and hardware securing
battery tray. (If installed)
53-12 FUSELAGE CENTER
C53-12-01 | Lower frame assembly. main landing gear Remove 5
attach, station 219 panels F4, F5,
F8and F9
C53-12-02 | Fuselage side frames at Stations 218.and | T.C.CF—78-17 | Remove cabin 5
219 FAAT78-26-02 | dado side
panels
C53-12-03 | Upper fwd spar beam, Station 200, and Remove 5
adapters, wing pickup, Station 200 ceiling panel
and wing top
center panel
C53-12-04 | Frame assembly, lower, main landing gear Remove 5
attach, Station 239 panels F5 and
F8
C53-12-05 | Frames (*hockey stick’) Station 239, wing Remove wing 5
attach top center

panel
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
53-12 FUSELAGE CENTER (CONT'D)
C53-12-06 | Top skin sandwich panels, center In'situ 5
fuselage, from station 111 to Station 10. Access upper
fuselage
surface
C53-12-07 | Aft cabin doors, LH and RH, hinge attach n situ 5
plates, upper and lower. Open door
C53-12-08 | Airstair door hinge plate Insitu 5
Lower door
C53-12-09 | Cabin floor rails| Remove or 5
stow cabin
seats and lift
floor boards
after de-
riveting board
side angles
C53-12-10 | Cabin floor boards, When above 5
Fuselage structure, Station 111 to Station Remove cabin 5
376, shell interior and exterior skins dado side
stringers and frames. panels, fuel

liners and fuel
cells,

53-13 FUSELAGE REAR

C53-13-01 | Aft LH baggage door hinge attach plates In'situ Open 5
door F6

C53-13-02 | Rear baggage compartment door hinge In situ Open 5

door F6
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AIRCRAFT CORROSION

CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and Service | Inspection | Reinstall | Time | Time |Inspection
Task Bulletins Access (mins) | (mins) | (mins) | Year
53-13 FUSELAGE REAR (CONT’D)
C83-13-03 | Rear baggage compartment door sl it Open 5
door Fé
C83-13-04 | Rear fuselage lower bukhead, Station Open door F6 5
376 and remove
rear floor panel
C83-13-05 | Battery bay, lower structure. Open door F6 5
and remove
fwd floor panel
53-14 FUSELAGE AFT
C53-14-01 | Af fuselage (o fin aftach adapter plates. | S8 6/454 See Notes 1 7
NOTE 1: If Pre Mod 1843 to 1848, N/A Mod incdrporated
remove horiz/vert stabilizer/ §
aft fuse top rib.
NOTE 2: If Post Mod 1843 to 1846,
inspect where accessible. N/A Mod incofporated
C83-14-02 | Rudder hinge fubular attach support Remove 7
structure. fairings T3, T4
and T14
54-00 NACELLE
C54-0001 | Forward frame engine mount plates and Lower engine 7

engine mount adapters.

cowling W7 o
W21, remove
cowling W29
or wa3
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AIRCRAFT CORROSION

CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
54-00 NACELLE (CONT'D)
C54-00-02 | Nacelle skin exhaust path and nacelle In'situ a
drag angles
55-10 HORIZONTAL STABILIZER
C55-10-01 | Horizontal Stabilizer/Elevator adapter In'situ a
plate inboard
C55-10-02 | Horizontal Stabilizer/Elevator adapter n'situ a
plate outboard
C55-10-03 | Elevalor center hinge arm TC. CF92:05 | Remove a
FAA94-14-22 | faifings T2 and
TI5
C55-10-04 | Tailplane front and rear mounting TC.CF-92-04 | Disassembly a
brackets TC.CF-85-10 | of Empennage
FAA83-26-05 | units is
recommended
55-20 ELEVATOR
C55-20-01 | Inboard attach adapter fitting in situ 1
C55-20-02 | Outboard attach adapter fitiing in situ 1
C55-20-03 | Trim tab hinge. in situ 1
C55-20-04 | Flap/Elevator interconnect tab hinge: In situ 4
C55-20-05 | RH and LH inboard hinge arms. insitu a
C55-20-06 | RH and LH outboard hinge arms In situ 4
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AIRCRAFT CORROSION

CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
55-30 VERTICAL STABILIZER
C55-30-01 | Rudder mid hinge attach plate. Remove a
Rudder
C55-30-02 | Rudder top hinge attach plate. Remove a
Rudder
C55-30-03 | Fin front and rear spar adapter fitings See Notes 1 a
NOTE 1: If Pre Mod 1841and 1842, N/A Mod incorporpfad =
remove horizivert stabilizer/
aft fuse top rib.
NOTE 2: If Post Mod 1841 and 1842,
inspect where accessible.
55-40 RUDDER
C55-40-01 | Lower hinge arm Remove a
panels T3 and
T4
C55-40-02 | Mid hinge bracket in situ 1
C55-40-03 | Upper hinge bracket in situ 1
C55-40-04 | Upper trim tab hinge in situ 1
C55-40-05 | Lower trim tab hinge insitu a
57-10 WINGS
C57-10-01 | Top skins adjacent to nacelle, ribs 5 t0 9 In situ Access, 123
LH and upper wing 4and5
RIH surface
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AIRCRAFT CORROSION

CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
57-10 WINGS (CONT'D)
C57-10-02 | Lower skins adjacent to nacelle, ribs 5 to In'situ 12,3,
LH and 9. 4ands
RIH
C57-10-03 | Rear spar cap aftachment adapters. TC.CF73-03 | Remove wing 23
FAA95-18-11 | top center
amdt 39- 9358 | fairing
S/B 6/295
C57-10-04 | Forward attachment adapters. TC. CF85-12 | Remove wing 23
FAA85-16-10 | top center
FAA94-04-01 | fairing
C57-10-05 | D' nose door assembly and hinge: Remove 23
panels W2 or
wi6
C57-10-06 | Leading edge skin outboard of nacelle. in situ 23
C57-10-07 | Hinge arm Station 97 5 in situ 23
Remove
shroud access
panel
C57-10-08 | Hinge arm adapters Stations 975, 1725 n'situ 23
2475 and 310 Remove
shroud access
panel
C57-1009 | Hinge arm Station 172.5 in'situ 23
Remove

shroud access
panel
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AIRCRAFT CORROSION

CARD No. CORR

Corrosion
Task

Description

Airworthiness
Directives
and Service
Bulletins

Inspection
Access

Access
Time and
Reinstall

(mins)

Inspect
Time
(mins)

Total
Time
(mins)

Inspection
Year

57-10

WINGS (CONT'D)

C57-10-10

Hinge arm Station 247.5

insitu
Remove
shroud access
panel

Ca7-10-11

Hinge arm Station 310

in situ
Remove
shroud access
panel

Ca7-10-12

Hinge arm Station 376.25,

Insitu
Remove wing
tip fairing

C&7-10-13

Main spar lower forward and aft cap
angles

TC
CF-87-02

FAA88-13-11
FAA 94-08-10

Access
through wing
lower skin
inspection
holes

Main spar wing strut attachment lug

Remove
fairings W5
and W6 or
W19 and W20

C&7-10-15

Main spar splice piate Station 152 6.

Access
through wing
lower skin
inspection
holes
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CARD No. CORR

Corrosion
Task

Description

Airworthiness
Directives
and Service
Bulletins

Inspection
Access

Access

Timeand | Inspect | Total

Reinstall | Time Time | Inspection
(mins) | (mins) | (mins) Year

57-10

WINGS (CONT'D)

C57-10-16

Rivets attaching ribs to upper skin
corrugation

Access
through wing
lower skin
inspection
holes

C57-10-17

Pre Mod 6/1117 wing-spar, strut-lug.
fastener holes.  N/A Mod incorporated|

171001200

High frequency
eddy current
See

PSM 1-6-7
PART 3

Ca7-10-18

‘Adapter assy — front spar-wing.

AD.
CF-2007-31

Access
through wing
lower skin
inspection
holes

(Refer to

SB 6/541)

57-40

WING STRUT

C57-40-01

Wing strut beam

T.C.CF85-14
FAA87-04-23

Remove
fairings F5 or
F8, W5 and
W6 or W19
and W20

C57-40-02

Strut finks.

Remove
fairings W6 or
w20
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AIRCRAFT CORROSION

CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
57-51 INBOARD FOREFLAP
C57-51-01 | Inboard hinge arm Station 345 Lower Flaps 23
C57-51-02 | Mid hinge arm Station 97.5. When lowered 23
C57-51-03 | Outboard hinge arm Station 172 58 When lowered 23
C57-51-04 | Pushrod attach fitling Station 97.5 When lowered 23
57-52 OUTBOARD FOREFLAP
C57-52-01 | Inboard hinge arm Station 173 5 When lowered 23
C57-52-02 | Inboard center hinge arm Station 247 11 When lowered 23
C57-52-03 | Outboard center hinge arm Station 310 When lowered 23
C57-52-04 | Outboard hinge arm Station 376 2 When lowered 23
C57-52-05 | Pushrod attach fiting Station 24711 When lowered 23
57-53 TRAILING FLAP
C57-53-01 | Inboard hinge end arm. When lowered 23
C57-53-02 | Center hinge arm When lowered 23
C57-53-03_| Outboard hinge end arm. When lowered 23
57-54 AILERON
C57-54-01 | Inboard hinge arm station 172.5. When lowered 23
C57-54-02 | Inboard center hinge arm Station 247 11 When lowered 23
C57-54-03 | Outboard center hinge arm Station 310 When lowered 23
C57-54-04 | Outboard hinge arm Station 376 2 When lowered 23
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C57-54-05 | Balance weight location channel S/B 6/507 When lowered
(D" nose). remove
leading edge
and weight
C57-54-06 | Trim tab hinge arm When lowered
C57-54-07 | Trim tab hinge. Vnen lowered
C57-54-08 | Gear tab hinge: When lowered





image9.png
,&, /PR 4




image10.png




image11.png




image12.png




image13.png




image14.png




image15.png




image16.png




image17.png




image18.png




image19.png




image20.png




image21.png




image22.png




image23.png
,&, /PR 4




image24.png




image25.png




image26.png




image27.png




image28.png




image29.png




image30.png




image31.png




image32.png




image33.png




image34.png




image35.png




image36.png




image37.png
foiTRbuid




image38.png




image39.png




image40.png




image41.png




image42.png




image43.png




image44.png
foiTRbuid




image45.png




image46.png




image47.png




image48.png




image49.png




image50.png




image51.png




image52.png




image53.png




image54.png




image1.png
r«‘.: Maritime Helicopters




image55.png




image56.png




image57.png




image58.png




image59.png




image60.png




image61.png




image62.png




image63.png




image64.png




image2.png




image65.png




image66.png




image67.png




image68.png




image69.png




image70.png




image71.png




image72.png




image73.png




image74.png




image3.png




image75.png




image76.png




image77.png




image78.png




image79.png
/24




image80.png




image81.png




image82.png




image83.png




image84.png




image4.png




image85.png
/24




image86.png




image87.png




image88.png




image89.png




image90.png
MARITIME HELICOPTERS PRE-WEIGHING CHECK LIST

STATION, DATE, ACNO.N,

MECH

1. Empty all fuel tanks and drain sumps.
Service both engine oil tanks to full
Service hydraulic tanks to normal full
Portable fire extinguishers (2 required)

Remove all operating items, (List on back of sheet for replacement)
Aircraft clean, exterior and interior

Cargo Nets Installed (Flight Configuration)

First Aid kit, Life Vests and Survival Kit installed.

9. Al crew member seats installed.
10. Position flaps up and all controls neutral. Use seat belts to hold yoke.
11. Prop locks and engine inlet covers removed

12. Aifcraftjacked to level condition

13. Scales properly calibrated, warmed, and zeroed

AIRCRAFT READY TO BE WEIGHED INSP.

bobobbobobooboboo
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BASIC AIRCRAFT WEIGHT CHANGE RECORD
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