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	1
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	CHECK:
	
	P 0100 – ENGINE INSPECTION

	FREQUENCY:
	
	EVERY 100 HOURS

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  DHC - 6 PSM 1-65-2 MM, Pratt & Whitney PT6A-34 MM 
	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	P 0100.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Pratt & Whitney PT6A MM
	
	

	
	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Pratt & Whitney PT6A MM
	
	

	
	
	
	

	P 0100.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 Examine the placards, decals, and markings in engine area. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your aircraft.
	
	
	

	
	
	
	

	P 0100.3  CORROSION CONTROL

	
	
	
	

	3.1 Perform a visual corrosion inspection on any area’s access during this CAMP inspection.
	Appendix

B
	
	

	
	
	
	

	P 0100.4 ENGINE EXTERNALS

	
	
	
	

	4.1 Inspect the following on all tubing, wiring, control linkages, hoses assemblies;
	
	
	

	
	
	
	

	4.1.1 All accessible connections, clamps and brackets for attachment.
	
	
	

	
	
	
	

	4.1.2 Accessible lockwire and safety cable for security and installation.
	
	
	

	
	
	
	

	4.1.3 Wear, chafing, cracks and corrosion.
	
	
	

	
	
	
	

	4.1.4 Fuel and oil lines for leaks.
	
	
	

	
	
	
	



	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	
	
	

	4.1.5 
	
	
	

	
	
	
	

	4.1.6 
	
	
	

	
	
	
	

	4.1.7 
	
	
	

	
	
	
	

	4.1.8 
	
	
	

	
	
	
	

	4.1.9 
	
	
	

	
	
	
	

	4.1.10 
	
	
	

	
	
	
	

	4.1.11 
	
	
	

	
	
	
	

	4.1.12 
	
	
	

	
	
	
	

	4.1.13 
	
	
	

	
	
	
	

	4.1.14 
	
	
	

	
	
	
	

	4.1.15 
	
	
	

	
	
	
	

	4.1.16 
	
	
	

	
	 
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	P 0100.5 SYSTEMS

	
	
	
	

	5.1 
	
	
	

	
	
	
	

	5.2 
	
	
	

	
	
	
	

	5.3 
	
	
	

	
	
	
	

	5.4 
	
	
	

	
	
	
	

	5.5 
	
	
	

	
	
	
	

	5.6 
	
	
	

	
	
	
	

	5.7 
	
	
	

	
	
	
	

	5.8 
	
	
	

	
	
	
	

	5.9 
	
	
	

	
	
	
	

	5.10 
	
	
	

	
	
	
	

	5.11 
	
	
	

	
	
	
	

	5.12 
	
	
	

	
	
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	
	
	

	5.13 Inspect pneumatic tubes and lines for cracks and damages especially at the end fittings and joints.
	
	
	

	
	
	
	

	P 0100.6 POST INSPECTION

	
	
	
	

	6.1 Inspect for operation and leaks.
	
	
	

	
	
	
	

	6.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	6.3 Perform Functional Check Flight if required per PT6A Maintenance Manual or AFM as appropriate.
	
	
	

	
	
	
	

	6.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	

	
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC- 6 – P 0100 – 100 Hour Powerplant Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	



