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	CHECK:
	
	P 0100 – ENGINE INSPECTION

	FREQUENCY:
	
	EVERY 100 HOURS

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


Reference:  DHC - 6 PSM 1-65-2 MM, Pratt & Whitney PT6A-34 MM 
	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	P 0100.1 GENERAL

	
	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	
	

	
	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	
	

	
	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Pratt & Whitney PT6A MM
	
	

	
	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Pratt & Whitney PT6A MM
	
	

	
	
	
	

	P 0100.2 PLACARDS AND MARKINGS

	
	
	
	

	2.1 Examine the placards, decals, and markings in engine area. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your aircraft.
	
	
	

	
	
	
	

	P 0100.3  CORROSION CONTROL

	
	
	
	

	3.1 Perform a visual corrosion inspection on any area’s access during this CAMP inspection.
	Appendix

C
	
	

	
	
	
	

	P 0100.4 ENGINE EXTERNALS

	
	
	
	

	4.1 Inspect the following on all tubing, wiring, control linkages, hoses assemblies;
	
	
	

	NOTE: Pay particular attention to rear linkage cam box, fuel control unit arm, telescopic rod and rod end fittings.
	
	
	

	4.1.1 All accessible connections, clamps and brackets for attachment.
	
	
	

	
	
	
	

	4.1.2 Accessible lockwire and safety cable for security and installation.
	
	
	

	
	
	
	

	4.1.3 Wear, chafing, cracks and corrosion.
	
	
	

	
	
	
	

	4.1.4 Fuel and oil lines for leaks.
	
	
	

	
	
	
	



	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	
	
	

	4.1.5 All insulated air tubes for sign of swelling, cracking, bulging of rubber sheath material. Refer to repair section and SB1687. Replace as necessary.
	
	
	

	
	
	
	

	4.1.6 Disconnect rod ends and clean using solvent (PWC11-027) or (PWC11-031).
	
	
	

	
	
	
	

	4.1.7 Examine rod end for corrosion, roughness in rotation, side play and radial play.
	
	
	

	
	
	
	

	4.1.8 Lubricate with light grease (PWC04-001) after engine external wash.
	
	
	

	
	
	
	

	4.1.9 After lubrication, reinstall rod ends and torque to specified value.
	
	
	

	
	
	
	

	4.1.10 Check free movement of linkage.
	
	
	

	
	
	
	

	4.1.11 Cleanliness of air inlet screen.
	
	
	

	
	
	
	

	4.1.12 Gas generator case external surfaces and fire seal mount ring brackets for cracks, distortion and corrosion
	
	
	

	
	
	
	

	4.1.13 Fire seal mount rings for cracks and attachment of brackets and seals.
	
	
	

	
	
	
	

	4.1.14 Exhaust duct for cracks and distortion.
	
	
	

	
	
	
	

	4.1.15 Propeller shaft seal for oil leaks.
	
	
	

	
	
	
	

	4.1.16 Accessories attachment and linkages, air, oil and fuel lines.


	
	
	

	
	 
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	P 0100.5 SYSTEMS

	
	
	
	

	5.1 Check oil level.
	SERVICING
	
	

	
	
	
	

	5.2 Check condition and locking of oil filler cap.
	72-60-00
	
	

	
	
	
	

	5.3 Inspect and clean oil filter elements and secondary screen (coarse hat-type screen attached to the inner end of the filter).
	79-20-02
	
	

	NOTE: Light traces of sediment only may be removed from the main filter screen. All other contamination requires replacement of filter Element. Any foreign material found in main oil filter or on chip detector, should be identified before further inspection/operation 79-20-02 MAINTENANCE PRACTICES.
	
	
	

	5.4 Perform a visual inspection of the fuel pump
	
	
	

	NOTE: If airframe fuel boost pump fails or is inadvertently left off for an accumulative time in excess of 10 hours, the engine driven fuel pump must be removed and replaced. The removed pump should be sent to an approved overhaul facility.
	
	
	

	5.5 Check scavenge oil pump housing for leaks
	
	
	

	
	
	
	

	5.6 Perform a visual inspection of the fuel pump for installation and leakage.
	72-10-02

Fuel Pump
	
	

	
	Maint Pract
	
	

	5.7 Inspect outlet filter for foreign matter or distortion.
	73-10-02
	
	

	
	
	
	

	5.8 Check drain valve for installation and leaks.
	73-10-06
	
	

	
	
	
	

	5.9 Inspect FCU for installation, linkages and pneumatic tubes.
	73-20-00
	
	

	
	
	
	

	5.10 Examine the FCU for bearing washout, shown by blue dye (grease and fuel mixed) at FCU vent.
	Fault Iso

Operating
	
	

	
	Problems
	
	

	5.11 Check starting flow control/flow divider for installation and leaks.
	73-10-04
	
	

	
	
	
	

	5.12 Check oil-to-fuel heater installation.
	73-10-00

Ign Exciter
	
	

	
	Maint Pract
	
	

	5.13 Check P3 filter for installation.
	
	
	

	NOTE: Visually inspect the P3 filter for corrosion. If the filter shows presence of corrosion, discard the filter and replace with a new filter.
	73-10-07
	
	


	
	
	MECH

INITIALS
	RII

INITIALS

	MAINTENANCE ACTION
	REF
	
	

	
	
	
	

	
	
	
	

	5.14 Inspect pneumatic tubes and lines for cracks and damages especially at the end fittings and joints.
	
	
	

	
	
	
	

	P 0100.6 POST INSPECTION

	
	
	
	

	6.1 Inspect for operation and leaks.
	
	
	

	
	
	
	

	6.2 Replace or close all applicable trim panels, covers, access and inspection doors/covers as necessary.
	
	
	

	
	
	
	

	6.3 Perform Functional Check Flight if required per PT6A Maintenance Manual or AFM as appropriate.
	
	
	

	
	
	
	

	6.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	
	

	
	
	
	


Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected all the items initialed by me in accordance with Maritime Helicopters DHC-400 Continuous Airworthiness Maintenance Program found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.
I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ DHC- 6 – P 0100 – 100 Hour Powerplant Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Engine Start Total Time:
	

	Engine S/N: 
	
	
	
	Engine Start Total Cycles:
	


	Signature:
	
	
	Certificate Type & No:
	



