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B
CORROSION CONTROL
C.1 
This corrosion control program to fulfill PSM 1-6-5, Part 3, Corrosion Manual requirements over a 5-year period
C.2 
Inspections shall be entered in the Work Order or aircraft log book as applicable when each even is complied with. Each inspection year will be tracked under the aircraft maintenance CALM program.
[image: image1.png]AIRCRAFT CORROSION

CARD No. CORR

AREA:

EXTERNAL and INTERNAL

TRADE:
AIRFRAME

MANHOURS: PREP
TOTAL:

‘An equalized corrosion inspection program to fulfil PSM 1
inspection should commence after the aircraft has previou:

inspections for that particular year

-6-5, Part 3, Corrosion Manual requi

rements over a 5 year period. The equalized

sly undergone the nitial 5 year corrosion inspection specified in Transport Canada
Ainworthiness Directive CF-94-12 when approval has been received from your Local Regulatory Authority. The periods of inspection are based
on a typical annual operation of 1200 flight hours accumulating 6000 flight hours over a 5 year period. The five yearly EMMA Cards identify the

CORROSION INDEX

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year

28-00 FUEL GALLERY

C28-00-00 | Fuel structure, piping. booster pumps. fuel Remove panel 1
strainer, crossfeed valve, sump plates and F13, Fi4and
electrical wiring and connections. F17

32-10 MAINLEG

C32-10-01 | Main landing gear leg upper platen Remove 1

o e fairing, and
C32-10-02 | Main landing gear leg upper platen links, ige‘ ‘zuzgM panek 4 F5 1
F8,F9.F18

C32-10-03 | Main landing gear leg lower platen and F20 1

C32-10-04 | Main landing gear leg rebound block base 1
plates

C32-10-05 | Main landing gear leg axle Jack aircraft 1

remove wheel

32-15 FLOAT  NOT APPLICABLE AT THIS TIME

C32-15:01 | Float installation - Front spreader bar, tie Beach aircraft 123
rod lugs, tie rod, vertical strut and in sity 4and5
hardware.
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year

3215 FLOAT (CONT'D) NOT APPLICABLE AT THIS TIME

C32-15:02 | Float installation - Top front strut bracket, When beached 123
front strut and hardware. In situ 4and5

C32-15-03 | Float installation - Bottom front strut lug. en beached 123
front strut and hardware. In situ 4and5

C32-15:04 | Float installation - Rear spreader bar, When beached 123
support strut bracket, rear support struts, In situ 4and5
swivel end fittings, main leg pivot lug and
hardware.

C32-15-05 | Float installation - Main strut, drag strut, RemoveTairing 123
fuselage lug, wing strut attachment and F4,F5, F8and 4and5
hardware. F9, remove

strut fairings

C32-15-06 | Float installation - Main strut, drag strut Remove strut 123
and hardware at float fairings panel 4and5

C32-15:07 | Float installation - Internal and external Remove 123
structure areas panels and 4and5

internal
bulkhead
panels
32-20 NOSELEG
C32-20-01 | Noseleg upper and lower forque finks, Insitu 1
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
32-20 NOSELEG (CONT’D)
C32-20-02 | Noseleg steering actuator lever. Open F1 or F2 1
door and
removeavionic
shields
C32-20-03 | Noseleg cylinder lower bearing assembly. During 1
overhaul
C32-20-04 | Noseleg fork where locknut bears against During 1
lower surface of fork overhaul
52-00 DOOR
C52-00-01 | Airstair door outer skin, adjacent fo hinge: Insitu 1
C52-00-02 | Airstair door hinge. Lower door 1
C52-00-03 | Cabin door RH, Upper and lower hinges. Insitu 1
Open doors
C52-00-04 | Nose baggage compartment door hinge in situ 1
Open F1 nose
cap or F2 door
53-11 FUSELAGE FORWARD
C53-11-01 | Noseleg lower attachment adapter fiting. in situ 5
Station 60
C53-11-02 | Noseleg upper mounting block, Station Open panels 5
60 F3and F10
C53-11-03 | Pilot door hinge, upper and lower In'situ 5

attachment plates, station 73.
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
53-11 FUSELAGE FORWARD (CONT'D)
C53-11-04 | Co-pilot door hinge, upper and lower In'situ 5
attachment plates, Station 73
C53-11-05 | Nose Attachment, exterior aluminum joint n'situ 5
straps and fasteners common to the nose.
station 44.
C53-11-06 | Battery tray structure, interior surface of Open nose 5
nose luggage compartment near battery luggage door
tray, fasteners and hardware securing
battery tray. (If installed)
53-12 FUSELAGE CENTER
C53-12-01 | Lower frame assembly. main landing gear Remove 5
attach, station 219 panels F4, F5,
F8and F9
C53-12-02 | Fuselage side frames at Stations 218.and | T.C.CF—78-17 | Remove cabin 5
219 FAAT78-26-02 | dado side
panels
C53-12-03 | Upper fwd spar beam, Station 200, and Remove 5
adapters, wing pickup, Station 200 ceiling panel
and wing top
center panel
C53-12-04 | Frame assembly, lower, main landing gear Remove 5
attach, Station 239 panels F5 and
F8
C53-12-05 | Frames (*hockey stick’) Station 239, wing Remove wing 5
attach top center

panel
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
53-12 FUSELAGE CENTER (CONT'D)
C53-12-06 | Top skin sandwich panels, center In'situ 5
fuselage, from station 111 to Station 10. Access upper
fuselage
surface
C53-12-07 | Aft cabin doors, LH and RH, hinge attach n situ 5
plates, upper and lower. Open door
C53-12-08 | Airstair door hinge plate Insitu 5
Lower door
C53-12-09 | Cabin floor rails| Remove or 5
stow cabin
seats and lift
floor boards
after de-
riveting board
side angles
C53-12-10 | Cabin floor boards, When above 5
Fuselage structure, Station 111 to Station Remove cabin 5
376, shell interior and exterior skins dado side
stringers and frames. panels, fuel

liners and fuel
cells,

53-13 FUSELAGE REAR

C53-13-01 | Aft LH baggage door hinge attach plates In'situ Open 5
door F6

C53-13-02 | Rear baggage compartment door hinge In situ Open 5

door F6
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and Service | Inspection | Reinstall | Time | Time |Inspection
Task Bulletins Access (mins) | (mins) | (mins) | Year
53-13 FUSELAGE REAR (CONT’D)
C83-13-03 | Rear baggage compartment door sl it Open 5
door Fé
C83-13-04 | Rear fuselage lower bukhead, Station Open door F6 5
376 and remove
rear floor panel
C83-13-05 | Battery bay, lower structure. Open door F6 5
and remove
fwd floor panel
53-14 FUSELAGE AFT
C53-14-01 | Af fuselage (o fin aftach adapter plates. | S8 6/454 See Notes 1 7
NOTE 1: If Pre Mod 1843 to 1848, N/A Mod incdrporated
remove horiz/vert stabilizer/ §
aft fuse top rib.
NOTE 2: If Post Mod 1843 to 1846,
inspect where accessible. N/A Mod incofporated
C83-14-02 | Rudder hinge fubular attach support Remove 7
structure. fairings T3, T4
and T14
54-00 NACELLE
C54-0001 | Forward frame engine mount plates and Lower engine 7

engine mount adapters.

cowling W7 o
W21, remove
cowling W29
or wa3
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
54-00 NACELLE (CONT'D)
C54-00-02 | Nacelle skin exhaust path and nacelle In'situ a
drag angles
55-10 HORIZONTAL STABILIZER
C55-10-01 | Horizontal Stabilizer/Elevator adapter In'situ a
plate inboard
C55-10-02 | Horizontal Stabilizer/Elevator adapter n'situ a
plate outboard
C55-10-03 | Elevalor center hinge arm TC. CF92:05 | Remove a
FAA94-14-22 | faifings T2 and
TI5
C55-10-04 | Tailplane front and rear mounting TC.CF-92-04 | Disassembly a
brackets TC.CF-85-10 | of Empennage
FAA83-26-05 | units is
recommended
55-20 ELEVATOR
C55-20-01 | Inboard attach adapter fitting in situ 1
C55-20-02 | Outboard attach adapter fitiing in situ 1
C55-20-03 | Trim tab hinge. in situ 1
C55-20-04 | Flap/Elevator interconnect tab hinge: In situ 4
C55-20-05 | RH and LH inboard hinge arms. insitu a
C55-20-06 | RH and LH outboard hinge arms In situ 4
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
55-30 VERTICAL STABILIZER
C55-30-01 | Rudder mid hinge attach plate. Remove a
Rudder
C55-30-02 | Rudder top hinge attach plate. Remove a
Rudder
C55-30-03 | Fin front and rear spar adapter fitings See Notes 1 a
NOTE 1: If Pre Mod 1841and 1842, N/A Mod incorporpfad =
remove horizivert stabilizer/
aft fuse top rib.
NOTE 2: If Post Mod 1841 and 1842,
inspect where accessible.
55-40 RUDDER
C55-40-01 | Lower hinge arm Remove a
panels T3 and
T4
C55-40-02 | Mid hinge bracket in situ 1
C55-40-03 | Upper hinge bracket in situ 1
C55-40-04 | Upper trim tab hinge in situ 1
C55-40-05 | Lower trim tab hinge insitu a
57-10 WINGS
C57-10-01 | Top skins adjacent to nacelle, ribs 5 t0 9 In situ Access, 123
LH and upper wing 4and5
RIH surface
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
57-10 WINGS (CONT'D)
C57-10-02 | Lower skins adjacent to nacelle, ribs 5 to In'situ 12,3,
LH and 9. 4ands
RIH
C57-10-03 | Rear spar cap aftachment adapters. TC.CF73-03 | Remove wing 23
FAA95-18-11 | top center
amdt 39- 9358 | fairing
S/B 6/295
C57-10-04 | Forward attachment adapters. TC. CF85-12 | Remove wing 23
FAA85-16-10 | top center
FAA94-04-01 | fairing
C57-10-05 | D' nose door assembly and hinge: Remove 23
panels W2 or
wi6
C57-10-06 | Leading edge skin outboard of nacelle. in situ 23
C57-10-07 | Hinge arm Station 97 5 in situ 23
Remove
shroud access
panel
C57-10-08 | Hinge arm adapters Stations 975, 1725 n'situ 23
2475 and 310 Remove
shroud access
panel
C57-1009 | Hinge arm Station 172.5 in'situ 23
Remove

shroud access
panel
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CARD No. CORR

Corrosion
Task

Description

Airworthiness
Directives
and Service
Bulletins

Inspection
Access

Access
Time and
Reinstall

(mins)

Inspect
Time
(mins)

Total
Time
(mins)

Inspection
Year

57-10

WINGS (CONT'D)

C57-10-10

Hinge arm Station 247.5

insitu
Remove
shroud access
panel

Ca7-10-11

Hinge arm Station 310

in situ
Remove
shroud access
panel

Ca7-10-12

Hinge arm Station 376.25,

Insitu
Remove wing
tip fairing

C&7-10-13

Main spar lower forward and aft cap
angles

TC
CF-87-02

FAA88-13-11
FAA 94-08-10

Access
through wing
lower skin
inspection
holes

Main spar wing strut attachment lug

Remove
fairings W5
and W6 or
W19 and W20

C&7-10-15

Main spar splice piate Station 152 6.

Access
through wing
lower skin
inspection
holes





[image: image11.png]AIRCRAFT CORROSION

CARD No. CORR

Corrosion
Task

Description

Airworthiness
Directives
and Service
Bulletins

Inspection
Access

Access

Timeand | Inspect | Total

Reinstall | Time Time | Inspection
(mins) | (mins) | (mins) Year

57-10

WINGS (CONT'D)

C57-10-16

Rivets attaching ribs to upper skin
corrugation

Access
through wing
lower skin
inspection
holes

C57-10-17

Pre Mod 6/1117 wing-spar, strut-lug.
fastener holes.  N/A Mod incorporated|

171001200

High frequency
eddy current
See

PSM 1-6-7
PART 3

Ca7-10-18

‘Adapter assy — front spar-wing.

AD.
CF-2007-31

Access
through wing
lower skin
inspection
holes

(Refer to

SB 6/541)

57-40

WING STRUT

C57-40-01

Wing strut beam

T.C.CF85-14
FAA87-04-23

Remove
fairings F5 or
F8, W5 and
W6 or W19
and W20

C57-40-02

Strut finks.

Remove
fairings W6 or
w20
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CARD No. CORR

Airworthiness Access
Directives Timeand | Inspect | Total
Corrosion Description and service Inspection | Reinstall | Time Time | Inspection
Task Bulletins Access (mins) | (mins) | (mins) Year
57-51 INBOARD FOREFLAP
C57-51-01 | Inboard hinge arm Station 345 Lower Flaps 23
C57-51-02 | Mid hinge arm Station 97.5. When lowered 23
C57-51-03 | Outboard hinge arm Station 172 58 When lowered 23
C57-51-04 | Pushrod attach fitling Station 97.5 When lowered 23
57-52 OUTBOARD FOREFLAP
C57-52-01 | Inboard hinge arm Station 173 5 When lowered 23
C57-52-02 | Inboard center hinge arm Station 247 11 When lowered 23
C57-52-03 | Outboard center hinge arm Station 310 When lowered 23
C57-52-04 | Outboard hinge arm Station 376 2 When lowered 23
C57-52-05 | Pushrod attach fiting Station 24711 When lowered 23
57-53 TRAILING FLAP
C57-53-01 | Inboard hinge end arm. When lowered 23
C57-53-02 | Center hinge arm When lowered 23
C57-53-03_| Outboard hinge end arm. When lowered 23
57-54 AILERON
C57-54-01 | Inboard hinge arm station 172.5. When lowered 23
C57-54-02 | Inboard center hinge arm Station 247 11 When lowered 23
C57-54-03 | Outboard center hinge arm Station 310 When lowered 23
C57-54-04 | Outboard hinge arm Station 376 2 When lowered 23





[image: image13.png]C57-54-05 | Balance weight location channel S/B 6/507 When lowered
(D" nose). remove
leading edge
and weight
C57-54-06 | Trim tab hinge arm When lowered
C57-54-07 | Trim tab hinge. Vnen lowered
C57-54-08 | Gear tab hinge: When lowered






