
Summary of Changes

Global
Page number system was changed to current CAMP/AAIP system for standardization, ease of revisions.
Powerplant Section removed.  These items were already in Viking airframe inspection making most duplicate.  Migrated all that were not into the A 0125 and B 0250 as appropriate to manufacturers interval requirements.
R A007 & R E007 now combined into single 7-day Routine Insp, R 0007

Table of Contents
Title Page – Rev 2
Pg iii – Section 7 now Aircraft Log Page. Section 8 Inspections.  Added ATTACHMENTS. Page iv was not needed for continuation, now Manual Control
Pg iv – Manual Control updated to Rev 2
[bookmark: _MailAutoSig]
Log of Effective Pages
Pg vi thru viii – Updated effected pages to Rev 2 12/30/21
Pg ix – Updated, removed POWERPLACE INSPECTIONS

Preamble
Pg 1-1 – Removed “Test” from some items; redundant. Section is already labeled INSPECTIONS/TESTS
Pg 4-2 – Corrected Section first letters from “B” to “C” for C inspections. Removed POWERPLANT INSPECTIONS 
Pg 7-1 – Added Aircraft Log Page
Pg 8-1 – Replaces Page 7-1 AIRFRAME INSPECTION with just 8 INSPECTIONS
NOTE; All pagination changes from end of preamble until ATTACHMENTS at end of document.  Now each each inspection has own numbering system, so will only address changes in the body of each inspection sheet.

R 0007 (A 0007 and E 0007 inspections combined & renamed to R 0007)
Page 1
Removed “7.1 ROUTIINE A INSPECTIONS” from title
3.1 - Changed Appendix C to B
4.2 - No escape hatch doors in this aircaft, removed
Page 2
3.2 – Removed Note from 5.5, not applicable
Page 3 & 4
Wing inspections from old R E007. POST INSPECTION RII inspections blocks now colored in; not required
Page 5
Updated new inspection name in sign off

A 0125
Page 1
Aded PT6A MM to Reference:
1.3, 1.4  –  Added PTA6 MM to REF column as inspections from old P 0100 have been incorporated
3.1 – Changed Appendix C to B
Added 32 - LANDING GEAR NOSE (company requuirement)
5.2, 6.2 –  Removed AD note on Overspeed Gov; no applicable
Page 2
6.4 – (Prop RH & LH) Added blending nicks to 6.4. 
5.5, 6.5 - No gas tach or prop gen, changed to Prop tach gen, 
5.6, 6.6- No prop synch, replaced with shaft seal
8.1,2 & 9.1,2 – Incorporated old Powerplant P 0100 inspections verbiag
10.1, – Incorporated old Powerplant P 0100 inspections verbiag
72 – ENGINE – RH Incorporated old Powerplant P 0100 inspections verbiag
Page 3
10.4,5 – Incorporated old Powerplant P 0100 inspections
11.1-5 – Incorporated old Powerplant P 0100 inspections
12.1-7 – Incorporated old Powerplant P 0100 inspections
Page 4
12.8 thru 13.9 – Incorporated old Powerplant P 0100 inspections, High Pressure filter element removed, same as 12.3, P3 insp’s moved to CALM
Page 5
16.2, 17.2 – Removed Prop gen, already previously addressed in 5.5 & 6.5 Pg 2
18.2, 19.2 – P 0100 items added
Page 5
79 – OIL – LH Mag chip tests are required every 100 hr, will be tracked on CALM as there is no 100 hr CAMP interval
Page 6
79 – OIL – RH Same with Mag test above. 
80 – STARTING LH & RH – Our aircraft does not have glow plugs, replaced with ignition current regulator
Page 7
No high pressure fuel filter in aircraft.
Filled in RII blocks. Log entry does not need an RII, or checking oil levels

A 0250
Page 1 
Aded PT6A MM to Reference:
1.3,4 – Added PTA6 MM (because powerplant inspections were merged in), 
21 – AIRCONDITIONING removed, not installed
Page 2
12.1, 13.1 - No 74-micron elements on this aircraft, 
12.4, 13.4 - No wing tanks
Page 4
Colored in Nose wheel assy RII block
Page 6
61 – PROPELLERS LH & RH Removed AD N/A 
23.1, 24.1 Nick, cracks and blending already done every 125 hr in A 0125 6.4 and 7.4
72 – ENGINE LH & RH Merged engine inspections from old P 0400
Page 7 
80 – STARTING LH & RH has merged in engine inspections from old P 0400
Page 8
Fill in RII block on 26.6
Page 9
Fill in RII block on 27.4 and 27.5

C 0500
Page 1
Added Viking MM to Reference:
3.1 – Changed to Appx B
21 – AIRCONDITIONING Removed, not installed
Page 2
6.7 - No VOR duel selector relay installed
6.10.3 - Shaded in Function Test RII block, clarified “ground” test
Page 3
No HF Radio or inverters installed (-300 aircraft), SOO 6371 not installed
7.16 SOO 6371 not installed, inserted inspection of cables
Page 4
8.1.6 - No “Portable ELT”, just used insp to look at ELT mounting
8.3 - No baggage restraints installed
Page 5
9.12 - No stall warning light
Page 6
28-FUEL – 10.3, shaded in RII. No wing fuel tanks installed (10.4&5)
29 - HYD PWR - Shadded in RII block for hyd filter
Page 7
30 -ICE AND RAIN No windshielf washer system (12.8&9), or engine air intake anti-cing boots (12.10&11)
13.1.2 – Shaded in RII block
Page 9
15.15 -  Removed, only 1 TCAS antenna
15.16 – Removed, no lower TCAS antenna
15.18 – Removed, only 1 ADF antenna
36 – PNEUMATIC no bleed air strainers (16.30)
 
Page 10
18.3 - No airstair door, aftermarket IKHAHA FWD door installed only
Page 11
18.6 – Removed, no cabin roof hatch installed
Page 12
61 – PROPELLERS – LH & RH No autofeather limit switches or propeller synchronizer systems
Page 14
Removed 73 – ENGINE FUEL & CONT LH & RH; applicable to the  -27 engine only.
76-ENG CONTROLS Removed Note, SB not applicable.
Page 15
80 – STARTING LH & RH No spark ignitors on our engines
Page 16
36.1.5.4 Removed, no Prop syncrhonizers
36.1.8.2 Removed, no instrument pneumatic system strainers 
 36.1.8.5 Removed, no HP fuel filters
Page 17
Filled in RII blocks, not requred

C 1000RT
Page 1
3.1 – Changed to Appx B
Page 2
RMI & Annuciator not installed on our aircraft
Page 4
Pilot’s/CoPilots “mating” surfaces are from mating tray to airframe
Page 6
10.1.7 Shaded in RII block
Page 11
Removed everything from “Inspect CVR” to next segment, already in 14.25 thru 14.28
Page 13
Removed everything from 11.10 until end of segment.  Wing tanks not installed
Page 21 & 22
A few RII blocks got shaded in for items that did not really need an RII
Page 38
Segment 73 – ENGINE FUEL AND CONT LH & RH removed, P3 now tracked on CALM
OPERATIONAL CHECKS – Engine driven air pumps not intalled on this aircraft (36.2&3)

C 1500RT
Page 1
3.1 – Changed to Appx B
Page 2
5.13 – Removed, DeVore bleed air ducts not installed
6.1 – VHF/FM Removed, not installed
7.2 Volt meter rempoved, not installed. 
7.3 Load meter removed, not installed
Page 3
11.5 & 6 removed, no wing tanks
Page 5
16.1 This type of light (brushes) not installed, changed to just inspect light
16.2 Removed, no lower beacon light
Page 6
17.1 - Already listed under 6.2 Communications
18.1.4 – Removed, no eng press ind installed. Now ID’s thru CAS system
18.1.5 - Removed, no eng driven air pumps installed 
18.1.6 - Removed, no eng air pump system installed, workes with bleed air valve in cockpit
18.1.12 - Removed, no engine pressure indicators installed. Done thru CAS system
18.1.13 - Removed, no engine driven air pumps 
18.1.14 - Removed, no eng air pump system installed, workes with bleed air valve in cockpit
18.1.15 - Removed, no Emergency instrument vacuum installed on 400 series
18.1.16 - Removed, no pressure and suction indicator installed on 400 series
Page 7
Shaded in multiple RII boxes that were inadvertently left open
Page 8
53 – FUSELAGE Shaded in RII boxes in that were inadvertently left open
Page 12
Removed strob light pwr supply, already covered in 33 - LIGHTS
Page 13
Removed strob light pwr supply, already covered in 33 - LIGHTS
Page 14
27.1.5 Shaded in RII 
Page 16
28.6 – No collector tanks, just changed to insp fuel drain lines.
28-10 – Removed, nacelle waste fuel return line and connections.  No collector tanks on our aircraft
28-11 – Removed, not installed on our aircraft

Page 19 
Shaded in RII for Function Check flight and Log Book Entry.

C 1700NT
Page 1
3.1 – Changed to Appx B
5.1.4 – Added tension requirements
Page 2
5.2.4 – Added tension requirements
5.3.4 – Added tension requirements
Page 2 
Removed 23 – COMMUNICATIONS Mod not installed
Page 6 
Removed 34 NAVIGATION Tracked on CALM
Page 8
Shaded in RII for Function Check flight and Log Book Entry.

C 3000NT
Page 1
3.1 – Changed to Appx B
Page 3
36 – PNEUMATIC Pneumatic, the system described in this section is for the earlier model Twin
Otters, 100, 200, and 300 series. Replacing with components that are currently installed on the 400 series aircraft.
15-1 – Removed, automatic water drain is not installed on the aircraft. 
15.2 – Modified inspection for installed system
Page 4
52 – DOORS removed, both items not installed on our aircraft
Page 5
17.12 – Removed, no cabin roof hatch installed
17.13 – Removed, repeat of 17.2 in same section
Page 8
61 – L/H PROPELLERS removed Prop sych & Beta range system, not installed. Now auto feather system relay box
61 – R/H PROPELLERS removed Prop sych & Beta range system, not installed. Now auto feather system relay box
Page 10 
Shaded in RII for Function Check flight and Log Book Entry.

CT 6000NT
Page 1 – Removed 7.4 COMPONENT TESTS from heading

F 3000NT
Page 1 – Removed 7.5 FUNCTIONAL CHECKS from heading

