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	Issue Date:
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	SECTION:
	
	A 0601 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	600 HOUR / 12 MONTH INSPECTION
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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 412 MM-2 Chapter 5

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0601.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.5 Review Special Inspections and carry out applicable Inspections.
	Chp 5
	

	
	
	

	1.6 Examine all inspection windows and sight glasses for cracking, crazing, and discoloration. If any of these conditions are present, the part must be removed and replaced prior to returning helicopter for service.
	Chp 5
	

	
	
	

	A 0601.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0601.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	A 0601.4 GENERAL

	
	
	

	4.1 Remove all panels, fairings, and cowlings required to satisfactorily carry out the inspection.
	
	

	
	
	

	A 0601.5 FLIGHT CONTROLS

	
	
	

	5.1 Collective flights controls;
	Chp 67
	

	
	
	

	5.1.1 Inspect friction shoes and liners for condition.
	
	

	
	
	

	5.1.2 Check collective lever friction adjuster for operation.
	
	

	
	
	

	5.1.3 Check for proper collective minimum friction.
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.1.4 Check collective flight controls for smooth movement throughout full range of travel.
	
	

	
	
	

	5.1.5 Inspect friction shoes and liners for condition.
	
	

	
	
	

	5.2 Cyclic flight controls;
	Chp 67
	

	
	
	

	5.2.1 Inspect flight control systems bellcrank and control tubes for damage, chafing, corrosion, and security of attachment.
	
	

	
	
	

	5.2.2 Check cyclic stick friction adjuster for proper operation.
	
	

	
	
	

	5.2.3 Check for proper cyclic minimum friction.
	
	

	
	
	

	5.2.4 Check cyclic flight controls for smooth movement throughout full range of travel.
	
	

	
	
	

	5.3 Anti-torque flight controls
	Chp 67
	

	
	
	

	5.3.1 Flight control systems bellcrank and control tubes for damage, chafing, corrosion, and security of attachment.
	
	

	
	
	

	5.3.2 Check anti-torque friction adjuster for proper friction.
	
	

	
	
	

	5.3.3 Check anti-torque flight controls for smooth movement throughout full range of travel.
	
	

	
	
	

	5.4 Engine controls;
	Chp 76
	

	
	
	

	5.4.1 Check collective lever throttle friction adjusters for proper operation.
	
	

	
	
	

	5.5 Inspect all exposed fuel lines and attachments for leakage,cdamage, and security.
	Chp 28 & 71
	

	
	
	

	5.6 Fuselage cabin structure;
	Chp 53
	

	
	
	

	5.6.1 Fuselage structure for corrosion and damage to finish and sealant. Pay particular attention to edges of joints and seams and around fastener heads.
	
	

	
	
	

	5.6.2 Ensure all drain holes are open.
	
	

	
	
	

	5.6.3 Engine compartment floor and service deck, FS 155.06 to 241.22, for damage, delamination, and corrosion.
	
	

	
	
	

	5.6.4 Fuselage bonded panels for damage and delamination.
	
	

	
	
	

	5.6.5 Pylon wall for damage, working fasteners, cracks, delamination, and corrosion.
	
	

	
	
	

	5.7 Electrical system;
	Chp 96
	

	
	
	

	5.7.1 Check inverters for security of mounting and connections.
	
	

	
	
	

	5.7.2 Check generator control units for damage and security of mounting and terminals.
	
	

	
	
	

	5.7.3 Inspect all exposed wire bundles, bundle supports, and connectors for damage, corrosion, and security. Pay particular attention to engine deck connectors and harnesses.
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.7.4 Inspect relays and main bus area for security of mounting and connections.
	
	

	
	
	

	5.7.5 Inspect bus insulation for damage and condition.
	
	

	
	
	

	5.8 Fire extinguishing system;
	Chp 4 & 26 & 96
	

	
	
	

	5.8.1 Functionally check voltage of engine fire extinguishing circuits.
	
	

	
	
	

	5.8.2 Replace engine fire extinguisher container firing cartridges in accordance with specified service life.
	
	

	
	
	

	5.8.3 Visually inspect the loop clamp installed on modified discharge tubes 212-060-921-001FM and -002FM for condition and security until Part III of referenced ASB is accomplished.
	ASB 412-12-152
	

	5.9 Remove four access doors, located just forward of the aft crosstube, from the underside of the fuselage. Inspect fuel lines for evidence of leakage, damage, and security.
	Chp 28
	

	
	
	

	5.10 
	
	

	
	
	

	5.11 
	
	

	
	
	

	5.12 
	
	

	
	
	

	A 0601.6 

	
	
	

	6.1 
	
	

	6.2 
	
	

	
	
	

	6.3 
	
	

	
	
	

	6.4 
	
	

	
	
	

	6.5 
	
	

	
	
	

	A 0601.7 

	
	
	

	7.1 
	
	

	7.2 
	
	

	
	
	

	7.3 
	
	

	
	
	

	7.4 
	
	

	
	
	

	7.5 
	
	

	
	
	

	A 0601.8 POST INSPECTION

	
	
	

	8.1 Replace or close all applicable trim panels, fairings, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	8.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-412-FM-1
	

	
	
	

	8.3 Perform Functional Check Flight if required per Bell 412 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	8.4 Perform maximum NG topping check.
	Chp 76
Pratt & Whitney
PT6T-3 Series Maintenance
	

	
	Manual
	

	8.5 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	

	8.6 Confirm all required RII have been completed and signed off.
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 412 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 412 CAMP – A 0601 – 600 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




