		
412 CAMP REVISION NOTES
[bookmark: _Hlk54182798]Incorporate a daily inspection. – Will put in Appendix

The daily inspections shall be performed by a qualified mechanic after each day of operation, excluding the day the daily inspection was performed. This inspection will be valid until the aircraft is operated or 3 calendar days. A separate logbook entry shall be made if the daily inspection is required after not operating for 3 days. Aircraft will have a current daily inspection prior to returning to service – Added Instructions Preface; Chp 2 SCOPE OF INSPECTIONS Para 2.8 

For the 25 HR inspection we only need to track the T/R AD’s (which is tracked on CALM report) and the lube. Can track 25hr lube on CALM as well – Removed, put lubes on CALM when approved.

The daily inspection will replace the A0025 inspection – Added Daily; 25 hour is more comprehensive so will have to keep. It can take the place of the daily when performed.

[bookmark: _Hlk47015041]Remove B0056 (in B0156 there is an exhaust duct insp) and create a 50hr inspection incorporating inspection items from A0025 – Added it to the Daily Insp (since just a visual) A0006.15

50hr inspection will be performed at intervals not to exceed 50 flight hours aircraft time in service since previous 50hr inspection. Inspection will be done in conjunction with a complete daily inspection. - No 50 hour inspection.  Do we want to create one? If so, what would be on it?

Add a section for required torques and after maintenance is performed checks in CAMP manual - Appendix E

Create a maintenance time limitation table in the CAMP – Appendix C

[bookmark: _Hlk47015591][bookmark: _Hlk47015607]Add a column to inspection forms for items that require an RII – Let me know which items on inspections need RII. Be frugal as there will not always be a second mech and the FAA will limit items we try and approve a Pilot to perform, especially if they are technical and required a tool.

[bookmark: _Hlk47014895]Remove A0100-100hr/120 day insp and add battery inspection on to daily – Will delete A0100, but let me know where you want the battery inspections located in the Daily sheet you sent.

A0101-A0103 should be incorporated into the 300hr and 600hr inspections and not stand alone inspections. Ref Bell 412 MM Ch. 5 para 5-6.
A0101 Cannot find the reference for this so will just delete. May require a CALM entry.
A0102 is a Tailboom insp required by ASB 412-00-100.  Do we want to just track that ASB on CALM?
A0103 incorporated into A0306

In the 300hr inspections, remove tail rotor crosshead, tail rotor control lever and anti-tq flight control tubes lube and add to 50hr inspection – No 50 hour inspection to move to.  Do we want to create one?

A0306-300hr/12mo para 5.1.1 and 5.1.5 are N/A for our aircraft. We do not have elastomeric rod ends on any flight control rod end.- Removed

B0100 Para 6.1- not required because we have post SB5398 fuel surge accumulators - Removed

B0100 Para 6.2- perform engine deceleration ck not required for our engines. IAW 71-00-00 para O, and SB 5398 – Removed, only applicable to POST SB 5398
B0150- Para 5.6.2.1 and Para 5.6.4.1 need to be removed because we have post SB5354 chip detectors (quick disconnect style) - Removed

B0312- Para 5.7.1 note needs to be removed and fuel pump gear set and coupling need to be tracked on CALM because different pumps have different TSN – Removed, need to put on CALM when approved.

B0312- Para 5.10 and Para 5.11 note needs to be removed. This statement is not required because the inspection is for chip detectors not the entire engine. - Removed

B0600- Para 6.1- inspection of seam welds is not required on our engines. IAW SB5239 effectivity of SB is for PT6T-3 & 3B engines only - Removed

B01200RT- Para 5.2.1- inspection of seam welds is not required IAW SB5239 - Removed

RII task card R01 and R34 are the same – Removed R34

Create RII task cards for components that are not on RII task card listing. - See CAMP para 5.6.4

RII task card R01 para 2.7.1 is not required. We have HP’s. - Removed

RII task card R25 para 3.1-3.2 and 4.2 need to be changed to reflect TR drive shafts with Thomas couplings. REF BH 412 MM Ch. 65 Para 65-16 – Changed.

Add a section for required torques and after maintenance is performed checks in CAMP manual. – Appendix E
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