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	ATA:
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	TYPE:
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	TASK:
	
	Aerodynamically Actuated Elevator



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	RII
INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R53-10-10.1 GENERAL

	
	
	

	1.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	1.2 Check for entry in the discrepancy section of the log book/Work Order for RII due. At a minimum the log book entry shall contain the following: A description stating that the RII for the maintenance item is due. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	R53-10-10.2 PRIOR TO STARTING TASK

	
	
	

	2.1 Verify any new parts used have correct paperwork.
	
	

	
	
	

	2.2 Verify the maintenance manual is the correct revision number. Check MM revision number against the MHI master publications list.
	
	

	
	
	

	2.3 Check computer tracking system for any item or inspection that could be affected by the maintenance task.
	
	

	
	
	

	2.4 Inspect all calibrated tool’s inspection decal that will be used in the task to confirm it is in current calibration.
	
	

	
	
	

	2.5 Verify that any new P/N used is compatible with aircraft S/N.
	
	

	
	
	

	2.6 Read the MM section describing the task.
	
	

	
	
	

	2.7 Ensure a POC required for adjustment or installation of elevator is entered in the aircraft Log Book.
	
	

	
	
	

	R53-10-10.3  INPROCESS INSPECTIONS

	
	

	3.1 Prior to installation of access panel;
	

	
	

	3.1.1 Confirm bolts have been installed and safety.
	
	

	
	
	

	3.1.2 Apply torque strip after bolts have been checked for torque. (this is not required on hardware that contains safety’s)
	
	

	
	
	


	
	
	RII

INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R53-10-10.4  POST TASK INSEPCTIONS

	
	
	

	4.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	4.2 Check that elevator moves freely with no binding of spring. Check for excessive play in elevator horn shimming.
	Bell MM 
Chapter 67
	

	
	
	

	4.3 Check access panel bolts for attachment and security.
	
	

	
	
	


Upon satisfactory completion of each inspection item, the RII Inspector shall initial the pertinent space as provided.  All RII Inspectors shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form the RII Inspector shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  
This form shall be attached to the aircraft W.O. 
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I certify that I have used this RII card throughout the inspection process and have made an entry into the aircraft log book.
RII Inspectors Signature; ______________________________  
RII INSPECTION AUTHORIZATION CARD CERTIFICATE NUMBER; ________________________________

