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	Page No:
	3

	Revision:
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	Issue Date:
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	ATA:
	
	R64-10-01

	TYPE:
	
	RII TASK CARD

	TASK:
	
	TR rigging check



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	RII
INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R64-10-01.1 GENERAL

	
	
	

	1.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	1.2 Check for entry in the discrepancy section of the log book/Work Order for RII due. At a minimum the log book entry shall contain the following: A description stating that the RII for the maintenance item is due. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	R64-10-01.2 PRIOR TO STARTING TASK

	
	
	

	2.1 Verify any new parts used have correct paperwork.
	
	

	
	
	

	2.2 Verify the maintenance manual is the correct revision number. Check MM revision number against the MHI master publications list.
	
	

	
	
	

	2.3 Check computer tracking system for any item or inspection that could be affected by the maintenance task.
	
	

	
	
	

	2.4 Inspect all calibrated tool’s inspection decal that will be used in the task to confirm it is in current calibration.
	
	

	
	
	

	2.5 Verify that any new P/N used is compatible with aircraft S/N.
	
	

	
	
	

	2.6 Read the MM section describing the task.
	
	

	
	
	

	2.7 Verify;
	

	
	

	2.7.1 This RII card is not for use on 412EP helicopters
	
	

	
	
	

	2.7.2 A POC is required if any adjustment is made to the TR rigging and that it is entered into the aircraft Log Book.
	
	

	
	
	

	2.7.3 This card is written assuming you do not have access to hydraulic power cart. Refer to MM if hydraulic cart is used.
	
	

	
	
	

	2.7.4 Verify stops on bell crank below Tail Rotor servo are retracted completely prior to start.
	
	

	
	
	

	2.7.5 Verify the length of series actuator when centered prior to rigging procedure.
	
	

	
	
	

	2.7.6 Refer to Tail Rotor fiction RII task card
	
	

	
	
	


	
	
	RII

INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R64-10-01.3  INPROCESS INSPECTIONS

	
	

	3.1 Verify; 
	

	
	

	3.1.1 The rod end thread exposure is within limits on any control rod adjusted.
	
	

	
	
	

	3.1.2 Rod end jam nuts are properly torqued on any control rod adjusted.
	
	

	
	
	

	3.1.3 Control rods are free to rotate several degrees about the longitudinal axis on any control rod adjusted.
	
	

	
	
	

	3.1.4 Control rod between pilot and copilot pedal adjuster is the correct length.
	
	

	
	
	

	3.1.5 Clearance between link and bell crank below TRGB.
	
	

	
	
	

	3.1.6 Control tube below engine CBOX is adjusted correctly.
	
	

	
	
	

	3.1.7 Stops on bell crank below servo are adjusted correctly.
	
	

	
	
	

	3.1.8 Clearance between TR blade and flap stop.
	
	

	
	
	

	3.1.9 Anti torque magnetic brake arm is installed correctly.
	
	

	
	
	

	3.1.10 Force gradient to pilot pedal adjuster is adjusted correctly.
	
	

	
	
	

	3.1.11 Clearance of force gradient while moving the pedals stop to stop.
	
	

	
	
	

	3.1.12 CMT transducers are adjusted to the correct length.
	
	

	
	
	

	R64-10-01.4 POST TASK INSPECTIONS

	
	
	

	4.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	4.2 Verify;
	
	

	
	
	

	4.2.1 Force gradient and transducer at the pilots pedal adjuster
	
	

	
	
	

	4.2.2 Control tube at copilots pedal adjuster
	
	

	
	
	

	4.2.3 Control tube at bell crank below the CBOX
	
	

	
	
	

	4.2.4 Link at TRGB
	
	

	
	
	

	4.2.5 PC link
	
	

	
	
	


Upon satisfactory completion of each inspection item, the RII Inspector shall initial the pertinent space as provided.  All RII Inspectors shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form the RII Inspector shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  
This form shall be attached to the aircraft W.O. 
	
	
	RII INSPECTOR

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I certify that I have used this RII card throughout the inspection process and have made an entry into the aircraft log book.
RII Inspectors Signature; ______________________________  
RII INSPECTION AUTHORIZATION CARD CERTIFICATE NUMBER; ________________________________

