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	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	RII
INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R 16.1 GENERAL

	
	
	

	1.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	1.2 Check for entry in the discrepancy section of the log book/Work Order for RII due. At a minimum the log book entry shall contain the following: A description stating that the RII for the maintenance item is due. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	R 16.2 PRIOR TO STARTING TASK

	
	
	

	2.1 Verify any new parts used have correct paperwork.
	
	

	
	
	

	2.2 Verify the maintenance manual is the correct revision number. Check MM revision number against the MHI master publications list.
	
	

	
	
	

	2.3 Check computer tracking system for any item or inspection that could be affected by the maintenance task.
	
	

	
	
	

	2.4 Inspect all calibrated tool’s inspection decal that will be used in the task to confirm it is in current calibration.
	
	

	
	
	

	2.5 Verify that any new P/N used is compatible with aircraft S/N.
	
	

	
	
	

	2.6 Read the MM section describing the task.
	
	

	
	
	

	2.7 An POC is required for adjustment of the throttles.
	
	

	
	
	

	R 16.3 INPROCESS INSPECTIONS

	
	

	3.1 Verify;
	

	
	

	3.1.1 Control tube rod ends have not exceeded the maximum exposed thread lengths.
	
	

	
	
	

	3.1.2 Safeties are installed in all locations.
	
	

	
	
	

	3.1.3 Correct torque was used on control tube jam nuts.
	
	

	
	
	

	3.1.4 Control tube rod ends are adjusted so both ends are centered on bellcranks allowing the maximum rotation of the control tube.
	
	

	
	
	

	3.1.5 Collective flex shaft to gear selector has proper engagement (pilot and copilot. Number one and two throttles).
	
	

	
	
	


	
	
	RII

INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	3.1.6 Pilot and co pilot throttles hit the collective lever stops at the same time.
	
	

	
	
	

	3.1.7 Number 1 and 2 FCU levers are positioned correctly on the shaft.
	
	

	
	
	

	3.1.8 Correct torque on nut of FCU lever if adjusted.
	
	

	
	
	

	3.1.9 Correct gap of fuel control interconnect.
	
	

	
	
	

	R 16.4 POST TASK INSEPCTIONS

	
	

	4.1 Verify;
	

	
	

	4.1.1 Smooth operation of the throttles through the entire range.
	
	

	
	
	

	4.1.2 Idle speeds are correct.
	
	

	
	
	

	4.1.3 Tube clearance in the area of the FCU tubing.
	
	

	
	
	

	4.1.4 Throttle cushions are the correct amount.
	
	

	
	
	

	4.1.5 Both throttles rotate approx the same degrees from stop to stop.
	
	

	
	
	

	4.1.6 FCU stops hit prior to collective lever stops.
	
	

	
	
	

	4.1.7 Cushions are equal on full open and full closed positions.
	
	

	
	
	

	4.2 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	


Upon satisfactory completion of each inspection item, the RII Inspector shall initial the pertinent space as provided.  All RII Inspectors shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form the RII Inspector shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  
This form shall be attached to the aircraft W.O./Log Book. 
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I certify that I have used this RII card throughout the inspection process and have made an entry into the aircraft log book.
RII Inspectors Signature; ______________________________  
RII INSPECTION AUTHORIZATION CARD CERTIFICATE NUMBER; ________________________________

