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1
MAINTENANCE EXCLUDED FROM CAMP 
Since the CAMP inspection program is not intended to prescribe maintenance functions, the following items will be tracked separately in the aircraft status report. 

A. Hand-held Fire Extinguishers
B. Static System and Altitude Reporting System per 14 CFR 91.411., BHT-412MM-CH05
C. ATC Transponder Test and Inspections per 14 CFR 91.413., BHT-412MM-CH05
D. Inspect Pitot-Static System per 14 CFR 91.411/413, BHT-412MM-CH05 
E. 36 Month Hydrostatic Retest of Emergency Floatation Gas Cylinder per AA-ICA407-11
F. 300 Hour / 12 Month Starter Generator Inspection per BHT-412MM-CH05
G. 600 Hour Engine Maximum Ng Topping Check per BHT-412MM-CH05
H. 600 Hour / 12 Month Lubrications per BHT-MM-2 Table 12-3 Lubrication Chart 
I. 300 Hour / 12 Month Fuel Pump Inspection per SB5003


