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After Maintenance Torque Checks and Inspections
	TASK
	REFERENCE

	Between 1 and 5 flight hours after main rotor hub installation
	BHT-412-MM-2

5-18

	Between 1 and 25 flight hours after expandable blade bolt installation
	BHT-412-MM-2

5-19

	Between 5 and 10 flight hours after tail rotor hub and blade installation
	BHT-412-MM-2

5-20

	Between 5 and 10 flight hours after tail rotor gear box installation
	BHT-412-MM-2

5-20

	Between 5 and 10 flight hours after intermediate gearbox installation
	BHT-412-MM-2

5-20

	Each 25 flight hours, for 100 hours, inspect tail rotor hanger bearing witness marks
	BHT-412-MM-2

5-21

	Each 25 flight hours of tail rotor operations inspection of tail rotor static stop
	BHT-412-MM-2

5-22

	50 hours after installation of tailboom, torque check anti-torque bellcrank support attachment nuts.
	BHT-415-22-MM-5-23

	50 hours after installation of rotor brake, torque check caliper and disk attachments bolts 
	BHT-415-22-MM-5-23

	100 hours after installation of tailboom, torque check attachment bolts.
	BHT-415-22-MM-5-24

	Recalibrate compass after removal/ installation or new unit
	IAW AC43-13.1b
Chp 12, Section 3

	
	

	
	

	
	


