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	AIRWORTHINESS CHECK

	
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
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	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0001.1 GENERAL

	
	
	

	1.1 Review aircraft computer status run, Deferred/MEL list and logbook ladder for maintenance and/or inspection requirements.  
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	A 0001.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0001.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	A 0001.4 TAIL BOOM L/H SIDE

	
	
	

	4.1 Tail boom structure for general condition, damage and corrosion.
	Chp 53
	

	
	
	

	4.2 Tail rotor drive shafts for condition, flex couplings and bearings for overheating, and grease leakage. Check overheat indicator stripe on bearing hanger for discoloration. When temp-plate indicators are installed, check temp-plates for discoloration.  If temp-plates are discolored or missing, refer to BHT-412-MM, Chapter 63 for Inspection Criteria Before Next Flight.
	Chp 65/67

BHT-412-MM, Chapter 63
	

	
	
	

	4.3 Clamp sets for proper installation and alignment.
	
	

	
	
	

	4.4 Tail rotor driveshaft covers for condition and security.
	
	

	
	
	

	4.5 Elevators for general condition and security.
	
	

	
	
	

	4.6 Smooth operation of elevator spring.
	
	

	
	
	

	4.7 Tail boom stinger for looseness and security.
	
	

	
	
	

	4.8 Vertical fin for general condition.
	
	

	
	
	

	4.9 Tail rotor gearbox for security, oil leaks, obvious damage and proper oil level.
	
	

	
	
	

	4.10 Tail rotor pitch change mechanism for general condition and excessive wear.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0001.5 TAIL BOOM R/H SIDE

	
	
	

	5.1 Tail rotor blades for obvious damage, security, and cleanliness. Check for compliance of daily AD 2008-10-03
	Chp 64
	

	
	
	

	5.2 Inspect P/N 212-011-713-103 flapping stop for yielding.
	
	

	
	
	

	5.3 Tail rotor crosshead and pitch change links for general condition and security.
	
	

	
	
	

	5.4 Binding of PC links with tail rotor to both full flapping positions. Binding is not acceptable.
	
	

	
	
	

	5.5 Inspect counterweights and counterweigh links for wear and excessive play.
	
	

	
	
	

	5.6 Inspect tail rotor blade to yoke bearings for excessive play.
	
	

	
	
	

	5.7 Inspect tail rotor trunnion bearings for excessive play.
	
	

	
	
	

	5.8 Lubricate Tail Rotor Trunnion Bearings (two). Do not intermix grease types. Purge until same grease appears
	Table 12-3

Lubrication Chart
	

	
	
	

	5.9 Tail rotor hub for condition and security.
	
	

	
	
	

	5.10 Tail rotor drive shafts for condition, flex couplings and bearings for overheating, and grease leakage.  When temp-plate indicators are installed, check temp-plates for discoloration.  If temp-plates are discolored or missing, refer to BHT-412-CR&O, Chapter 63 for Inspection Criteria Before Next Flight.
	BHT-412-CR&O, Chapter 63
	

	
	
	

	5.11 T/R driveshaft Thomas couplings for condition and security.
	
	

	
	
	

	5.12 Tail rotor driveshaft covers for condition and security.
	
	

	
	
	

	5.13 Vertical fin for general condition.
	
	

	
	
	

	5.14 42 degree gearbox for security, oil leaks, obvious damage and proper oil level.
	Chp 65
	

	
	
	

	5.15 Elevators for general condition and security, control tube for positive spring action and freedom of movement.
	Chpt 67
	

	
	
	

	5.16 Tail boom for general condition, avionics equipment for condition and security.
	Chp 53/97
	

	
	
	

	5.17 Baggage compartment door for proper operation. Check compartment for condition and cleanliness.
	Chp 53
	

	A 0001.6 FUSELAGE R/H SIDE AND NOSE

	
	
	

	6.1 Fuselage exterior for obvious damage, evidence of fuel and oil leaks, damage to protective finish and pitot static ports for obstructions.
	
	

	6.2 Oil coolers for damage, corrosion and obstruction, hoses and tubes for leakage, damage and fraying.
	Chp 79
	

	
	
	

	6.3 Tail rotor servo compartment for cleanliness, corrosion, and leaks.
	Chp 29/67
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	6.4 Tail rotor hydraulic actuator for leaks and security, control tubes for condition.
	Chp 29/67
	

	
	
	

	6.5 Visible flight controls for attachment and security.
	
	

	
	
	

	6.6 Tail boom attachment points for cracks, security and evidence of fretting.
	Chp 53
	

	
	
	

	6.7 Heater compartment for general condition, security and cleanliness. Structure for damage and corrosion (including connections and fasteners).
	Chp 21
	

	
	
	

	6.8 Avionics and Electrical compartment for general condition, water entrapment.
	
	

	
	
	

	6.9 Combining gearbox for evidence of fuel or oil leaks and any obvious damage, security and condition of plumbing, electrical systems, and accessories.
	
	

	
	
	

	6.10 Combining gearbox for proper oil level.
	
	

	
	
	

	6.11 Engine and reduction gearbox mounts for loose bearings, condition and security.
	Chp 71
	

	
	
	

	6.12 Oil cooler blowers for damage, corrosion and obstruction.
	
	

	
	
	

	6.13 Engine fire extinguisher bottles, proper charge, and security.
	Chp 26
	

	
	
	

	6.14 Engine mounts for condition and security.
	
	

	
	
	

	6.15 Exhaust ejector for condition and security.
	
	

	
	
	

	6.16 Engine cowling for condition, security, and proper operation of latches.
	
	

	
	
	

	6.17 Tail rotor drive shafts for condition, flex couplings and bearings for overheating, and grease leakage.  When temp-plate indicators are installed, check temp-plates for discoloration.  If temp-plates are discolored or missing, refer to BHT-412-MM, Chapter 63 for Inspection Criteria Before Next Flight.
	BHT-412-CR&O, Chapter 63
	

	
	
	

	6.18 T/R driveshaft Thomas couplings for condition and security.
	
	

	
	
	

	6.19 Firewalls for general condition, cracks, and deteriorated gaskets.
	
	

	
	
	

	6.20 Power section for evidence of fuel or oil leaks and any obvious damage, security and condition of plumbing, electrical systems, and accessories
	
	

	
	
	

	6.21 Power section 1 for proper oil level.
	
	

	
	
	

	6.22 Engine mounts for condition and security.
	
	

	
	
	

	6.23 Exposed area of main beam adjacent to engine fwd mount for cracks.
	
	

	
	
	

	6.24 Fuel cap for security and proper operation.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	6.25 Sliding door for wear and proper operation.
	
	

	
	
	

	6.26 Transmission for proper oil level.
	
	

	
	
	

	6.27 Transmission tail rotor output quill for grease leakage and for evidence of overheating. When temp-plate indicators are installed, check temp-plates for discoloration.  If temp-plates are discolored or missing, refer to BHT-412-MM, Chapter 63 for Inspection Criteria Before Next Flight.
	
	

	
	
	

	6.28 Interior of pilot and passenger compartment for proper storage of loose equipment, map case, cleanliness, and overall condition; and passenger briefing cards are in the aircraft.  Check first aid kit for proper sealing and inspection due date.
	Chp 25
	

	
	
	

	6.29 Condition, cleanliness, excessive deterioration, tears and security of crew and passenger seating. Check restraint assemblies for condition and security.
	Chp 25
	

	
	
	

	6.30 Life vests for general condition, inspection due date, CO2 bottles for tightness and inflation valve locks for integrity.  Check life raft (in cabin) general appearance, security and inspection due date. (if installed)
	
	

	
	
	

	6.31 Supplementary emergency lighting (if installed) for security and general condition.
	
	

	
	
	

	6.32 Hydraulic filter bypass indicator buttons. (In hell hole) – not extended.
	Chp 29
	

	
	
	

	6.33 Cabin fire extinguishers for damage and corrosion; security and proper operation of mounting brackets.  Ensure safety pin is installed and that it is secured in place with plastic safety tie.
	Chp 26
	

	
	
	

	6.34 Landing gear and floats for obvious damage, supports for wear, corrosion or damage and security of attachment.
	Chp 32
	

	
	
	

	6.35 Crew and passenger access steps for condition and security.
	
	

	
	
	

	6.36 Crew doors (and surrounding structure) for proper operation and condition. Check for security of emergency release system.
	Chp 52
	

	
	
	

	6.37 Pitot and static ports for blockage and damage.
	
	

	
	
	

	6.38 Windows and windshield for obvious damage and cleanliness. Check windshield wipers and blades for condition and security.
	Chp 52
Chp 30
	

	
	
	

	6.39 Remote hydraulic filter bypass indicator for bypass condition.
	Chp 29
	

	
	
	

	6.40 Tail rotor pedals and visible flight controls for attachment and security.
	
	

	
	
	

	6.41 Transmission chip detector cat eye indicators are not tripped.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	6.42 Heating and venting components, air ducts, for condition and security.
	Chp 21
	

	
	
	

	6.43 Battery, mounts, external connections and vents for corrosion, security and condition, vent and drains for blockage. Service as needed I/A/W manufactures recommendations.
	
	

	
	
	

	6.44 Avionics bay for general condition of electrical wires, security of equipment and water entrapment.
	Chp 97
	

	
	
	

	A 0001.7 FUSELAGE NOSE AND L/H SIDE

	
	
	

	7.1 Windows and windshield for obvious damage and cleanliness.
	Chp 52
	

	
	
	

	7.2 If installed, emergency float reservoir for correct pressure and inflation valve safety pin is removed and properly stowed.
	
	

	
	
	

	7.3 Tail rotor pedals and visible flight controls for attachment and security.
	
	

	
	
	

	7.4 Pitot and static ports for blockage and damage.
	Chp 95
	

	
	
	

	7.5 Crew door for proper operation, condition and security of emergency release system.
	
	

	
	
	

	7.6 Crew and passenger access steps for condition and security.
	
	

	
	
	

	7.7 Landing gear and floats for obvious damage.
	Chp 32
	

	
	
	

	7.8 Sliding door for wear and proper operation.
	
	

	
	
	

	7.9 Exposed area of main beam adjacent to engine fwd mount for cracks.
	
	

	
	
	

	7.10 Engine and reduction gearbox mounts for loose bearings, condition and security.
	Chp 71
	

	
	
	

	7.11 Power section 2 for proper oil level.
	
	

	
	
	

	7.12 Power section for evidence of fuel or oil leaks and any obvious damage, security and condition of plumbing, electrical systems, and accessories.
	
	

	
	
	

	7.13 Firewalls for general condition, cracks, and deteriorated seal or gaskets.
	Chp 71
	

	
	
	

	7.14 Engine cowling for condition, security, and proper operation of latches.
	Chp 71
	

	
	
	

	7.15 Exhaust ejector for condition and security.
	
	

	
	
	

	7.16 Exhaust ducts for cracks and/or distortion, condition and security.
	
	

	
	
	

	7.17 Engine fire extinguisher bottles, proper charge, and security.
	
	

	
	
	

	7.18 Oil cooler blowers for damage and obstruction.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	7.19 Combining gearbox for evidence of fuel or oil leaks and any obvious damage, security and condition of plumbing, electrical systems, and accessories.
	
	

	
	
	

	7.20 Reduction gearbox oil filter impending bypass indicator button - not extended
	
	

	
	
	

	7.21 Avionics/electrical compartments for general condition, water entrapment.
	Chp 96/97
	

	
	
	

	A 0001.8 FUSELAGE BOTTOM

	
	
	

	8.1 Life raft bottle for security and proper charge.
	
	

	
	
	

	8.2 Belly for evidence of fuel or oil leaks and any obvious damage, security and condition of plumbing, electrical systems, and accessories.
	Chp 53
	

	
	
	

	8.3 The “hell hole” for evidence of fuel or oil leaks and any obvious damage, security and condition of plumbing, electrical systems, and accessories.
	Chp 53
	

	
	
	

	8.4 Inspect “hell hole” visible flight controls for attachment and security.
	
	

	
	
	

	8.5 Hydraulic servos, valves, and lines for leakage and general condition.
	Chp 29
	

	
	
	

	8.6 Cargo hook function and security.
	
	

	
	
	

	8.7 Drains are free of obstructions.
	
	

	
	
	

	8.8 Antennas for condition and security.
	
	

	
	
	

	A 0001.9 FUSELAGE TOP

	
	
	

	9.1 Antennas for condition and security.
	
	

	
	
	

	9.2 Hydraulic reservoirs #1 and #2 for proper fluid level.
	Chp 29
	

	
	
	

	9.3 Transmission and transmission oil lines, for oil leaks, obvious damage, loose accessories, and fittings.
	Chp 63
	

	
	
	

	9.4 Rotor brake for leakage and security, disc for warpage, evident of overheat, caliper switches and wiring for condition and security.
	Chp 63
	

	
	BHT-412-SI-12
	

	9.5 Hydraulic lines, valves and filter modules & pumps for leaks damage and security.
	Chp 29
	

	
	
	

	9.6 Transmission external oil filter for bypass indication.
	
	

	
	
	

	9.7 Main driveshaft forward and aft couplings for grease leakage and evidence of overheating.  When template indicators are installed check temp-plates for discoloration.  If temp-plates are discolored or missing, refer to BHT-412-MM, Chapter 63 for Inspection Criteria Before Next Flight.
	Chp 63
	

	
	
	

	9.8 Flight controls system from servos to main rotor head for obvious damage and security.
	
	

	
	
	

	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	9.9 Mast assembly for obvious damage, bearing seal for leaks.
	Chp 63
	

	
	
	

	9.10 Main rotor pitch links for security, bearings for wear
	Chp 62
	

	
	
	

	9.11 Rephasing levers for bearing looseness and security.
	Chp 62
	

	
	
	

	9.12 Main rotor P/C link rod end bearings using work aid as per chapter 62 of the MM.
	Chp 62
	

	
	
	

	9.13 Main rotor hub for obvious damage, pendulum dampers for condition and security.  Lubricate pendulum damper bearings with Mobil 28 grease.
	Chp 62
	

	
	
	

	9.14 Pitch horns for cracks in areas surrounding torque transfer pin holes.
	Chp 62
	

	
	
	

	9.15 Condition of MR head elastomeric components.
	Chp 62
	

	
	
	

	9.16 Main rotor blades for obvious damage.
	Chp 62
	

	
	
	

	9.17 Engine #1 and #2 air intake ducts for condition and obstructions.
	
	

	
	
	

	A 0001.10 ELECTRICAL

	
	
	

	10.1 Drain fuel sumps and fuel filters, check for presence of water and other contaminates
	Chp 28
	

	
	
	

	10.2 Operation of door lights.
	
	

	
	
	

	10.3 Operation of pitot and static ports heat.
	
	

	
	
	

	10.4 All exterior navigation, anti-collision, landing and search lights for condition and proper operation.
	
	

	
	
	

	10.5 Master caution panel and interior lighting for proper operation, baggage compartment smoke detector press to test functions.
	
	

	
	
	

	10.6 BHVM (HUMMS) and engine monitoring system for indication of exceedances. Ensure data has been uploaded to the website at least once a day or any time of suspected exceedance.
	
	

	
	
	

	10.7 Placards, decals, and markings for legibility and appearance.
	
	

	
	
	


	
	
	MECHANIC’S

INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0001.11 POST INSPECTION

	
	
	

	11.1 Condition and security of all cowling and access panels, all secure.
	
	

	
	
	

	11.2 Aircraft documents for proper entries.
	GMM 2.1
	

	
	
	


