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	Registration No.:
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	RII
INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R 14.1 GENERAL

	
	
	

	1.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	1.2 Check for entry in the discrepancy section of the log book/Work Order for RII due. At a minimum the log book entry shall contain the following: A description stating that the RII for the maintenance item is due. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	R 14.2 PRIOR TO STARTING TASK

	
	
	

	2.1 Verify any new parts used have correct paperwork.
	
	

	
	
	

	2.2 Verify the maintenance manual is the correct revision number. Check MM revision number against the MHI master publications list.
	
	

	
	
	

	2.3 Check computer tracking system for any item or inspection that could be affected by the maintenance task.
	
	

	
	
	

	2.4 Inspect all calibrated tool’s inspection decal that will be used in the task to confirm it is in current calibration.
	
	

	
	
	

	2.5 Verify that any new P/N used is compatible with aircraft S/N.
	
	

	
	
	

	2.6 Read the MM section describing the task.
	
	

	
	
	

	2.7 Prior to Installation verify integrity of lock wiring and locking seals on unit.
	
	

	
	
	

	R 14.3 INPROCESS INSPECTIONS

	
	
	

	3.1 For PT6T-3B Engines verify MFCU seal drain port is installed.
	
	

	
	
	

	3.2 Verify that strainer (34) and seat (33) have been installed prior to installing fuel inter-connect tube into AFCU port.
	
	

	
	
	

	3.3 Ensure retaining plate(28) has been installed, torqued, and safetied.
	
	

	
	
	

	3.4 Ensure proper packings are placed in fuel ports at MFCU/Fuel Pump mating surfaces. (If there are still old packings in these recesses they must be discarded and replaced)
	
	

	
	
	

	3.5 On all Post-SB5041 and PT6T-3B/-3BE engines ensure Pressure Regulating Valve has been properly installed.
	
	

	
	
	


	
	
	RII

INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	3.6 Before MFCU/AFCU linkage is installed ensure that a fits and clearances check has been performed IAW P&W PT6T-3B MM.
	
	

	
	
	

	R 14.4 POST TASK INSEPCTIONS

	
	

	4.1 Verify;
	

	
	

	4.1.1 MFCU/AFCU interconnect linkage is attached.
	
	

	
	
	

	4.1.2 Ensure Bolts securing MFCU to Fuel Pump have been properly torqued and torque striped.
	
	

	
	
	

	4.1.3 Ensure all attached fuel lines have been secured and torqued properly.
	
	

	
	
	

	4.1.4 All lines with holes drilled in the B-Nut have been safetied wired properly.
	
	

	
	
	

	4.1.5 That following engine checks are written up in the logbook;
	

	
	

	4.1.5.1 Dry Motoring Run
	
	

	
	
	

	4.1.5.2 Wet Motoring Run
	
	

	
	
	

	4.1.5.3 Max Ng. and Manual/Automatic Interconnect Linkage Adjustment
	
	

	
	
	

	4.1.5.4 Power Turbine Governor Check
	
	

	
	
	

	4.1.5.5 Power Check
	
	

	
	
	

	4.1.5.6 Acceleration Check
	
	

	
	
	

	4.1.5.7 Deceleration Check
	
	

	
	
	


Upon satisfactory completion of each inspection item, the RII Inspector shall initial the pertinent space as provided.  All RII Inspectors shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form the RII Inspector shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  
This form shall be attached to the aircraft W.O/Log Book. 
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I certify that I have used this RII card throughout the inspection process and have made an entry into the aircraft log book.
RII Inspectors Signature; ______________________________  
RII INSPECTION AUTHORIZATION CARD CERTIFICATE NUMBER; ________________________________


