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	Page No:
	4

	Revision:
	Reissue

	Issue Date:
	08/15/15

	SECTION:
	
	R 29 – BELL 412 CAMP

	TYPE:
	
	RII TASK CARD

	TASK:
	
	Bell 412 Main Rotor Spindles



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	RII
INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R 29.1 GENERAL

	
	
	

	1.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	1.2 Check for entry in the discrepancy section of the log book/Work Order for RII due. At a minimum the log book entry shall contain the following: A description stating that the RII for the maintenance item is due. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	R 29.2 PRIOR TO STARTING TASK

	
	
	

	2.1 Verify any new parts used have correct paperwork.
	
	

	
	
	

	2.2 Verify the maintenance manual is the correct revision number. Check MM revision number against the MHI master publications list.
	
	

	
	
	

	2.3 Check computer tracking system for any item or inspection that could be affected by the maintenance task.
	
	

	
	
	

	2.4 Inspect all calibrated tool’s inspection decal that will be used in the task to confirm it is in current calibration.
	
	

	
	
	

	2.5 Verify that any new P/N used is compatible with aircraft S/N.
	
	

	
	
	

	2.6 Read the MM section describing the task.
	
	

	
	
	

	2.7 Ensure a POC required is entered in log book for the replacement of MR spindles.
	
	

	
	
	

	2.8 Refer to Main Rotor Head task card if MR Head is removed.
	
	

	
	
	

	2.9 Refer to MR PC link task card.
	
	

	
	
	

	2.10 Refer to MR blade task card.
	
	

	
	
	

	2.11 Mark damper bridge locations for reinstallation prior to removal.
	
	

	
	
	

	2.12 Mark pendulum dampers position for reinstallation. (if removed)
	
	

	
	
	

	2.13 Mark droop restraints position for reinstallation prior to removal.
	
	

	
	
	


	
	
	RII

INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R 29.3 INPROCESS INSPECTIONS

	
	

	3.1 Verify;
	

	
	

	3.1.1 Pins in pivot bearings are properly seated in spindle.
	
	

	
	
	

	3.1.2 Pivot bearings are installed using wet primer.
	
	

	
	
	

	3.1.3 Pins are installed in the pitch horn to spindle.
	
	

	
	
	

	3.1.4 Pins in pivot bearings are properly seated in fitting.
	
	

	
	
	

	3.1.5 Damper sets SN’s are matched.
	
	

	
	
	

	3.1.6 Shims are correct thickness.
	TB 412-90-92
	

	
	
	

	3.1.7 Dampers are bonded in bridge.
	
	

	
	
	

	R 29.4 POST TASK INSEPCTIONS

	
	

	4.1 Verify;
	

	
	

	4.1.1 Spindles are installed with blade bolt lock pin in the up position.
	
	

	
	
	

	4.1.2 The correct torque was used on;
	

	
	

	4.1.2.1 Hardware connecting pitch horn to spindle.
	
	

	
	
	

	4.1.2.2 Spindle to pivot bearings.
	
	

	
	
	

	4.1.2.3 Pivot bearings to yoke.
	
	

	
	
	

	4.1.2.4 Bridge damper to yoke.
	
	

	
	
	

	4.1.2.5 Damper to damper bearing.
	
	

	
	
	

	4.1.2.6 Pendulum damper to yoke.
	
	

	
	
	

	4.1.3 Droop stops are installed in correct location.
	
	

	
	
	

	4.1.4 Torque and safeties on droop stop dampers.
	
	

	
	
	

	4.1.5 Safeties are installed.
	
	

	
	
	

	4.1.6 Damper bridge is installed in correct locations as marked when removed.
	
	

	
	
	

	4.1.7 Pendulum dampers are installed in correct locations as marked when removed. (if removed)
	
	

	
	
	


	
	
	RII

INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	4.2 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	


Upon satisfactory completion of each inspection item, the RII Inspector shall initial the pertinent space as provided.  All RII Inspectors shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form the RII Inspector shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  
This form shall be attached to the aircraft W.O./Log Book. 
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I certify that I have used this RII card throughout the inspection process and have made an entry into the aircraft log book.
RII Inspectors Signature; ______________________________  
RII INSPECTION AUTHORIZATION CARD CERTIFICATE NUMBER; ________________________________


