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	Page No:
	4
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	SECTION:
	
	R 31 – BELL 412 CAMP

	TYPE:
	
	RII TASK CARD

	TASK:
	
	Bell 412 Engine Installation (Twin Pack)



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


	
	
	RII
INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	R 31.1 GENERAL

	
	
	

	1.1 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	1.2 Check for entry in the discrepancy section of the log book/Work Order for RII due. At a minimum the log book entry shall contain the following: A description stating that the RII for the maintenance item is due. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	

	R 31.2 PRIOR TO STARTING TASK

	
	
	

	2.1 Verify any new parts used have correct paperwork.
	
	

	
	
	

	2.2 Verify the maintenance manual is the correct revision number. Check MM revision number against the MHI master publications list.
	
	

	
	
	

	2.3 Check computer tracking system for any item or inspection that could be affected by the maintenance task.
	
	

	
	
	

	2.4 Inspect all calibrated tool’s inspection decal that will be used in the task to confirm it is in current calibration.
	
	

	
	
	

	2.5 Verify that any new P/N used is compatible with aircraft S/N.
	
	

	
	
	

	2.6 Read the MM section describing the task.
	
	

	
	
	

	2.7 Verify POC is entered in Log Book.
	
	

	
	
	

	2.8 Refer to AFCU, MFCU, governor, main driveshaft, N1 rigging, N2 rigging, NG topping, TCU limiting task cards.
	
	

	
	
	

	R 31.3 INPROCESS INSPECTIONS

	
	
	

	3.1 Inspect inside air box for loose hardware and FOD.
	
	

	
	
	

	3.2 Verify;
	

	
	

	3.2.1 Proper torque was used on forward engine mounts and check for safeties.
	
	

	
	
	

	3.2.2 All tubing, hoses, electrical, and clamping is secured and safeties on front of accessory gearbox.
	
	

	
	
	

	3.2.3 Fire detector “cigarettes” are installed in fire detector harness connectors.
	
	

	
	
	


	
	
	RII

INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	3.2.4 Oil filters are installed.
	
	

	
	
	

	3.2.5 Filters are installed.
	
	

	
	
	

	3.2.6 P3 filters are installed. Qty 2 (alternate Qty 2)
	
	

	
	
	

	R 31.4 POST TASK INSEPCTIONS

	
	

	4.1 Verify;
	

	
	

	4.1.1 Oil cooler blower boots are installed correctly.
	
	

	
	
	

	4.1.2 All tubing, hoses, electrical, and clamping is secured and safeties on reduction gearbox. Pay particular attention to electrical connectors above the driveshaft.
	
	

	
	
	

	4.1.3 Proper torque and safeties on rear engine mounts.
	
	

	
	
	

	4.1.4 N2 control rod hardware is torqued and safeties.
	
	

	
	
	

	4.1.5 All tubing, hoses, electrical, and clamping is secured and safeties on power sections.
	
	

	
	
	

	4.1.6 Calibration of the torque transmitter system is complied with.
	
	

	
	
	

	4.1.7 Internal thermocouple resistance check was complied with.
	
	

	
	
	

	4.1.8 Igniters have been tested for operation.
	
	

	
	
	

	4.1.9 Firewalls and firewall seals are properly aligned.
	
	

	
	
	

	4.1.10 All firewalls for loose or missing hardware.
	
	

	
	
	

	4.1.11 Engine and reduction gearbox is properly serviced.
	
	

	
	
	

	4.1.12 Bonding straps are properly installed.
	
	

	
	
	

	4.1.13 Starter generator cables and v bands for proper torque and safeties.
	
	

	
	
	

	4.1.14 N1 control rod hardware is torqued and safeties.
	
	

	
	
	

	4.1.15 The N1 control tube boot is secure.
	
	

	
	
	

	4.1.16 Control tube has clearance throughout the entire range of operation.
	
	

	
	
	

	4.1.17 Tannis heater pads are installed. Pay particular attention to the FCU vent holes to ensure they were not covered by the pad.
	
	

	
	
	


	
	
	RII

INSPECTORS
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	4.1.18 Lock wire and cotter pins are properly installed.
	
	

	
	
	

	4.1.19 HUMMS sensors are installed.
	
	

	
	
	

	4.1.20 Ejectors and cowlings are properly installed.
	
	

	
	
	

	4.1.21 All checks in Pratt and Whitney “Checks after component repair or replacement” table have been complied with on all components that have been removed including power section.
	
	

	
	
	

	4.1.22 Leak check is complied with.
	
	

	
	
	

	4.1.23 SCC’s are complied with for all related components.
	
	

	
	
	

	4.2 Check inlets for FOD.
	
	

	
	
	

	4.3 Check for entry in the corrective action section of the log book for the maintenance task. At a minimum the log book entry shall contain the following: A description of the maintenance task. A reference to the acceptable data used. Aircraft TT. Date. Signature. A&P number.
	
	

	
	
	


Upon satisfactory completion of each inspection item, the RII Inspector shall initial the pertinent space as provided.  All RII Inspectors shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form the RII Inspector shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  
This form shall be attached to the aircraft W.O./Log Book. 
	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


I certify that I have used this RII card throughout the inspection process and have made an entry into the aircraft log book.
RII Inspectors Signature; ______________________________  
RII INSPECTION AUTHORIZATION CARD CERTIFICATE NUMBER; ________________________________


