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	300 HOUR / 12 MONTH INSPECTION
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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 412 MM-2 Chapter 5

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0301.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.5 Review Special Inspections and carry out applicable Inspections.
	Chp 5
	

	
	
	

	1.6 Examine all inspection windows and sight glasses for cracking, crazing, and discoloration. If any of these conditions are present, the part must be removed and replaced prior to returning helicopter for service.
	Chp 5
	

	
	
	

	A 0301.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0301.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	A 0301.4 GENERAL

	
	
	

	4.1 Remove all panels, fairings, and cowlings required to satisfactorily carry out the inspection.
	
	

	
	
	

	A 0301.5 FUSELAGE — CABIN

	
	
	

	5.1 Forward fuselage;
	Chp 53
	

	
	
	

	5.1.1 Cabin exterior structure for corrosion and damage.
	
	

	
	
	

	5.1.2 Cabin interior structure for corrosion and damage.
	
	

	
	
	

	5.1.3 Ensure all drain holes are open.
	
	

	
	
	

	5.1.4 All compartments for evidence of water entrapment and corrosion.
	
	

	
	
	

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.2 Doors and windows;
	Chp 52
	

	
	
	

	5.2.1 Crew doors structure for corrosion, damage, distortion, and positive locking mechanisms. Seals for tears and separations.
	
	

	
	
	

	5.2.2 Crew door emergency jettison mechanism for condition and security. Perform operational check.
	
	

	
	
	

	5.2.3 Passenger door structure for corrosion, damage, distortion, and positive locking mechanisms
	
	

	
	
	

	5.2.4 Nose, electrical, and equipment compartment access doors for corrosion, damage, distortion, and positive locking mechanisms.
	
	

	
	
	

	5.2.5 Passenger door window retainers and fillers for damage. Seals for adherence, tears, separations, and deterioration.
	
	

	
	
	

	5.2.6 If installed, inspect heated windshield for condition and proper installation.
	
	

	
	
	

	5.3 Landing gear assembly;
	Chp 32
	

	
	
	

	5.3.1 Landing gear skid shoes for excessive wear, cracks, damage, corrosion, and security of attachment.
	
	

	
	
	

	5.3.2 Aft cross tube support beam for cracks, damage, corrosion, and security of attachment.
	
	

	
	
	

	5.3.3 Retighten cross tube to skid tube saddle bolts.
	
	

	
	
	

	5.3.4 Torque forward and aft cross tube support fittings U-bolts to 80 to 100 inch-pounds.
	
	

	
	
	

	5.3.5 Torque check ground handling wheel attachment eyebolts on skid tubes 40 to 58 foot-pounds.
	
	

	NOTE:  Eyebolts that rotate prior to reaching 40 foot-pounds shall be removed and inspected for evidence of bending. No bending is permitted.
	

	5.3.6 If gross weight towing kit provisions are installed, inspect fitting assembly for condition and security. Torque check attachment bolts 160 to 190 inch-pounds If bolts are found loose, inspect for condition
	BHT-412-SI-58
	

	
	
	

	5.4 Underside of fuselage;
	Chp 53
	

	
	
	

	5.4.1 Fuselage structure for damage, corrosion, and working rivets.
	
	

	
	
	

	5.4.2 Exterior finish for condition and cleanliness.
	
	

	
	
	

	5.4.3 Evidence of excessive fluid leakage.
	
	

	
	
	

	5.4.4 Structure around landing gear for condition.
	
	

	
	
	

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.5 Forward crosstube support structure for working fasteners, cracks, corrosion, and excessive wear.
	
	

	
	
	

	5.6 Aft crosstube support structure for working fasteners,cracks, corrosion, and excessive wear.
	
	

	
	
	

	A 0301.6 ENGINE FUEL AND POWER CONTROLS

	
	
	

	6.1 Engine control linkages for looseness, lost motion, chafing, damage, and security of attachment.
	Chp 76
	

	
	
	

	6.2 Bellcranks, mounts, and jackshafts for looseness, damage, and security of attachment.
	Chp 76
	

	
	
	

	6.3 Check controls for smooth movement throughout full range of travel.
	Chp 76
	

	
	
	

	6.4 Engine fire detection systems for condition and security.
	Chp 26
	

	
	
	

	A 0301.7 CABIN ROOF

	
	
	

	7.1 Cabin roof structure.
	Chp 52/53
	

	7.1.1 Cabin roof structure, cowlings and fairings for damage, delamination, and general condition.
	
	

	
	
	

	7.1.2 Cabin roof and cowling/fairing mounted antennas for condition and security.
	
	

	
	
	

	7.2 Inspect the left side and right side engine air inlet cowlings for gaps between the lower surface of the cowling firewall and the mating horizontal engine firewall.
	Chp 71
ASB 412-10-140
	

	
	
	

	7.3 Inspect all exposed fuel lines and attachments for leakage, damage, and security.
	Chp 28 & 71
	

	
	
	

	A 0301.8 BAGGAGE COMPARTMENT

	
	
	

	8.1 Baggage compartment door for corrosion, damage, distortion, and positive locking mechanism.
	Chp 52
	

	
	
	

	8.2 Baggage compartment smoke detector for condition and security.
	Chp 26
	

	
	
	

	8.3 Inspect wire bundles and clamping for chafing, condition, and security.
	Chp 96
	

	
	
	

	A 0301.9 LUBRICATION

	
	
	

	9.1 Lubricate tail rotor crosshead bearing. Do not intermix grease types. Two shots every 50 hours.
	Table 12-3
Lubrication Chart
	

	
	
	

	9.2 Lubricate anti-torque flight control tube bearings. Do not intermix grease types. Purge until same grease appears.
	Table 12-3
Lubrication Chart
	

	NOTE:  Fittings not present on all helicopters
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	9.3 Lubricate tail rotor control lever (three places). Do not intermix grease types. Purge until same grease appears.
	Table 12-3
Lubrication Chart
	

	
	
	

	A 0301.10 POST INSPECTION

	
	
	

	10.1 Replace or close all applicable trim panels, fairings, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	10.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-412-FM-1
	

	
	
	

	10.3 Perform Functional Check Flight if required per Bell 412 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	10.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	

	10.5 Confirm all required RII have been completed and signed off.
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 412 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 412 CAMP – A 0301 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




