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	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 412 MM-2 Chapter 5

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0304.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.5 Review Special Inspections and carry out applicable Inspections.
	Chp 5
	

	
	
	

	1.6 Examine all inspection windows and sight glasses for cracking, crazing, and discoloration. If any of these conditions are present, the part must be removed and replaced prior to returning helicopter for service.
	Chp 5
	

	
	
	

	A 0304.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0304.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	A 0304.4 GENERAL

	
	
	

	4.1 Remove all panels, fairings, and cowlings required to satisfactorily carry out the inspection.
	
	

	
	
	

	A 0304.5 TAILBOOM

	
	
	

	5.1 Tailboom structure;
	Chapter 53
	

	
	
	

	5.1.1 Tailboom exterior structure for corrosion and damage.
	
	

	
	
	

	5.1.2 Tailboom interior structure for corrosion and damage.
	
	

	
	
	

	5.1.3 Inspect tailboom joints, splices, longerons, attach fittings, and attaching hardware for corrosion, damage, and cracks
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.1.4 Remove plug button at BS 99.00.
	ASB 412-90-49
	

	NOTE:  Paint fissures are common in the splice area, cracks will be evident by black powder emanating from cracked area, corrosion will leave evidence of white powder.
	
	

	5.1.5 Using a borescope or other suitable means, inspect inside of longeron paying particular attention to cracking and/or corrosion in area of splice.
	
	

	
	
	

	5.1.6 Report any cracks to Product Support Engineering.
	
	

	
	
	

	5.1.7 Install plug button with sealant (C-308).
	
	

	
	
	

	5.1.8 Ensure all drain holes are open.
	
	

	
	
	

	5.1.9 Vertical fin spar caps forward side and web from upper tailboom skin to approximately 4.0 inches (101.6 mm) below upper tailboom skin as follows: remove aft tailboom access door. Face aft and use bright light and small mirror to inspect area for cracks, especially near rivet holes.
	
	

	NOTE:  If necessary, clean area with cloth dampened with MEK (C-309) or equivalent. Ventilate area to prevent breathing fumes.
	

	5.2 Anti-torque controls;
	Chp 67
	

	
	
	

	5.2.1 Tail rotor control tubes between tail rotor pedals and tail rotor gearbox for corrosion, wear, and damage.
	
	

	
	
	

	5.2.2 Control tube bellcranks, supports, and attaching hardware for corrosion, security, wear, and damage.
	
	

	
	
	

	5.2.3 Tail rotor hydraulic actuator for leaks and security of attachment, damage, corrosion, and bearings and linkages for looseness.
	
	

	
	
	

	5.3 Aerodynamically actuated elevator;
	Chp 67
	

	
	
	

	5.3.1 Elevator control tube between forward support bracket and elevator horn for corrosion, wear, and damage.
	
	

	
	
	

	5.3.2 Control tube support and attaching hardware for security, corrosion, wear, and damage.
	
	

	
	
	

	5.3.3 Elevators and support structure for loose or missing rivets and cracks in the skin.
	
	

	
	
	

	5.3.4 Trailing edge tabs and tip caps for condition and security.
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	

	5.3.5 Functionally check operation of tube as follows;
	

	CAUTION

DO NOT RELEASE ELEVATOR AND ALLOW THE
SPRING TO DRIVE ELEVATOR BACK TO
ORIGINAL POSITION
	

	5.3.5.1 Move elevator to extreme nose down position and while holding allow elevator to slowly return to original position. Failure to return to original position, binding and/or lock-up are not acceptable.
	
	

	
	
	

	5.3.5.2 If any of these conditions exist, replace tube.
	
	

	
	
	

	5.3.6 Remove elevator control tube and measure spring breakout force for 90 to 100 pounds. Install elevator control tube.
	
	

	
	
	

	5.3.7 Functionally check elevator rigging for proper setting and travel.
	
	

	
	
	

	5.3.8 Inspect and measure elevator trailing edge tab for 16° ±1/4° angle down from upper surface of elevator.
	
	

	
	
	

	A 0304.6 LUBRICATION

	
	
	

	6.1 Lubricate tail rotor crosshead bearing. Do not intermix grease types. Two shots every 50 hours.
	Table 12-3
Lubrication Chart
	

	
	
	

	6.2 Lubricate anti-torque flight control tube bearings. Do not intermix grease types. Purge until same grease appears.
	Table 12-3
Lubrication Chart
	

	NOTE:  Fittings not present on all helicopters
	

	6.3 Lubricate tail rotor control lever (three places). Do not intermix grease types. Purge until same grease appears.
	Table 12-3
Lubrication Chart
	

	
	
	

	A 0304.7 POST INSPECTION

	
	
	

	7.1 Replace or close all applicable trim panels, fairings, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	7.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-412-FM-1
	

	
	
	

	7.3 Perform Functional Check Flight if required per Bell 412 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	7.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	

	7.5 Confirm all required RII have been completed and signed off.
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 412 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 412 CAMP – A 0304 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




