	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 412 MM-2 Chapter 5

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0306.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.5 Review Special Inspections and carry out applicable Inspections.
	Chp 5
	

	
	
	

	1.6 Examine all inspection windows and sight glasses for cracking, crazing, and discoloration. If any of these conditions are present, the part must be removed and replaced prior to returning helicopter for service.
	Chp 5
	

	
	
	

	A 0306.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0306.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	A 0306.4 GENERAL

	
	
	

	4.1 Remove all panels, fairings, and cowlings required to satisfactorily carry out the inspection.
	
	

	
	
	

	A 0306.5 MAIN ROTOR

	
	
	

	5.1 Main rotor controls;
	Chp 62
	

	
	
	

	5.1.1 Torque check swashplate outer ring through bolts to 165 to 175 inch-pounds.
	
	

	
	
	




	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.1.2 Torque check four hub and sleeve to rephasing lever attachment bolts to 24 to 34 foot-pounds for ½ inch bolts or to 160 to 200 inch-pounds for 3/8 inch bolts (if installed).
	
	

	
	
	

	5.1.3 Torque check four drive link to rephasing lever attachment bolts to 165 to 200 inch-pounds.
	
	

	
	
	

	5.1.4 Torque check swashplate support to mast plate bolts AN5H-6A to 130 to 140 inch-pounds.
	
	

	
	
	

	5.1.5 Purge lubricate Swashplate and collective lever trunnions and trunnion rod ends as follows: Rotate and simultaneously purge lubricate trunnions and trunnion rod ends to remove as much of the “old” lubricate as possible.
	Fig 12-3
Note 9
	

	
	
	

	5.2 Main rotor hub and blade assembly;
	Chp 62
	

	
	
	

	5.2.1 Main rotor blades upper and lower surfaces for condition of bond lines and doublers. Leading edge for erosion. Blade surfaces for corrosion, cracks, damage, and voids.
	
	

	
	
	

	5.2.2 Main rotor hub assembly for corrosion and damage.
	
	

	
	
	

	5.2.3 Blade retention bolts for condition and security.
	
	

	
	
	

	5.2.4 Torque check eight main rotor yoke assembly through bolt nuts to 70 to 80 foot-pounds.
	
	

	
	
	

	5.2.5 Ensure bolts EWB0420 are installed (16 places) for simple pendulum absorber bracket. Torque check bolts. Apply 29 to 33 foot-pounds in increasing torque direction.
	
	

	
	
	

	A 0306.6 MAIN ROTOR CONTROLS

	NOTE:  Disconnect pitch link upper rod ends from the pitch horns to determine main rotor control bearing wear.
	

	
	

	6.1 Inspect:
	

	
	

	6.1.1 Swashplate and support assembly for condition and security with special attention to gimbal ring attachment lugs.
	
	

	NOTE:  The presence of black oxide powder will require investigation to determine the cause.
	

	6.1.2 Gimble ring bearings, liners, and attaching hardware for excessive looseness and wear. Gimble ring bearing and attaching bolt axial or radial looseness shall not exceed 0.005 inch (0.127 mm) with no binding allowed.
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	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	6.1.3 Trunnion bearings and attaching hardware for excessive looseness and wear. Bearings shall not exceed 0.020-inch axial looseness
	
	

	
	
	

	6.1.4 Drive hub and rephasing levers for wear and bearing looseness
	
	

	
	
	

	6.1.5 Drive links’ spherical bearings for axial looseness. They shall not exceed 0.007 inch radial or 0.015 inch.
	
	

	
	
	

	6.1.6 Swashplate link non-elastomeric bearing for looseness. It shall not exceed 0.015-inch axial.
	
	

	
	
	

	6.1.7 Collective lever trunnion bearing for axial looseness. It shall not exceed 0.020 inch.
	
	

	
	
	

	6.1.8 Pitch link’s non-elastomeric bearing for looseness.  It shall not exceed 0.007-inch radial or 0.015-inch axial.
	
	

	
	
	

	A 0306.7 ELECTRICAL

	7.1 Emergency bus interconnect circuit breaker and diodes;
	Chp 96
	

	
	
	

	7.1.1 Inspect EMERG BUS INTC circuit breaker for wear. Operate circuit breaker manually and check by feel. Worn or loose circuit breaker is not acceptable. Close circuit breaker.
	
	

	
	
	

	7.1.2 Place all switches in OFF or NORM position and close all circuit breakers.
	
	

	
	
	

	7.1.3 Connect battery.
	
	

	
	
	

	7.1.4 Place BATTERY BUS 1 switch and BATTERY BUS 2 switch in the ON position. Position INV 1 and INV 2 switches in the ON position. Caution panel INVERTER 1 and INVERTER 2 segments should not be illuminated.
	
	

	
	
	

	7.1.5 Check emergency bus power by pressing the FIRE EXT PRESS TO TEST button momentarily. Observe both FIRE PULL handle warning lights illuminate.
	
	

	
	
	

	7.1.6 Position emergency bus switch to EMERG LOAD position. Check emergency bus power by pressing the FIRE EXT PRESS TO TEST button momentarily. Observe both FIRE PULL handles illuminate. Verify INVERTER 1 and INVERTER 2 segments are illuminated on the caution panel.
	
	

	NOTE:  S/N 33108 and subsequent — Check INVERTER 1 light segment on the caution panel is not illuminated and INVERTER 2 segment is illuminated.
	

	7.1.7 Position BATTERY BUS 1 and BATTERY BUS 2 switches off. Check emergency bus power by pressing FIRE EXT PRESS TO TEST button momentarily. Observe FIRE PULL handles illuminate.
	
	

	
	
	



	

	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	7.1.8 Position INVERTER 1 and INVERTER 2 switches OFF. Position emergency bus switch to NORMAL. Disconnect battery.
	
	

	
	
	

	7.1.9 Install screw, spacer, and washer in the emergency load switch guard if removed.
	
	

	
	
	

	7.2 Perform functional check of power diodes.
	Chp 96
	

	
	
	

	A 0306.8 LUBRICATION

	
	
	

	8.1 Lubricate tail rotor crosshead bearing. Do not intermix grease types. Two shots every 50 hours.
	Table 12-3
Lubrication Chart
	

	
	
	

	8.2 Lubricate anti-torque flight control tube bearings. Do not intermix grease types. Purge until same grease appears.
	Table 12-3
Lubrication Chart
	

	NOTE:  Fittings not present on all helicopters
	

	8.3 Lubricate tail rotor control lever (three places). Do not intermix grease types. Purge until same grease appears.
	Table 12-3
Lubrication Chart
	

	
	
	

	A 0306.9 POST INSPECTION

	9.1 Replace or close all applicable trim panels, fairings, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	9.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-412-FM-1
	

	
	
	

	9.3 Perform Functional Check Flight if required per Bell 412 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	9.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	

	9.5 Confirm all required RII have been completed and signed off.
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 412 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 412 CAMP – A 0306 – 300 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




