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	2
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	SECTION:
	
	A 0603 – AIRFRAME INSPECTION PROGRAM

	TYPE:
	
	600 HOUR / 12 MONTH INSPECTION

	NOTE:
	
	



	Registration No.:
	N
	Start
	
	Aircraft Start Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Start Total Cycles:
	


Reference:  BHT 412 MM-2 Chapter 5

	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	A 0603.1 GENERAL

	
	
	

	1.1 Logbook review for recorded discrepancies. Correct discrepancies on installed equipment.
	
	

	
	
	

	1.2 Ensure all applicable and required Special Inspections, Alert Service Bulletins (ASB’s), Engine Service Bulletins, and Airworthiness Directives (AD’s) are accomplished.
	
	

	
	
	

	1.3 Replace all life limited components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.4 Overhaul all components that have completed published operating limits.
	Bell 412 MP
	

	
	
	

	1.5 Review Special Inspections and carry out applicable Inspections.
	Chp 5
	

	
	
	

	1.6 Examine all inspection windows and sight glasses for cracking, crazing, and discoloration. If any of these conditions are present, the part must be removed and replaced prior to returning helicopter for service.
	Chp 5
	

	
	
	

	A 0603.2 PLACARDS AND MARKINGS

	
	
	

	2.1 Examine the placards, decals, and markings. Make sure you can read them, they are applied correctly, and they are in agreement with the applicable configuration of your helicopter.
	Chapter 11
	

	A 0603.3 CORROSION CONTROL

	
	
	

	3.1 Perform corrosion inspection in accordance with the Corrosion Guide on any area’s access during this CAMP inspection.
	CSSD-PSE-87-001
	

	
	
	

	A 0603.4 GENERAL

	
	
	

	4.1 Remove all panels, fairings, and cowlings required to satisfactorily carry out the inspection.
	
	

	
	
	

	A 0603.5 HYDRAULIC

	
	
	

	5.1 Hydraulic system;
	Chp 29
	

	NOTE:  Hydraulic filter elements 205-076-034-003 are non-cleanable. It is recommended they be replaced every 600 hours or 12 months. Filter elements 205-076-034-007 are cleanable. The -003 and -007 elements are interchangeable; intermixing of different element types is not permitted.
	
	

	5.1.1 Remove and inspect hydraulic filter elements.
	
	

	
	
	

	5.1.2 Discard or clean filter elements as applicable.
	
	

	
	
	



	
	
	MECHANIC’S
INITIALS

	MAINTENANCE ACTION
	REFERENCE
	

	
	
	

	
	
	

	5.1.3 Install hydraulic filter elements.
	
	

	
	
	

	5.1.4 Install 0 to 500 PSI (0 to 3447 kPa) gauge in quick disconnect at rotor brake caliper. Slowly pull rotor brake handle through travel. Cylinder should generate 240 to 260 PSI at any handle velocity and shall maintain 150 PSI minimum in over center position for 3 minutes. Adjust as necessary.
	Chp 63
	

	
	
	

	5.1.5 Inspect hydraulic system filler caps for proper functioning and sealing. Make sure the sealing O-rings within the filler caps are in good condition. Repair or replace the filler caps or replace sealing O-rings as required.
	
	

	
	
	

	5.1.6 Inspect brake linings for wear (minimum thickness 0.150 inch (3.81 mm)).
	
	

	
	
	

	A 0603.6 POST INSPECTION

	
	
	

	6.1 Replace or close all applicable trim panels, fairings, covers, access and inspection doors/covers as necessary.
	
	

	
	
	

	6.2 Complete a ground run at 100% NR to check for leaks and confirm system operation.
	BHT-412-FM-1
	

	
	
	

	6.3 Perform Functional Check Flight if required per Bell 412 Maintenance Manual or RFM as appropriate.
	
	

	
	
	

	6.4 Make an entry in the appropriate logbook (refer to the following page for wording of approval for return to service).
	
	

	
	
	

	6.5 Confirm all required RII have been completed and signed off.
	
	

	
	
	



Upon satisfactory completion of each inspection item, the mechanic shall initial the pertinent space as provided.  All mechanics shall sign and initial, in the space provided, at the end of the form.

At the completion of each inspection form, an A&P mechanic shall check the entire form for completion and then enter his/her signature, certificate type and number, and date in the space provided at the end of the form.  The same individual is also responsible for making the logbook entry shown at the conclusion of this inspection.

I certify that I have inspected and/or completed all the items initialed by me in accordance with Maritime Helicopters’ Bell 412 Continuous Airworthiness Maintenance Program and found them to be in an airworthy condition except as may be noted in the Aircraft Logbook.

	
	
	

	INITIALS
	SIGNATURE
	CERTIFICATE TYPE & NUMBER

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	



I have reviewed this inspection form to verify that all items have been completed and have made an entry in the Aircraft Log Book.

I certify that this aircraft has been inspected in accordance with Maritime Helicopters’ Bell 412 CAMP – A 0603 – 600 Hour / 12 Month Inspection and was determined to be in an airworthy condition.

	Registration No.:
	N
	End
	
	Aircraft Ending Total Time:
	

	Aircraft S/N:
	
	Date:
	
	Aircraft Ending Total Cycles:
	



	Signature:
	
	
	Certificate Type & No:
	




